(kicad_pcb (version 20171130) (host pcbnew "(5.1.2-1)-1")
  (general
    (thickness 1.6)
    (drawings 30)
    (tracks 251)
    (zones 0)
    (modules 5)
    (nets 24)
  )
  (page USLetter)
  (title_block
    (title BlueGeckoBreakout)
    (date 2019-05-09)
    (rev 1)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.6)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.16)
    (mod_text_size 0.9 0.9)
    (mod_text_width 0.16)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/"))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad5)")
  (net 2 "Net-(J1-Pad6)")
  (net 3 "Net-(J1-Pad7)")
  (net 4 "Net-(J1-Pad8)")
  (net 5 "Net-(J1-Pad9)")
  (net 6 "Net-(J1-Pad12)")
  (net 7 "Net-(J2-Pad12)")
  (net 8 "Net-(J2-Pad11)")
  (net 9 "Net-(J2-Pad10)")
  (net 10 "Net-(J2-Pad9)")
  (net 11 "Net-(J2-Pad8)")
  (net 12 "Net-(J2-Pad7)")
  (net 13 "Net-(J2-Pad6)")
  (net 14 "Net-(J2-Pad5)")
  (net 15 "Net-(J2-Pad4)")
  (net 16 "Net-(J2-Pad3)")
  (net 17 "Net-(J2-Pad2)")
  (net 18 GND)
  (net 19 VDD)
  (net 20 PF1)
  (net 21 PF0)
  (net 22 PF2)
  (net 23 PF3)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J2-Pad9)")
    (add_net PF0)
    (add_net PF1)
    (add_net PF2)
    (add_net PF3)
  )
  (net_class VDD ""
    (clearance 0.3)
    (trace_width 0.5)
    (via_dia 1)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net VDD)
  )
  (module BGM113Breakout:BGM113 (layer F.Cu) (tedit 5D1D5399)
    (at 140.97 95.504)
    (attr smd)
    (fp_text reference U1 (at 3.048 9.144) (layer F.SilkS))
    (fp_text value BGM113 (at 7.874 -5.715 180) (layer F.SilkS))
    (pad 24 smd oval (at 2 6.95 90) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J2-Pad3)") (clearance 0.1524))
    (pad 23 smd oval (at 1.2 6.95 90) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (clearance 0.1524))
    (pad 22 smd oval (at 0.4 6.95 90) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J2-Pad2)") (clearance 0.1524))
    (pad 21 smd oval (at -0.4 6.95 90) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad12)") (clearance 0.1524))
    (pad 20 smd oval (at -1.2 6.95 90) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 23 PF3) (clearance 0.1524))
    (pad 19 smd oval (at -2 6.95 90) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 22 PF2) (clearance 0.1524))
    (pad 36 smd oval (at 3.675 -2.4) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 18 GND) (clearance 0.1524))
    (pad 35 smd oval (at 3.675 -1.6) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (clearance 0.1524))
    (pad 28 smd oval (at 3.675 4) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J2-Pad6)") (clearance 0.1524))
    (pad 26 smd oval (at 3.675 5.6) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J2-Pad4)") (clearance 0.1524))
    (pad 31 smd oval (at 3.675 1.6) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J2-Pad9)") (clearance 0.1524))
    (pad 29 smd oval (at 3.675 3.2) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J2-Pad7)") (clearance 0.1524))
    (pad 30 smd oval (at 3.675 2.4) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J2-Pad8)") (clearance 0.1524))
    (pad 25 smd oval (at 3.675 6.4) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 18 GND) (clearance 0.1524))
    (pad 34 smd oval (at 3.675 -0.8) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J2-Pad12)") (clearance 0.1524))
    (pad 27 smd oval (at 3.675 4.8) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J2-Pad5)") (clearance 0.1524))
    (pad 33 smd oval (at 3.675 0) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J2-Pad11)") (clearance 0.1524))
    (pad 32 smd oval (at 3.675 0.8) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J2-Pad10)") (clearance 0.1524))
    (pad 18 smd oval (at -3.675 6.4) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 18 GND) (clearance 0.1524))
    (pad 17 smd oval (at -3.675 5.6) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 19 VDD) (clearance 0.1524))
    (pad 16 smd oval (at -3.675 4.8) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (clearance 0.1524))
    (pad 15 smd oval (at -3.675 4) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad9)") (clearance 0.1524))
    (pad 14 smd oval (at -3.675 3.2) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad8)") (clearance 0.1524))
    (pad 13 smd oval (at -3.675 2.4) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad7)") (clearance 0.1524))
    (pad 12 smd oval (at -3.675 1.6) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad6)") (clearance 0.1524))
    (pad 11 smd oval (at -3.675 0.8) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad5)") (clearance 0.1524))
    (pad 10 smd oval (at -3.675 0) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 21 PF0) (clearance 0.1524))
    (pad 9 smd oval (at -3.675 -0.8) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 20 PF1) (clearance 0.1524))
    (pad 8 smd oval (at -3.675 -1.6) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 19 VDD) (clearance 0.1524))
    (pad 7 smd oval (at -3.675 -2.4) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 18 GND) (clearance 0.1524))
    (pad 6 smd oval (at -3.675 -3.2) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 18 GND) (clearance 0.1524))
    (pad 5 smd oval (at -3.675 -4) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 18 GND) (clearance 0.1524))
    (pad 4 smd oval (at -3.675 -4.8) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 18 GND) (clearance 0.1524))
    (pad 3 smd oval (at -3.675 -5.6) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 18 GND) (clearance 0.1524))
    (pad 2 smd oval (at -3.675 -6.4) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 18 GND) (clearance 0.1524))
    (pad 1 smd oval (at -3.675 -7.2) (size 2 0.5) (layers F.Cu F.Paste F.Mask)
      (net 18 GND) (clearance 0.1524))
    (model "${KIPRJMOD}/User Library-BGM113.step"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical_SMD (layer F.Cu) (tedit 59FED6E3)
    (at 141.052 120.396)
    (descr "surface-mounted straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x05 1.27mm double row")
    (attr smd)
    (fp_text reference J3 (at -4.146 3.302) (layer F.SilkS) hide)
    (fp_text value Conn_ARM_JTAG_SWD_10 (at 0 4.235) (layer F.Fab) hide)
    (fp_text user %R (at -2.368 -4.826 180) (layer F.Fab) hide)
    (pad 10 smd rect (at 1.95 2.54) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J2-Pad12)"))
    (pad 9 smd rect (at -1.95 2.54) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 8 smd rect (at 1.95 1.27) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 23 PF3))
    (pad 7 smd rect (at -1.95 1.27) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 1.95 0) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 22 PF2))
    (pad 5 smd rect (at -1.95 0) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 4 smd rect (at 1.95 -1.27) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 21 PF0))
    (pad 3 smd rect (at -1.95 -1.27) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 18 GND))
    (pad 2 smd rect (at 1.95 -2.54) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 20 PF1))
    (pad 1 smd rect (at -1.95 -2.54) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 19 VDD))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 133.1325 90.424 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 1.8145 1.778) (layer F.SilkS))
    (fp_text value 10uf (at 3.3385 -0.762) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 18 GND))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 19 VDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x12_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 132.08 93.98)
    (descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x12 2.54mm single row")
    (fp_text reference J1 (at 0 29.972) (layer F.SilkS))
    (fp_text value Conn_01x12_Male (at 0 30.27) (layer F.Fab) hide)
    (fp_text user %R (at 0 13.97 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 VDD))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 PF1))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 PF0))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 PF2))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 PF3))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad12)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x12_P2.54mm_Vertical.wrl
      (offset (xyz 0 0 -2))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -180 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x12_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 149.86 121.92 180)
    (descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x12 2.54mm single row")
    (fp_text reference J2 (at 0 -2.032) (layer F.SilkS))
    (fp_text value Conn_01x12_Male (at -10.16 30.27) (layer F.Fab) hide)
    (fp_text user %R (at 0 13.97 90) (layer F.Fab))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad12)"))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad11)"))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad10)"))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad9)"))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x12_P2.54mm_Vertical.wrl
      (offset (xyz 0 0 -2))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -180 0))
    )
  )
  (gr_text "BGM113 Breakout V1.2" (at 134.112 101.6 90) (layer B.SilkS))
  (gr_text JTAG (at 140.97 116.459) (layer F.SilkS))
  (gr_text PC10 (at 148.463 106.68) (layer F.SilkS))
  (gr_text RES (at 147.193 93.98) (layer F.SilkS))
  (gr_text PD13 (at 147.955 96.52 90) (layer F.SilkS))
  (gr_text PD14 (at 146.558 99.06 90) (layer F.SilkS))
  (gr_text PF3 (at 148.463 101.6) (layer F.SilkS))
  (gr_text PF2 (at 148.463 104.14) (layer F.SilkS))
  (gr_text PC11 (at 148.463 109.22) (layer F.SilkS))
  (gr_text PA0 (at 148.463 111.76) (layer F.SilkS))
  (gr_text PD15 (at 148.463 114.3) (layer F.SilkS))
  (gr_text PD15 (at 148.463 116.84) (layer F.SilkS))
  (gr_text PC10 (at 148.463 119.38) (layer F.SilkS))
  (gr_text GND (at 147.193 121.92) (layer F.SilkS))
  (gr_line (start 130.048 124.714) (end 130.048 87.63) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 151.892 124.714) (end 130.048 124.714) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 151.892 87.63) (end 151.892 124.714) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 130.048 87.63) (end 151.892 87.63) (layer Edge.Cuts) (width 0.05))
  (gr_text PC11 (at 133.477 121.92) (layer F.SilkS))
  (gr_text PF3 (at 133.477 119.38) (layer F.SilkS))
  (gr_text PF2 (at 133.477 116.84) (layer F.SilkS))
  (gr_text PB11 (at 133.477 114.3) (layer F.SilkS))
  (gr_text PB12 (at 133.477 111.76) (layer F.SilkS))
  (gr_text PA1 (at 133.477 106.68) (layer F.SilkS))
  (gr_text PB13 (at 133.477 109.22) (layer F.SilkS))
  (gr_text PD13 (at 134.493 102.489 270) (layer F.SilkS))
  (gr_text PF0 (at 133.477 101.6) (layer F.SilkS))
  (gr_text PF1 (at 133.477 99.06) (layer F.SilkS))
  (gr_text VDD (at 134.747 96.52) (layer F.SilkS))
  (gr_text GND (at 134.747 93.98) (layer F.SilkS))
  (zone (net 18) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 130.302 87.884) (xy 151.638 87.884) (xy 151.638 124.46) (xy 130.302 124.46)
      )
    )
  )
  (zone (net 18) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 130.302 87.884) (xy 151.638 87.884) (xy 151.638 124.46) (xy 130.302 124.46)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.208 87.884) (xy 140.208 91.948) (xy 151.638 91.948) (xy 151.638 87.884)
      )
    )
  )
)
