(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 12)
    (no_connects 0)
    (area 143.566667 80.95 186.675001 103.241242)
    (thickness 1.6)
    (drawings 18)
    (tracks 26)
    (zones 0)
    (modules 11)
    (nets 10)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.1)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.1)
    (pcb_text_size 1 1)
    (mod_edge_width 0.1)
    (mod_text_size 1 1)
    (mod_text_width 0.1)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(P1-Pad1)")
  (net 2 "Net-(P2-Pad1)")
  (net 3 "Net-(P3-Pad1)")
  (net 4 "Net-(P4-Pad1)")
  (net 5 "Net-(P5-Pad1)")
  (net 6 "Net-(P6-Pad1)")
  (net 7 "Net-(P7-Pad1)")
  (net 8 "Net-(P8-Pad1)")
  (net 9 GND)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.3)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P6-Pad1)")
    (add_net "Net-(P7-Pad1)")
    (add_net "Net-(P8-Pad1)")
  )
  (module Pot_Bourns-PTD90-double-quad (layer F.Cu) (tedit 58E2ABE8)
    (at 171.4 93.2 180)
    (descr "Potentiometer, double, dual,  Alps, RK97, single,")
    (tags "Potentiometer, double, dual, Alps, RK16, single, RevA, 30 July 2010,")
    (fp_text reference RV2 (at -2.54 0 180) (layer F.SilkS) hide)
    (fp_text value POT_Dual (at 2.776 -0.3 270) (layer F.SilkS) hide)
    (pad 6 thru_hole circle (at 7.5 2.5 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 4 "Net-(P4-Pad1)"))
    (pad 3 thru_hole circle (at 5 2.5 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 3 "Net-(P3-Pad1)"))
    (pad 4 thru_hole circle (at 7.5 -2.5 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 9 GND))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 7 "Net-(P7-Pad1)"))
    (pad 5 thru_hole circle (at 7.5 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 8 "Net-(P8-Pad1)"))
    (pad 1 thru_hole circle (at 5 -2.5 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 9 GND))
  )
  (module Spino:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58DCADF8)
    (at 166.8 87.2 180)
    (fp_text reference P3 (at 0 2.54 180) (layer F.SilkS) hide)
    (fp_text value "IN 3" (at 0 -2.54 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask B.SilkS)
      (net 3 "Net-(P3-Pad1)"))
  )
  (module Spino:Pot_Bourns-PTD90-double-quad (layer F.Cu) (tedit 58DBFC87)
    (at 163.9 93.2 180)
    (descr "Potentiometer, double, dual,  Alps, RK97, single,")
    (tags "Potentiometer, double, dual, Alps, RK16, single, RevA, 30 July 2010,")
    (fp_text reference RV1 (at -2.54 0 180) (layer F.SilkS) hide)
    (fp_text value POT_Dual (at 2.776 -0.3 270) (layer F.SilkS) hide)
    (pad 6 thru_hole circle (at 7.5 2.5 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 2 "Net-(P2-Pad1)"))
    (pad 3 thru_hole circle (at 5 2.5 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 1 "Net-(P1-Pad1)"))
    (pad 4 thru_hole circle (at 7.5 -2.5 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 9 GND))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 5 "Net-(P5-Pad1)"))
    (pad 5 thru_hole circle (at 7.5 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 6 "Net-(P6-Pad1)"))
    (pad 1 thru_hole circle (at 5 -2.5 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 9 GND))
  )
  (module Spino:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58D678DA)
    (at 160 87.2 180)
    (fp_text reference P1 (at 0 2.54 180) (layer F.SilkS) hide)
    (fp_text value "IN 1" (at 0 -2.54 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask B.SilkS)
      (net 1 "Net-(P1-Pad1)"))
  )
  (module Spino:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58D678DA)
    (at 156.6 87.2 180)
    (fp_text reference P2 (at 0 2.54 180) (layer F.SilkS) hide)
    (fp_text value "IN 2" (at 0 -2.54 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask B.SilkS)
      (net 2 "Net-(P2-Pad1)"))
  )
  (module Spino:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58D678DA)
    (at 163.4 87.2 180)
    (fp_text reference P4 (at 0 2.54 180) (layer F.SilkS) hide)
    (fp_text value "IN 4" (at 0 -2.54 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask B.SilkS)
      (net 4 "Net-(P4-Pad1)"))
  )
  (module Spino:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58D678DA)
    (at 153 95 180)
    (fp_text reference P5 (at 0 2.54 180) (layer F.SilkS) hide)
    (fp_text value "OUT 1" (at 0 -2.54 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask B.SilkS)
      (net 5 "Net-(P5-Pad1)"))
  )
  (module Spino:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58D678DA)
    (at 153 98 180)
    (fp_text reference P6 (at 0 2.54 180) (layer F.SilkS) hide)
    (fp_text value "OUT 2" (at 0 -2.54 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask B.SilkS)
      (net 6 "Net-(P6-Pad1)"))
  )
  (module Spino:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58D678DA)
    (at 153 89 180)
    (fp_text reference P7 (at 0 2.54 180) (layer F.SilkS) hide)
    (fp_text value "OUT 3" (at 0 -2.54 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask B.SilkS)
      (net 7 "Net-(P7-Pad1)"))
  )
  (module Spino:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58D678DA)
    (at 153 92 180)
    (fp_text reference P8 (at 0 2.54 180) (layer F.SilkS) hide)
    (fp_text value "OUT 4" (at 0 -2.54 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask B.SilkS)
      (net 8 "Net-(P8-Pad1)"))
  )
  (module Spino:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 58D678DA)
    (at 157.6 99.2 180)
    (fp_text reference P9 (at 0 2.54 180) (layer F.SilkS) hide)
    (fp_text value GND (at 0 -2.54 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask B.SilkS)
      (net 9 GND))
  )
  (dimension 18.6 (width 0.1) (layer Cmts.User)
    (gr_text "18.600 mm" (at 161.1 81.7) (layer Cmts.User))
    (feature1 (pts (xy 170.4 84) (xy 170.4 81)))
    (feature2 (pts (xy 151.8 84) (xy 151.8 81)))
    (crossbar (pts (xy 151.8 82.4) (xy 170.4 82.4)))
    (arrow1a (pts (xy 170.4 82.4) (xy 169.273496 82.986421)))
    (arrow1b (pts (xy 170.4 82.4) (xy 169.273496 81.813579)))
    (arrow2a (pts (xy 151.8 82.4) (xy 152.926504 82.986421)))
    (arrow2b (pts (xy 151.8 82.4) (xy 152.926504 81.813579)))
  )
  (dimension 14.4 (width 0.1) (layer Cmts.User)
    (gr_text "14.400 mm" (at 147.9 93.2 270) (layer Cmts.User))
    (feature1 (pts (xy 150 100.4) (xy 147.2 100.4)))
    (feature2 (pts (xy 150 86) (xy 147.2 86)))
    (crossbar (pts (xy 148.6 86) (xy 148.6 100.4)))
    (arrow1a (pts (xy 148.6 100.4) (xy 148.013579 99.273496)))
    (arrow1b (pts (xy 148.6 100.4) (xy 149.186421 99.273496)))
    (arrow2a (pts (xy 148.6 86) (xy 148.013579 87.126504)))
    (arrow2b (pts (xy 148.6 86) (xy 149.186421 87.126504)))
  )
  (gr_line (start 170.4 100.4) (end 170.4 86) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151.8 100.4) (end 170.4 100.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151.8 86) (end 170.4 86) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151.8 100.4) (end 151.8 86) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text spaitz@gmail.com (at 164.5 99.3 180) (layer F.SilkS))
  (gr_text "PTD904-20K\n" (at 161.7 93.1 90) (layer F.SilkS))
  (gr_text spaitz@gmail.com (at 169 94 90) (layer B.SilkS))
  (gr_text BK (at 159.8 99.3) (layer B.SilkS))
  (gr_text GRY (at 153.5 99.6) (layer B.SilkS))
  (gr_text PR (at 154.9 94.7) (layer B.SilkS))
  (gr_text BL (at 154.75 92) (layer B.SilkS))
  (gr_text GRN (at 153.5 87.4) (layer B.SilkS))
  (gr_text YE (at 156.6 88.8) (layer B.SilkS))
  (gr_text OR (at 160 88.8) (layer B.SilkS))
  (gr_text RE (at 163.5 88.8) (layer B.SilkS))
  (gr_text BR (at 168.8 87.2) (layer B.SilkS))
  (zone (net 9) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.9 86.1) (xy 170.3 86.1) (xy 170.3 100.3) (xy 151.9 100.3)
      )
    )
  )
)
