<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="50.8" x2="0" y2="2.54" width="0.2032" layer="20"/>
<wire x1="0" y1="2.54" x2="2.54" y2="0" width="0.2032" layer="20"/>
<wire x1="2.54" y1="0" x2="57.15" y2="0" width="0.2032" layer="20"/>
<wire x1="57.15" y1="0" x2="57.15" y2="2.54" width="0.2032" layer="20"/>
<wire x1="57.15" y1="2.54" x2="59.69" y2="5.08" width="0.2032" layer="20"/>
<wire x1="59.69" y1="5.08" x2="59.69" y2="35.56" width="0.2032" layer="20"/>
<wire x1="59.69" y1="35.56" x2="62.23" y2="35.56" width="0.2032" layer="20"/>
<wire x1="62.23" y1="35.56" x2="64.77" y2="38.1" width="0.2032" layer="20"/>
<wire x1="64.77" y1="38.1" x2="64.77" y2="50.8" width="0.2032" layer="20"/>
<wire x1="64.77" y1="50.8" x2="62.23" y2="53.34" width="0.2032" layer="20"/>
<wire x1="62.23" y1="53.34" x2="2.54" y2="53.34" width="0.2032" layer="20"/>
<wire x1="2.54" y1="53.34" x2="0" y2="50.8" width="0.2032" layer="20"/>
<text>GND</text>
<text>1</text>
<text>5</text>
<text>3.3</text>
<text>RAW</text>
<text>RST</text>
<text>GND</text>
<text>REF</text>
<text>GND</text>
<text>A0</text>
<text>A1</text>
<text>A2</text>
<text>A3</text>
<text>A4</text>
<text>A5</text>
<text>D5</text>
<text>D4</text>
<text>D3</text>
<text>D2</text>
<text>D1</text>
<text>D0</text>
<text>D11</text>
<text>D10</text>
<text>D9</text>
<text>D8</text>
<text>D7</text>
<text>D6</text>
<text>D12</text>
<text>D13</text>
<text>D1</text>
<text>D0</text>
<text>5V</text>
<text>GND</text>
<hole x="57.15" y="7.62" drill="3.2"/>
<hole x="6.35" y="50.8" drill="3.2"/>
<text>D9</text>
<text>D10</text>
<text>INT1</text>
<text>INT0</text>
<text>CANL</text>
<text>CANH</text>
<text>PetraSoft</text>
<text>CAN Shield V.1</text>
<text>RESET</text>
</plain>
<libraries>
<library name="pinhead">
<packages>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="1X06">
</package>
<package name="AXIAL-0.3">
</package>
<package name="1X08">
</package>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="CAP-PTH-SMALL2">
</package>
<package name="CREATIVE_COMMONS">
</package>
</packages>
</library>
<library name="can">
<description>CAN Components</description>
<packages>
<package name="DIL18">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;&lt;p&gt;
package type P</description>
</package>
<package name="DIL08">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03">
</package>
<package name="DB9_MALE">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="1X02">
</package>
<package name="1X01">
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RESONATOR-PTH">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALL">
</package>
</packages>
</library>
<library name="con-phoenix-350">
<description>&lt;b&gt;Phoenix Connectors&lt;/b&gt; Grid 3.50 mm&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1751248">
<description>&lt;b&gt;MKDS 1/ 2-3,5&lt;/b&gt; Printklemme&lt;p&gt;
Nennstrom: 10 A&lt;br&gt;
Bemessungsspannung: 160 V&lt;br&gt;
Raster: 3,5 mm&lt;br&gt;
Polzahl: 2&lt;br&gt;
Montageart: Löten&lt;br&gt;
Anschlussart: Schraubanschluss&lt;br&gt;
Anschlussrichtung vom Leiter zur Platine: 0°&lt;br&gt;
Source: http://eshop.phoenixcontact.com .. 1751248.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ICSP" library="pinhead" package="2X03" value="ICSP">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun" package="AXIAL-0.3" value="1k">
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun" package="AXIAL-0.3" value="1k">
<attribute name="VALUE"/>
</element>
<element name="RX" library="SparkFun" package="LED3MM" value=""/>
<element name="TX" library="SparkFun" package="LED3MM" value=""/>
<element name="JP1" library="SparkFun" package="1X06" value="Power"/>
<element name="JP3" library="SparkFun" package="1X06" value="Analog"/>
<element name="JP4" library="SparkFun" package="1X08" value="Digital2"/>
<element name="JP2" library="SparkFun" package="1X08" value="Digital1"/>
<element name="SL5" library="SparkFun" package="1X08" value="">
<attribute name="VALUE"/>
</element>
<element name="SL6" library="SparkFun" package="1X08" value="">
<attribute name="VALUE"/>
</element>
<element name="SL7" library="SparkFun" package="1X06" value="">
<attribute name="VALUE"/>
</element>
<element name="SL8" library="SparkFun" package="1X06" value="">
<attribute name="VALUE"/>
</element>
<element name="S2" library="SparkFun" package="TACTILE-PTH" value=""/>
<element name="R4" library="SparkFun" package="AXIAL-0.3" value="10K">
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun" package="CAP-PTH-SMALL2" value="0.1uF">
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun" package="CAP-PTH-SMALL2" value="0.1uF">
<attribute name="VALUE"/>
</element>
<element name="JP7" library="SparkFun" package="1X06" value="BlueSMiRF"/>
<element name="U$2" library="SparkFun" package="CREATIVE_COMMONS" value="CREATIVE_COMMONS"/>
<element name="IC1" library="can" package="DIL18" value="MCP2515">
<attribute name="VALUE"/>
</element>
<element name="IC2" library="can" package="DIL08" value="MCP2551">
<attribute name="VALUE"/>
</element>
<element name="INT" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="CS" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="SparkFun-Connectors" package="DB9_MALE" value="">
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun" package="AXIAL-0.3" value="120">
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun" package="AXIAL-0.3" value="10k">
<attribute name="VALUE"/>
</element>
<element name="Y1" library="SparkFun-FreqCtrl" package="RESONATOR-PTH" value="RESONATORPTH"/>
<element name="C3" library="SparkFun-Passives" package="CAP-PTH-SMALL" value="">
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Passives" package="CAP-PTH-SMALL" value="">
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun" package="AXIAL-0.3" value="Rs">
<attribute name="VALUE"/>
</element>
<element name="X2" library="con-phoenix-350" package="1751248" value="1751248">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="TERM" library="SparkFun-Connectors" package="1X02" value=""/>
<element name="JP5" library="SparkFun-Connectors" package="1X01" value="M01PTH"/>
<element name="JP6" library="SparkFun-Connectors" package="1X01" value="M01PTH"/>
<element name="JP8" library="SparkFun-Connectors" package="1X01" value="M01PTH"/>
<element name="JP9" library="SparkFun-Connectors" package="1X01" value="M01PTH"/>
<element name="JP10" library="SparkFun-Connectors" package="1X01" value="M01PTH"/>
</elements>
<signals>
<signal name="GND">
<contactref element="SL6" pad="7"/>
<contactref element="JP4" pad="7"/>
<contactref element="SL8" pad="4"/>
<contactref element="JP1" pad="4"/>
<contactref element="SL8" pad="5"/>
<contactref element="JP1" pad="5"/>
<contactref element="S2" pad="1"/>
<contactref element="S2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="ICSP" pad="6"/>
<contactref element="JP7" pad="3"/>
<contactref element="IC1" pad="9"/>
<contactref element="IC2" pad="2"/>
<contactref element="Y1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="R7" pad="P$1"/>
<contactref element="X1" pad="3"/>
<contactref element="X1" pad="5"/>
<contactref element="X1" pad="8"/>
</signal>
<signal name="RX">
<contactref element="SL5" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP7" pad="4"/>
</signal>
<signal name="TX">
<contactref element="JP2" pad="2"/>
<contactref element="SL5" pad="2"/>
<contactref element="JP7" pad="5"/>
</signal>
<signal name="D2">
<contactref element="SL5" pad="3"/>
<contactref element="JP2" pad="3"/>
<contactref element="INT" pad="3"/>
</signal>
<signal name="D3">
<contactref element="JP2" pad="4"/>
<contactref element="SL5" pad="4"/>
<contactref element="INT" pad="1"/>
</signal>
<signal name="D4">
<contactref element="SL5" pad="5"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="D5">
<contactref element="JP2" pad="6"/>
<contactref element="SL5" pad="6"/>
</signal>
<signal name="D6">
<contactref element="SL5" pad="7"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="D7">
<contactref element="JP2" pad="8"/>
<contactref element="SL5" pad="8"/>
</signal>
<signal name="D8">
<contactref element="SL6" pad="1"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="D9">
<contactref element="JP4" pad="2"/>
<contactref element="SL6" pad="2"/>
<contactref element="CS" pad="3"/>
</signal>
<signal name="D10">
<contactref element="SL6" pad="3"/>
<contactref element="JP4" pad="3"/>
<contactref element="CS" pad="1"/>
</signal>
<signal name="D11">
<contactref element="JP4" pad="4"/>
<contactref element="SL6" pad="4"/>
</signal>
<signal name="D12">
<contactref element="SL6" pad="5"/>
<contactref element="JP4" pad="5"/>
</signal>
<signal name="D13">
<contactref element="JP4" pad="6"/>
<contactref element="SL6" pad="6"/>
</signal>
<signal name="AREF">
<contactref element="JP4" pad="8"/>
<contactref element="SL6" pad="8"/>
</signal>
<signal name="A3">
<contactref element="JP3" pad="3"/>
<contactref element="SL7" pad="3"/>
</signal>
<signal name="A4">
<contactref element="SL7" pad="2"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="3.3V">
<contactref element="SL8" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="RESET">
<contactref element="SL8" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="ICSP" pad="5"/>
<contactref element="S2" pad="3"/>
<contactref element="R4" pad="P$1"/>
<contactref element="S2" pad="4"/>
</signal>
<signal name="5V">
<contactref element="SL8" pad="3"/>
<contactref element="JP1" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="ICSP" pad="2"/>
<contactref element="JP7" pad="2"/>
<contactref element="R4" pad="P$2"/>
<contactref element="IC1" pad="18"/>
<contactref element="IC2" pad="3"/>
<contactref element="R3" pad="P$2"/>
<contactref element="R2" pad="P$2"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="VIN">
<contactref element="SL8" pad="6"/>
<contactref element="JP1" pad="6"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="A5">
<contactref element="SL7" pad="1"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="ICSP" pad="4"/>
<contactref element="IC1" pad="14"/>
</signal>
<signal name="MISO">
<contactref element="ICSP" pad="1"/>
<contactref element="IC1" pad="15"/>
</signal>
<signal name="SCK">
<contactref element="ICSP" pad="3"/>
<contactref element="IC1" pad="13"/>
</signal>
<signal name="A2">
<contactref element="SL7" pad="4"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="A1">
<contactref element="JP3" pad="5"/>
<contactref element="SL7" pad="5"/>
</signal>
<signal name="A0">
<contactref element="SL7" pad="6"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="CANL">
<contactref element="X2" pad="1"/>
<contactref element="X1" pad="2"/>
<contactref element="IC2" pad="6"/>
<contactref element="TERM" pad="1"/>
</signal>
<signal name="CANH">
<contactref element="IC2" pad="7"/>
<contactref element="R5" pad="P$1"/>
<contactref element="X2" pad="2"/>
<contactref element="X1" pad="7"/>
</signal>
<signal name="TXCAN">
<contactref element="IC1" pad="1"/>
<contactref element="IC2" pad="1"/>
<contactref element="TX" pad="K"/>
</signal>
<signal name="RXCAN">
<contactref element="IC1" pad="2"/>
<contactref element="IC2" pad="4"/>
<contactref element="RX" pad="K"/>
</signal>
<signal name="INT">
<contactref element="IC1" pad="12"/>
<contactref element="INT" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="IC1" pad="17"/>
<contactref element="R3" pad="P$1"/>
</signal>
<signal name="CS">
<contactref element="IC1" pad="16"/>
<contactref element="CS" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="R5" pad="P$2"/>
<contactref element="TERM" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="P$1"/>
<contactref element="RX" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="P$1"/>
<contactref element="TX" pad="A"/>
</signal>
<signal name="OSC1">
<contactref element="IC1" pad="8"/>
<contactref element="C3" pad="1"/>
<contactref element="Y1" pad="1"/>
</signal>
<signal name="OSC2">
<contactref element="IC1" pad="7"/>
<contactref element="C4" pad="1"/>
<contactref element="Y1" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="R7" pad="P$2"/>
<contactref element="IC2" pad="8"/>
</signal>
<signal name="TX0RTS">
<contactref element="IC1" pad="4"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="TX1RTS">
<contactref element="IC1" pad="5"/>
<contactref element="JP6" pad="1"/>
</signal>
<signal name="TX2RTS">
<contactref element="IC1" pad="6"/>
<contactref element="JP8" pad="1"/>
</signal>
<signal name="RX0BF">
<contactref element="IC1" pad="11"/>
<contactref element="JP9" pad="1"/>
</signal>
<signal name="RX1BF">
<contactref element="IC1" pad="10"/>
<contactref element="JP10" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
