(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 80)
    (no_connects 0)
    (area 105.45 54.65 186.65 154.9)
    (thickness 1.6)
    (drawings 22)
    (tracks 527)
    (zones 0)
    (modules 26)
    (nets 45)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.6 1.6)
    (pad_drill 0.8)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 107.95 57.15)
    (visible_elements 7FFED77F)
    (pcbplotparams
      (layerselection 0x000f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /TX_H)
  (net 2 /RX_H)
  (net 3 /WF_RST_H)
  (net 4 GND)
  (net 5 /X_STEP)
  (net 6 /Y_Step)
  (net 7 /Z_Step)
  (net 8 /X_Dir)
  (net 9 /Y_Dir)
  (net 10 /Z_Dir)
  (net 11 /WF_CE_H)
  (net 12 /RST/Abort)
  (net 13 /Cycle_Start/Resme)
  (net 14 +5VD)
  (net 15 +3.3VP)
  (net 16 /A_Dir)
  (net 17 /A_Step)
  (net 18 /RX_L)
  (net 19 /TX_L)
  (net 20 /WF_CHPD)
  (net 21 /WF_RST)
  (net 22 /Limit_X)
  (net 23 /Limit_Y)
  (net 24 /Limit_Z)
  (net 25 /Probe)
  (net 26 /Spindle_PWM)
  (net 27 /Feed_Hold)
  (net 28 /Splindle_ENA)
  (net 29 "Net-(J1-Pad14)")
  (net 30 "Net-(J1-Pad15)")
  (net 31 "Net-(J1-Pad16)")
  (net 32 "Net-(J1-Pad17)")
  (net 33 "Net-(SW1-Pad1)")
  (net 34 "Net-(SW1-Pad2)")
  (net 35 /WF_GPIO2)
  (net 36 /WF_GPIO0)
  (net 37 /Stepper_ENA/DIS)
  (net 38 "Net-(U4-Pad17)")
  (net 39 "Net-(U4-Pad18)")
  (net 40 /NA/Reservd)
  (net 41 "Net-(U4-Pad25)")
  (net 42 "Net-(U4-Pad26)")
  (net 43 VDD)
  (net 44 /A_RST)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /A_Dir)
    (add_net /A_RST)
    (add_net /A_Step)
    (add_net /Cycle_Start/Resme)
    (add_net /Feed_Hold)
    (add_net /Limit_X)
    (add_net /Limit_Y)
    (add_net /Limit_Z)
    (add_net /NA/Reservd)
    (add_net /Probe)
    (add_net /RST/Abort)
    (add_net /RX_H)
    (add_net /RX_L)
    (add_net /Spindle_PWM)
    (add_net /Splindle_ENA)
    (add_net /Stepper_ENA/DIS)
    (add_net /TX_H)
    (add_net /TX_L)
    (add_net /WF_CE_H)
    (add_net /WF_CHPD)
    (add_net /WF_GPIO0)
    (add_net /WF_GPIO2)
    (add_net /WF_RST)
    (add_net /WF_RST_H)
    (add_net /X_Dir)
    (add_net /X_STEP)
    (add_net /Y_Dir)
    (add_net /Y_Step)
    (add_net /Z_Dir)
    (add_net /Z_Step)
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(SW1-Pad1)")
    (add_net "Net-(SW1-Pad2)")
    (add_net "Net-(U4-Pad17)")
    (add_net "Net-(U4-Pad18)")
    (add_net "Net-(U4-Pad25)")
    (add_net "Net-(U4-Pad26)")
    (add_net VDD)
  )
  (net_class PWR ""
    (clearance 0.3)
    (trace_width 0.5)
    (via_dia 1)
    (via_drill 0.5)
    (uvia_dia 1)
    (uvia_drill 0.5)
    (add_net +3.3VP)
    (add_net +5VD)
    (add_net GND)
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58389CA5)
    (at 134.62 111.887 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at -0.127 2.032 180) (layer B.SilkS))
    (fp_text value R (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 21 /WF_RST))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 15 +3.3VP))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer B.Cu) (tedit 58389C55)
    (at 143.51 83.566 90)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C8 (at 4.191 0.254 180) (layer B.SilkS))
    (fp_text value C (at 0 -2.7 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 44 /A_RST))
    (pad 2 smd rect (at 2 0 90) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_1210_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58389C5F)
    (at 136.906 89.662 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 1.778 -2.032 180) (layer B.SilkS))
    (fp_text value R (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 /WF_RST_H))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 44 /A_RST))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:DB25FC (layer F.Cu) (tedit 583769E6)
    (at 166.37 104.902 270)
    (descr "Connecteur DB25 femelle couche")
    (tags "CONN DB25")
    (fp_text reference J1 (at 21.463 4.953 270) (layer F.SilkS))
    (fp_text value DB25 (at 0 -6.35 270) (layer F.Fab))
    (pad "" thru_hole circle (at 23.495 -1.27 270) (size 3.81 3.81) (drill 3.048) (layers *.Cu *.Mask F.SilkS))
    (pad "" thru_hole circle (at -23.495 -1.27 270) (size 3.81 3.81) (drill 3.048) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole rect (at -16.51 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 +5VD))
    (pad 2 thru_hole circle (at -13.716 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /X_Dir))
    (pad 3 thru_hole circle (at -11.049 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /X_STEP))
    (pad 4 thru_hole circle (at -8.255 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /Y_Dir))
    (pad 5 thru_hole circle (at -5.461 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /Y_Step))
    (pad 6 thru_hole circle (at -2.667 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /Z_Dir))
    (pad 7 thru_hole circle (at 0 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /Z_Step))
    (pad 8 thru_hole circle (at 2.794 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /A_Dir))
    (pad 9 thru_hole circle (at 5.588 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /A_Step))
    (pad 10 thru_hole circle (at 8.382 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /Probe))
    (pad 11 thru_hole circle (at 11.049 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /Limit_X))
    (pad 12 thru_hole circle (at 13.843 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /Limit_Y))
    (pad 13 thru_hole circle (at 16.637 1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /Limit_Z))
    (pad 14 thru_hole circle (at -14.9352 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(J1-Pad14)"))
    (pad 15 thru_hole circle (at -12.3952 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(J1-Pad15)"))
    (pad 16 thru_hole circle (at -9.6012 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(J1-Pad16)"))
    (pad 17 thru_hole circle (at -6.858 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(J1-Pad17)"))
    (pad 18 thru_hole circle (at -4.1148 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 19 thru_hole circle (at -1.3208 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 20 thru_hole circle (at 1.4224 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 21 thru_hole circle (at 4.1656 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 22 thru_hole circle (at 7.0104 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 23 thru_hole circle (at 9.7028 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 24 thru_hole circle (at 12.446 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 25 thru_hole circle (at 15.24 -1.27 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (model Connect.3dshapes/DB25FC.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ESP8266:ESP-01 (layer F.Cu) (tedit 58376A0B)
    (at 131.826 118.364 180)
    (descr "Module, ESP-8266, ESP-01, 8 pin")
    (tags "Module ESP-8266 ESP8266")
    (fp_text reference U1 (at -2.921 -0.127 270) (layer F.SilkS))
    (fp_text value ESP-01v090 (at 12.192 3.556 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /TX_L))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /WF_CHPD))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /WF_GPIO2))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /WF_RST))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 /WF_GPIO0))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 +3.3VP))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /RX_L))
  )
  (module Housings_DIP:DIP-32_W15.24mm_LongPads (layer F.Cu) (tedit 58376958)
    (at 139.954 81.534)
    (descr "32-lead dip package, row spacing 15.24 mm (600 mils), longer pads")
    (tags "dil dip 2.54 600")
    (fp_text reference U4 (at 8.001 -3.302) (layer F.SilkS))
    (fp_text value ARDUINO_NANO (at 7.62 19.05) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 /TX_H))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 /RX_H))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 44 /A_RST))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 /X_STEP))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 /Y_Step))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 /Z_Step))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 /X_Dir))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 /Y_Dir))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 /Z_Dir))
    (pad 11 thru_hole oval (at 0 25.4) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 37 /Stepper_ENA/DIS))
    (pad 12 thru_hole oval (at 0 27.94) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 22 /Limit_X))
    (pad 13 thru_hole oval (at 0 30.48) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 23 /Limit_Y))
    (pad 14 thru_hole oval (at 0 33.02) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 26 /Spindle_PWM))
    (pad 15 thru_hole oval (at 0 35.56) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 24 /Limit_Z))
    (pad 16 thru_hole oval (at 15.24 35.56) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 /WF_CE_H))
    (pad 17 thru_hole oval (at 15.24 33.02) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(U4-Pad17)"))
    (pad 18 thru_hole oval (at 15.24 30.48) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(U4-Pad18)"))
    (pad 19 thru_hole oval (at 15.24 27.94) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 /RST/Abort))
    (pad 20 thru_hole oval (at 15.24 25.4) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 27 /Feed_Hold))
    (pad 21 thru_hole oval (at 15.24 22.86) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 /Cycle_Start/Resme))
    (pad 22 thru_hole oval (at 15.24 20.32) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 28 /Splindle_ENA))
    (pad 23 thru_hole oval (at 15.24 17.78) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 40 /NA/Reservd))
    (pad 24 thru_hole oval (at 15.24 15.24) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 25 /Probe))
    (pad 25 thru_hole oval (at 15.24 12.7) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(U4-Pad25)"))
    (pad 26 thru_hole oval (at 15.24 10.16) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(U4-Pad26)"))
    (pad 27 thru_hole oval (at 15.24 7.62) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 +5VD))
    (pad 28 thru_hole oval (at 15.24 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 44 /A_RST))
    (pad 29 thru_hole oval (at 15.24 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 30 thru_hole oval (at 15.24 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 43 VDD))
    (model Housings_DIP.3dshapes/DIP-32_W15.24mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-14_W7.62mm (layer F.Cu) (tedit 58376A2A)
    (at 118.872 102.108 90)
    (descr "14-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U2 (at 8.382 15.113 90) (layer F.SilkS))
    (fp_text value QuadBidir5to3.3vstpdn (at 5.08 15.24 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 /RX_L))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 /TX_L))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 +3.3VP))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 20 /WF_CHPD))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 21 /WF_RST))
    (pad 7 thru_hole oval (at 10.16 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 /WF_RST_H))
    (pad 8 thru_hole oval (at 10.16 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 /WF_CE_H))
    (pad 9 thru_hole oval (at 10.16 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 10 thru_hole oval (at 10.16 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 +5VD))
    (pad 11 thru_hole oval (at 10.16 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 /RX_H))
    (pad 12 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 /TX_H))
    (model Housings_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer B.Cu) (tedit 58389CB5)
    (at 129.794 107.696 180)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C1 (at 0.127 2.286 180) (layer B.SilkS))
    (fp_text value C (at 0 -2.7 180) (layer B.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 15 +3.3VP))
    (pad 2 smd rect (at 2 0 180) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_1210_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer B.Cu) (tedit 581429C2)
    (at 127.762 81.28)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C2 (at 0 -2.54) (layer B.SilkS))
    (fp_text value C (at 0 -2.7) (layer B.Fab))
    (pad 1 smd rect (at -2 0) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 15 +3.3VP))
    (pad 2 smd rect (at 2 0) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_1210_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer B.Cu) (tedit 58389CF4)
    (at 128.016 136.525 90)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C3 (at 0.889 -2.921 180) (layer B.SilkS))
    (fp_text value C (at 0 -2.7 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 14 +5VD))
    (pad 2 smd rect (at 2 0 90) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_1210_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer B.Cu) (tedit 58389CDA)
    (at 161.29 86.36 270)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C4 (at 0 3.048 360) (layer B.SilkS))
    (fp_text value C (at 0 -2.7 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 2 0 270) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 14 +5VD))
    (model Capacitors_SMD.3dshapes/C_1210_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer B.Cu) (tedit 58389CC3)
    (at 125.476 99.314)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C5 (at -0.381 -2.54) (layer B.SilkS))
    (fp_text value C (at 0 -2.7) (layer B.Fab))
    (pad 1 smd rect (at -2 0) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 15 +3.3VP))
    (pad 2 smd rect (at 2 0) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_1210_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer B.Cu) (tedit 58389C69)
    (at 151.892 87.122 270)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C6 (at 0 2.667 360) (layer B.SilkS))
    (fp_text value C (at 0 -2.7 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 2 0 270) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 14 +5VD))
    (model Capacitors_SMD.3dshapes/C_1210_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer B.Cu) (tedit 5837686C)
    (at 120.396 81.28 180)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C7 (at 0 2.54 180) (layer B.SilkS))
    (fp_text value C (at 0 -2.7 180) (layer B.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 14 +5VD))
    (pad 2 smd rect (at 2 0 180) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_1210_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58389C8D)
    (at 162.56 95.25 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -2.159 180) (layer B.SilkS))
    (fp_text value R (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 17 /A_Step))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 5 /X_STEP))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58389C85)
    (at 162.56 106.172 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0.254 -2.032 180) (layer B.SilkS))
    (fp_text value R (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 16 /A_Dir))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 8 /X_Dir))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 583768DE)
    (at 157.48 132.08 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 1.651 -1.651 270) (layer B.SilkS))
    (fp_text value R (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 12 /RST/Abort))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 14 +5VD))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58389D08)
    (at 152.4 132.08 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 1.27 1.778 450) (layer B.SilkS))
    (fp_text value R (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 14 +5VD))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 27 /Feed_Hold))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 583768CE)
    (at 147.32 132.08 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at -1.778 2.032 270) (layer B.SilkS))
    (fp_text value R (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 14 +5VD))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 13 /Cycle_Start/Resme))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 58376A1D)
    (at 125.476 85.09)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference U3 (at 0.381 -4.064) (layer F.SilkS))
    (fp_text value 5V_to_3.3V_StpDn (at 0.254 2.54) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 15 +3.3VP))
    (pad 3 thru_hole oval (at 2.54 0) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 1 thru_hole oval (at -2.54 0) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 14 +5VD))
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_MPT-2.54mm_12pol (layer F.Cu) (tedit 58376CD3)
    (at 160.02 138.43 180)
    (descr "12-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference P1 (at 13.589 5.08 180) (layer F.SilkS))
    (fp_text value CONN_01X12 (at 14.478 -2.032 180) (layer F.Fab))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 27 /Feed_Hold))
    (pad 1 thru_hole rect (at 0 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 12 /RST/Abort))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 13 /Cycle_Start/Resme))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 28 /Splindle_ENA))
    (pad 9 thru_hole oval (at 20.32 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 10 thru_hole oval (at 22.86 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 26 /Spindle_PWM))
    (pad 11 thru_hole oval (at 25.4 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 12 thru_hole oval (at 27.94 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 14 +5VD))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MPT-2.54mm_12pol.wrl
      (at (xyz 0.55 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_4.3mm_M4_ISO7380_Pad (layer F.Cu) (tedit 5837614B)
    (at 120.65 71.12)
    (descr "Mounting Hole 4.3mm, M4, ISO7380")
    (tags "mounting hole 4.3mm m4 iso7380")
    (fp_text reference "" (at 0 -4.8) (layer F.SilkS) hide)
    (fp_text value "" (at 0 4.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 7.6 7.6) (drill 4.3) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_4.3mm_M4_ISO7380_Pad (layer F.Cu) (tedit 5837615F)
    (at 171.45 138.43)
    (descr "Mounting Hole 4.3mm, M4, ISO7380")
    (tags "mounting hole 4.3mm m4 iso7380")
    (fp_text reference "" (at 0 -4.8) (layer F.SilkS) hide)
    (fp_text value "" (at 0 4.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 7.6 7.6) (drill 4.3) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_4.3mm_M4_ISO7380_Pad (layer F.Cu) (tedit 5837616D)
    (at 120.65 138.43)
    (descr "Mounting Hole 4.3mm, M4, ISO7380")
    (tags "mounting hole 4.3mm m4 iso7380")
    (fp_text reference "" (at 0 -4.8) (layer F.SilkS) hide)
    (fp_text value "" (at 0 4.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 7.6 7.6) (drill 4.3) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_4.3mm_M4_ISO7380_Pad (layer F.Cu) (tedit 58376139)
    (at 171.45 71.12)
    (descr "Mounting Hole 4.3mm, M4, ISO7380")
    (tags "mounting hole 4.3mm m4 iso7380")
    (fp_text reference "" (at 0 -4.8) (layer F.SilkS) hide)
    (fp_text value "" (at 0 4.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 7.6 7.6) (drill 4.3) (layers *.Cu *.Mask))
  )
  (module Buttons_Switches_ThroughHole:Push_E-Switch_KS01Q01 (layer F.Cu) (tedit 58389BFF)
    (at 139.827 125.222 270)
    (descr "E-Switch KS01Q01")
    (tags "Push Button")
    (fp_text reference SW1 (at -0.762 9.652 360) (layer F.SilkS))
    (fp_text value Switch_DPST (at 2.5 -2.04914 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 33 "Net-(SW1-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 34 "Net-(SW1-Pad2)"))
    (pad 4 thru_hole circle (at 5 5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole circle (at 0 5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 21 /WF_RST))
    (model Buttons_Switches_ThroughHole.3dshapes/Push_E-Switch_KS01Q01.wrl
      (at (xyz 0.1 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Bottom Back" (at 147.32 71.12) (layer B.Cu))
  (gr_text "Top Front" (at 146.05 69.85) (layer F.Cu))
  (gr_text ABRT (at 157.48 142.875) (layer F.SilkS))
  (gr_text FDHLD (at 152.4 142.875) (layer F.SilkS))
  (gr_text RSM (at 147.193 142.875) (layer F.SilkS))
  (gr_text SENA (at 142.24 142.875) (layer F.SilkS))
  (gr_text PWM (at 137.287 142.875) (layer F.SilkS))
  (gr_text +5 (at 131.953 142.875) (layer F.SilkS))
  (target plus (at 184.15 152.4) (size 5) (width 0.15) (layer Edge.Cuts))
  (target plus (at 107.95 57.15) (size 5) (width 0.15) (layer Edge.Cuts))
  (gr_line (start 114.3 144.78) (end 114.3 64.77) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.8 144.78) (end 114.3 144.78) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.8 64.77) (end 177.8 144.78) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114.3 64.77) (end 177.8 64.77) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "2 Abort\n4 Feed Hold\n6 Cycle Start/Resume\n8 Spindle Ena\n10 Spindle PWM\n12 +5V out" (at 118.11 128.397) (layer F.SilkS))
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 176.53 143.51) (xy 115.57 143.51) (xy 115.57 66.04) (xy 176.53 66.04)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 176.53 143.51) (xy 115.57 143.51) (xy 115.57 66.04) (xy 176.53 66.04)
      )
    )
  )
)
