(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 6)
    (tracks 31)
    (zones 0)
    (modules 8)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.254000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 16)
  (net 4 17)
  (net 5 BH)
  (net 6 10)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 10)
    (add_net 16)
    (add_net 17)
    (add_net BH)
    (add_net GND)
    (add_net VCC)
  )
  (module AOR_custom:JOYSTICK (layer F.Cu) (tedit 5D003120)
    (at 131.404 95.344)
    (fp_text reference RV1 (at 1 -0.7) (layer F.SilkS) hide)
    (fp_text value joystick (at 1.75 -0.7) (layer F.SilkS) hide)
    (pad 14 thru_hole roundrect (at -7 8) (size 2.032 2.032) (drill oval 1.778 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 13 thru_hole roundrect (at 6.5 8) (size 2.032 2.032) (drill oval 1.778 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 12 thru_hole roundrect (at 6.5 -8) (size 2.032 2.032) (drill oval 1.778 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 11 thru_hole roundrect (at -7 -8) (size 2.032 2.032) (drill oval 1.778 1.016) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 10 thru_hole circle (at 12.5 3) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 10))
    (pad 9 thru_hole circle (at 8 3) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 BH))
    (pad 8 thru_hole circle (at 12.5 -3) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 10))
    (pad 7 thru_hole circle (at 8 -3) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 BH))
    (pad 6 thru_hole roundrect (at -10.5 2.5) (size 1.524 1.524) (drill oval 0.889 1.27) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 5 thru_hole roundrect (at -10.5 0) (size 1.524 1.524) (drill oval 0.889 1.27) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 4 17))
    (pad 4 thru_hole roundrect (at -10.5 -2.5) (size 1.524 1.524) (drill oval 0.889 1.27) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (pad 3 thru_hole roundrect (at 2.5 -10) (size 1.524 1.524) (drill oval 1.27 0.889) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 thru_hole roundrect (at 0 -10) (size 1.524 1.524) (drill oval 1.27 0.889) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 3 16))
    (pad 1 thru_hole roundrect (at -2.5 -10) (size 1.524 1.524) (drill oval 1.27 0.889) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
  )
  (module AOR_custom:AOR_LOGO (layer B.Cu) (tedit 5C26ADAA)
    (at 130.302 98.552 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value AOR_LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5CC50E71)
    (at 116.078 83.82)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5CC50E71)
    (at 116.078 104.648)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5CC50E71)
    (at 142.494 104.648)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 121.92 82.296 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x06 (at 0 15.03 90) (layer F.Fab))
    (fp_text user %R (at 0 6.35 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 16))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 17))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 BH))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 10))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5CC50E71)
    (at 142.494 83.82)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module AOR_custom:AOR_LOGO (layer F.Cu) (tedit 5C26ADAA)
    (at 130.048 105.918)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value AOR_LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (gr_text "ACP3-X-JOY-PCB\nREV B, 6-11-2019" (at 130.302 94.996) (layer B.SilkS))
  (gr_text "ACP3-X-JOY-PCB\nREV B, 6-11-2019" (at 116.078 93.98 90) (layer F.SilkS))
  (gr_line (start 146.304 80.01) (end 112.268 80.01) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 146.304 108.204) (end 146.304 80.01) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 112.268 108.204) (end 146.304 108.204) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 112.268 80.01) (end 112.268 108.204) (layer Edge.Cuts) (width 0.2))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.268 80.01) (xy 146.304 80.01) (xy 146.304 108.204) (xy 112.268 108.204)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.268 80.01) (xy 146.304 80.01) (xy 146.304 108.204) (xy 112.268 108.204)
      )
    )
  )
)
