(kicad_pcb (version 20170922) (host pcbnew "(2017-10-12 revision e0b9a2141)-master")
(general
  (thickness 1.6)
  (drawings 10)
  (tracks 15)
  (zones 0)
  (modules 2)
  (nets 8)
)
(page A4)
(layers
  (0 F.Cu signal)
  (31 B.Cu signal)
  (32 B.Adhes user)
  (33 F.Adhes user)
  (34 B.Paste user)
  (35 F.Paste user)
  (36 B.SilkS user)
  (37 F.SilkS user)
  (38 B.Mask user)
  (39 F.Mask user)
  (40 Dwgs.User user)
  (41 Cmts.User user)
  (42 Eco1.User user)
  (43 Eco2.User user)
  (44 Edge.Cuts user)
  (45 Margin user)
  (46 B.CrtYd user)
  (47 F.CrtYd user)
  (48 B.Fab user)
  (49 F.Fab user)
)
(general
  (thickness 1.6)
  (drawings 10)
  (tracks 15)
  (zones 0)
  (modules 2)
  (nets 8)
)
(page A4)
(layers
  (0 F.Cu signal)
  (31 B.Cu signal)
  (32 B.Adhes user)
  (33 F.Adhes user)
  (34 B.Paste user)
  (35 F.Paste user)
  (36 B.SilkS user)
  (37 F.SilkS user)
  (38 B.Mask user)
  (39 F.Mask user)
  (40 Dwgs.User user)
  (41 Cmts.User user)
  (42 Eco1.User user)
  (43 Eco2.User user)
  (44 Edge.Cuts user)
  (45 Margin user)
  (46 B.CrtYd user)
  (47 F.CrtYd user)
  (48 B.Fab user)
  (49 F.Fab user)
)
(setup
  (last_trace_width 0.254)
  (trace_clearance 0.127)
  (zone_clearance 0.508)
  (zone_45_only no)
  (trace_min 0.2)
  (segment_width 0.2)
  (edge_width 0.15)
  (via_size 1.27)
  (via_drill 0.508)
  (via_min_size 0.4)
  (via_min_drill 0.3)
  (uvia_size 0.3)
  (uvia_drill 0.1)
  (uvias_allowed no)
  (uvia_min_size 0.2)
  (uvia_min_drill 0.1)
  (pcb_text_width 0.3)
  (pcb_text_size 1.5 1.5)
  (mod_edge_width 0.15)
  (mod_text_size 1 1)
  (mod_text_width 0.15)
  (pad_size 1.524 1.524)
  (pad_drill 0.762)
  (pad_to_mask_clearance 0.2)
  (aux_axis_origin 0 0)
  (visible_elements FFFFFF7F)
  (pcbplotparams
    (layerselection 0x00030_ffffffff)
    (usegerberextensions false)
    (usegerberattributes true)
    (usegerberadvancedattributes true)
    (creategerberjobfile true)
    (excludeedgelayer true)
    (linewidth 0.100000)
    (plotframeref false)
    (viasonmask false)
    (mode 1)
    (useauxorigin false)
    (hpglpennumber 1)
    (hpglpenspeed 20)
    (hpglpendiameter 15)
    (psnegative false)
    (psa4output false)
    (plotreference true)
    (plotvalue true)
    (plotinvisibletext false)
    (padsonsilk false)
    (subtractmaskfromsilk false)
    (outputformat 1)
    (mirror false)
    (drillshape 1)
    (scaleselection 1)
    (outputdirectory ""))
)
(net 0 "")
(net 1 "Net-(CON1-Pad6)")
(net 2 "Net-(CON1-Pad5)")
(net 3 "Net-(CON1-Pad4)")
(net 4 "Net-(CON1-Pad3)")
(net 5 "Net-(CON1-Pad2)")
(net 6 "Net-(CON1-Pad1)")
(net 7 "Net-(J1-Pad6)")
(net_class Default "This is the default net class."
  (clearance 0.127)
  (trace_width 0.254)
  (via_dia 1.27)
  (via_drill 0.508)
  (uvia_dia 0.3)
  (uvia_drill 0.1)
  (add_net "Net-(CON1-Pad1)")
  (add_net "Net-(CON1-Pad2)")
  (add_net "Net-(CON1-Pad3)")
  (add_net "Net-(CON1-Pad4)")
  (add_net "Net-(CON1-Pad5)")
  (add_net "Net-(CON1-Pad6)")
  (add_net "Net-(J1-Pad6)")
)
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 5A1DFFF7)
    (at 76.2 63.5)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference MINIPRO (at 2.286 6.35 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x06 (at 0 15.03) (layer F.Fab))
    (fp_text user %R (at 0 6.35 90) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(CON1-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(CON1-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(CON1-Pad6)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(CON1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(CON1-Pad5)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5A1DFFF4)
    (at 69.85 67.31)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference ISP (at 1.524 7.62) (layer F.SilkS) hide)
    (fp_text value AVR-ISP-6 (at 1.27 7.41) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(CON1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(CON1-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(CON1-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(CON1-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(CON1-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(CON1-Pad6)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 1 (at 74.168 63.5) (layer B.SilkS))
  (gr_text 1 (at 70.358 65.278) (layer B.SilkS))
  (gr_text 1 (at 70.358 65.278) (layer F.SilkS))
  (gr_text 1 (at 74.168 63.5) (layer F.SilkS))
  (gr_line (start 77.724 77.724) (end 77.724 61.976) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 74.676 77.724) (end 77.724 77.724) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 68.326 73.914) (end 74.676 77.724) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 68.326 65.786) (end 68.326 73.914) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 74.676 61.976) (end 68.326 65.786) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 77.724 61.976) (end 74.676 61.976) (layer Edge.Cuts) (width 0.15))
)
