<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="-1.27" y1="0" x2="64.75" y2="0" width="0" layer="20"/>
<wire x1="64.75" y1="0" x2="64.75" y2="26.34" width="0" layer="20"/>
<wire x1="64.75" y1="26.34" x2="-1.27" y2="26.34" width="0" layer="20"/>
<wire x1="-1.27" y1="26.34" x2="-1.27" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="powerpoles">
<description>Anderson Powerpole footprints</description>
<packages>
<package name="POWERPOLE_PAIR_45A">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="powerpoles" package="POWERPOLE_PAIR_45A" value="POWERPOLE_POWER45A"/>
<element name="J2" library="powerpoles" package="POWERPOLE_PAIR_45A" value="POWERPOLE_POWER45A"/>
<element name="J3" library="powerpoles" package="POWERPOLE_PAIR_45A" value="POWERPOLE_POWER45A"/>
<element name="J4" library="powerpoles" package="POWERPOLE_PAIR_45A" value="POWERPOLE_POWER45A"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="J1" pad="RED"/>
<contactref element="J2" pad="RED"/>
<contactref element="J3" pad="RED"/>
<contactref element="J4" pad="RED"/>
</signal>
<signal name="N$2">
<contactref element="J1" pad="BLACK"/>
<contactref element="J2" pad="BLACK"/>
<contactref element="J3" pad="BLACK"/>
<contactref element="J4" pad="BLACK"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
