<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="68.58" y1="42.18" x2="93.98" y2="42.18" width="0.2" layer="20"/>
<wire x1="93.98" y1="42.18" x2="93.98" y2="11.43" width="0.2" layer="20"/>
<wire x1="93.98" y1="11.43" x2="68.58" y2="11.43" width="0.2" layer="20"/>
<wire x1="68.58" y1="11.43" x2="68.58" y2="42.18" width="0.2" layer="20"/>
<text>ANT</text>
<text>1</text>
<text>+V</text>
<text>D</text>
<text>0V</text>
<text>TinySensor V0.1</text>
<text>http://555circuitslab.com</text>
<text>TinySensor V0.1</text>
</plain>
<libraries>
<library name="JeeParts">
<packages>
<package name="RFM12B">
<description>RFM12B radio module by HopeRF</description>
</package>
</packages>
</library>
<library name="avr-5">
<packages>
<package name="SOIC14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="resistor">
<packages>
<package name="0204/5">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 5 mm</description>
</package>
</packages>
</library>
<library name="wirepad">
<packages>
<package name="1,6/0,8">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="ohw-logo">
<packages>
<package name="OSHW_FILLX100_NOTEXT">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BATTCOM_20MM_PTH">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC2" library="JeeParts" package="RFM12B" value="RFM12B">
<attribute name="NAME"/>
</element>
<element name="IC1" library="avr-5" package="SOIC14" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="resistor" package="0204/5" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PAD1" library="wirepad" package="1,6/0,8" value="ANT">
<attribute name="VALUE"/>
</element>
<element name="U$2" library="ohw-logo" package="OSHW_FILLX100_NOTEXT" value=""/>
<element name="BAT1" library="SparkFun-Electromechanical" package="BATTCOM_20MM_PTH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PAD4" library="wirepad" package="1,6/0,8" value="+VDD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PAD2" library="wirepad" package="1,6/0,8" value="Data">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PAD3" library="wirepad" package="1,6/0,8" value="GND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="pinhead" package="2X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PAD5" library="wirepad" package="1,6/0,8" value="">
<attribute name="VALUE"/>
</element>
<element name="PAD6" library="wirepad" package="1,6/0,8" value="ANT">
<attribute name="VALUE"/>
</element>
<element name="PAD7" library="wirepad" package="1,6/0,8" value="ANT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PAD8" library="wirepad" package="1,6/0,8" value="ANT">
<attribute name="VALUE"/>
</element>
<element name="PAD9" library="wirepad" package="1,6/0,8" value="ANT">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$3">
<contactref element="IC1" pad="8"/>
<contactref element="IC2" pad="SDI"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="7"/>
<contactref element="IC2" pad="SDO"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="IC2" pad="SCK"/>
<contactref element="IC1" pad="9"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="IC2" pad="SEL"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="IC2" pad="IRQ"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="13"/>
<contactref element="R1" pad="1"/>
<contactref element="PAD2" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="IC2" pad="ANT"/>
<contactref element="PAD1" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="IC2" pad="VDD"/>
<contactref element="IC1" pad="1"/>
<contactref element="BAT1" pad="1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="14"/>
<contactref element="IC2" pad="GND"/>
<contactref element="BAT1" pad="2"/>
<contactref element="PAD3" pad="1"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="N$10">
<contactref element="IC1" pad="12"/>
<contactref element="R1" pad="2"/>
<contactref element="PAD4" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="4"/>
<contactref element="JP1" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
