(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 177)
    (no_connects 0)
    (area 74.820429 25.916 212.453572 120.742)
    (thickness 1.6002)
    (drawings 9)
    (tracks 682)
    (zones 0)
    (modules 75)
    (nets 67)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu power)
    (2 In2.Cu power)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.127)
    (trace_clearance 0.127)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.127)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.5334)
    (via_drill 0.254)
    (via_min_size 0.5334)
    (via_min_drill 0.254)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.2 2.2)
    (pad_drill 2.2)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000007)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "C:/Users/rc.tech/Desktop/New Gerbers/"))
  )
  (net 0 "")
  (net 1 SW_READ2)
  (net 2 VCC)
  (net 3 3.3V)
  (net 4 SS_2)
  (net 5 RES)
  (net 6 "Net-(B1-Pad6)")
  (net 7 "Net-(B1-Pad7)")
  (net 8 "Net-(B1-Pad8)")
  (net 9 16V)
  (net 10 GND)
  (net 11 SW_READ1)
  (net 12 SS_1)
  (net 13 "Net-(B2-Pad6)")
  (net 14 "Net-(B2-Pad7)")
  (net 15 "Net-(B2-Pad8)")
  (net 16 SW_READ3)
  (net 17 SS_3)
  (net 18 "Net-(B3-Pad6)")
  (net 19 "Net-(B3-Pad7)")
  (net 20 "Net-(B3-Pad8)")
  (net 21 SS_4)
  (net 22 "Net-(B4-Pad6)")
  (net 23 "Net-(B4-Pad7)")
  (net 24 "Net-(B4-Pad8)")
  (net 25 "Net-(C4-Pad1)")
  (net 26 "Net-(C6-Pad2)")
  (net 27 "Net-(C11-Pad2)")
  (net 28 "Net-(D1-Pad1)")
  (net 29 "Net-(D1-Pad2)")
  (net 30 "Net-(D2-Pad1)")
  (net 31 "Net-(D2-Pad2)")
  (net 32 "Net-(D3-Pad1)")
  (net 33 "Net-(D3-Pad2)")
  (net 34 "Net-(D4-Pad1)")
  (net 35 "Net-(D4-Pad2)")
  (net 36 "Net-(D5-Pad1)")
  (net 37 "Net-(D5-Pad2)")
  (net 38 "Net-(D6-Pad1)")
  (net 39 "Net-(D6-Pad2)")
  (net 40 "Net-(D7-Pad1)")
  (net 41 "Net-(D7-Pad2)")
  (net 42 "Net-(D8-Pad1)")
  (net 43 "Net-(D8-Pad2)")
  (net 44 "Net-(D9-Pad2)")
  (net 45 SW_4)
  (net 46 SW_READ4)
  (net 47 "Net-(P1-Pad22)")
  (net 48 "Net-(P1-Pad24)")
  (net 49 "Net-(P1-Pad26)")
  (net 50 "Net-(P1-Pad28)")
  (net 51 "Net-(P1-Pad30)")
  (net 52 SW_3)
  (net 53 SW_2)
  (net 54 SW_1)
  (net 55 SDI)
  (net 56 SCLK)
  (net 57 Control_4)
  (net 58 Control_3)
  (net 59 D/C)
  (net 60 Control_2)
  (net 61 SHDN)
  (net 62 Control_1)
  (net 63 "Net-(U3-Pad1)")
  (net 64 "Net-(U5-Pad1)")
  (net 65 "Net-(U8-Pad1)")
  (net 66 "Net-(U11-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.127)
    (via_dia 0.5334)
    (via_drill 0.254)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net 16V)
    (add_net 3.3V)
    (add_net Control_1)
    (add_net Control_2)
    (add_net Control_3)
    (add_net Control_4)
    (add_net D/C)
    (add_net GND)
    (add_net "Net-(B1-Pad6)")
    (add_net "Net-(B1-Pad7)")
    (add_net "Net-(B1-Pad8)")
    (add_net "Net-(B2-Pad6)")
    (add_net "Net-(B2-Pad7)")
    (add_net "Net-(B2-Pad8)")
    (add_net "Net-(B3-Pad6)")
    (add_net "Net-(B3-Pad7)")
    (add_net "Net-(B3-Pad8)")
    (add_net "Net-(B4-Pad6)")
    (add_net "Net-(B4-Pad7)")
    (add_net "Net-(B4-Pad8)")
    (add_net "Net-(C11-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(D9-Pad2)")
    (add_net "Net-(P1-Pad22)")
    (add_net "Net-(P1-Pad24)")
    (add_net "Net-(P1-Pad26)")
    (add_net "Net-(P1-Pad28)")
    (add_net "Net-(P1-Pad30)")
    (add_net "Net-(U11-Pad1)")
    (add_net "Net-(U3-Pad1)")
    (add_net "Net-(U5-Pad1)")
    (add_net "Net-(U8-Pad1)")
    (add_net RES)
    (add_net SCLK)
    (add_net SDI)
    (add_net SHDN)
    (add_net SS_1)
    (add_net SS_2)
    (add_net SS_3)
    (add_net SS_4)
    (add_net SW_1)
    (add_net SW_2)
    (add_net SW_3)
    (add_net SW_4)
    (add_net SW_READ1)
    (add_net SW_READ2)
    (add_net SW_READ3)
    (add_net SW_READ4)
    (add_net VCC)
  )
  (module UDP:MOLEX4Pin (layer B.Cu) (tedit 58A77397)
    (at 129.54 41.402 180)
    (fp_text reference U6 (at 0 -6.35 180) (layer B.SilkS))
    (fp_text value DG_PBSW (at 0 8.89 180) (layer B.Fab) hide)
    (pad 4 thru_hole circle (at 1.75 -2.3 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 35 "Net-(D4-Pad2)"))
    (pad 2 thru_hole circle (at 1.75 2.3 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 3 thru_hole circle (at -1.75 -2.3 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 33 "Net-(D3-Pad2)"))
    (pad 1 thru_hole circle (at -1.75 2.3 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 53 SW_2))
  )
  (module UDP:ISC15ANP4 (layer F.Cu) (tedit 58B06D0E)
    (at 124.714 76.962)
    (fp_text reference B1 (at 0 11.43) (layer F.SilkS))
    (fp_text value ISC15ANP4 (at 0 -11.43) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 8 -3.81) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 SW_READ2))
    (pad 1 thru_hole circle (at 8 3.81) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 3 thru_hole circle (at -9.05 3.5) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 3.3V))
    (pad 4 thru_hole circle (at -7.05 2.5) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 SS_2))
    (pad 5 thru_hole circle (at -9.05 1.5) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 RES))
    (pad 6 thru_hole circle (at -7.05 0.5) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 6 "Net-(B1-Pad6)"))
    (pad 7 thru_hole circle (at -9.05 -0.5) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 7 "Net-(B1-Pad7)"))
    (pad 8 thru_hole circle (at -7.05 -1.5) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 8 "Net-(B1-Pad8)"))
    (pad 9 thru_hole circle (at -9.05 -2.5) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 9 16V))
    (pad 10 thru_hole circle (at -7.05 -3.5) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 10 GND))
  )
  (module UDP:ISC15ANP4 (layer F.Cu) (tedit 58B06D12)
    (at 162.56 76.962)
    (fp_text reference B2 (at 0 11.43) (layer F.SilkS))
    (fp_text value ISC15ANP4 (at 0 -11.43) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 8 -3.81) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 11 SW_READ1))
    (pad 1 thru_hole circle (at 8 3.81) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 3 thru_hole circle (at -9.05 3.5) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 3.3V))
    (pad 4 thru_hole circle (at -7.05 2.5) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 12 SS_1))
    (pad 5 thru_hole circle (at -9.05 1.5) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 RES))
    (pad 6 thru_hole circle (at -7.05 0.5) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 13 "Net-(B2-Pad6)"))
    (pad 7 thru_hole circle (at -9.05 -0.5) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 14 "Net-(B2-Pad7)"))
    (pad 8 thru_hole circle (at -7.05 -1.5) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 15 "Net-(B2-Pad8)"))
    (pad 9 thru_hole circle (at -9.05 -2.5) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 9 16V))
    (pad 10 thru_hole circle (at -7.05 -3.5) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 10 GND))
  )
  (module UDP:ISC15ANP4 (layer F.Cu) (tedit 58B06D09)
    (at 124.714 102.362)
    (fp_text reference B3 (at 0 11.43) (layer F.SilkS))
    (fp_text value ISC15ANP4 (at 0 -11.43) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 8 -3.81) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 16 SW_READ3))
    (pad 1 thru_hole circle (at 8 3.81) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 3 thru_hole circle (at -9.05 3.5) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 3.3V))
    (pad 4 thru_hole circle (at -7.05 2.5) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 17 SS_3))
    (pad 5 thru_hole circle (at -9.05 1.5) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 RES))
    (pad 6 thru_hole circle (at -7.05 0.5) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 18 "Net-(B3-Pad6)"))
    (pad 7 thru_hole circle (at -9.05 -0.5) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 19 "Net-(B3-Pad7)"))
    (pad 8 thru_hole circle (at -7.05 -1.5) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 20 "Net-(B3-Pad8)"))
    (pad 9 thru_hole circle (at -9.05 -2.5) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 9 16V))
    (pad 10 thru_hole circle (at -7.05 -3.5) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 10 GND))
  )
  (module UDP:ISC15ANP4 (layer F.Cu) (tedit 58B06D17)
    (at 162.56 102.362)
    (fp_text reference B4 (at 0 11.43) (layer F.SilkS))
    (fp_text value ISC15ANP4 (at 0 -11.43) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 8 -3.81) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 16 SW_READ3))
    (pad 1 thru_hole circle (at 8 3.81) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 3 thru_hole circle (at -9.05 3.5) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 3.3V))
    (pad 4 thru_hole circle (at -7.05 2.5) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 21 SS_4))
    (pad 5 thru_hole circle (at -9.05 1.5) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 RES))
    (pad 6 thru_hole circle (at -7.05 0.5) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 22 "Net-(B4-Pad6)"))
    (pad 7 thru_hole circle (at -9.05 -0.5) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 23 "Net-(B4-Pad7)"))
    (pad 8 thru_hole circle (at -7.05 -1.5) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 24 "Net-(B4-Pad8)"))
    (pad 9 thru_hole circle (at -9.05 -2.5) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 9 16V))
    (pad 10 thru_hole circle (at -7.05 -3.5) (size 1.2 1.2) (drill 0.75) (layers *.Cu *.Mask)
      (net 10 GND))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AF73F0)
    (at 180.848 51.054 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value 1u (at 0 -2.1 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58B060DE)
    (at 160.782 82.962)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 2.1) (layer B.SilkS))
    (fp_text value 0.1u (at 0 -2.1) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 3.3V))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58B06375)
    (at 122.936 108.362)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 2.1) (layer B.SilkS))
    (fp_text value 0.1u (at 0 -2.1) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 3.3V))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AF73E2)
    (at 175.26 56.134)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 2.1) (layer B.SilkS))
    (fp_text value 10n (at 0 -2.1) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AF73E9)
    (at 175.26 51.054)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 2.1) (layer B.SilkS))
    (fp_text value 2.2u (at 0 -2.1) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 3.3V))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58A75CA8)
    (at 101.854 60.452 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 10p (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 9 16V))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(C6-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58B065A0)
    (at 160.782 108.362)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 2.1) (layer B.SilkS))
    (fp_text value 0.1u (at 0 -2.1) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 3.3V))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AF748D)
    (at 122.936 82.962)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 0 2.1) (layer B.SilkS))
    (fp_text value 0.1u (at 0 -2.1) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 3.3V))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58A75C95)
    (at 97.282 55.88 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value 1u (at 0 -2.1 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 3.3V))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58A75CB2)
    (at 96.52 66.294 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 1u (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 9 16V))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58A75C33)
    (at 92.964 54.864 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at 0 2.1 270) (layer B.SilkS))
    (fp_text value 4.7u (at 0 -2.1 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(C11-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module UDP:PJ-0002BH-SMT (layer B.Cu) (tedit 58ADA74F)
    (at 94.234 88.138)
    (fp_text reference CON1 (at -1.27 -8.89) (layer B.SilkS))
    (fp_text value PJ-002BH-SMT (at -2.54 8.89) (layer B.Fab) hide)
    (pad 1 smd rect (at -4.5 5.9) (size 2.4 2.8) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 1 smd rect (at 1.6 5.9) (size 2.4 2.8) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at -4.5 -5.9) (size 2.4 2.8) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 3 smd rect (at 1.6 -5.9) (size 2.4 2.8) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad "" np_thru_hole circle (at 0 0) (size 1.8 1.8) (drill 1.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -4.5 0) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
  )
  (module Diodes_SMD:SOD-123 (layer B.Cu) (tedit 58A7630A)
    (at 114.046 43.942 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at 0 2 270) (layer B.SilkS))
    (fp_text value MBR0560 (at 0 -2.1 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.635 0 270) (size 0.91 1.22) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.635 0 270) (size 0.91 1.22) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(D1-Pad2)"))
  )
  (module Diodes_SMD:SOD-123 (layer B.Cu) (tedit 58A762D6)
    (at 114.046 35.56 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D2 (at 0 2 270) (layer B.SilkS))
    (fp_text value MBR0560 (at 0 -2.1 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.635 0 270) (size 0.91 1.22) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 1.635 0 270) (size 0.91 1.22) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(D2-Pad2)"))
  )
  (module Diodes_SMD:SOD-123 (layer B.Cu) (tedit 58ADA6CD)
    (at 142.24 43.942 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D3 (at 0 2 270) (layer B.SilkS))
    (fp_text value MBR0560 (at 0 -2.1 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.635 0 270) (size 0.91 1.22) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 1.635 0 270) (size 0.91 1.22) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(D3-Pad2)"))
  )
  (module Diodes_SMD:SOD-123 (layer B.Cu) (tedit 58A762F2)
    (at 142.24 35.56 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D4 (at 0 2 270) (layer B.SilkS))
    (fp_text value MBR0560 (at 0 -2.1 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.635 0 270) (size 0.91 1.22) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 1.635 0 270) (size 0.91 1.22) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(D4-Pad2)"))
  )
  (module Diodes_SMD:SOD-123 (layer B.Cu) (tedit 58A770D0)
    (at 170.434 43.942 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D5 (at 0 2 270) (layer B.SilkS))
    (fp_text value MBR0560 (at 0 -2.1 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.635 0 270) (size 0.91 1.22) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at 1.635 0 270) (size 0.91 1.22) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(D5-Pad2)"))
  )
  (module Diodes_SMD:SOD-123 (layer B.Cu) (tedit 58ADAFF9)
    (at 170.434 35.56 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D6 (at 0 2 270) (layer B.SilkS))
    (fp_text value MBR0560 (at 0 -2.1 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.635 0 270) (size 0.91 1.22) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(D6-Pad1)"))
    (pad 2 smd rect (at 1.635 0 270) (size 0.91 1.22) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(D6-Pad2)"))
  )
  (module Diodes_SMD:SOD-123 (layer B.Cu) (tedit 58AF0268)
    (at 198.628 43.942 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D7 (at 0 2 270) (layer B.SilkS))
    (fp_text value MBR0560 (at 0 -2.1 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.635 0 270) (size 0.91 1.22) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(D7-Pad1)"))
    (pad 2 smd rect (at 1.635 0 270) (size 0.91 1.22) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(D7-Pad2)"))
  )
  (module Diodes_SMD:SOD-123 (layer B.Cu) (tedit 58AF027D)
    (at 198.628 35.56 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D8 (at 0 2 270) (layer B.SilkS))
    (fp_text value MBR0560 (at 0 -2.1 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.635 0 270) (size 0.91 1.22) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(D8-Pad1)"))
    (pad 2 smd rect (at 1.635 0 270) (size 0.91 1.22) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(D8-Pad2)"))
  )
  (module Diodes_SMD:SOD-123 (layer B.Cu) (tedit 58A75C08)
    (at 92.71 62.992 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D9 (at 0 2 90) (layer B.SilkS))
    (fp_text value BAT42W-V-GS08 (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.635 0 90) (size 0.91 1.22) (layers B.Cu B.Paste B.Mask)
      (net 9 16V))
    (pad 2 smd rect (at 1.635 0 90) (size 0.91 1.22) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(D9-Pad2)"))
  )
  (module UDP:WM8046ND (layer F.Cu) (tedit 58B05FE9)
    (at 197.866 73.279 90)
    (fp_text reference P1 (at 0 3.81 90) (layer F.SilkS))
    (fp_text value CONN_02X15 (at 0 -3.81 90) (layer F.Fab) hide)
    (pad 17 thru_hole circle (at 2.54 -1.27 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 SW_READ1))
    (pad 16 thru_hole circle (at 0 1.27 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 3.3V))
    (pad 15 thru_hole circle (at 0 -1.27 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 SW_4))
    (pad 19 thru_hole circle (at 5.08 -1.27 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 SW_READ2))
    (pad 21 thru_hole circle (at 7.62 -1.27 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 SW_READ3))
    (pad 23 thru_hole circle (at 10.16 -1.27 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 SW_READ4))
    (pad 25 thru_hole circle (at 12.7 -1.27 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 SS_1))
    (pad 27 thru_hole circle (at 15.24 -1.27 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 SS_2))
    (pad 29 thru_hole circle (at 17.78 -1.27 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 SS_3))
    (pad 18 thru_hole circle (at 2.54 1.27 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 20 thru_hole circle (at 5.08 1.27 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 22 thru_hole circle (at 7.62 1.27 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(P1-Pad22)"))
    (pad 24 thru_hole circle (at 10.16 1.27 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(P1-Pad24)"))
    (pad 26 thru_hole circle (at 12.7 1.27 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(P1-Pad26)"))
    (pad 28 thru_hole circle (at 15.24 1.27 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(P1-Pad28)"))
    (pad 30 thru_hole circle (at 17.78 1.27 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(P1-Pad30)"))
    (pad 13 thru_hole circle (at -2.54 -1.27 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 SW_3))
    (pad 14 thru_hole circle (at -2.54 1.27 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 16V))
    (pad 12 thru_hole circle (at -5.08 1.27 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 RES))
    (pad 11 thru_hole circle (at -5.08 -1.27 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 SW_2))
    (pad 9 thru_hole circle (at -7.62 -1.27 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 SW_1))
    (pad 10 thru_hole circle (at -7.62 1.27 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 SDI))
    (pad 8 thru_hole circle (at -10.16 1.27 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 SCLK))
    (pad 7 thru_hole circle (at -10.16 -1.27 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 Control_4))
    (pad 5 thru_hole circle (at -12.7 -1.27 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 Control_3))
    (pad 6 thru_hole circle (at -12.7 1.27 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 D/C))
    (pad 3 thru_hole circle (at -15.24 -1.27 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 Control_2))
    (pad 4 thru_hole circle (at -15.24 1.27 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 SHDN))
    (pad 1 thru_hole circle (at -17.78 -1.27 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 Control_1))
    (pad 2 thru_hole circle (at -17.78 1.27 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 SS_4))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58A762A1)
    (at 107.442 43.942 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 43 (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(D1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58AC5BC4)
    (at 107.442 35.56 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 90 (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(D2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58A7621B)
    (at 101.346 30.226)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 2.1) (layer B.SilkS))
    (fp_text value 10k (at 0 -2.1) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 54 SW_1))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58A77180)
    (at 135.636 43.942 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 43 (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(D3-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58A7716B)
    (at 135.636 35.56 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 90 (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(D4-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(D4-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58A7737B)
    (at 129.54 30.226)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 2.1) (layer B.SilkS))
    (fp_text value 10k (at 0 -2.1) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 53 SW_2))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58ADB00A)
    (at 163.83 43.942 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 43 (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(D5-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(D5-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58ADB004)
    (at 163.83 35.56 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 90 (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(D6-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(D6-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58ADAFFE)
    (at 157.734 30.226)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 0 2.1) (layer B.SilkS))
    (fp_text value 10k (at 0 -2.1) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 45 SW_4))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58AF026D)
    (at 192.024 43.942 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 43 (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(D7-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(D7-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58AF0282)
    (at 192.024 35.56 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 90 (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(D8-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(D8-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58AF0202)
    (at 185.928 30.226)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at 0 2.1) (layer B.SilkS))
    (fp_text value 10k (at 0 -2.1) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 45 SW_4))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58AF7487)
    (at 140.462 73.152)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at 0 2.1) (layer B.SilkS))
    (fp_text value 10k (at 0 -2.1) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 SW_READ2))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58B060D9)
    (at 178.308 73.152)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at 0 2.1) (layer B.SilkS))
    (fp_text value 10k (at 0 -2.1) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 11 SW_READ1))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58B06355)
    (at 140.462 98.552)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R15 (at 0 2.1) (layer B.SilkS))
    (fp_text value 10k (at 0 -2.1) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 16 SW_READ3))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58B060D3)
    (at 160.782 78.962 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R16 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value 25 (at 0 -2.1 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 59 D/C))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(B2-Pad6)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58B05E74)
    (at 160.782 70.962 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R17 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value 25 (at 0 -2.1 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 56 SCLK))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(B2-Pad7)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58B0608D)
    (at 160.782 74.962 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R18 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value 25 (at 0 -2.1 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 55 SDI))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(B2-Pad8)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58B0636F)
    (at 122.936 104.362 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R19 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value 25 (at 0 -2.1 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 59 D/C))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(B3-Pad6)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58B0635F)
    (at 122.936 96.362 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R20 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value 25 (at 0 -2.1 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 56 SCLK))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(B3-Pad7)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58B0635B)
    (at 122.936 100.362 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R21 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value 25 (at 0 -2.1 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 55 SDI))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(B3-Pad8)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58A75CAC)
    (at 106.68 60.452 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R22 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 6.04M (at 0 -2.1 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 9 16V))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(C6-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58A75C9F)
    (at 104.394 55.372)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R23 (at 0 2.1) (layer B.SilkS))
    (fp_text value 499k (at 0 -2.1) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(C6-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58B05AA8)
    (at 178.308 98.552)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R24 (at 0 2.1) (layer B.SilkS))
    (fp_text value 10k (at 0 -2.1) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 16 SW_READ3))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58B05A9F)
    (at 160.782 104.362 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R25 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value 25 (at 0 -2.1 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 59 D/C))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(B4-Pad6)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58B05A99)
    (at 160.782 96.362 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R26 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value 25 (at 0 -2.1 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 56 SCLK))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(B4-Pad7)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58B05A93)
    (at 160.782 100.362 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R27 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value 25 (at 0 -2.1 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 55 SDI))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(B4-Pad8)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58AF7497)
    (at 122.936 78.962 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R28 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value 25 (at 0 -2.1 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 59 D/C))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(B1-Pad6)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58AF749D)
    (at 122.936 70.962 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R29 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value 25 (at 0 -2.1 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 56 SCLK))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(B1-Pad7)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58AF7492)
    (at 122.936 74.962 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R30 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value 25 (at 0 -2.1 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 55 SDI))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(B1-Pad8)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module UDP:NC7SZ08 (layer B.Cu) (tedit 58A7620A)
    (at 93.472 36.4 180)
    (fp_text reference U1 (at 0 -2 180) (layer B.SilkS))
    (fp_text value NC7SZ08 (at 0 2 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.65 -0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 62 Control_1))
    (pad 2 smd rect (at 0 -0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 62 Control_1))
    (pad 3 smd rect (at 0.65 -0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 5 smd rect (at -0.65 0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 4 smd rect (at 0.65 0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(D1-Pad1)"))
  )
  (module UDP:MOLEX4Pin (layer B.Cu) (tedit 58A7620F)
    (at 101.346 41.402 180)
    (fp_text reference U2 (at 0 -6.35 180) (layer B.SilkS))
    (fp_text value DG_PBSW (at 0 8.89 180) (layer B.Fab) hide)
    (pad 4 thru_hole circle (at 1.75 -2.3 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 31 "Net-(D2-Pad2)"))
    (pad 2 thru_hole circle (at 1.75 2.3 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 3 thru_hole circle (at -1.75 -2.3 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 29 "Net-(D1-Pad2)"))
    (pad 1 thru_hole circle (at -1.75 2.3 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 54 SW_1))
  )
  (module UDP:NC7SZ04 (layer B.Cu) (tedit 58A76215)
    (at 93.472 42.4 180)
    (fp_text reference U3 (at 0 -2 180) (layer B.SilkS))
    (fp_text value NC7SZ04 (at 0 2 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.65 -0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 63 "Net-(U3-Pad1)"))
    (pad 2 smd rect (at 0 -0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 62 Control_1))
    (pad 3 smd rect (at 0.65 -0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 4 smd rect (at 0.65 0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(D2-Pad1)"))
    (pad 5 smd rect (at -0.65 0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
  )
  (module UDP:NC7SZ08 (layer B.Cu) (tedit 58A76E62)
    (at 121.412 36.4 180)
    (fp_text reference U4 (at 0 -2 180) (layer B.SilkS))
    (fp_text value NC7SZ08 (at 0 2 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.65 -0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 60 Control_2))
    (pad 2 smd rect (at 0 -0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 60 Control_2))
    (pad 3 smd rect (at 0.65 -0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 5 smd rect (at -0.65 0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 4 smd rect (at 0.65 0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(D3-Pad1)"))
  )
  (module UDP:NC7SZ04 (layer B.Cu) (tedit 58A76EE2)
    (at 121.412 42.4 180)
    (fp_text reference U5 (at 0 -2 180) (layer B.SilkS))
    (fp_text value NC7SZ04 (at 0 2 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.65 -0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 64 "Net-(U5-Pad1)"))
    (pad 2 smd rect (at 0 -0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 60 Control_2))
    (pad 3 smd rect (at 0.65 -0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 4 smd rect (at 0.65 0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(D4-Pad1)"))
    (pad 5 smd rect (at -0.65 0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
  )
  (module UDP:NC7SZ08 (layer B.Cu) (tedit 58ADAF8E)
    (at 149.86 36.4 180)
    (fp_text reference U7 (at 0 -2 180) (layer B.SilkS))
    (fp_text value NC7SZ08 (at 0 2 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.65 -0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 58 Control_3))
    (pad 2 smd rect (at 0 -0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 58 Control_3))
    (pad 3 smd rect (at 0.65 -0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 5 smd rect (at -0.65 0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 4 smd rect (at 0.65 0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(D5-Pad1)"))
  )
  (module UDP:NC7SZ04 (layer B.Cu) (tedit 58ADAFA9)
    (at 149.86 42.4 180)
    (fp_text reference U8 (at 0 -2 180) (layer B.SilkS))
    (fp_text value NC7SZ04 (at 0 2 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.65 -0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 65 "Net-(U8-Pad1)"))
    (pad 2 smd rect (at 0 -0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 58 Control_3))
    (pad 3 smd rect (at 0.65 -0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 4 smd rect (at 0.65 0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(D6-Pad1)"))
    (pad 5 smd rect (at -0.65 0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
  )
  (module UDP:MOLEX4Pin (layer B.Cu) (tedit 58A7624F)
    (at 157.734 41.402 180)
    (fp_text reference U9 (at 0 -6.35 180) (layer B.SilkS))
    (fp_text value DG_PBSW (at 0 8.89 180) (layer B.Fab) hide)
    (pad 4 thru_hole circle (at 1.75 -2.3 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 39 "Net-(D6-Pad2)"))
    (pad 2 thru_hole circle (at 1.75 2.3 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 3 thru_hole circle (at -1.75 -2.3 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 37 "Net-(D5-Pad2)"))
    (pad 1 thru_hole circle (at -1.75 2.3 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 45 SW_4))
  )
  (module UDP:NC7SZ08 (layer B.Cu) (tedit 58AF0278)
    (at 178.054 36.4 180)
    (fp_text reference U10 (at 0 -2 180) (layer B.SilkS))
    (fp_text value NC7SZ08 (at 0 2 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.65 -0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 57 Control_4))
    (pad 2 smd rect (at 0 -0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 57 Control_4))
    (pad 3 smd rect (at 0.65 -0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 5 smd rect (at -0.65 0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 4 smd rect (at 0.65 0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(D7-Pad1)"))
  )
  (module UDP:NC7SZ04 (layer B.Cu) (tedit 58AF0272)
    (at 178.054 42.4 180)
    (fp_text reference U11 (at 0 -2 180) (layer B.SilkS))
    (fp_text value NC7SZ04 (at 0 2 180) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.65 -0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 66 "Net-(U11-Pad1)"))
    (pad 2 smd rect (at 0 -0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 57 Control_4))
    (pad 3 smd rect (at 0.65 -0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 4 smd rect (at 0.65 0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(D8-Pad1)"))
    (pad 5 smd rect (at -0.65 0.95 180) (size 0.4 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
  )
  (module UDP:MOLEX4Pin (layer B.Cu) (tedit 58A77392)
    (at 185.928 41.402 180)
    (fp_text reference U12 (at 0 -6.35 180) (layer B.SilkS))
    (fp_text value DG_PBSW (at 0 8.89 180) (layer B.Fab) hide)
    (pad 4 thru_hole circle (at 1.75 -2.3 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 43 "Net-(D8-Pad2)"))
    (pad 2 thru_hole circle (at 1.75 2.3 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 3 thru_hole circle (at -1.75 -2.3 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 41 "Net-(D7-Pad2)"))
    (pad 1 thru_hole circle (at -1.75 2.3 180) (size 1.7 1.7) (drill 1.02) (layers *.Cu *.Mask)
      (net 45 SW_4))
  )
  (module UDP:CAT6219 (layer B.Cu) (tedit 58AF7399)
    (at 180.848 56.134 180)
    (fp_text reference U13 (at 0 -2.54 180) (layer B.SilkS))
    (fp_text value CAT6219 (at 0 2.54 180) (layer B.Fab) hide)
    (pad 5 smd rect (at 1.165 0.96 270) (size 0.7 1) (layers B.Cu B.Paste B.Mask)
      (net 3 3.3V))
    (pad 2 smd rect (at -1.235 0.01 270) (size 0.7 1) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 3 smd rect (at -1.235 -0.94 270) (size 0.7 1) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 4 smd rect (at 1.165 -0.94 270) (size 0.7 1) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(C4-Pad1)"))
    (pad 1 smd rect (at -1.235 0.96 270) (size 0.7 1) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
  )
  (module UDP:MAX8574 (layer B.Cu) (tedit 58A75C8E)
    (at 97.282 60.198 180)
    (fp_text reference U14 (at 0 -2.54 180) (layer B.SilkS))
    (fp_text value MAX8574 (at 0 2.54 180) (layer B.Fab) hide)
    (pad 4 smd rect (at 1.2 -0.95 180) (size 1.33 0.54) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(D9-Pad2)"))
    (pad 5 smd rect (at 1.2 0 180) (size 1.33 0.54) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(C11-Pad2)"))
    (pad 6 smd rect (at 1.2 0.95 180) (size 1.33 0.54) (layers B.Cu B.Paste B.Mask)
      (net 3 3.3V))
    (pad 3 smd rect (at -1.2 -0.95 180) (size 1.33 0.54) (layers B.Cu B.Paste B.Mask)
      (net 61 SHDN))
    (pad 2 smd rect (at -1.2 0 180) (size 1.33 0.54) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 1 smd rect (at -1.2 0.95 180) (size 1.33 0.54) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(C6-Pad2)"))
  )
  (module UDP:LQH32C (layer B.Cu) (tedit 58B08D41)
    (at 89.916 59.182 270)
    (fp_text reference L1 (at 0 -2.54 270) (layer B.SilkS))
    (fp_text value 10u (at 0 2.54 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.7 0 270) (size 2.1 2) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(C11-Pad2)"))
    (pad 2 smd rect (at 1.7 0 270) (size 2.1 2) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(D9-Pad2)"))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_DIN965 (layer F.Cu) (tedit 58B0A560)
    (at 199.898 29.718)
    (descr "Mounting Hole 2.2mm, no annular, M2, DIN965")
    (tags "mounting hole 2.2mm no annular m2 din965")
    (fp_text reference REF** (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_DIN965 (at 0 2.9) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_DIN965 (layer F.Cu) (tedit 58B0A627)
    (at 87.376 29.718)
    (descr "Mounting Hole 2.2mm, no annular, M2, DIN965")
    (tags "mounting hole 2.2mm no annular m2 din965")
    (fp_text reference REF** (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_DIN965 (at 0 2.9) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_DIN965 (layer F.Cu) (tedit 58B0A6F6)
    (at 87.376 116.84)
    (descr "Mounting Hole 2.2mm, no annular, M2, DIN965")
    (tags "mounting hole 2.2mm no annular m2 din965")
    (fp_text reference REF** (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_DIN965 (at 0 2.9) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_DIN965 (layer F.Cu) (tedit 58B0A783)
    (at 199.898 116.84)
    (descr "Mounting Hole 2.2mm, no annular, M2, DIN965")
    (tags "mounting hole 2.2mm no annular m2 din965")
    (fp_text reference REF** (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_DIN965 (at 0 2.9) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask F.SilkS))
  )
  (gr_line (start 84.328 119.888) (end 202.946 119.888) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 84.328 79.248) (end 84.328 119.888) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 84.328 26.924) (end 84.328 31.496) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 84.328 26.924) (end 84.328 26.67) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 106.426 26.67) (end 84.328 26.67) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 176.53 26.67) (end 202.946 26.67) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 202.946 26.67) (end 202.946 119.888) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 106.426 26.67) (end 176.53 26.67) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 84.328 79.248) (end 84.328 31.496) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 10) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 202.946 119.888) (xy 84.328 119.888) (xy 84.328 26.67) (xy 202.946 26.67)
      )
    )
  )
  (zone (net 2) (net_name VCC) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 202.946 119.888) (xy 84.328 119.888) (xy 84.328 26.67) (xy 202.946 26.67)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 202.946 119.888) (xy 84.328 119.888) (xy 84.328 26.67) (xy 202.946 26.67)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 202.946 119.888) (xy 84.328 119.888) (xy 84.328 26.67) (xy 202.946 26.67)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.44 62.484) (xy 88.392 62.484) (xy 88.392 55.88) (xy 91.44 55.88)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.44 62.484) (xy 88.392 62.484) (xy 88.392 55.88) (xy 91.44 55.88)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.44 62.484) (xy 88.392 62.484) (xy 88.392 55.88) (xy 91.44 55.88)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 91.44 62.484) (xy 88.392 62.484) (xy 88.392 55.88) (xy 91.44 55.88)
      )
    )
  )
)
