(kicad_pcb (version 20171130) (host pcbnew "(5.1.0)-1")
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 114)
    (zones 0)
    (modules 13)
    (nets 12)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 0.6)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFEF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber"))
  )
  (net 0 "")
  (net 1 /+5)
  (net 2 /GND)
  (net 3 /EN)
  (net 4 "Net-(RN1-Pad1)")
  (net 5 "Net-(RN1-Pad4)")
  (net 6 /XE)
  (net 7 /CI)
  (net 8 "Net-(RN1-Pad8)")
  (net 9 /CE)
  (net 10 /PI)
  (net 11 /XI)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /+5)
    (add_net /CE)
    (add_net /CI)
    (add_net /EN)
    (add_net /GND)
    (add_net /PI)
    (add_net /XE)
    (add_net /XI)
    (add_net "Net-(RN1-Pad1)")
    (add_net "Net-(RN1-Pad4)")
    (add_net "Net-(RN1-Pad8)")
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 112 124)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference J1 (at -5.5 -1.648) (layer F.SilkS) hide)
    (fp_text value PE (at 2.5 0) (layer F.SilkS))
    (fp_text user %R (at -5.5 -0.5) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 9 /CE))
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 121.5 124.5 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0.01 1.29 180) (layer F.SilkS))
    (fp_text value .1u (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 /+5))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 117 124.5)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -0.15 -1.34 180) (layer F.SilkS))
    (fp_text value 47K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /EN))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-14_3.9x8.7mm_P1.27mm (layer F.Cu) (tedit 5E98C1B1)
    (at 119.5 130.5)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at -0.5 -3.5) (layer F.SilkS))
    (fp_text value 4066 (at 0 5.375) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /CE))
    (pad 2 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /XE))
    (pad 3 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(RN1-Pad4)"))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (pad 5 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /EN))
    (pad 6 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /EN))
    (pad 7 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 /GND))
    (pad 8 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 /PI))
    (pad 9 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /CI))
    (pad 10 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /CI))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 /XI))
    (pad 12 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(RN1-Pad4)"))
    (pad 13 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(RN1-Pad4)"))
    (pad 14 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 /+5))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 122.5 138)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference J2 (at 0 5) (layer F.SilkS) hide)
    (fp_text value CE (at 0 -2) (layer F.SilkS))
    (fp_text user %R (at 0 8) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 9 /CE))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 115.5 138)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference J3 (at 0 6) (layer F.SilkS) hide)
    (fp_text value XI (at 0 -2) (layer F.SilkS))
    (fp_text user %R (at 0 8) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 11 /XI))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 112 138)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference J4 (at -5 -4) (layer F.SilkS) hide)
    (fp_text value XE (at 1.5 -1.5) (layer F.SilkS))
    (fp_text user %R (at -8 -4) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 6 /XE))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 119 138)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference J5 (at 0 5) (layer F.SilkS) hide)
    (fp_text value CI (at 0 -2) (layer F.SilkS))
    (fp_text user %R (at 0 9) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 7 /CI))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 112 127.5)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference J6 (at -7 -1) (layer F.SilkS) hide)
    (fp_text value EN (at 2.5 0) (layer F.SilkS))
    (fp_text user %R (at -5 -1) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 3 /EN))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 112 120.5)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference J7 (at -6 0) (layer F.SilkS) hide)
    (fp_text value PI (at 2.21 0.01) (layer F.SilkS))
    (fp_text user %R (at -5 0) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 10 /PI))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 112 134.5)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference J8 (at -6 -2) (layer F.SilkS) hide)
    (fp_text value +5 (at 2.5 0) (layer F.SilkS))
    (fp_text user %R (at -6 -2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 1 /+5))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer F.Cu) (tedit 5A0F774F)
    (at 112 131)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference J9 (at -7 -2) (layer F.SilkS) hide)
    (fp_text value GND (at 2.36 0.03 90) (layer F.SilkS))
    (fp_text user %R (at -7 -2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 2 /GND))
  )
  (module Resistor_SMD:R_Array_Convex_4x0603 (layer F.Cu) (tedit 58E0A8B2)
    (at 119.18 121.16 90)
    (descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN1 (at 0.1 2.74 90) (layer F.SilkS))
    (fp_text value 10K (at 0 2.8 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.9 -1.2 90) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(RN1-Pad1)"))
    (pad 3 smd rect (at -0.9 0.4 90) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 7 /CI))
    (pad 2 smd rect (at -0.9 -0.4 90) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 6 /XE))
    (pad 4 smd rect (at -0.9 1.2 90) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(RN1-Pad4)"))
    (pad 7 smd rect (at 0.9 -0.4 90) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 /+5))
    (pad 8 smd rect (at 0.9 -1.2 90) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(RN1-Pad8)"))
    (pad 6 smd rect (at 0.9 0.4 90) (size 0.8 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 /+5))
    (pad 5 smd rect (at 0.9 1.2 90) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 /+5))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text @citrus3000psi (at 123 125 90) (layer B.SilkS))
  (gr_text "PISO SWITCHBOARD" (at 121 126.5 90) (layer B.SilkS))
  (gr_arc (start 123.5 139) (end 123.5 140) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 111 139) (end 110 139) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 111 119.5) (end 111 118.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 123.5 119.5) (end 124.5 119.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 110 119.5) (end 110 139) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 123.5 118.5) (end 111 118.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 124.5 139) (end 124.5 119.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 111 140) (end 123.5 140) (layer Edge.Cuts) (width 0.05))
)
