(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "Flock: RCBUS Compatible FDC and RTC Module")
    (date "2023-09-27")
    (rev "2.0")
    (company "Designed by Sergey Kiselev")
    (comment 2 "Licensed under CERN-OHL-S: https://cern-ohl.web.cern.ch")
    (comment 3 "Documentation and design files: https://github.com/skiselev/flock-v2")
    (comment 4 "Flock is an open source hardware project")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010f0_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "VCC")
  (net 3 "/A15")
  (net 4 "/A14")
  (net 5 "/A13")
  (net 6 "/A12")
  (net 7 "/A11")
  (net 8 "/A10")
  (net 9 "/A9")
  (net 10 "/A8")
  (net 11 "/A7")
  (net 12 "/A6")
  (net 13 "/A5")
  (net 14 "/A4")
  (net 15 "/A3")
  (net 16 "/A2")
  (net 17 "/A1")
  (net 18 "/A0")
  (net 19 "/~{M1}")
  (net 20 "/~{RESET}")
  (net 21 "Net-(C8-Pad1)")
  (net 22 "/~{WR}")
  (net 23 "/~{RD}")
  (net 24 "/~{IORQ}")
  (net 25 "/D0")
  (net 26 "/D1")
  (net 27 "/D2")
  (net 28 "/D3")
  (net 29 "/D4")
  (net 30 "/D5")
  (net 31 "/D6")
  (net 32 "/D7")
  (net 33 "/~{RFSH}")
  (net 34 "Net-(C9-Pad1)")
  (net 35 "Net-(BT1-Pad1)")
  (net 36 "/~{DENSEL}")
  (net 37 "unconnected-(J1-Pad4)")
  (net 38 "unconnected-(J1-Pad6)")
  (net 39 "/~{INDEX}")
  (net 40 "/~{MEA}")
  (net 41 "/~{DSB}")
  (net 42 "/~{DSA}")
  (net 43 "/~{MEB}")
  (net 44 "/~{DIR}")
  (net 45 "/~{STEP}")
  (net 46 "/~{WDATA}")
  (net 47 "/~{WE}")
  (net 48 "/~{TRK0}")
  (net 49 "/~{HDSEL}")
  (net 50 "/~{RDATA}")
  (net 51 "/~{WP}")
  (net 52 "/~{DC}")
  (net 53 "/RESET")
  (net 54 "/~{FDC_CS}")
  (net 55 "/~{DACK}")
  (net 56 "unconnected-(U1-Pad15)")
  (net 57 "/~{DOR_WR}")
  (net 58 "/~{CCR_WR}")
  (net 59 "unconnected-(U1-Pad38)")
  (net 60 "/RTC_CE")
  (net 61 "/RTC_IO")
  (net 62 "Net-(C10-Pad1)")
  (net 63 "Net-(C11-Pad1)")
  (net 64 "unconnected-(J3-Pad22)")
  (net 65 "/~{RTC_WR}")
  (net 66 "/~{RTC_RD}")
  (net 67 "Net-(U2-Pad2)")
  (net 68 "Net-(U2-Pad3)")
  (net 69 "unconnected-(J3-Pad37)")
  (net 70 "unconnected-(J3-Pad66)")
  (net 71 "unconnected-(J3-Pad21)")
  (net 72 "unconnected-(J3-Pad23)")
  (net 73 "unconnected-(J3-Pad35)")
  (net 74 "unconnected-(J3-Pad36)")
  (net 75 "unconnected-(J3-Pad77)")
  (net 76 "unconnected-(J3-Pad38)")
  (net 77 "unconnected-(J3-Pad39)")
  (net 78 "unconnected-(J3-Pad40)")
  (net 79 "unconnected-(J3-Pad41)")
  (net 80 "unconnected-(J3-Pad42)")
  (net 81 "unconnected-(J3-Pad43)")
  (net 82 "unconnected-(J3-Pad44)")
  (net 83 "unconnected-(J3-Pad45)")
  (net 84 "unconnected-(J3-Pad46)")
  (net 85 "unconnected-(J3-Pad47)")
  (net 86 "unconnected-(J3-Pad48)")
  (net 87 "unconnected-(J3-Pad49)")
  (net 88 "unconnected-(J3-Pad50)")
  (net 89 "unconnected-(J3-Pad51)")
  (net 90 "unconnected-(J3-Pad52)")
  (net 91 "unconnected-(J3-Pad53)")
  (net 92 "unconnected-(J3-Pad54)")
  (net 93 "unconnected-(J3-Pad55)")
  (net 94 "unconnected-(J3-Pad56)")
  (net 95 "unconnected-(J3-Pad60)")
  (net 96 "unconnected-(J3-Pad61)")
  (net 97 "unconnected-(J3-Pad62)")
  (net 98 "unconnected-(J3-Pad63)")
  (net 99 "unconnected-(J3-Pad64)")
  (net 100 "unconnected-(J3-Pad65)")
  (net 101 "unconnected-(J3-Pad67)")
  (net 102 "unconnected-(J3-Pad68)")
  (net 103 "unconnected-(J3-Pad69)")
  (net 104 "unconnected-(J3-Pad70)")
  (net 105 "unconnected-(J3-Pad71)")
  (net 106 "unconnected-(J3-Pad72)")
  (net 107 "unconnected-(J3-Pad73)")
  (net 108 "unconnected-(J3-Pad74)")
  (net 109 "unconnected-(J3-Pad75)")
  (net 110 "unconnected-(J3-Pad76)")
  (net 111 "unconnected-(J3-Pad78)")
  (net 112 "unconnected-(J3-Pad79)")
  (net 113 "unconnected-(J3-Pad80)")
  (net 114 "/OUT_D2")
  (net 115 "/IRQ")
  (net 116 "Net-(JP3-Pad2)")
  (net 117 "/RTC_SCLK")
  (net 118 "/RTC_DOUT")
  (net 119 "/~{RTC_WE}")
  (net 120 "unconnected-(J1-Pad33)")
  (net 121 "unconnected-(J1-Pad27)")
  (net 122 "unconnected-(J1-Pad17)")
  (net 123 "unconnected-(J1-Pad9)")
  (net 124 "unconnected-(J1-Pad3)")
  (net 125 "/RTC_ADDR")
  (net 126 "/~{RTC_RD_ENA}")
  (net 127 "/OUT_D0")
  (net 128 "/IN_D7")
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 130.81 95.25)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -3.8) (layer "F.Fab"))
    (fp_text value "3.2mm" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "My_Components:Cap_Cer_508" (layer "F.Cu")
    (tedit 619D8A0D)
    (at 186.69 99.06 90)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags "Cap_Cer_508")
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C1" (at -5.08 0 90) (layer "F.SilkS"))
    (fp_text value "100nF" (at 5.715 0 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle locked (at -2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "VCC") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (model "discret/capa_2pas_5x5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Cap_Cer_508" (layer "F.Cu")
    (tedit 619D8A0D)
    (at 156.21 115.57 90)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags "Cap_Cer_508")
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C3" (at -5.08 0 90) (layer "F.SilkS"))
    (fp_text value "100nF" (at -0.635 -1.905 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle locked (at -2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "VCC") (pintype "passive"))
    (model "discret/capa_2pas_5x5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Conn_TE_2-644488-2_2P_2.54mm" (layer "F.Cu")
    (tedit 6271FC4E)
    (at 166.37 85.09 180)
    (descr "Connector, Friction Lock, 2 Positions, 2.54mm Pitch")
    (tags "CONN FRICTION LOCK 2P")
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 7.112 5.3975) (layer "F.SilkS"))
    (fp_text value "Floppy 5V" (at 6.985 3.81) (layer "F.SilkS"))
    (pad "1" thru_hole rect (at -1.27 0 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.27 0 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "pin_array/pins_array_8x2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Cap_Cer_508" (layer "F.Cu")
    (tedit 619D8A0D)
    (at 156.21 104.14 -90)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags "Cap_Cer_508")
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C4" (at 5.08 0 90) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.905 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle locked (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "VCC") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (model "discret/capa_2pas_5x5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Cap_Cer_508" (layer "F.Cu")
    (tedit 619D8A0D)
    (at 147.32 90.17)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags "Cap_Cer_508")
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C2" (at -2.54 -1.905) (layer "F.SilkS"))
    (fp_text value "100nF" (at 1.5875 -1.905) (layer "F.SilkS"))
    (pad "1" thru_hole circle locked (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "VCC") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (model "discret/capa_2pas_5x5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Cap_Cer_508" (layer "F.Cu")
    (tedit 619D8A0D)
    (at 156.21 92.71 -90)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags "Cap_Cer_508")
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C5" (at 2.54 1.905 90) (layer "F.SilkS"))
    (fp_text value "100nF" (at -1.5875 1.905 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle locked (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "VCC") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (model "discret/capa_2pas_5x5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Cap_Cer_508" (layer "F.Cu")
    (tedit 6001348F)
    (at 222.25 93.98)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags "Cap_Cer_508")
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C9" (at -2.54 -2.2225) (layer "F.SilkS"))
    (fp_text value "15pF" (at 1.905 -2.2225) (layer "F.SilkS"))
    (pad "1" thru_hole circle locked (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask "F.SilkS")
      (net 34 "Net-(C9-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask "F.SilkS")
      (net 1 "GND") (pintype "passive"))
    (model "discret/capa_2pas_5x5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Cap_Elec_Radial_6.3mm" (layer "F.Cu")
    (tedit 61A5155F)
    (at 149.86 95.25 -90)
    (descr "Electrolythic Capacitor, Radial, 6.3 mm diameter,  2.5 mm lead spacing")
    (tags "CAPACITOR CP")
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C6" (at 4.445 0 180) (layer "F.SilkS"))
    (fp_text value "47uF" (at 5.715 0 180) (layer "F.SilkS"))
    (fp_text user "+" (at -2.794 -2.794 -90) (layer "F.SilkS"))
    (pad "1" thru_hole rect locked (at -1.25 0 270) (size 1.49098 1.49098) (drill 0.8001) (layers *.Cu *.Mask)
      (net 2 "VCC") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 1.25 0 270) (size 1.49098 1.49098) (drill 0.8001) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (model "discret/c_vert_c2v10.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:IC_DIP20_300" (layer "F.Cu")
    (tedit 619E89FD)
    (at 171.45 104.14)
    (descr "20 pins DIL package, round pads")
    (tags "DIP DIL DIP20 DIL20")
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U3" (at -10.16 5.715) (layer "F.SilkS"))
    (fp_text value "ATF16V8B" (at 8.89 5.715) (layer "F.SilkS"))
    (pad "1" thru_hole rect locked (at -11.43 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 17 "/A1") (pinfunction "I/CLK") (pintype "input"))
    (pad "2" thru_hole circle locked (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 16 "/A2") (pinfunction "I1") (pintype "input"))
    (pad "3" thru_hole circle locked (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 15 "/A3") (pinfunction "I2") (pintype "input"))
    (pad "4" thru_hole circle locked (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 14 "/A4") (pinfunction "I3") (pintype "input"))
    (pad "5" thru_hole circle locked (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 13 "/A5") (pinfunction "I4") (pintype "input"))
    (pad "6" thru_hole circle locked (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 12 "/A6") (pinfunction "I5") (pintype "input"))
    (pad "7" thru_hole circle locked (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 11 "/A7") (pinfunction "I6") (pintype "input"))
    (pad "8" thru_hole circle locked (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 19 "/~{M1}") (pinfunction "I7") (pintype "input"))
    (pad "9" thru_hole circle locked (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 24 "/~{IORQ}") (pinfunction "I8") (pintype "input"))
    (pad "10" thru_hole circle locked (at 11.43 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "11" thru_hole circle locked (at 11.43 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 23 "/~{RD}") (pinfunction "I9/~{OE}") (pintype "input"))
    (pad "12" thru_hole circle locked (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 22 "/~{WR}") (pinfunction "I/O8") (pintype "bidirectional"))
    (pad "13" thru_hole circle locked (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 54 "/~{FDC_CS}") (pinfunction "I/O7") (pintype "bidirectional"))
    (pad "14" thru_hole circle locked (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 55 "/~{DACK}") (pinfunction "I/O6") (pintype "bidirectional"))
    (pad "15" thru_hole circle locked (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 58 "/~{CCR_WR}") (pinfunction "I/O5") (pintype "bidirectional"))
    (pad "16" thru_hole circle locked (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 57 "/~{DOR_WR}") (pinfunction "I/O4") (pintype "bidirectional"))
    (pad "17" thru_hole circle locked (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 66 "/~{RTC_RD}") (pinfunction "I/O3") (pintype "bidirectional"))
    (pad "18" thru_hole circle locked (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 65 "/~{RTC_WR}") (pinfunction "I/O2") (pintype "bidirectional"))
    (pad "19" thru_hole circle locked (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 125 "/RTC_ADDR") (pinfunction "I/O1") (pintype "bidirectional"))
    (pad "20" thru_hole circle locked (at -11.43 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (model "dil/dil_20.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Battery_Holder_CR2032_Universal" (layer "F.Cu")
    (tedit 619D8A07)
    (at 138.43 110.49 180)
    (descr "Battery Holder, CR2032, Through Hole, Universal")
    (tags "BATT HOLDER CR2032 TH")
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "BT1" (at -10.16 -9.525) (layer "F.SilkS"))
    (fp_text value "CR2032" (at -10.16 -11.1125) (layer "F.SilkS"))
    (fp_text user "+" (at -13.9954 2.0066) (layer "F.SilkS"))
    (fp_text user "-" (at 5.9436 1.9812 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle locked (at -14.00048 0 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask "F.SilkS")
      (net 35 "Net-(BT1-Pad1)") (pinfunction "+") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5.99948 0 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask "F.SilkS")
      (net 1 "GND") (pinfunction "-") (pintype "passive"))
  )
  (footprint "My_Components:Crystal_HC-49U_Vert" (layer "F.Cu")
    (tedit 60825482)
    (at 214.63 96.52 -90)
    (descr "Quartz Crystal, HC-49U, Vertical")
    (tags "QUARTZ CRYSTAL HC49U VERT")
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (autoplace_cost180 10)
    (attr through_hole)
    (fp_text reference "Y1" (at 3.175 -3.175 90) (layer "F.SilkS"))
    (fp_text value "16MHz" (at -1.905 -3.175 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle locked (at -2.44094 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 34 "Net-(C9-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.44094 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 21 "Net-(C8-Pad1)") (pinfunction "2") (pintype "passive"))
    (model "discret/crystal_hc18u_vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Crystal_32K_Horiz" (layer "F.Cu")
    (tedit 603D2699)
    (at 144.691316 85.0975 90)
    (descr "crystal resonator for RTC, 32768 Hz")
    (tags "CRYSTAL RTC")
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Y2" (at 5.0875 6.438684) (layer "F.SilkS"))
    (fp_text value "32768Hz" (at 3.1825 6.438684) (layer "F.SilkS"))
    (pad "1" thru_hole circle locked (at -1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 67 "Net-(U2-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 68 "Net-(U2-Pad3)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -1.5875 5.08 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "3") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 1.5875 5.08 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "3") (pintype "passive"))
    (model "discret/c_vert_c1v5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Res_762" (layer "F.Cu")
    (tedit 626C4978)
    (at 181.61 92.71 -90)
    (descr "Resistor, 7.62mm lead spacing")
    (tags "RESISTOR")
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (autoplace_cost180 10)
    (attr through_hole)
    (fp_text reference "R2" (at 5.715 0 90) (layer "F.SilkS"))
    (fp_text value "10k" (at -5.715 -0.635 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 53 "/RESET") (pintype "passive"))
    (model "discret/resistor.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:IC_DIP14_300" (layer "F.Cu")
    (tedit 619D8A4B)
    (at 167.64 92.71)
    (descr "16 pins DIL package, round pads")
    (tags "DIP DIL DIP16 DIL16")
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U5" (at -6.35 5.715) (layer "F.SilkS"))
    (fp_text value "74HCT125" (at 5.08 5.715) (layer "F.SilkS"))
    (pad "1" thru_hole rect locked (at -7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 20 "/~{RESET}") (pintype "input"))
    (pad "2" thru_hole circle locked (at -5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "VCC") (pintype "input"))
    (pad "3" thru_hole circle locked (at -2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 53 "/RESET") (pintype "tri_state"))
    (pad "4" thru_hole circle locked (at 0 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 126 "/~{RTC_RD_ENA}") (pintype "input"))
    (pad "5" thru_hole circle locked (at 2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 128 "/IN_D7") (pintype "input"))
    (pad "6" thru_hole circle locked (at 5.08 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 32 "/D7") (pintype "tri_state"))
    (pad "7" thru_hole circle locked (at 7.62 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "8" thru_hole circle locked (at 7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 25 "/D0") (pintype "tri_state"))
    (pad "9" thru_hole circle locked (at 5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 61 "/RTC_IO") (pintype "input"))
    (pad "10" thru_hole circle locked (at 2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 126 "/~{RTC_RD_ENA}") (pintype "input"))
    (pad "11" thru_hole circle locked (at 0 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 61 "/RTC_IO") (pintype "tri_state"))
    (pad "12" thru_hole circle locked (at -2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 118 "/RTC_DOUT") (pintype "input"))
    (pad "13" thru_hole circle locked (at -5.08 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 119 "/~{RTC_WE}") (pintype "input"))
    (pad "14" thru_hole circle locked (at -7.62 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (model "dil/dil_16.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Cap_Cer_508" (layer "F.Cu")
    (tedit 619D8A0D)
    (at 219.71 113.03 -90)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags "Cap_Cer_508")
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C11" (at 1.905 -1.905 90) (layer "F.SilkS"))
    (fp_text value "56pF" (at -1.905 -1.905 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle locked (at -2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 63 "Net-(C11-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.54 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (model "discret/capa_2pas_5x5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Res_762" (layer "F.Cu")
    (tedit 626C4978)
    (at 179.07 92.71 -90)
    (descr "Resistor, 7.62mm lead spacing")
    (tags "RESISTOR")
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (autoplace_cost180 10)
    (attr through_hole)
    (fp_text reference "R3" (at 5.715 0 90) (layer "F.SilkS"))
    (fp_text value "10k" (at -5.715 0.635 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "VCC") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 128 "/IN_D7") (pintype "passive"))
    (model "discret/resistor.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:IC_DIP8_300" (layer "F.Cu")
    (tedit 619E89A5)
    (at 138.43 85.09 90)
    (descr "8 pins DIL package, round pads")
    (tags "DIP DIL DIP8 DIL8")
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 6.35 -3.81 180) (layer "F.SilkS"))
    (fp_text value "DS1302+" (at 6.35 1.905) (layer "F.SilkS"))
    (pad "1" thru_hole rect locked (at -3.81 3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "VCC2") (pintype "power_in"))
    (pad "2" thru_hole circle locked (at -1.27 3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 67 "Net-(U2-Pad2)") (pinfunction "X1") (pintype "input"))
    (pad "3" thru_hole circle locked (at 1.27 3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 68 "Net-(U2-Pad3)") (pinfunction "X2") (pintype "input"))
    (pad "4" thru_hole circle locked (at 3.81 3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" thru_hole circle locked (at 3.81 -3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 60 "/RTC_CE") (pinfunction "CE") (pintype "input"))
    (pad "6" thru_hole circle locked (at 1.27 -3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 61 "/RTC_IO") (pinfunction "I/O") (pintype "bidirectional"))
    (pad "7" thru_hole circle locked (at -1.27 -3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 117 "/RTC_SCLK") (pinfunction "SCLK") (pintype "input"))
    (pad "8" thru_hole circle locked (at -3.81 -3.81 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 35 "Net-(BT1-Pad1)") (pinfunction "VCC1") (pintype "power_in"))
    (model "dil/dil_8.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Conn_SIL6" (layer "F.Cu")
    (tedit 603D2E41)
    (at 214.63 88.9)
    (descr "Footprint, SIL-6")
    (tags "CONN SIL-6")
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "RN1" (at -6.0325 -2.2225) (layer "F.SilkS"))
    (fp_text value "1k" (at 6.6675 -2.2225) (layer "F.SilkS"))
    (pad "1" thru_hole rect locked (at -6.35 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "common") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 39 "/~{INDEX}") (pinfunction "R1") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 48 "/~{TRK0}") (pinfunction "R2") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 51 "/~{WP}") (pinfunction "R3") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 50 "/~{RDATA}") (pinfunction "R4") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 6.35 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 52 "/~{DC}") (pinfunction "R5") (pintype "passive"))
  )
  (footprint "My_Components:Crystal_HC-49U_Vert" (layer "F.Cu")
    (tedit 60825482)
    (at 214.63 109.22 90)
    (descr "Quartz Crystal, HC-49U, Vertical")
    (tags "QUARTZ CRYSTAL HC49U VERT")
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (autoplace_cost180 10)
    (attr through_hole)
    (fp_text reference "Y3" (at -3.175 3.175 90) (layer "F.SilkS"))
    (fp_text value "9.6MHz" (at 1.905 3.175 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle locked (at -2.44094 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 63 "Net-(C11-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.44094 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 62 "Net-(C10-Pad1)") (pinfunction "2") (pintype "passive"))
    (model "discret/crystal_hc18u_vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Cap_Super_Radial_13.5mm" (layer "F.Cu")
    (tedit 626ABAF1)
    (at 140.67973 110.49 180)
    (descr "Electrolythic Capacitor, Radial, 6.3 mm diameter,  2.5 mm lead spacing")
    (tags "CAPACITOR CP")
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C7" (at 1.5875 -7.62) (layer "F.SilkS"))
    (fp_text value "0.22F" (at -2.2225 -7.62) (layer "F.SilkS"))
    (fp_text user "+" (at -5.3975 -5.3975) (layer "F.SilkS"))
    (pad "1" thru_hole rect (at -2.5 0 180) (size 2.2 2.2) (drill 1.4) (layers *.Cu *.Mask)
      (net 35 "Net-(BT1-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 180) (size 2.2 2.2) (drill 1.4) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (model "discret/c_vert_c2v10.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:IC_PLCC44_TH" (layer "F.Cu")
    (tedit 61A920C2)
    (at 199.39 102.87 90)
    (descr "PLCC44 Socket, Through Hole")
    (tags "PLCC PLCC44")
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at -12.3825 -3.81 180) (layer "F.SilkS"))
    (fp_text value "37C65" (at -12.3825 3.81 180) (layer "F.SilkS"))
    (pad "1" thru_hole rect locked (at 1.27 -6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 23 "/~{RD}") (pinfunction "~{RD}") (pintype "input"))
    (pad "2" thru_hole circle locked (at -1.27 -8.89) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 22 "/~{WR}") (pinfunction "~{WR}") (pintype "input"))
    (pad "3" thru_hole circle locked (at -1.27 -6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 54 "/~{FDC_CS}") (pinfunction "~{CS}") (pintype "input"))
    (pad "4" thru_hole circle locked (at -3.81 -8.89) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 18 "/A0") (pinfunction "A0") (pintype "input"))
    (pad "5" thru_hole circle locked (at -3.81 -6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 55 "/~{DACK}") (pinfunction "~{DACK}") (pintype "input"))
    (pad "6" thru_hole circle locked (at -6.35 -8.89) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "TC") (pintype "input"))
    (pad "7" thru_hole circle locked (at -8.89 -6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 25 "/D0") (pinfunction "DB0") (pintype "tri_state"))
    (pad "8" thru_hole circle locked (at -6.35 -6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 26 "/D1") (pinfunction "DB1") (pintype "tri_state"))
    (pad "9" thru_hole circle locked (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 27 "/D2") (pinfunction "DB2") (pintype "tri_state"))
    (pad "10" thru_hole circle locked (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 28 "/D3") (pinfunction "DB3") (pintype "tri_state"))
    (pad "11" thru_hole circle locked (at -8.89 -1.27) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 29 "/D4") (pinfunction "DB4") (pintype "tri_state"))
    (pad "12" thru_hole circle locked (at -6.35 -1.27) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 30 "/D5") (pinfunction "DB5") (pintype "tri_state"))
    (pad "13" thru_hole circle locked (at -8.89 1.27) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 31 "/D6") (pinfunction "DB6") (pintype "tri_state"))
    (pad "14" thru_hole circle locked (at -6.35 1.27) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 32 "/D7") (pinfunction "DB7") (pintype "tri_state"))
    (pad "15" thru_hole circle locked (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 56 "unconnected-(U1-Pad15)") (pinfunction "DMA") (pintype "output+no_connect"))
    (pad "16" thru_hole circle locked (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 115 "/IRQ") (pinfunction "IRQ") (pintype "output"))
    (pad "17" thru_hole circle locked (at -8.89 6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "~{DCHGEN}") (pintype "input"))
    (pad "18" thru_hole circle locked (at -6.35 8.89) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 57 "/~{DOR_WR}") (pinfunction "~{LDOR}") (pintype "input"))
    (pad "19" thru_hole circle locked (at -6.35 6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 58 "/~{CCR_WR}") (pinfunction "~{LDCR}") (pintype "input"))
    (pad "20" thru_hole circle locked (at -3.81 8.89) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 53 "/RESET") (pinfunction "RST") (pintype "input"))
    (pad "21" thru_hole circle locked (at -3.81 6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 50 "/~{RDATA}") (pinfunction "~{RDD}") (pintype "input"))
    (pad "22" thru_hole circle locked (at -1.27 8.89) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 62 "Net-(C10-Pad1)") (pinfunction "~{XT2}") (pintype "input"))
    (pad "23" thru_hole circle locked (at -1.27 6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 63 "Net-(C11-Pad1)") (pinfunction "XT2") (pintype "input"))
    (pad "24" thru_hole circle locked (at 1.27 8.89) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 116 "Net-(JP3-Pad2)") (pinfunction "DRV") (pintype "input"))
    (pad "25" thru_hole circle locked (at 1.27 6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 21 "Net-(C8-Pad1)") (pinfunction "~{XT1}") (pintype "input"))
    (pad "26" thru_hole circle locked (at 3.81 8.89) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 34 "Net-(C9-Pad1)") (pinfunction "XT1") (pintype "input"))
    (pad "27" thru_hole circle locked (at 3.81 6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "PCVAL") (pintype "input"))
    (pad "28" thru_hole circle locked (at 6.35 8.89) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 49 "/~{HDSEL}") (pinfunction "~{HS}") (pintype "output"))
    (pad "29" thru_hole circle locked (at 8.89 6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 47 "/~{WE}") (pinfunction "~{WE}") (pintype "output"))
    (pad "30" thru_hole circle locked (at 6.35 6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 46 "/~{WDATA}") (pinfunction "~{WD}") (pintype "output"))
    (pad "31" thru_hole circle locked (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 44 "/~{DIR}") (pinfunction "~{DIRC}") (pintype "output"))
    (pad "32" thru_hole circle locked (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 45 "/~{STEP}") (pinfunction "~{STEP}") (pintype "output"))
    (pad "33" thru_hole circle locked (at 8.89 1.27) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 42 "/~{DSA}") (pinfunction "~{DS1}") (pintype "output"))
    (pad "34" thru_hole circle locked (at 6.35 1.27) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "35" thru_hole circle locked (at 8.89 -1.27) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 41 "/~{DSB}") (pinfunction "~{DS2}") (pintype "output"))
    (pad "36" thru_hole circle locked (at 6.35 -1.27) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 40 "/~{MEA}") (pinfunction "~{DS3}/~{MO1}") (pintype "output"))
    (pad "37" thru_hole circle locked (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 43 "/~{MEB}") (pinfunction "~{DS4}/~{MO2}") (pintype "output"))
    (pad "38" thru_hole circle locked (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 59 "unconnected-(U1-Pad38)") (pinfunction "~{HDL}") (pintype "output+no_connect"))
    (pad "39" thru_hole circle locked (at 8.89 -6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 36 "/~{DENSEL}") (pinfunction "~{RWC}/~{RPM}") (pintype "output"))
    (pad "40" thru_hole circle locked (at 6.35 -8.89) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 52 "/~{DC}") (pinfunction "~{DCHG}") (pintype "input"))
    (pad "41" thru_hole circle locked (at 6.35 -6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 51 "/~{WP}") (pinfunction "~{WP}") (pintype "input"))
    (pad "42" thru_hole circle locked (at 3.81 -8.89) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 48 "/~{TRK0}") (pinfunction "~{TR00}") (pintype "input"))
    (pad "43" thru_hole circle locked (at 3.81 -6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 39 "/~{INDEX}") (pinfunction "~{IDX}") (pintype "input"))
    (pad "44" thru_hole circle locked (at 1.27 -8.89) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "VCC") (pintype "power_in"))
  )
  (footprint "My_Components:IC_DIP16_300" (layer "F.Cu")
    (tedit 619D8A53)
    (at 168.91 115.57)
    (descr "16 pins DIL package, round pads")
    (tags "DIP DIL DIP16 DIL16")
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U4" (at -7.62 5.715) (layer "F.SilkS"))
    (fp_text value "74AHCT174" (at 6.0325 5.715) (layer "F.SilkS"))
    (pad "1" thru_hole rect locked (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 20 "/~{RESET}") (pinfunction "~{Mr}") (pintype "input"))
    (pad "2" thru_hole circle locked (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 119 "/~{RTC_WE}") (pinfunction "Q0") (pintype "output"))
    (pad "3" thru_hole circle locked (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 30 "/D5") (pinfunction "D0") (pintype "input"))
    (pad "4" thru_hole circle locked (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 31 "/D6") (pinfunction "D1") (pintype "input"))
    (pad "5" thru_hole circle locked (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 117 "/RTC_SCLK") (pinfunction "Q1") (pintype "output"))
    (pad "6" thru_hole circle locked (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 27 "/D2") (pinfunction "D2") (pintype "input"))
    (pad "7" thru_hole circle locked (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 114 "/OUT_D2") (pinfunction "Q2") (pintype "output"))
    (pad "8" thru_hole circle locked (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "9" thru_hole circle locked (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 65 "/~{RTC_WR}") (pinfunction "Cp") (pintype "input"))
    (pad "10" thru_hole circle locked (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 127 "/OUT_D0") (pinfunction "Q3") (pintype "output"))
    (pad "11" thru_hole circle locked (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 25 "/D0") (pinfunction "D3") (pintype "input"))
    (pad "12" thru_hole circle locked (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 118 "/RTC_DOUT") (pinfunction "Q4") (pintype "output"))
    (pad "13" thru_hole circle locked (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 32 "/D7") (pinfunction "D4") (pintype "input"))
    (pad "14" thru_hole circle locked (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 29 "/D4") (pinfunction "D5") (pintype "input"))
    (pad "15" thru_hole circle locked (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 60 "/RTC_CE") (pinfunction "Q5") (pintype "output"))
    (pad "16" thru_hole circle locked (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (model "dil/dil_16.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Res_762" (layer "F.Cu")
    (tedit 626C4978)
    (at 184.15 92.71 -90)
    (descr "Resistor, 7.62mm lead spacing")
    (tags "RESISTOR")
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (autoplace_cost180 10)
    (attr through_hole)
    (fp_text reference "R1" (at 5.715 0 90) (layer "F.SilkS"))
    (fp_text value "10k" (at -5.715 0 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 125 "/RTC_ADDR") (pintype "passive"))
    (model "discret/resistor.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Conn_Pin_Header_5x1_2.54mm" (layer "F.Cu")
    (tedit 61A6C618)
    (at 224.79 111.76 90)
    (descr "Pin Header, 5x1, 2.54mm pitch")
    (tags "CONN 5x1")
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at -7.3025 0 90) (layer "F.SilkS"))
    (fp_text value "GPIO" (at 8.255 0 90) (layer "F.SilkS"))
    (pad "1" thru_hole rect locked (at -5.08 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -2.54 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 128 "/IN_D7") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 0 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 127 "/OUT_D0") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 2.54 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 114 "/OUT_D2") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 5.08 0 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "Pin_5") (pintype "passive"))
    (model "pin_array/pins_array_8x2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Conn_Pin_Header_17x2_2.54mm_Shrouded_RA" (layer "F.Cu")
    (tedit 650B227C)
    (at 200.66 82.55)
    (descr "Pin Header, 13x2, 2.54mm pitch, shrouded")
    (tags "CONN PIN HEADER 13x2")
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -10.16 3.81) (layer "F.SilkS"))
    (fp_text value "Floppy" (at -3.81 3.81) (layer "F.SilkS"))
    (pad "1" thru_hole rect (at -20.32 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at -20.32 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 36 "/~{DENSEL}") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at -17.78 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 124 "unconnected-(J1-Pad3)") (pinfunction "Pin_3") (pintype "passive+no_connect"))
    (pad "4" thru_hole circle (at -17.78 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 37 "unconnected-(J1-Pad4)") (pinfunction "Pin_4") (pintype "passive+no_connect"))
    (pad "5" thru_hole circle (at -15.24 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at -15.24 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 38 "unconnected-(J1-Pad6)") (pinfunction "Pin_6") (pintype "passive+no_connect"))
    (pad "7" thru_hole circle (at -12.7 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle (at -12.7 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 39 "/~{INDEX}") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole circle (at -10.16 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 123 "unconnected-(J1-Pad9)") (pinfunction "Pin_9") (pintype "passive+no_connect"))
    (pad "10" thru_hole circle (at -10.16 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 40 "/~{MEA}") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole circle (at -7.62 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole circle (at -7.62 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 41 "/~{DSB}") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole circle (at -5.08 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole circle (at -5.08 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 42 "/~{DSA}") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole circle (at -2.54 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole circle (at -2.54 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 43 "/~{MEB}") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole circle (at 0 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 122 "unconnected-(J1-Pad17)") (pinfunction "Pin_17") (pintype "passive+no_connect"))
    (pad "18" thru_hole circle (at 0 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 44 "/~{DIR}") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole circle (at 2.54 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole circle (at 2.54 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 45 "/~{STEP}") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" thru_hole circle (at 5.08 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" thru_hole circle (at 5.08 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 46 "/~{WDATA}") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" thru_hole circle (at 7.62 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" thru_hole circle (at 7.62 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 47 "/~{WE}") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" thru_hole circle (at 10.16 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" thru_hole circle (at 10.16 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 48 "/~{TRK0}") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" thru_hole circle (at 12.7 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 121 "unconnected-(J1-Pad27)") (pinfunction "Pin_27") (pintype "passive+no_connect"))
    (pad "28" thru_hole circle (at 12.7 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 51 "/~{WP}") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" thru_hole circle (at 15.24 1.27 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" thru_hole circle (at 15.24 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 50 "/~{RDATA}") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" thru_hole circle (at 17.78 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" thru_hole circle (at 17.78 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 49 "/~{HDSEL}") (pinfunction "Pin_32") (pintype "passive"))
    (pad "33" thru_hole circle (at 20.32 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 120 "unconnected-(J1-Pad33)") (pinfunction "Pin_33") (pintype "passive+no_connect"))
    (pad "34" thru_hole circle (at 20.32 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 52 "/~{DC}") (pinfunction "Pin_34") (pintype "passive"))
    (model "pin_array/pins_array_13x2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Cap_Cer_508" (layer "F.Cu")
    (tedit 619D8A0D)
    (at 219.71 105.7275 90)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags "Cap_Cer_508")
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C10" (at -1.905 1.905 90) (layer "F.SilkS"))
    (fp_text value "68pF" (at 1.905 1.905 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle locked (at -2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 62 "Net-(C10-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.54 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (model "discret/capa_2pas_5x5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Symbol:OSHW-Logo_5.7x6mm_SilkScreen" (layer "F.Cu")
    (tedit 0)
    (at 196.85 119.38)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "LOGO2" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "Logo_Open_Hardware_Small" (at 0.75 0) (layer "F.Fab") hide)
  )
  (footprint "My_Components:Cap_Cer_508" (layer "F.Cu")
    (tedit 619D8A0D)
    (at 222.25 99.06)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags "Cap_Cer_508")
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C8" (at -2.54 -2.2225) (layer "F.SilkS"))
    (fp_text value "47pF" (at 1.905 -2.2225) (layer "F.SilkS"))
    (pad "1" thru_hole circle locked (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 21 "Net-(C8-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (model "discret/capa_2pas_5x5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:RCBUS_Logo" (layer "F.Cu")
    (tedit 0)
    (at 194.6275 89.2175)
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (attr board_only exclude_from_pos_files)
    (fp_text reference "LOGO3" (at 0 0) (layer "F.Fab"))
    (fp_text value "RCBUS_Logo" (at 0.75 0) (layer "F.Fab") hide)
  )
  (footprint "My_Components:Conn_Pin_Header_40x2_2.54mm_Right_Angle_RCBus80" (layer "F.Cu")
    (tedit 6503996F)
    (at 175.26 127)
    (descr "Pin Header, 39x1, 2.54mm pitch")
    (tags "CONN 39x1")
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0 5.08) (layer "F.Fab"))
    (fp_text value "RCBus-80" (at 0 6.985) (layer "F.Fab"))
    (fp_text user "D15" (at 35.56 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "A21" (at -22.86 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "A15" (at -48.26 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "p79" (at 48.26 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "nINT" (at 5.08 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "A6" (at -25.402162 1.892215 unlocked) (layer "B.SilkS"))
    (fp_text user "TX2" (at 38.1 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "D0" (at 17.78 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "p78" (at 45.72 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "A1" (at -12.7 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "nBRQ" (at 10.16 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "D6" (at 33.02 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "A3" (at -17.78 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "A16" (at -10.16 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "GND" (at -7.62 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "A5" (at -22.86 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "D3" (at 25.4 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "A23" (at -27.94 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "A7" (at -27.94 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "nIRQ2" (at 43.18 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "USR4" (at 50.8 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "PAGE" (at 0 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "D7" (at 35.56 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "TX" (at 38.1 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "p48" (at -30.48 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "D11" (at 25.4 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "nIORQ" (at 15.24 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "A8" (at -30.499465 1.892215 unlocked) (layer "B.SilkS"))
    (fp_text user "p45" (at -38.1 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "A9" (at -33.02 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "p46" (at -35.56 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "D4" (at 27.94 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "IRQ1n" (at 43.18 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "p44" (at -40.64 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "p47" (at -33.02 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "IEI" (at 45.72 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "D8" (at 17.78 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "D10" (at 22.86 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "A0" (at -10.16 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "D12" (at 27.94 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "D1" (at 20.32 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "BAO" (at -43.18 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "nWR" (at 10.16 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "D9" (at 20.32 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "D5" (at 30.48 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "nNMI" (at 15.24 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "A17" (at -12.7 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "+5V" (at -5.08 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "nHLT" (at 7.62 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "USR8" (at 50.8 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "GND" (at -7.62 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "A20" (at -20.32 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "A19" (at -17.78 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "+5V" (at -5.08 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "nBAK" (at 5.08 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "nWAIT" (at 12.7 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "nM1" (at -2.54 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "D2" (at 22.86 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "A18" (at -15.24 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "nMRQ" (at 7.62 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "A13" (at -43.18 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "BAI" (at -45.72 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "A2" (at -15.24 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "A22" (at -25.4 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "nRFSH" (at -2.54 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "nRST" (at 0 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "nRD" (at 12.7 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "D13" (at 30.48 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "RX2" (at 40.64 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "A10" (at -35.56 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "A4" (at -20.32 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "CLK" (at 2.54 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "A14" (at -45.72 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "p41" (at -48.26 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "A12" (at -40.64 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "A11" (at -38.1 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "CLK2" (at 2.54 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "D14" (at 33.02 -4.445 unlocked) (layer "B.SilkS"))
    (fp_text user "IEO" (at 48.26 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "RX" (at 40.64 1.905 unlocked) (layer "B.SilkS"))
    (fp_text user "1" (at -48.26 -5.08 unlocked) (layer "F.SilkS"))
    (pad "1" thru_hole rect (at -48.26 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "/A15") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at -45.72 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "/A14") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at -43.18 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "/A13") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at -40.64 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "/A12") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at -38.1 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "/A11") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at -35.56 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "/A10") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at -33.02 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "/A9") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle (at -30.48 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "/A8") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole circle (at -27.94 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "/A7") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole circle (at -25.4 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "/A6") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole circle (at -22.86 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "/A5") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole circle (at -20.32 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "/A4") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole circle (at -17.78 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "/A3") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole circle (at -15.24 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 "/A2") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole circle (at -12.7 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "/A1") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole circle (at -10.16 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 "/A0") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole circle (at -7.62 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole circle (at -5.08 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole circle (at -2.54 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 "/~{M1}") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole circle (at 0 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "/~{RESET}") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 71 "unconnected-(J3-Pad21)") (pinfunction "Pin_21") (pintype "passive+no_connect"))
    (pad "22" thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 64 "unconnected-(J3-Pad22)") (pinfunction "Pin_22") (pintype "passive+no_connect"))
    (pad "23" thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 72 "unconnected-(J3-Pad23)") (pinfunction "Pin_23") (pintype "passive+no_connect"))
    (pad "24" thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 "/~{WR}") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" thru_hole circle (at 12.7 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 "/~{RD}") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" thru_hole circle (at 15.24 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 "/~{IORQ}") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" thru_hole circle (at 17.78 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 "/D0") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" thru_hole circle (at 20.32 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "/D1") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" thru_hole circle (at 22.86 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 "/D2") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" thru_hole circle (at 25.4 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 "/D3") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" thru_hole circle (at 27.94 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 "/D4") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" thru_hole circle (at 30.48 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 "/D5") (pinfunction "Pin_32") (pintype "passive"))
    (pad "33" thru_hole circle (at 33.02 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 "/D6") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" thru_hole circle (at 35.56 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 "/D7") (pinfunction "Pin_34") (pintype "passive"))
    (pad "35" thru_hole circle (at 38.1 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 73 "unconnected-(J3-Pad35)") (pinfunction "Pin_35") (pintype "passive+no_connect"))
    (pad "36" thru_hole circle (at 40.64 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 74 "unconnected-(J3-Pad36)") (pinfunction "Pin_36") (pintype "passive+no_connect"))
    (pad "37" thru_hole circle (at 43.18 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 69 "unconnected-(J3-Pad37)") (pinfunction "Pin_37") (pintype "passive+no_connect"))
    (pad "38" thru_hole circle (at 45.72 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 76 "unconnected-(J3-Pad38)") (pinfunction "Pin_38") (pintype "passive+no_connect"))
    (pad "39" thru_hole circle (at 48.26 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 77 "unconnected-(J3-Pad39)") (pinfunction "Pin_39") (pintype "passive+no_connect"))
    (pad "40" thru_hole circle (at 50.8 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 78 "unconnected-(J3-Pad40)") (pinfunction "Pin_40") (pintype "passive+no_connect"))
    (pad "41" thru_hole circle (at -48.26 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 79 "unconnected-(J3-Pad41)") (pinfunction "Pin_41") (pintype "passive+no_connect"))
    (pad "42" thru_hole circle (at -45.72 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 80 "unconnected-(J3-Pad42)") (pinfunction "Pin_42") (pintype "passive+no_connect"))
    (pad "43" thru_hole circle (at -43.18 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 81 "unconnected-(J3-Pad43)") (pinfunction "Pin_43") (pintype "passive+no_connect"))
    (pad "44" thru_hole circle (at -40.64 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 82 "unconnected-(J3-Pad44)") (pinfunction "Pin_44") (pintype "passive+no_connect"))
    (pad "45" thru_hole circle (at -38.1 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 83 "unconnected-(J3-Pad45)") (pinfunction "Pin_45") (pintype "passive+no_connect"))
    (pad "46" thru_hole circle (at -35.56 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 84 "unconnected-(J3-Pad46)") (pinfunction "Pin_46") (pintype "passive+no_connect"))
    (pad "47" thru_hole circle (at -33.02 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 85 "unconnected-(J3-Pad47)") (pinfunction "Pin_47") (pintype "passive+no_connect"))
    (pad "48" thru_hole circle (at -30.48 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 86 "unconnected-(J3-Pad48)") (pinfunction "Pin_48") (pintype "passive+no_connect"))
    (pad "49" thru_hole circle (at -27.94 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 87 "unconnected-(J3-Pad49)") (pinfunction "Pin_49") (pintype "passive+no_connect"))
    (pad "50" thru_hole circle (at -25.4 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 88 "unconnected-(J3-Pad50)") (pinfunction "Pin_50") (pintype "passive+no_connect"))
    (pad "51" thru_hole circle (at -22.86 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 89 "unconnected-(J3-Pad51)") (pinfunction "Pin_51") (pintype "passive+no_connect"))
    (pad "52" thru_hole circle (at -20.32 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 90 "unconnected-(J3-Pad52)") (pinfunction "Pin_52") (pintype "passive+no_connect"))
    (pad "53" thru_hole circle (at -17.78 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 91 "unconnected-(J3-Pad53)") (pinfunction "Pin_53") (pintype "passive+no_connect"))
    (pad "54" thru_hole circle (at -15.24 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 92 "unconnected-(J3-Pad54)") (pinfunction "Pin_54") (pintype "passive+no_connect"))
    (pad "55" thru_hole circle (at -12.7 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 93 "unconnected-(J3-Pad55)") (pinfunction "Pin_55") (pintype "passive+no_connect"))
    (pad "56" thru_hole circle (at -10.16 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 94 "unconnected-(J3-Pad56)") (pinfunction "Pin_56") (pintype "passive+no_connect"))
    (pad "57" thru_hole circle (at -7.62 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_57") (pintype "passive"))
    (pad "58" thru_hole circle (at -5.08 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "Pin_58") (pintype "passive"))
    (pad "59" thru_hole circle (at -2.54 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 "/~{RFSH}") (pinfunction "Pin_59") (pintype "passive"))
    (pad "60" thru_hole circle (at 0 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 95 "unconnected-(J3-Pad60)") (pinfunction "Pin_60") (pintype "passive+no_connect"))
    (pad "61" thru_hole circle (at 2.54 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 96 "unconnected-(J3-Pad61)") (pinfunction "Pin_61") (pintype "passive+no_connect"))
    (pad "62" thru_hole circle (at 5.08 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 97 "unconnected-(J3-Pad62)") (pinfunction "Pin_62") (pintype "passive+no_connect"))
    (pad "63" thru_hole circle (at 7.62 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 98 "unconnected-(J3-Pad63)") (pinfunction "Pin_63") (pintype "passive+no_connect"))
    (pad "64" thru_hole circle (at 10.16 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 99 "unconnected-(J3-Pad64)") (pinfunction "Pin_64") (pintype "passive+no_connect"))
    (pad "65" thru_hole circle (at 12.7 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 100 "unconnected-(J3-Pad65)") (pinfunction "Pin_65") (pintype "passive+no_connect"))
    (pad "66" thru_hole circle (at 15.24 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 70 "unconnected-(J3-Pad66)") (pinfunction "Pin_66") (pintype "passive+no_connect"))
    (pad "67" thru_hole circle (at 17.78 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 101 "unconnected-(J3-Pad67)") (pinfunction "Pin_67") (pintype "passive+no_connect"))
    (pad "68" thru_hole circle (at 20.32 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 102 "unconnected-(J3-Pad68)") (pinfunction "Pin_68") (pintype "passive+no_connect"))
    (pad "69" thru_hole circle (at 22.86 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 103 "unconnected-(J3-Pad69)") (pinfunction "Pin_69") (pintype "passive+no_connect"))
    (pad "70" thru_hole circle (at 25.4 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 104 "unconnected-(J3-Pad70)") (pinfunction "Pin_70") (pintype "passive+no_connect"))
    (pad "71" thru_hole circle (at 27.94 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 105 "unconnected-(J3-Pad71)") (pinfunction "Pin_71") (pintype "passive+no_connect"))
    (pad "72" thru_hole circle (at 30.48 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 106 "unconnected-(J3-Pad72)") (pinfunction "Pin_72") (pintype "passive+no_connect"))
    (pad "73" thru_hole circle (at 33.02 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 107 "unconnected-(J3-Pad73)") (pinfunction "Pin_73") (pintype "passive+no_connect"))
    (pad "74" thru_hole circle (at 35.56 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 108 "unconnected-(J3-Pad74)") (pinfunction "Pin_74") (pintype "passive+no_connect"))
    (pad "75" thru_hole circle (at 38.1 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 109 "unconnected-(J3-Pad75)") (pinfunction "Pin_75") (pintype "passive+no_connect"))
    (pad "76" thru_hole circle (at 40.64 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 110 "unconnected-(J3-Pad76)") (pinfunction "Pin_76") (pintype "passive+no_connect"))
    (pad "77" thru_hole circle (at 43.18 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 75 "unconnected-(J3-Pad77)") (pinfunction "Pin_77") (pintype "passive+no_connect"))
    (pad "78" thru_hole circle (at 45.72 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 111 "unconnected-(J3-Pad78)") (pinfunction "Pin_78") (pintype "passive+no_connect"))
    (pad "79" thru_hole circle (at 48.26 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 112 "unconnected-(J3-Pad79)") (pinfunction "Pin_79") (pintype "passive+no_connect"))
    (pad "80" thru_hole circle (at 50.8 -2.54) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 113 "unconnected-(J3-Pad80)") (pinfunction "Pin_80") (pintype "passive+no_connect"))
    (model "pin_array/pins_array_8x2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Conn_Pin_Header_2x1_2.54mm_NoKey" (layer "F.Cu")
    (tedit 619E9CE4)
    (at 140.97 93.98)
    (descr "Pin Header, 2x1, 2.54mm pitch, no key")
    (tags "CONN 2x1 NOKEY")
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "JP1" (at -4.7625 -2.2225) (layer "F.SilkS"))
    (fp_text value "RTC_Address" (at 1.5875 -2.2225) (layer "F.SilkS"))
    (pad "1" thru_hole circle locked (at -1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "VCC") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 125 "/RTC_ADDR") (pinfunction "B") (pintype "passive"))
    (model "pin_array/pins_array_8x2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Symbol:OSHW-Logo_5.7x6mm_SilkScreen" (layer "B.Cu")
    (tedit 0)
    (at 196.85 118.11 180)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "LOGO1" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "Logo_Open_Hardware_Small" (at 0.75 0) (layer "B.Fab") hide)
  )
  (footprint "Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm_NumberLabels" (layer "B.Cu")
    (tedit 5C745336)
    (at 214.63 102.87 180)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip, labeled with numbers")
    (tags "net tie solder jumper bridged")
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "JP3" (at 0 1.8) (layer "B.SilkS"))
    (fp_text value "DRV" (at 0 -1.9) (layer "B.SilkS"))
    (fp_text user "1" (at -2.6 0) (layer "B.SilkS"))
    (fp_text user "3" (at 2.6 0) (layer "B.SilkS"))
    (pad "1" smd custom (at -1.3 0 180) (size 1 0.5) (layers "B.Cu" "B.Mask")
      (net 1 "GND") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0.55 -0.75)
            (xy 0 -0.75)
            (xy 0 0.75)
            (xy 0.55 0.75)
          ) (width 0) (fill yes))
            (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
            (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
      ))
    (pad "2" smd rect (at 0 0 180) (size 1 1.5) (layers "B.Cu" "B.Mask")
      (net 116 "Net-(JP3-Pad2)") (pinfunction "C") (pintype "passive"))
    (pad "3" smd custom (at 1.3 0 180) (size 1 0.5) (layers "B.Cu" "B.Mask")
      (net 2 "VCC") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_poly (pts
            (xy 0 -0.75)
            (xy -0.55 -0.75)
            (xy -0.55 0.75)
            (xy 0 0.75)
          ) (width 0) (fill yes))
      ))
  )
  (footprint "Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm_NumberLabels" (layer "B.Cu")
    (tedit 5C745336)
    (at 167.64 94.615 180)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip, labeled with numbers")
    (tags "net tie solder jumper bridged")
    (property "Sheetfile" "Z80-FDC-V2.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "JP2" (at 0 3.4925) (layer "B.SilkS"))
    (fp_text value "RTC_ENA" (at 0 1.905) (layer "B.SilkS"))
    (fp_text user "1" (at -2.6 0) (layer "B.SilkS"))
    (fp_text user "3" (at 2.6 0) (layer "B.SilkS"))
    (pad "1" smd custom (at -1.3 0 180) (size 1 0.5) (layers "B.Cu" "B.Mask")
      (net 66 "/~{RTC_RD}") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0.55 -0.75)
            (xy 0 -0.75)
            (xy 0 0.75)
            (xy 0.55 0.75)
          ) (width 0) (fill yes))
            (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
            (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
      ))
    (pad "2" smd rect (at 0 0 180) (size 1 1.5) (layers "B.Cu" "B.Mask")
      (net 126 "/~{RTC_RD_ENA}") (pinfunction "C") (pintype "passive"))
    (pad "3" smd custom (at 1.3 0 180) (size 1 0.5) (layers "B.Cu" "B.Mask")
      (net 2 "VCC") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_poly (pts
            (xy 0 -0.75)
            (xy -0.55 -0.75)
            (xy -0.55 0.75)
            (xy 0 0.75)
          ) (width 0) (fill yes))
      ))
  )
  (gr_line (start 227.33 78.74) (end 227.33 129.54) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 127 130.81) (mid 126.101974 130.438026) (end 125.73 129.54) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 227.33 129.54) (mid 226.958026 130.438026) (end 226.06 130.81) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 125.73 129.54) (end 125.73 85.09) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 226.06 130.81) (end 127 130.81) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 226.06 77.47) (mid 226.958026 77.841974) (end 227.33 78.74) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 133.35 77.47) (end 125.73 85.09) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 133.35 77.47) (end 226.06 77.47) (layer "Edge.Cuts") (width 0.05))
  (gr_text "Flock - Floppy Disk Controller and Real Time Clock - Version 2.0\nCopyright (C) 2022-2023 Sergey Kiselev" (at 222.25 86.36) (layer "B.SilkS"))
  (gr_text "Designed\nin\nOregon" (at 205.779605 118.584308) (layer "B.SilkS"))
  (gr_text "GND" (at 223.8375 116.84) (layer "B.SilkS"))
  (gr_text "OUT_D0" (at 223.8375 111.76) (layer "B.SilkS"))
  (gr_text "FDC I/O Registers:\nMSR(r):    0x50   CCR(w)/DIR(r): 0x48\nData(r/w): 0x51   DOR(w)/TC(r):  0x58 " (at 154.305 115.57) (layer "B.SilkS"))
  (gr_text "IN_D7" (at 223.8375 114.3) (layer "B.SilkS"))
  (gr_text "Floppy Disk Controller (FDC):\nReal Time Clock (RTC), JP1 open:\nReal Time Clock (RTC), JP1 closed:" (at 187.325 115.57) (layer "B.SilkS"))
  (gr_text "Module's I/O Addresses:" (at 187.325 109.855) (layer "B.SilkS"))
  (gr_text "OUT_D2" (at 223.8375 109.22) (layer "B.SilkS"))
  (gr_text "SK102" (at 224.79 84.1375 -90) (layer "B.SilkS"))
  (gr_text "!" (at 187.96 103.8225) (layer "B.SilkS"))
  (gr_text "J2 is an unfused 5V power supply\nfor a single 3.5{dblquote} floppy disk drive\nAvoid overloading and short-circuiting\n" (at 186.055 103.505) (layer "B.SilkS"))
  (gr_text "+5V" (at 223.8375 106.68) (layer "B.SilkS"))
  (gr_text "Design files and documentation:\nLicensed under CERN-OHL-S:" (at 226.06 91.44) (layer "B.SilkS"))
  (gr_text "https://github.com/skiselev/flock-v2\nhttps://cern-ohl.web.cern.ch" (at 200.025 91.44) (layer "B.SilkS"))
  (gr_text "Jumpers settings [default]:\nJP2: [1-2]: Enable RTC\nJP2:  2-3 : Disable RTC\nJP3: [1-2]: Y3 crystal not installed\n     disable 300 Kbps transfer rate\nJP3:  2-3 : Y3 crystal installed\n     enable 300 Kbps transfer rate" (at 154.305 103.1875) (layer "B.SilkS"))
  (gr_text "0x48 - 0x59\n0xC0 - 0xC1\n0x0C - 0x0D\n" (at 165.1 115.57) (layer "B.SilkS"))
  (gr_text "www.malinov.com" (at 186.055 121.285) (layer "F.SilkS"))
  (gr_text "SK102" (at 224.79 84.1375 90) (layer "F.SilkS"))
  (gr_text "Designed\nin\nOregon" (at 206.069603 120.015) (layer "F.SilkS"))
  (gr_text "-" (at 165.1 86.995) (layer "F.SilkS"))
  (gr_text "JLCJLCJLCJLC" (at 171.45 104.14) (layer "F.SilkS"))
  (gr_text "Open:   0xC0\nClosed: 0x0C" (at 140.335 97.155) (layer "F.SilkS"))
  (gr_text "+" (at 167.64 86.995) (layer "F.SilkS"))
  (gr_text "Y3, C10, and C11\nare optional;\nrequired for 300 Kbps\ntransfer rate support" (at 210.5025 119.6975) (layer "F.SilkS"))
  (gr_text "Flock - V2.0\nCopyright (C)\nSergey Kiselev" (at 130.81 86.995 90) (layer "F.SilkS"))
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 227.33 130.81)
        (xy 125.73 130.81)
        (xy 125.73 85.09)
        (xy 133.35 77.47)
        (xy 227.33 77.47)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 227.33 130.81)
        (xy 125.73 130.81)
        (xy 125.73 85.09)
        (xy 133.35 77.47)
        (xy 227.33 77.47)
      )
    )
  )
)
