<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="60" y1="0" x2="60" y2="60" width="0.254" layer="20"/>
<wire x1="60" y1="60" x2="0" y2="60" width="0.254" layer="20"/>
<wire x1="0" y1="60" x2="0" y2="0" width="0.254" layer="20"/>
<text>EightByEight RevE 2016-07</text>
<text>Blinkinlabs, LLC</text>
<wire x1="60" y1="0" x2="0" y2="0" width="0.254" layer="20"/>
<text>Off</text>
<text>On</text>
<text>Charge</text>
<text>Power</text>
<text>16</text>
<text>5</text>
<text>GND</text>
<text>3.3V</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R0402">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
<package name="SOD-123">
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="blinkinlabs">
<description>Library of parts that we use for our Blinkinlabs designs. Some parts copied (and modified) from the excellent Sparkfun libraries.
</description>
<packages>
<package name="USB_MICRO_THRUHOLE">
</package>
<package name="QFN32_5X5_LONGLEADS">
</package>
<package name="TD-07XB">
</package>
<package name="TSSOP16">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 14&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="SSOP24-150">
</package>
<package name="CRSYTAL_2520">
</package>
<package name="SWITCH_6P-2POS">
<description>This is one we found in the parts drawer, need to get details for it.</description>
</package>
<package name="ESP_WROOM_02">
</package>
<package name="LED_3528">
</package>
<package name="BATTERY_AA_SMD">
</package>
<package name="INDUCTOR_CD43">
</package>
<package name="SO08-150">
<description>&lt;b&gt;Small Outline package 8&lt;/b&gt; 150 mil</description>
</package>
</packages>
</library>
<library name="PaxInstrument-T400">
<description>Generated from &lt;b&gt;lumberdaq.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="SPARKFUN-RESISTORS_0603-RES">
</package>
</packages>
</library>
<library name="teensy_adapter">
<packages>
<package name="SC70-6L">
<description>&lt;b&gt;SC-70 Package&lt;/b&gt;</description>
</package>
<package name="VFDFN-10">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-ARV">
<description>&lt;b&gt;Chip Resistor Array&lt;/b&gt; size 4 × 0603&lt;p&gt;
convex termination - Phycomp Components&lt;br&gt;
Source: RS Components</description>
</package>
<package name="SJ_2S-TRACE">
<description>Solder jumper, small, shorted with trace. No paste layer. Trace is cuttable.</description>
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B1,27">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="DevicesToMerge">
<packages>
<package name="IO_HOLE_3MM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U2" library="blinkinlabs" package="SSOP24-150" value="ICN2026">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="adafruit" package="C0402" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="R0402" value="1.6k 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="adafruit" package="R0402" value="33">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="adafruit" package="R0402" value="33">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="blinkinlabs" package="USB_MICRO_THRUHOLE" value="USB_MICROSMT+THRUHULE">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R6" library="adafruit" package="R0402" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="adafruit" package="C0402" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="blinkinlabs" package="SWITCH_6P-2POS" value="SWITCH_SPDT"/>
<element name="C2" library="adafruit" package="C0402" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="adafruit" package="C0402" value="2.2uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="adafruit" package="C0402" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="adafruit" package="C0402" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="blinkinlabs" package="QFN32_5X5_LONGLEADS" value="MK20DN64VFM5">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="adafruit" package="C0402" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW2" library="blinkinlabs" package="TD-07XB" value="BRIGHTNESS">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="blinkinlabs" package="TSSOP16" value="74138">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="blinkinlabs" package="CRSYTAL_2520" value="16MHz">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="Z1" library="PaxInstrument-T400" package="SPARKFUN-RESISTORS_0603-RES" value="PGB1010603">
<attribute name="MPN" value="PGB1010603NRHF"/>
<attribute name="MF" value="Littelfuse"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Z2" library="PaxInstrument-T400" package="SPARKFUN-RESISTORS_0603-RES" value="PGB1010603">
<attribute name="MPN" value="PGB1010603NRHF"/>
<attribute name="MF" value="Littelfuse"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="R0402" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="R0402" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="adafruit" package="R0402" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="adafruit" package="R0402" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="blinkinlabs" package="SSOP24-150" value="ICN2026">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="adafruit" package="R0402" value="2k 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="adafruit" package="C0402" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U6" library="blinkinlabs" package="ESP_WROOM_02" value="ESP_WROOM_02">
<attribute name="NAME"/>
</element>
<element name="LED_1" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_2" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_3" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_4" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_5" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_6" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_7" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_8" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_9" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_10" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_11" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_12" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_13" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_14" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_15" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_16" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_17" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_18" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_19" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_20" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_21" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_22" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_23" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_24" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_25" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_26" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_27" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_28" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_29" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_30" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_31" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_32" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_33" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_34" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_35" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_36" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_37" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_38" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_39" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_40" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_41" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_42" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_43" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_44" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_45" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_46" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_47" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_48" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_49" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_50" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_51" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_52" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_53" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_54" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_55" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_56" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_57" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_58" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_59" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_60" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_61" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_62" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_63" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="LED_64" library="blinkinlabs" package="LED_3528" value="LED_RGB_CA"/>
<element name="R13" library="adafruit" package="R0402" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="adafruit" package="R0402" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="adafruit" package="R0402" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="adafruit" package="R0402" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="blinkinlabs" package="BATTERY_AA_SMD" value="BATTERY">
<attribute name="NAME"/>
</element>
<element name="U10" library="teensy_adapter" package="SC70-6L" value="FDG6316P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U9" library="teensy_adapter" package="SC70-6L" value="FDG6316P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U11" library="teensy_adapter" package="SC70-6L" value="FDG6316P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U12" library="teensy_adapter" package="SC70-6L" value="FDG6316P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="SparkFun-Passives" package="0603-ARV" value="200">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="SparkFun-Passives" package="0603-ARV" value="200">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U8" library="teensy_adapter" package="VFDFN-10" value="MMA8653FC"/>
<element name="R17" library="adafruit" package="R0402" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="adafruit" package="R0402" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="adafruit" package="C0402" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="adafruit" package="C0402" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="adafruit" package="C0402" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="adafruit" package="R0402" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="adafruit" package="R0402" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="adafruit" package="R0402" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="adafruit" package="R0402" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="adafruit" package="R0402" value="DNP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U7" library="blinkinlabs" package="SO08-150" value="MP3401A">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="L1" library="blinkinlabs" package="INDUCTOR_CD43" value="2.2uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="adafruit" package="CHIP-LED0603" value="ORANGE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="adafruit" package="R0603" value="1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="adafruit" package="C0603" value="2.2nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="adafruit" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="adafruit" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="adafruit" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U5" library="SparkFun-PowerIC" package="SOT23-5" value="MIC5219 3.3V">
<attribute name="PROD_ID" value="VREG-09872"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="adafruit" package="C0402" value="47pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="adafruit" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="adafruit" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="adafruit" package="SOD-123" value="RB161M-20">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="adafruit" package="SOD-123" value="RB161M-20">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="adafruit" package="R0805" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="adafruit" package="R0402" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP16" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="R21" library="adafruit" package="R0402" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="adafruit" package="CHIP-LED0603" value="PURPLE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP1" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="TP2" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="TP3" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP4" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="TP5" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="TP6" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="TP7" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP8" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="TP9" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="TP10" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="TP11" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="TP12" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="TP13" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="TP14" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="TP15" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="TP17" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP18" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="TP19" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="TP20" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="TP21" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="TP22" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="TP23" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="TP24" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="TP25" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="SparkFun-Passives" package="SJ_2S-TRACE" value="SOLDERJUMPERTRACE">
<attribute name="NAME"/>
</element>
<element name="Z3" library="PaxInstrument-T400" package="SPARKFUN-RESISTORS_0603-RES" value="PGB1010603">
<attribute name="MPN" value="PGB1010603NRHF"/>
<attribute name="MF" value="Littelfuse"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="DevicesToMerge" package="IO_HOLE_3MM" value="TEST_POINT"/>
<element name="U$6" library="DevicesToMerge" package="IO_HOLE_3MM" value="TEST_POINT"/>
<element name="U$9" library="DevicesToMerge" package="IO_HOLE_3MM" value="TEST_POINT"/>
<element name="U$10" library="DevicesToMerge" package="IO_HOLE_3MM" value="TEST_POINT"/>
</elements>
<signals>
<signal name="1ROW0">
<contactref element="LED_1" pad="2"/>
<contactref element="LED_2" pad="2"/>
<contactref element="LED_3" pad="2"/>
<contactref element="LED_4" pad="2"/>
<contactref element="LED_5" pad="2"/>
<contactref element="LED_6" pad="2"/>
<contactref element="LED_7" pad="2"/>
<contactref element="LED_8" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="U10" pad="6"/>
</signal>
<signal name="1ROW1">
<contactref element="LED_9" pad="2"/>
<contactref element="LED_10" pad="2"/>
<contactref element="LED_11" pad="2"/>
<contactref element="LED_12" pad="2"/>
<contactref element="LED_13" pad="2"/>
<contactref element="LED_14" pad="2"/>
<contactref element="LED_15" pad="2"/>
<contactref element="LED_16" pad="2"/>
<contactref element="U10" pad="3"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="1ROW2">
<contactref element="LED_17" pad="2"/>
<contactref element="LED_18" pad="2"/>
<contactref element="LED_19" pad="2"/>
<contactref element="LED_20" pad="2"/>
<contactref element="LED_21" pad="2"/>
<contactref element="LED_22" pad="2"/>
<contactref element="LED_23" pad="2"/>
<contactref element="LED_24" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="U9" pad="6"/>
</signal>
<signal name="1ROW3">
<contactref element="LED_25" pad="2"/>
<contactref element="LED_26" pad="2"/>
<contactref element="LED_27" pad="2"/>
<contactref element="LED_28" pad="2"/>
<contactref element="LED_29" pad="2"/>
<contactref element="LED_30" pad="2"/>
<contactref element="LED_31" pad="2"/>
<contactref element="LED_32" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="U9" pad="3"/>
</signal>
<signal name="GND">
<contactref element="U2" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="C8" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="U1" pad="PAD@9"/>
<contactref element="U1" pad="PAD@11"/>
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="PAD@1"/>
<contactref element="U1" pad="PAD@4"/>
<contactref element="U1" pad="8"/>
<contactref element="SW2" pad="3"/>
<contactref element="SW2" pad="4"/>
<contactref element="SW2" pad="5"/>
<contactref element="U3" pad="8"/>
<contactref element="U3" pad="5"/>
<contactref element="J1" pad="PIN$5"/>
<contactref element="Q1" pad="P$2"/>
<contactref element="Q1" pad="P$4"/>
<contactref element="Z1" pad="1"/>
<contactref element="Z2" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="U4" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="C11" pad="2"/>
<contactref element="U6" pad="GND$1"/>
<contactref element="U6" pad="GND$2"/>
<contactref element="U6" pad="GND$3"/>
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R13" pad="1"/>
<contactref element="R14" pad="1"/>
<contactref element="R15" pad="1"/>
<contactref element="R16" pad="1"/>
<contactref element="J2" pad="-"/>
<contactref element="U8" pad="P$7"/>
<contactref element="U8" pad="P$9"/>
<contactref element="U8" pad="P$6"/>
<contactref element="C13" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="R25" pad="1"/>
<contactref element="U7" pad="2"/>
<contactref element="U7" pad="7"/>
<contactref element="C10" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="U5" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="R11" pad="1"/>
<contactref element="R21" pad="1"/>
<contactref element="TP18" pad="TP"/>
<contactref element="SJ1" pad="1"/>
<contactref element="Z3" pad="1"/>
<contactref element="J1" pad="PAD$3"/>
<contactref element="J1" pad="PAD$9"/>
<contactref element="J1" pad="PAD$7"/>
<contactref element="J1" pad="PAD$5"/>
<contactref element="J1" pad="PAD$8"/>
<contactref element="J1" pad="PAD$10"/>
<contactref element="J1" pad="PAD$2"/>
<contactref element="J1" pad="PAD$1"/>
<contactref element="J1" pad="PAD$4"/>
<contactref element="J1" pad="PAD$6"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="LED_STB">
<contactref element="U2" pad="4"/>
<contactref element="U1" pad="29"/>
<contactref element="U4" pad="4"/>
<contactref element="TP3" pad="TP"/>
</signal>
<signal name="LED_CLK">
<contactref element="U2" pad="3"/>
<contactref element="U4" pad="3"/>
<contactref element="U1" pad="26"/>
<contactref element="TP2" pad="TP"/>
</signal>
<signal name="LED_DAT_0">
<contactref element="U2" pad="2"/>
<contactref element="U1" pad="27"/>
<contactref element="TP1" pad="TP"/>
</signal>
<signal name="LED_OE">
<contactref element="U2" pad="21"/>
<contactref element="U1" pad="16"/>
<contactref element="U4" pad="21"/>
<contactref element="R6" pad="1"/>
<contactref element="U3" pad="4"/>
<contactref element="TP4" pad="TP"/>
</signal>
<signal name="N$18">
<contactref element="U2" pad="23"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="R7" pad="1"/>
<contactref element="J1" pad="PIN$2"/>
<contactref element="Z1" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="R8" pad="1"/>
<contactref element="J1" pad="PIN$3"/>
<contactref element="Z2" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="C8" pad="1"/>
<contactref element="U1" pad="6"/>
<contactref element="C4" pad="1"/>
<contactref element="U3" pad="16"/>
<contactref element="U10" pad="1"/>
<contactref element="U10" pad="4"/>
<contactref element="U9" pad="1"/>
<contactref element="U9" pad="4"/>
<contactref element="U11" pad="1"/>
<contactref element="U11" pad="4"/>
<contactref element="U12" pad="1"/>
<contactref element="U12" pad="4"/>
<contactref element="U5" pad="3"/>
<contactref element="U5" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="SW1" pad="P0"/>
<contactref element="SW1" pad="P1"/>
<contactref element="TP7" pad="TP"/>
</signal>
<signal name="+3V3">
<contactref element="U6" pad="3V3"/>
<contactref element="R23" pad="2"/>
<contactref element="R26" pad="2"/>
<contactref element="R27" pad="2"/>
<contactref element="U8" pad="P$8"/>
<contactref element="U8" pad="P$1"/>
<contactref element="C14" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="R28" pad="2"/>
<contactref element="R17" pad="2"/>
<contactref element="R18" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="U5" pad="5"/>
<contactref element="R12" pad="2"/>
<contactref element="U$10" pad="1"/>
</signal>
<signal name="ARM_TCK">
<contactref element="U1" pad="12"/>
<contactref element="TP11" pad="TP"/>
</signal>
<signal name="ARM_TMS">
<contactref element="U1" pad="15"/>
<contactref element="TP10" pad="TP"/>
</signal>
<signal name="LED_S0">
<contactref element="U3" pad="15"/>
<contactref element="U10" pad="2"/>
</signal>
<signal name="LED_S1">
<contactref element="U3" pad="14"/>
<contactref element="U10" pad="5"/>
</signal>
<signal name="LED_S2">
<contactref element="U3" pad="13"/>
<contactref element="U9" pad="2"/>
</signal>
<signal name="LED_S3">
<contactref element="U3" pad="12"/>
<contactref element="U9" pad="5"/>
</signal>
<signal name="ARM_RESET">
<contactref element="U1" pad="19"/>
<contactref element="TP14" pad="TP"/>
</signal>
<signal name="VBAT">
<contactref element="U7" pad="3"/>
<contactref element="L1" pad="P$1"/>
<contactref element="J2" pad="+"/>
<contactref element="C12" pad="1"/>
<contactref element="TP8" pad="TP"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="17"/>
<contactref element="Q1" pad="P$3"/>
</signal>
<signal name="N$61">
<contactref element="U1" pad="18"/>
<contactref element="Q1" pad="P$1"/>
</signal>
<signal name="USB_D-">
<contactref element="R7" pad="2"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="USB_D+">
<contactref element="R8" pad="2"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="BUTTON">
<contactref element="SW2" pad="1"/>
<contactref element="SW2" pad="2"/>
<contactref element="R28" pad="1"/>
<contactref element="U6" pad="IO4"/>
<contactref element="TP25" pad="TP"/>
</signal>
<signal name="LED_ROW_A">
<contactref element="U3" pad="1"/>
<contactref element="U1" pad="30"/>
<contactref element="TP19" pad="TP"/>
</signal>
<signal name="LED_ROW_B">
<contactref element="U3" pad="2"/>
<contactref element="U1" pad="31"/>
<contactref element="TP20" pad="TP"/>
</signal>
<signal name="N$2">
<contactref element="U4" pad="23"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="GCOL0">
<contactref element="U4" pad="5"/>
<contactref element="LED_1" pad="4"/>
<contactref element="LED_9" pad="4"/>
<contactref element="LED_17" pad="4"/>
<contactref element="LED_25" pad="4"/>
<contactref element="LED_33" pad="4"/>
<contactref element="LED_41" pad="4"/>
<contactref element="LED_49" pad="4"/>
<contactref element="LED_57" pad="4"/>
</signal>
<signal name="GCOL1">
<contactref element="U4" pad="6"/>
<contactref element="LED_2" pad="4"/>
<contactref element="LED_10" pad="4"/>
<contactref element="LED_18" pad="4"/>
<contactref element="LED_26" pad="4"/>
<contactref element="LED_34" pad="4"/>
<contactref element="LED_42" pad="4"/>
<contactref element="LED_50" pad="4"/>
<contactref element="LED_58" pad="4"/>
</signal>
<signal name="GCOL2">
<contactref element="U4" pad="7"/>
<contactref element="LED_3" pad="4"/>
<contactref element="LED_11" pad="4"/>
<contactref element="LED_19" pad="4"/>
<contactref element="LED_27" pad="4"/>
<contactref element="LED_35" pad="4"/>
<contactref element="LED_43" pad="4"/>
<contactref element="LED_51" pad="4"/>
<contactref element="LED_59" pad="4"/>
</signal>
<signal name="GCOL3">
<contactref element="U4" pad="8"/>
<contactref element="LED_4" pad="4"/>
<contactref element="LED_12" pad="4"/>
<contactref element="LED_20" pad="4"/>
<contactref element="LED_28" pad="4"/>
<contactref element="LED_36" pad="4"/>
<contactref element="LED_44" pad="4"/>
<contactref element="LED_52" pad="4"/>
<contactref element="LED_60" pad="4"/>
</signal>
<signal name="GCOL4">
<contactref element="U4" pad="9"/>
<contactref element="LED_5" pad="4"/>
<contactref element="LED_13" pad="4"/>
<contactref element="LED_21" pad="4"/>
<contactref element="LED_29" pad="4"/>
<contactref element="LED_37" pad="4"/>
<contactref element="LED_45" pad="4"/>
<contactref element="LED_53" pad="4"/>
<contactref element="LED_61" pad="4"/>
</signal>
<signal name="GCOL5">
<contactref element="U4" pad="10"/>
<contactref element="LED_6" pad="4"/>
<contactref element="LED_14" pad="4"/>
<contactref element="LED_22" pad="4"/>
<contactref element="LED_30" pad="4"/>
<contactref element="LED_38" pad="4"/>
<contactref element="LED_46" pad="4"/>
<contactref element="LED_54" pad="4"/>
<contactref element="LED_62" pad="4"/>
</signal>
<signal name="GCOL6">
<contactref element="U4" pad="11"/>
<contactref element="LED_7" pad="4"/>
<contactref element="LED_15" pad="4"/>
<contactref element="LED_23" pad="4"/>
<contactref element="LED_31" pad="4"/>
<contactref element="LED_39" pad="4"/>
<contactref element="LED_47" pad="4"/>
<contactref element="LED_55" pad="4"/>
<contactref element="LED_63" pad="4"/>
</signal>
<signal name="GCOL7">
<contactref element="U4" pad="12"/>
<contactref element="LED_8" pad="4"/>
<contactref element="LED_16" pad="4"/>
<contactref element="LED_24" pad="4"/>
<contactref element="LED_32" pad="4"/>
<contactref element="LED_40" pad="4"/>
<contactref element="LED_48" pad="4"/>
<contactref element="LED_56" pad="4"/>
<contactref element="LED_64" pad="4"/>
</signal>
<signal name="BCOL0">
<contactref element="LED_1" pad="3"/>
<contactref element="LED_9" pad="3"/>
<contactref element="LED_17" pad="3"/>
<contactref element="LED_25" pad="3"/>
<contactref element="LED_33" pad="3"/>
<contactref element="LED_41" pad="3"/>
<contactref element="LED_49" pad="3"/>
<contactref element="LED_57" pad="3"/>
<contactref element="U2" pad="13"/>
</signal>
<signal name="BCOL1">
<contactref element="LED_2" pad="3"/>
<contactref element="LED_10" pad="3"/>
<contactref element="LED_18" pad="3"/>
<contactref element="LED_26" pad="3"/>
<contactref element="LED_34" pad="3"/>
<contactref element="LED_42" pad="3"/>
<contactref element="LED_50" pad="3"/>
<contactref element="LED_58" pad="3"/>
<contactref element="U2" pad="14"/>
</signal>
<signal name="BCOL2">
<contactref element="LED_3" pad="3"/>
<contactref element="LED_11" pad="3"/>
<contactref element="LED_19" pad="3"/>
<contactref element="LED_27" pad="3"/>
<contactref element="LED_35" pad="3"/>
<contactref element="LED_43" pad="3"/>
<contactref element="LED_51" pad="3"/>
<contactref element="LED_59" pad="3"/>
<contactref element="U2" pad="15"/>
</signal>
<signal name="BCOL3">
<contactref element="LED_4" pad="3"/>
<contactref element="LED_12" pad="3"/>
<contactref element="LED_20" pad="3"/>
<contactref element="LED_28" pad="3"/>
<contactref element="LED_36" pad="3"/>
<contactref element="LED_44" pad="3"/>
<contactref element="LED_52" pad="3"/>
<contactref element="LED_60" pad="3"/>
<contactref element="U2" pad="16"/>
</signal>
<signal name="BCOL4">
<contactref element="LED_5" pad="3"/>
<contactref element="LED_13" pad="3"/>
<contactref element="LED_21" pad="3"/>
<contactref element="LED_29" pad="3"/>
<contactref element="LED_37" pad="3"/>
<contactref element="LED_45" pad="3"/>
<contactref element="LED_53" pad="3"/>
<contactref element="LED_61" pad="3"/>
<contactref element="U2" pad="17"/>
</signal>
<signal name="BCOL5">
<contactref element="LED_6" pad="3"/>
<contactref element="LED_14" pad="3"/>
<contactref element="LED_22" pad="3"/>
<contactref element="LED_30" pad="3"/>
<contactref element="LED_38" pad="3"/>
<contactref element="LED_46" pad="3"/>
<contactref element="LED_54" pad="3"/>
<contactref element="LED_62" pad="3"/>
<contactref element="U2" pad="18"/>
</signal>
<signal name="BCOL6">
<contactref element="LED_7" pad="3"/>
<contactref element="LED_15" pad="3"/>
<contactref element="LED_23" pad="3"/>
<contactref element="LED_31" pad="3"/>
<contactref element="LED_39" pad="3"/>
<contactref element="LED_47" pad="3"/>
<contactref element="LED_55" pad="3"/>
<contactref element="LED_63" pad="3"/>
<contactref element="U2" pad="19"/>
</signal>
<signal name="BCOL7">
<contactref element="LED_8" pad="3"/>
<contactref element="LED_16" pad="3"/>
<contactref element="LED_24" pad="3"/>
<contactref element="LED_32" pad="3"/>
<contactref element="LED_40" pad="3"/>
<contactref element="LED_48" pad="3"/>
<contactref element="LED_56" pad="3"/>
<contactref element="LED_64" pad="3"/>
<contactref element="U2" pad="20"/>
</signal>
<signal name="LED_DAT_1">
<contactref element="U2" pad="22"/>
<contactref element="U4" pad="2"/>
</signal>
<signal name="RCOL0">
<contactref element="R19" pad="5"/>
<contactref element="LED_1" pad="1"/>
<contactref element="LED_9" pad="1"/>
<contactref element="LED_17" pad="1"/>
<contactref element="LED_25" pad="1"/>
<contactref element="LED_33" pad="1"/>
<contactref element="LED_41" pad="1"/>
<contactref element="LED_49" pad="1"/>
<contactref element="LED_57" pad="1"/>
</signal>
<signal name="RCOL1">
<contactref element="R19" pad="6"/>
<contactref element="LED_2" pad="1"/>
<contactref element="LED_10" pad="1"/>
<contactref element="LED_18" pad="1"/>
<contactref element="LED_26" pad="1"/>
<contactref element="LED_34" pad="1"/>
<contactref element="LED_42" pad="1"/>
<contactref element="LED_50" pad="1"/>
<contactref element="LED_58" pad="1"/>
</signal>
<signal name="RCOL2">
<contactref element="R19" pad="7"/>
<contactref element="LED_3" pad="1"/>
<contactref element="LED_11" pad="1"/>
<contactref element="LED_19" pad="1"/>
<contactref element="LED_27" pad="1"/>
<contactref element="LED_35" pad="1"/>
<contactref element="LED_43" pad="1"/>
<contactref element="LED_51" pad="1"/>
<contactref element="LED_59" pad="1"/>
</signal>
<signal name="RCOL3">
<contactref element="R19" pad="8"/>
<contactref element="LED_4" pad="1"/>
<contactref element="LED_12" pad="1"/>
<contactref element="LED_20" pad="1"/>
<contactref element="LED_28" pad="1"/>
<contactref element="LED_36" pad="1"/>
<contactref element="LED_44" pad="1"/>
<contactref element="LED_52" pad="1"/>
<contactref element="LED_60" pad="1"/>
</signal>
<signal name="RCOL4">
<contactref element="R20" pad="5"/>
<contactref element="LED_5" pad="1"/>
<contactref element="LED_13" pad="1"/>
<contactref element="LED_21" pad="1"/>
<contactref element="LED_29" pad="1"/>
<contactref element="LED_37" pad="1"/>
<contactref element="LED_45" pad="1"/>
<contactref element="LED_53" pad="1"/>
<contactref element="LED_61" pad="1"/>
</signal>
<signal name="RCOL5">
<contactref element="R20" pad="6"/>
<contactref element="LED_6" pad="1"/>
<contactref element="LED_14" pad="1"/>
<contactref element="LED_22" pad="1"/>
<contactref element="LED_30" pad="1"/>
<contactref element="LED_38" pad="1"/>
<contactref element="LED_46" pad="1"/>
<contactref element="LED_54" pad="1"/>
<contactref element="LED_62" pad="1"/>
</signal>
<signal name="RCOL6">
<contactref element="R20" pad="7"/>
<contactref element="LED_7" pad="1"/>
<contactref element="LED_15" pad="1"/>
<contactref element="LED_23" pad="1"/>
<contactref element="LED_31" pad="1"/>
<contactref element="LED_39" pad="1"/>
<contactref element="LED_47" pad="1"/>
<contactref element="LED_55" pad="1"/>
<contactref element="LED_63" pad="1"/>
</signal>
<signal name="RCOL7">
<contactref element="R20" pad="8"/>
<contactref element="LED_8" pad="1"/>
<contactref element="LED_16" pad="1"/>
<contactref element="LED_24" pad="1"/>
<contactref element="LED_32" pad="1"/>
<contactref element="LED_40" pad="1"/>
<contactref element="LED_48" pad="1"/>
<contactref element="LED_56" pad="1"/>
<contactref element="LED_64" pad="1"/>
</signal>
<signal name="1ROW4">
<contactref element="LED_33" pad="2"/>
<contactref element="LED_34" pad="2"/>
<contactref element="LED_35" pad="2"/>
<contactref element="LED_36" pad="2"/>
<contactref element="LED_37" pad="2"/>
<contactref element="LED_38" pad="2"/>
<contactref element="LED_39" pad="2"/>
<contactref element="LED_40" pad="2"/>
<contactref element="R13" pad="2"/>
<contactref element="U11" pad="6"/>
</signal>
<signal name="1ROW5">
<contactref element="LED_41" pad="2"/>
<contactref element="LED_42" pad="2"/>
<contactref element="LED_43" pad="2"/>
<contactref element="LED_44" pad="2"/>
<contactref element="LED_45" pad="2"/>
<contactref element="LED_46" pad="2"/>
<contactref element="LED_47" pad="2"/>
<contactref element="LED_48" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="U11" pad="3"/>
</signal>
<signal name="1ROW6">
<contactref element="LED_49" pad="2"/>
<contactref element="LED_50" pad="2"/>
<contactref element="LED_51" pad="2"/>
<contactref element="LED_52" pad="2"/>
<contactref element="LED_53" pad="2"/>
<contactref element="LED_54" pad="2"/>
<contactref element="LED_55" pad="2"/>
<contactref element="LED_56" pad="2"/>
<contactref element="R15" pad="2"/>
<contactref element="U12" pad="6"/>
</signal>
<signal name="1ROW7">
<contactref element="LED_57" pad="2"/>
<contactref element="LED_58" pad="2"/>
<contactref element="LED_59" pad="2"/>
<contactref element="LED_60" pad="2"/>
<contactref element="LED_61" pad="2"/>
<contactref element="LED_62" pad="2"/>
<contactref element="LED_63" pad="2"/>
<contactref element="LED_64" pad="2"/>
<contactref element="R16" pad="2"/>
<contactref element="U12" pad="3"/>
</signal>
<signal name="ARM_TX">
<contactref element="U1" pad="14"/>
<contactref element="U6" pad="RXD"/>
<contactref element="TP12" pad="TP"/>
</signal>
<signal name="ARM_RX">
<contactref element="U1" pad="13"/>
<contactref element="U6" pad="TXD"/>
<contactref element="TP13" pad="TP"/>
</signal>
<signal name="LED_S4">
<contactref element="U3" pad="11"/>
<contactref element="U11" pad="2"/>
</signal>
<signal name="LED_S5">
<contactref element="U3" pad="10"/>
<contactref element="U11" pad="5"/>
</signal>
<signal name="LED_S6">
<contactref element="U3" pad="9"/>
<contactref element="U12" pad="2"/>
</signal>
<signal name="LED_S7">
<contactref element="U3" pad="7"/>
<contactref element="U12" pad="5"/>
</signal>
<signal name="LED_ROW_C">
<contactref element="U3" pad="3"/>
<contactref element="U1" pad="32"/>
<contactref element="TP21" pad="TP"/>
</signal>
<signal name="RCOL0_">
<contactref element="U2" pad="5"/>
<contactref element="R19" pad="4"/>
</signal>
<signal name="RCOL1_">
<contactref element="U2" pad="6"/>
<contactref element="R19" pad="3"/>
</signal>
<signal name="RCOL2_">
<contactref element="U2" pad="7"/>
<contactref element="R19" pad="2"/>
</signal>
<signal name="RCOL3_">
<contactref element="U2" pad="8"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="RCOL4_">
<contactref element="U2" pad="9"/>
<contactref element="R20" pad="4"/>
</signal>
<signal name="RCOL5_">
<contactref element="U2" pad="10"/>
<contactref element="R20" pad="3"/>
</signal>
<signal name="RCOL6_">
<contactref element="U2" pad="11"/>
<contactref element="R20" pad="2"/>
</signal>
<signal name="RCOL7_">
<contactref element="U2" pad="12"/>
<contactref element="R20" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U8" pad="P$4"/>
<contactref element="C13" pad="1"/>
</signal>
<signal name="ACC_INT1">
<contactref element="U8" pad="P$3"/>
<contactref element="U6" pad="IO13"/>
</signal>
<signal name="I2C_SCL">
<contactref element="U8" pad="P$2"/>
<contactref element="R18" pad="1"/>
<contactref element="U6" pad="IO14"/>
<contactref element="TP6" pad="TP"/>
</signal>
<signal name="ESP_GPIO0">
<contactref element="U6" pad="IO0"/>
<contactref element="R23" pad="1"/>
<contactref element="U1" pad="21"/>
<contactref element="TP15" pad="TP"/>
</signal>
<signal name="ESP_GPIO15">
<contactref element="U6" pad="IO15"/>
<contactref element="R25" pad="2"/>
</signal>
<signal name="ESP_ENABLE">
<contactref element="U6" pad="EN"/>
<contactref element="R26" pad="1"/>
</signal>
<signal name="ESP_RESET">
<contactref element="U6" pad="RST"/>
<contactref element="R27" pad="1"/>
<contactref element="U1" pad="20"/>
<contactref element="TP17" pad="TP"/>
</signal>
<signal name="ARM_3V3">
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="11"/>
<contactref element="C5" pad="1"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="7"/>
<contactref element="C3" pad="1"/>
<contactref element="U2" pad="24"/>
<contactref element="R6" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="U4" pad="24"/>
<contactref element="C11" pad="1"/>
<contactref element="TP9" pad="TP"/>
</signal>
<signal name="CHARGE">
<contactref element="U7" pad="6"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="USB_5V">
<contactref element="U7" pad="4"/>
<contactref element="C17" pad="1"/>
<contactref element="D3" pad="A"/>
<contactref element="J1" pad="PIN$1"/>
<contactref element="Z3" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U7" pad="1"/>
<contactref element="L1" pad="P$2"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="BOOST_5V">
<contactref element="U7" pad="8"/>
<contactref element="C9" pad="1"/>
<contactref element="D2" pad="A"/>
<contactref element="TP24" pad="TP"/>
</signal>
<signal name="N$7">
<contactref element="R10" pad="2"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="U5" pad="4"/>
<contactref element="C16" pad="1"/>
</signal>
<signal name="+5V_SWITCH">
<contactref element="D2" pad="C"/>
<contactref element="SW1" pad="S1"/>
<contactref element="SW1" pad="S0"/>
<contactref element="D3" pad="C"/>
</signal>
<signal name="EXP_GPIO5">
<contactref element="U6" pad="IO5"/>
<contactref element="U$6" pad="1"/>
</signal>
<signal name="ESP_GPIO16">
<contactref element="U6" pad="IO18"/>
<contactref element="U$9" pad="1"/>
</signal>
<signal name="ESP_TOUT">
<contactref element="U6" pad="TOUT"/>
</signal>
<signal name="ARM_RX1">
<contactref element="U1" pad="24"/>
<contactref element="U6" pad="IO2"/>
<contactref element="R12" pad="1"/>
<contactref element="TP23" pad="TP"/>
</signal>
<signal name="I2C_SDA">
<contactref element="U6" pad="IO12"/>
<contactref element="R17" pad="1"/>
<contactref element="U8" pad="P$10"/>
<contactref element="TP5" pad="TP"/>
</signal>
<signal name="ARM_BOOTLOADER">
<contactref element="TP16" pad="TP"/>
<contactref element="U1" pad="25"/>
</signal>
<signal name="LED_HS_EN">
<contactref element="R21" pad="2"/>
<contactref element="U3" pad="6"/>
<contactref element="U1" pad="22"/>
<contactref element="TP22" pad="TP"/>
</signal>
<signal name="+5V_BLEED">
<contactref element="SW1" pad="O1"/>
<contactref element="SW1" pad="O0"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="DISCHARGE">
<contactref element="U7" pad="5"/>
<contactref element="D4" pad="A"/>
</signal>
<signal name="N$1">
<contactref element="D4" pad="C"/>
<contactref element="D1" pad="C"/>
<contactref element="SJ1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
