(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 42)
    (no_connects 0)
    (area 112.554999 61.244999 181.7 124.415)
    (thickness 1.6)
    (drawings 5)
    (tracks 215)
    (zones 0)
    (modules 10)
    (nets 26)
  )
  (page A4)
  (title_block
    (title Panel)
    (date 2017-03-28)
    (rev 1)
    (company "CU Rocket Engineering")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(D1-Pad3)")
  (net 4 "Net-(D1-Pad4)")
  (net 5 "Net-(D2-Pad1)")
  (net 6 "Net-(D2-Pad3)")
  (net 7 "Net-(D2-Pad4)")
  (net 8 "Net-(D3-Pad1)")
  (net 9 "Net-(D3-Pad3)")
  (net 10 "Net-(D3-Pad4)")
  (net 11 "Net-(D4-Pad1)")
  (net 12 "Net-(D4-Pad3)")
  (net 13 "Net-(D4-Pad4)")
  (net 14 "Net-(D5-Pad1)")
  (net 15 "Net-(D5-Pad3)")
  (net 16 "Net-(D5-Pad4)")
  (net 17 VCC)
  (net 18 "Net-(J1-Pad3)")
  (net 19 "Net-(J1-Pad4)")
  (net 20 "Net-(J1-Pad5)")
  (net 21 "Net-(J1-Pad6)")
  (net 22 "Net-(J1-Pad7)")
  (net 23 "Net-(U1-Pad9)")
  (net 24 "Net-(U2-Pad9)")
  (net 25 "Net-(U2-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad3)")
    (add_net "Net-(D1-Pad4)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad3)")
    (add_net "Net-(D2-Pad4)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad3)")
    (add_net "Net-(D3-Pad4)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad3)")
    (add_net "Net-(D4-Pad4)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D5-Pad3)")
    (add_net "Net-(D5-Pad4)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad9)")
    (add_net VCC)
  )
  (module LEDs:LED_D5.0mm-4 (layer F.Cu) (tedit 587A3A7B)
    (at 129.54 119.38)
    (descr "LED, diameter 5.0mm, 2 pins, diameter 5.0mm, 3 pins, diameter 5.0mm, 4 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-154A4SUREQBFZGEW(Ver.9A).pdf")
    (tags "LED diameter 5.0mm 2 pins diameter 5.0mm 3 pins diameter 5.0mm 4 pins")
    (fp_text reference D1 (at 1.905 -3.96) (layer F.SilkS))
    (fp_text value Debug1 (at 1.905 3.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad3)"))
    (pad 4 thru_hole oval (at 3.81 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad4)"))
    (model LEDs.3dshapes/LED_D5.0mm-4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm-4 (layer F.Cu) (tedit 587A3A7B)
    (at 138.43 119.38)
    (descr "LED, diameter 5.0mm, 2 pins, diameter 5.0mm, 3 pins, diameter 5.0mm, 4 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-154A4SUREQBFZGEW(Ver.9A).pdf")
    (tags "LED diameter 5.0mm 2 pins diameter 5.0mm 3 pins diameter 5.0mm 4 pins")
    (fp_text reference D2 (at 1.905 -3.96) (layer F.SilkS))
    (fp_text value Debug2 (at 1.905 3.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(D2-Pad3)"))
    (pad 4 thru_hole oval (at 3.81 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(D2-Pad4)"))
    (model LEDs.3dshapes/LED_D5.0mm-4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm-4 (layer F.Cu) (tedit 587A3A7B)
    (at 147.32 119.38)
    (descr "LED, diameter 5.0mm, 2 pins, diameter 5.0mm, 3 pins, diameter 5.0mm, 4 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-154A4SUREQBFZGEW(Ver.9A).pdf")
    (tags "LED diameter 5.0mm 2 pins diameter 5.0mm 3 pins diameter 5.0mm 4 pins")
    (fp_text reference D3 (at 1.905 -3.96) (layer F.SilkS))
    (fp_text value Debug3 (at 1.905 3.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(D3-Pad3)"))
    (pad 4 thru_hole oval (at 3.81 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 "Net-(D3-Pad4)"))
    (model LEDs.3dshapes/LED_D5.0mm-4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm-4 (layer F.Cu) (tedit 587A3A7B)
    (at 156.21 119.38)
    (descr "LED, diameter 5.0mm, 2 pins, diameter 5.0mm, 3 pins, diameter 5.0mm, 4 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-154A4SUREQBFZGEW(Ver.9A).pdf")
    (tags "LED diameter 5.0mm 2 pins diameter 5.0mm 3 pins diameter 5.0mm 4 pins")
    (fp_text reference D4 (at 1.905 -3.96) (layer F.SilkS))
    (fp_text value Debug4 (at 1.905 3.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 "Net-(D4-Pad1)"))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "Net-(D4-Pad3)"))
    (pad 4 thru_hole oval (at 3.81 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 "Net-(D4-Pad4)"))
    (model LEDs.3dshapes/LED_D5.0mm-4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm-4 (layer F.Cu) (tedit 587A3A7B)
    (at 165.1 119.38)
    (descr "LED, diameter 5.0mm, 2 pins, diameter 5.0mm, 3 pins, diameter 5.0mm, 4 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-154A4SUREQBFZGEW(Ver.9A).pdf")
    (tags "LED diameter 5.0mm 2 pins diameter 5.0mm 3 pins diameter 5.0mm 4 pins")
    (fp_text reference D5 (at 1.905 -3.96) (layer F.SilkS))
    (fp_text value Debug5 (at 1.905 3.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "Net-(D5-Pad1)"))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Net-(D5-Pad3)"))
    (pad 4 thru_hole oval (at 3.81 0) (size 1.07 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 "Net-(D5-Pad4)"))
    (model LEDs.3dshapes/LED_D5.0mm-4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:DB9FC (layer B.Cu) (tedit 587FDE78)
    (at 138.43 72.39 270)
    (descr "Connecteur DB9 femelle couche")
    (tags "CONN DB9")
    (fp_text reference J1 (at 5.46 -2.28 270) (layer B.SilkS))
    (fp_text value PanelTerm (at 6.73 5.08 270) (layer B.Fab))
    (pad "" thru_hole circle (at 18.29 2.54 270) (size 3.81 3.81) (drill 3.05) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -7.11 2.54 270) (size 3.81 3.81) (drill 3.05) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 17 VCC))
    (pad 2 thru_hole circle (at 2.79 0 270) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 5.46 0 270) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at 8.26 0 270) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad4)"))
    (pad 5 thru_hole circle (at 11.05 0 270) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad5)"))
    (pad 6 thru_hole circle (at 1.4 2.54 270) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad6)"))
    (pad 7 thru_hole circle (at 4.19 2.54 270) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask)
      (net 22 "Net-(J1-Pad7)"))
    (pad 8 thru_hole circle (at 6.86 2.54 270) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 9.65 2.54 270) (size 1.52 1.52) (drill 1.02) (layers *.Cu *.Mask))
    (model Connectors.3dshapes/DB9FC.wrl
      (at (xyz 0.208661 0.05315 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH-12mm (layer F.Cu) (tedit 53FD9538)
    (at 138.43 105.41)
    (fp_text reference SW1 (at 0 -0.762) (layer F.SilkS))
    (fp_text value ReadyButton (at 0 1.016) (layer F.Fab))
    (pad 1 thru_hole oval (at 6.35 -2.54) (size 3.048 1.7272) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 6.35 2.54) (size 3.048 1.7272) (drill 0.8128) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad6)"))
    (pad 1 thru_hole oval (at -6.35 -2.54) (size 3.048 1.7272) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at -6.35 2.54) (size 3.048 1.7272) (drill 0.8128) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad6)"))
    (model Buttons_Switches_THT.3dshapes/SW_PUSH-12mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 4 4 4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH-12mm (layer F.Cu) (tedit 53FD9538)
    (at 160.02 105.41)
    (fp_text reference SW2 (at 0 -0.762) (layer F.SilkS))
    (fp_text value ResetButton (at 0 1.016) (layer F.Fab))
    (pad 1 thru_hole oval (at 6.35 -2.54) (size 3.048 1.7272) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 6.35 2.54) (size 3.048 1.7272) (drill 0.8128) (layers *.Cu *.Mask)
      (net 22 "Net-(J1-Pad7)"))
    (pad 1 thru_hole oval (at -6.35 -2.54) (size 3.048 1.7272) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at -6.35 2.54) (size 3.048 1.7272) (drill 0.8128) (layers *.Cu *.Mask)
      (net 22 "Net-(J1-Pad7)"))
    (model Buttons_Switches_THT.3dshapes/SW_PUSH-12mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 4 4 4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer B.Cu) (tedit 586281B4)
    (at 152.4 86.36)
    (descr "16-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 3.81 2.39) (layer B.SilkS))
    (fp_text value 74HC595 (at 3.81 -20.17) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad4)"))
    (pad 9 thru_hole oval (at 7.62 -17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(U1-Pad9)"))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 10 thru_hole oval (at 7.62 -15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 VCC))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(D2-Pad3)"))
    (pad 11 thru_hole oval (at 7.62 -12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad4)"))
    (pad 4 thru_hole oval (at 0 -7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(D2-Pad4)"))
    (pad 12 thru_hole oval (at 7.62 -10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad5)"))
    (pad 5 thru_hole oval (at 0 -10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad 13 thru_hole oval (at 7.62 -7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 0 -12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(D3-Pad3)"))
    (pad 14 thru_hole oval (at 7.62 -5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad3)"))
    (pad 7 thru_hole oval (at 0 -15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(D3-Pad4)"))
    (pad 15 thru_hole oval (at 7.62 -2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad3)"))
    (pad 8 thru_hole oval (at 0 -17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 16 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 VCC))
    (model Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer B.Cu) (tedit 586281B4)
    (at 171.45 86.36)
    (descr "16-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U2 (at 3.81 2.39) (layer B.SilkS))
    (fp_text value 74HC595 (at 3.81 -20.17) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(D4-Pad3)"))
    (pad 9 thru_hole oval (at 7.62 -17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(U2-Pad9)"))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(D4-Pad4)"))
    (pad 10 thru_hole oval (at 7.62 -15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 VCC))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(D4-Pad1)"))
    (pad 11 thru_hole oval (at 7.62 -12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad4)"))
    (pad 4 thru_hole oval (at 0 -7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(D5-Pad3)"))
    (pad 12 thru_hole oval (at 7.62 -10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad5)"))
    (pad 5 thru_hole oval (at 0 -10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(D5-Pad4)"))
    (pad 13 thru_hole oval (at 7.62 -7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 0 -12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(D5-Pad1)"))
    (pad 14 thru_hole oval (at 7.62 -5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(U1-Pad9)"))
    (pad 7 thru_hole oval (at 0 -15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(U2-Pad7)"))
    (pad 15 thru_hole oval (at 7.62 -2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(D3-Pad1)"))
    (pad 8 thru_hole oval (at 0 -17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 16 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 VCC))
    (model Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 120.65 124.46) (end 120.65 60.96) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 181.61 124.46) (end 120.65 124.46) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 181.61 60.96) (end 181.61 124.46) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 120.65 60.96) (end 181.61 60.96) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "CU Rocket Engineering\nPanel Board\nRevision 1" (at 177.8 92.71 90) (layer B.SilkS))
)
