<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="31.2166" y1="34.671" x2="41.4274" y2="34.671" width="0.0254" layer="20"/>
<wire x1="41.4274" y1="34.671" x2="41.4274" y2="24.4094" width="0.0254" layer="20"/>
<wire x1="41.4274" y1="24.4094" x2="31.2166" y2="24.4094" width="0.0254" layer="20"/>
<wire x1="31.2166" y1="24.4094" x2="31.2166" y2="34.671" width="0.0254" layer="20"/>
<text>i2c</text>
<text>addr:</text>
<text>gnd</text>
<text>Vin</text>
<text>sda</text>
<text>scl</text>
<text>1</text>
<text>v0.2</text>
<text>LED
Brd</text>
<text>LED</text>
<text>0</text>
<text>0</text>
<text>1</text>
<text>a0</text>
<text>a1</text>
<text>11000a1a0</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="1X01-CLEANBIG">
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="NXP_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 14:27:46</description>
<packages>
<package name="SOP50P490X110-10N">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-TRICOLOR-PLCC">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PAD-JUMPER-3-NO_NO_SILK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="NXP_By_element14_Batch_1" package="SOP50P490X110-10N" value="PCA9632DP2,118">
<attribute name="SUPPLIER" value="NXP"/>
<attribute name="MPN" value="PCA9632DP2,118"/>
<attribute name="OC_FARNELL" value="1867849"/>
<attribute name="PACKAGE" value="TSSOP-10"/>
<attribute name="OC_NEWARK" value="70R6723"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="adafruit" package="1X01-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="GND" library="adafruit" package="1X01-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="JP3" library="adafruit" package="1X01-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="JP4" library="adafruit" package="1X01-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="R0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="R0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="R0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SparkFun-LED" package="LED-TRICOLOR-PLCC" value="LED-TRICOLORPLCC"/>
<element name="JP6" library="SparkFun-Passives" package="PAD-JUMPER-3-NO_NO_SILK" value="JUMPER-PAD-3-NONOSILK">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Passives" package="PAD-JUMPER-3-NO_NO_SILK" value="JUMPER-PAD-3-NONOSILK">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="JP1" pad="1"/>
<contactref element="IC1" pad="10"/>
<contactref element="U$1" pad="PAD1"/>
<contactref element="JP6" pad="1"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="JP4" pad="1"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="SCL">
<contactref element="JP3" pad="1"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="GND">
<contactref element="GND" pad="1"/>
<contactref element="IC1" pad="6"/>
<contactref element="JP6" pad="3"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="PAD4"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="2"/>
<contactref element="U$1" pad="PAD2"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="PAD3"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="RED">
<contactref element="R1" pad="1"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="BLU">
<contactref element="R2" pad="1"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="GRN">
<contactref element="R3" pad="1"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="A1">
<contactref element="IC1" pad="7"/>
<contactref element="JP6" pad="2"/>
</signal>
<signal name="A0">
<contactref element="IC1" pad="5"/>
<contactref element="JP2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
