(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 11)
    (tracks 46)
    (zones 0)
    (modules 7)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (trace_clearance 0.25)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.25)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 125.222 90.424)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x01020_fffffffe)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.050000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 "Net-(J1-Pad4)")
  (net 4 "Net-(J1-Pad3)")
  (net 5 "Net-(U1-Pad6)")
  (net 6 "Net-(JP1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.25)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.45)
    (diff_pair_width 0.35)
    (add_net GND)
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(JP1-Pad2)")
    (add_net "Net-(U1-Pad6)")
    (add_net VCC)
  )
  (module "CPB:Jumper 1-2-3 0.5mm" (layer B.Cu) (tedit 5D4B6EE2)
    (at 137.5 87.7 90)
    (fp_text reference JP1 (at 0.1 2.1 180) (layer B.SilkS))
    (fp_text value ADDR (at -0.1 1.4 90) (layer B.Fab))
    (pad 3 smd trapezoid (at 1.5 0 270) (size 1 0.7) (rect_delta -0.3 0 ) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 1 smd trapezoid (at -1.5 0 90) (size 1 0.7) (rect_delta -0.3 0 ) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 0 90) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(JP1-Pad2)"))
  )
  (module CPB:AHT10 (layer B.Cu) (tedit 5D48D185)
    (at 132.2 87)
    (fp_text reference U1 (at -3 -0.1) (layer B.SilkS))
    (fp_text value AHT10 (at -1.8 3.6) (layer B.Fab))
    (pad 6 smd rect (at 1.35 1.27) (size 1 0.8) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(U1-Pad6)"))
    (pad 5 smd rect (at 1.35 0) (size 1 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.35 -1.27) (size 1 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 3 smd rect (at -1.35 -1.27) (size 1 0.8) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 2 smd rect (at -1.35 0) (size 1 0.8) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J1-Pad4)"))
    (pad 1 smd oval (at -1.35 1.27) (size 1 0.8) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(JP1-Pad2)"))
  )
  (module CPB:Socket_Strip_Straight_1x04_Oval_Pitch2.54mm (layer F.Cu) (tedit 5D38F24C)
    (at 127 81.28)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x04 (at 0 9.95) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33) (layer F.Fab) hide)
    (pad 4 thru_hole oval (at 0 7.62) (size 2.2 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.2 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.2 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.9 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x04_Pitch2.54mm.wrl
      (offset (xyz 0 -3.809999942779541 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5D38F1FB)
    (at 139.954 85.09)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 58AA8463)
    (at 135.89 84.058 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -1.058 -1.81) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.5 270) (layer B.Fab))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 58E0A804)
    (at 132.6 82.05 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -0.95 -1.766) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J1-Pad4)"))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 58E0A804)
    (at 130.6 82.05 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -0.85 1.8 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text x39 (at 136.1 86.7 270) (layer B.SilkS))
  (gr_text x38 (at 136.1 89 270) (layer B.SilkS))
  (gr_text VCC (at 129.794 81.28) (layer F.SilkS))
  (gr_text GND (at 129.794 83.82) (layer F.SilkS))
  (gr_text SCL (at 129.794 86.36) (layer F.SilkS))
  (gr_line (start 125.222 90.424) (end 137.16 90.424) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125.222 79.756) (end 125.222 90.424) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.16 79.756) (end 125.222 79.756) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 137.16 85.09) (end 137.16 90.424) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_text "AHT10\ncperiod\n2019" (at 134.62 85.09 270) (layer F.SilkS))
  (gr_text SDA (at 129.794 89) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123 77) (xy 144 77) (xy 144 93) (xy 123 93)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124.968 79.502) (xy 143.764 79.502) (xy 144.018 91.694) (xy 124.968 91.186)
      )
    )
  )
)
