(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 16)
    (no_connects 0)
    (area 149.022999 86.284999 175.843001 110.311001)
    (thickness 1.6)
    (drawings 23)
    (tracks 38)
    (zones 0)
    (modules 9)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.08)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 LED)
  (net 3 Vin)
  (net 4 "Net-(P3-Pad2)")
  (net 5 FX-Out)
  (net 6 FX-In)
  (net 7 "Net-(R1-Pad2)")
  (net 8 "Net-(P4-Pad1)")
  (net 9 "Net-(R2-Pad2)")
  (net 10 "Net-(R3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net FX-In)
    (add_net FX-Out)
    (add_net GND)
    (add_net LED)
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net Vin)
  )
  (module 3PDT:Switches_Stomp_Switch_3PDT (layer F.Cu) (tedit 5B2C3F5F)
    (at 162.433 101.473)
    (fp_text reference SW1 (at 7.62 8.001) (layer F.SilkS) hide)
    (fp_text value 3PDT (at 0 13) (layer F.SilkS))
    (pad 8 thru_hole oval (at 0 5) (size 2.5 3) (drill 2.5) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at 0 -5) (size 2.5 3) (drill 2.5) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(R2-Pad2)"))
    (pad 3 thru_hole oval (at 5 -5) (size 2.5 3) (drill 2.5) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(R3-Pad1)"))
    (pad 9 thru_hole oval (at 5 5) (size 2.5 3) (drill 2.5) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P4-Pad1)"))
    (pad 7 thru_hole oval (at -5 5) (size 2.5 3) (drill 2.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole oval (at -5 -5) (size 2.5 3) (drill 2.5) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P4-Pad1)"))
    (pad 4 thru_hole oval (at -5 0) (size 2.5 3) (drill 2.5) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(R1-Pad2)"))
    (pad 5 thru_hole oval (at 0 0) (size 2.5 3) (drill 2.5) (layers *.Cu *.Mask F.SilkS)
      (net 3 Vin))
    (pad 6 thru_hole oval (at 5 0) (size 2.5 3) (drill 2.5) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(P3-Pad2)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5B2C4112)
    (at 173.99 91.059 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P1 (at -2.54 1.143 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 4.93 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 LED))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5B2C410C)
    (at 150.876 91.059 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P2 (at 2.667 1.143 180) (layer F.SilkS) hide)
    (fp_text value Power (at 0 4.93 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 Vin))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5B2C4153)
    (at 173.99 94.361)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P3 (at 3.937 1.524) (layer F.SilkS) hide)
    (fp_text value OutJack (at 0 4.93) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(P3-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5B2C4110)
    (at 150.876 96.901 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P4 (at 2.54 1.397 180) (layer F.SilkS) hide)
    (fp_text value InJack (at 0 4.93 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(P4-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 593B5ED9)
    (at 166.37 88.519 270)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P5 (at -2.032 3.81 360) (layer F.SilkS) hide)
    (fp_text value CONN_01X04 (at 0 10.01 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 FX-Out))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 Vin))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 FX-In))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5B2C40C9)
    (at 156.464 88.519 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at -1.27 0 360) (layer F.SilkS))
    (fp_text value 33k (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 FX-In))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5B2C43DE)
    (at 171.577 89.027 270)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at 0.635 1.143 360) (layer F.SilkS))
    (fp_text value 220R (at 0 1.8 270) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 LED))
    (pad 2 smd rect (at 0.45 0 270) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5B2C40D7)
    (at 168.783 88.519 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R3 (at 1.27 0 180) (layer F.SilkS))
    (fp_text value 33k (at 0 1.8 90) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 FX-Out))
    (model Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 170.434 107.188) (end 170.434 106.426) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.48 110.236) (end 167.386 110.236) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170.434 107.188) (end 167.386 110.236) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170.434 99.822) (end 172.72 99.822) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170.434 106.426) (end 170.434 99.822) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.432 107.188) (end 157.48 110.236) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.432 99.822) (end 154.432 107.188) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.146 99.822) (end 154.432 99.822) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.768 86.36) (end 149.098 86.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.098 99.822) (end 149.098 86.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.146 99.822) (end 149.098 99.822) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.768 99.822) (end 172.72 99.822) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.768 86.36) (end 175.768 99.822) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "SDLLC - 2018.06.21" (at 158.369 108.966) (layer F.SilkS))
  (gr_text Out (at 173.863 99.06) (layer F.SilkS))
  (gr_text In (at 150.876 99.06) (layer F.SilkS))
  (gr_text LED+ (at 171.196 87.249) (layer F.SilkS))
  (gr_text G (at 153.035 91.059) (layer F.SilkS))
  (gr_text G (at 163.83 90.805) (layer F.SilkS))
  (gr_text "EO\n" (at 166.37 90.805) (layer F.SilkS))
  (gr_text EI (at 158.623 90.805) (layer F.SilkS))
  (gr_text V+ (at 161.417 90.805) (layer F.SilkS))
  (gr_text V+ (at 153.543 88.519) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.768 99.822) (xy 170.434 99.822) (xy 170.434 107.188) (xy 167.386 110.236) (xy 157.48 110.236)
        (xy 154.432 107.188) (xy 154.432 99.822) (xy 149.098 99.822) (xy 149.098 86.36) (xy 175.768 86.36)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.768 99.822) (xy 170.434 99.822) (xy 170.434 107.188) (xy 167.386 110.236) (xy 157.48 110.236)
        (xy 154.432 107.188) (xy 154.432 99.822) (xy 149.098 99.822) (xy 149.098 86.36) (xy 175.768 86.36)
      )
    )
  )
)
