(kicad_pcb (version 4) (host pcbnew 4.0.1-stable)
  (general
    (links 39)
    (no_connects 0)
    (area 163.500999 103.048999 183.463001 139.267001)
    (thickness 1.6)
    (drawings 11)
    (tracks 170)
    (zones 0)
    (modules 22)
    (nets 19)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 "Net-(IC1-Pad1)")
  (net 4 "Net-(IC1-Pad2)")
  (net 5 "Net-(IC1-Pad3)")
  (net 6 "Net-(IC1-Pad5)")
  (net 7 "Net-(IC1-Pad6)")
  (net 8 "Net-(IC1-Pad7)")
  (net 9 +12V)
  (net 10 "Net-(P1-Pad2)")
  (net 11 "Net-(P2-Pad2)")
  (net 12 "Net-(P3-Pad2)")
  (net 13 "Net-(Q1-Pad1)")
  (net 14 "Net-(Q1-Pad3)")
  (net 15 "Net-(Q3-Pad1)")
  (net 16 "Net-(Q3-Pad3)")
  (net 17 "Net-(Q5-Pad1)")
  (net 18 "Net-(Q5-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad3)")
    (add_net "Net-(IC1-Pad5)")
    (add_net "Net-(IC1-Pad6)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(Q3-Pad1)")
    (add_net "Net-(Q3-Pad3)")
    (add_net "Net-(Q5-Pad1)")
    (add_net "Net-(Q5-Pad3)")
  )
  (net_class v12 ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 57A9746C)
    (at 178.435 116.205 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0.889 -1.905 180) (layer F.SilkS))
    (fp_text value 0.1u (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 57A97461)
    (at 173.99 109.22 270)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference IC1 (at 2.54 -1.016 270) (layer F.SilkS))
    (fp_text value ATTINY85 (at 0 -3.72 270) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(IC1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(IC1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(IC1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(IC1-Pad5)"))
    (pad 6 thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(IC1-Pad6)"))
    (pad 7 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(IC1-Pad7)"))
    (pad 8 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 57A97496)
    (at 180.34 132.08)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 2.54 -1.016 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 +12V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P1-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 57A97486)
    (at 180.34 125.73)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 2.54 -1.016 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 +12V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P2-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 57A974A9)
    (at 180.34 119.38)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 2.54 -1.016 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 +12V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P3-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 553634F8)
    (at 167.005 134.62 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.25 270) (layer F.SilkS))
    (fp_text value BC847 (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 -0.99822 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(Q1-Pad3)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 57A975B7)
    (at 176.53 134.62 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 2.794 -1.016 270) (layer F.SilkS))
    (fp_text value IRLML2502TRPBF (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(Q1-Pad3)"))
    (pad 2 smd rect (at 0.95 1.00076 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(Q1-Pad1)"))
    (pad 3 smd rect (at 0 -0.99822 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(P1-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 553634F8)
    (at 167.005 128.27 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at 0 -2.25 270) (layer F.SilkS))
    (fp_text value BC847 (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(Q3-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 -0.99822 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(Q3-Pad3)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 57A975BE)
    (at 176.53 128.27 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q4 (at 2.794 -1.016 270) (layer F.SilkS))
    (fp_text value IRLML2502TRPBF (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(Q3-Pad3)"))
    (pad 2 smd rect (at 0.95 1.00076 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(Q3-Pad1)"))
    (pad 3 smd rect (at 0 -0.99822 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(P2-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 553634F8)
    (at 167.005 121.92 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q5 (at 0 -2.25 270) (layer F.SilkS))
    (fp_text value BC847 (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(Q5-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 -0.99822 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(Q5-Pad3)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 57A975C1)
    (at 176.53 121.92 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q6 (at 2.794 -1.016 270) (layer F.SilkS))
    (fp_text value IRLML2502TRPBF (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(Q5-Pad3)"))
    (pad 2 smd rect (at 0.95 1.00076 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(Q5-Pad1)"))
    (pad 3 smd rect (at 0 -0.99822 270) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(P3-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57A97560)
    (at 167.005 137.16 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -2.159 -1.27 180) (layer F.SilkS))
    (fp_text value 100 (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(Q1-Pad3)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(IC1-Pad5)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57A97580)
    (at 171.45 133.985)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 2.54 -1.143) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(Q1-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 57A975B4)
    (at 172.085 136.525 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at -3.175 -0.889 180) (layer F.SilkS))
    (fp_text value 1 (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57A97566)
    (at 167.005 130.81 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at -2.159 -1.27 180) (layer F.SilkS))
    (fp_text value 100 (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(Q3-Pad3)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(IC1-Pad6)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57A9758A)
    (at 171.45 127.635)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 2.54 -0.889) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(Q3-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 57A975AB)
    (at 172.085 130.175 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R6 (at -3.175 -0.889 180) (layer F.SilkS))
    (fp_text value 1 (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(Q3-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57A9756C)
    (at 167.005 124.46 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at -2.159 -1.27 180) (layer F.SilkS))
    (fp_text value 100 (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(Q5-Pad3)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad7)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 57A97595)
    (at 171.45 121.285)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 2.54 -0.889) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(Q5-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 57A975A7)
    (at 172.085 123.825 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R9 (at -2.921 -0.889 180) (layer F.SilkS))
    (fp_text value 1 (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(Q5-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 57A9766B)
    (at 171.45 105.41 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at -1.016 -2.794 360) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 +12V))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 178.435 109.22)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(IC1-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "+12, +5, GND" (at 169.672 107.442) (layer B.SilkS))
  (gr_text +12-12 (at 182.372 133.096 90) (layer B.SilkS))
  (gr_text +12-12 (at 182.372 126.746 90) (layer B.SilkS))
  (gr_text +12-12 (at 182.372 120.396 90) (layer B.SilkS))
  (gr_text "RC Model Light\n(c) 2016\nwww.arduinoslovakia.eu" (at 175.006 137.922 90) (layer B.SilkS))
  (dimension 36.068 (width 0.3) (layer Dwgs.User)
    (gr_text "36,068 mm" (at 190.326 121.158 90) (layer Dwgs.User))
    (feature1 (pts (xy 184.404 103.124) (xy 191.676 103.124)))
    (feature2 (pts (xy 184.404 139.192) (xy 191.676 139.192)))
    (crossbar (pts (xy 188.976 139.192) (xy 188.976 103.124)))
    (arrow1a (pts (xy 188.976 103.124) (xy 189.562421 104.250504)))
    (arrow1b (pts (xy 188.976 103.124) (xy 188.389579 104.250504)))
    (arrow2a (pts (xy 188.976 139.192) (xy 189.562421 138.065496)))
    (arrow2b (pts (xy 188.976 139.192) (xy 188.389579 138.065496)))
  )
  (dimension 19.812 (width 0.3) (layer Dwgs.User)
    (gr_text "19,812 mm" (at 173.482 145.114) (layer Dwgs.User))
    (feature1 (pts (xy 183.388 140.716) (xy 183.388 146.464)))
    (feature2 (pts (xy 163.576 140.716) (xy 163.576 146.464)))
    (crossbar (pts (xy 163.576 143.764) (xy 183.388 143.764)))
    (arrow1a (pts (xy 183.388 143.764) (xy 182.261496 144.350421)))
    (arrow1b (pts (xy 183.388 143.764) (xy 182.261496 143.177579)))
    (arrow2a (pts (xy 163.576 143.764) (xy 164.702504 144.350421)))
    (arrow2b (pts (xy 163.576 143.764) (xy 164.702504 143.177579)))
  )
  (gr_line (start 183.388 103.124) (end 163.576 103.124) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 183.388 139.192) (end 183.388 103.124) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.576 139.192) (end 183.388 139.192) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.576 103.124) (end 163.576 139.192) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 163.83 103.378) (xy 183.134 103.378) (xy 183.134 138.938) (xy 163.83 138.938)
      )
    )
  )
)
