(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 18)
    (no_connects 0)
    (area 90.124847 75.824847 155.875153 141.575153)
    (thickness 1.6)
    (drawings 5)
    (tracks 21)
    (zones 0)
    (modules 16)
    (nets 11)
  )
  (page USLetter)
  (title_block
    (title "Mason Jar Lamp")
    (date 2016-07-06)
    (rev B)
    (company "DPW 2016")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerbers/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(D1-Pad2)")
  (net 4 "Net-(D3-Pad2)")
  (net 5 "Net-(D5-Pad2)")
  (net 6 "Net-(D5-Pad1)")
  (net 7 "Net-(D6-Pad1)")
  (net 8 "Net-(D8-Pad2)")
  (net 9 "Net-(D8-Pad1)")
  (net 10 "Net-(D10-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(D8-Pad2)")
  )
  (module Capacitors_SMD:c_elec_4x5.3 (layer F.Cu) (tedit 57713DE5)
    (at 116 109 270)
    (descr "SMT capacitor, aluminium electrolytic, 4x5.3")
    (attr smd)
    (fp_text reference C1 (at 0.1 3.8 360) (layer F.SilkS))
    (fp_text value 6u8 (at 0 3.175 270) (layer F.Fab))
    (pad 1 smd rect (at 1.80086 0 270) (size 2.60096 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at -1.80086 0 270) (size 2.60096 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/c_elec_4x5.3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 55BDE2E8)
    (at 106 119 120)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D5 (at 0 -2 120) (layer F.SilkS))
    (fp_text value "Warm White LED" (at 0 2 120) (layer F.Fab))
    (pad 2 smd rect (at 1.41986 0 300) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D5-Pad2)"))
    (pad 1 smd rect (at -1.41986 0 300) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D5-Pad1)"))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 55BDE2E8)
    (at 140 119 240)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D6 (at 0 -2 240) (layer F.SilkS))
    (fp_text value "Warm White LED" (at 0 2 240) (layer F.Fab))
    (pad 2 smd rect (at 1.41986 0 60) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D5-Pad1)"))
    (pad 1 smd rect (at -1.41986 0 60) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D6-Pad1)"))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 55BDE2E8)
    (at 123 89)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D7 (at 0 -2) (layer F.SilkS))
    (fp_text value "Warm White LED" (at 0 2) (layer F.Fab))
    (pad 2 smd rect (at 1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D6-Pad1)"))
    (pad 1 smd rect (at -1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 55BDE2E8)
    (at 123 129 180)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D8 (at 0 -2 180) (layer F.SilkS))
    (fp_text value "Warm White LED" (at 0 2 180) (layer F.Fab))
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D8-Pad2)"))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D8-Pad1)"))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 55BDE2E8)
    (at 140 99 300)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D9 (at 0 -2 300) (layer F.SilkS))
    (fp_text value "Warm White LED" (at 0 2 300) (layer F.Fab))
    (pad 2 smd rect (at 1.41986 0 120) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D8-Pad1)"))
    (pad 1 smd rect (at -1.41986 0 120) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D10-Pad2)"))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 55BDE2E8)
    (at 106 99 60)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D10 (at 0 -2 60) (layer F.SilkS))
    (fp_text value "Warm White LED" (at 0 2 60) (layer F.Fab))
    (pad 2 smd rect (at 1.41986 0 240) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D10-Pad2)"))
    (pad 1 smd rect (at -1.41986 0 240) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 57713DC1)
    (at 133.5 108.6 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 2.8 1.2 360) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D3-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(D1-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 57713DCB)
    (at 105.2 108.7)
    (fp_text reference P2 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value "Loop Mounting Hole" (at -0.635 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask F.SilkS))
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 57713DC7)
    (at 140.7 108.5)
    (fp_text reference P3 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value "Loop Mounting Hole" (at -0.635 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask F.SilkS))
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 57713DDD)
    (at 114 118)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0.1 2.2) (layer F.SilkS))
    (fp_text value 56 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D5-Pad2)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5418A20D)
    (at 114 115)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 -2.3) (layer F.SilkS))
    (fp_text value 56 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D8-Pad2)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 55BDE2E8)
    (at 123 111)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D1 (at 0 -2) (layer F.SilkS))
    (fp_text value D (at 0 2) (layer F.Fab))
    (pad 2 smd rect (at 1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 55BDE2E8)
    (at 123 107 180)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D2 (at 0 -2 180) (layer F.SilkS))
    (fp_text value D (at 0 2 180) (layer F.Fab))
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 55BDE2E8)
    (at 123 115)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D3 (at 0 -2) (layer F.SilkS))
    (fp_text value D (at 0 2) (layer F.Fab))
    (pad 2 smd rect (at 1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 55BDE2E8)
    (at 123 103 180)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D4 (at 0 -2 180) (layer F.SilkS))
    (fp_text value D (at 0 2 180) (layer F.Fab))
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D3-Pad2)"))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (gr_text "DPW 2016" (at 123.1 96.2) (layer F.SilkS))
  (gr_circle (center 123 108.7) (end 155.8 108.8) (layer Edge.Cuts) (width 0.15))
  (zone (net 6) (net_name "Net-(D5-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.016418 119.398507) (xy 114 119.4) (xy 114 119.3) (xy 114.016418 119.398507)
      )
    )
  )
  (zone (net 10) (net_name "Net-(D10-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109 100) (xy 96 93) (xy 99 89) (xy 102 86) (xy 107 82)
        (xy 114 79) (xy 120 78) (xy 126 78) (xy 132 79) (xy 137 81)
        (xy 142 84) (xy 147 89) (xy 150 93) (xy 137 100) (xy 136 98)
        (xy 142 91) (xy 137 87) (xy 131 84) (xy 127 83) (xy 119 83)
        (xy 114 84) (xy 109 87) (xy 104 91) (xy 110 98) (xy 109 100)
      )
    )
  )
  (zone (net 9) (net_name "Net-(D8-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 152 97) (xy 154 105) (xy 154 112) (xy 153 118) (xy 151 123)
        (xy 147 129) (xy 143 133) (xy 139 136) (xy 132 139) (xy 126 140)
        (xy 124 140) (xy 124 126) (xy 126 126) (xy 131 134) (xy 137 131)
        (xy 141 128) (xy 145 123) (xy 148 117) (xy 149 112) (xy 149 106)
        (xy 148 101) (xy 138 102) (xy 138 101) (xy 150 94) (xy 152 97)
      )
    )
  )
  (zone (net 8) (net_name "Net-(D8-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113 116) (xy 109 116) (xy 107 114) (xy 104 114) (xy 102 116)
        (xy 98 116) (xy 100 122) (xy 105 128) (xy 111 132) (xy 117 134)
        (xy 120 126) (xy 122 126) (xy 122 140) (xy 114 139) (xy 107 136)
        (xy 99 129) (xy 94 121) (xy 92 114) (xy 92 112) (xy 113 112)
        (xy 113 116)
      )
    )
  )
  (zone (net 5) (net_name "Net-(D5-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 104 116) (xy 107 116) (xy 108 117) (xy 113 117) (xy 113 120)
        (xy 109 120) (xy 108 118) (xy 107 118) (xy 104 119) (xy 103 119)
        (xy 103 122) (xy 101 122) (xy 100 119) (xy 100 117) (xy 103 117)
        (xy 104 116)
      )
    )
  )
  (zone (net 6) (net_name "Net-(D5-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 144 122) (xy 141 126) (xy 138 128) (xy 134 131) (xy 132 131)
        (xy 128 125) (xy 127 124) (xy 117 124) (xy 115 131) (xy 111 130)
        (xy 108 128) (xy 104 124) (xy 104 120) (xy 105 120) (xy 107 119)
        (xy 108 121) (xy 136 121) (xy 138 119) (xy 144 122)
      )
    )
  )
  (zone (net 7) (net_name "Net-(D6-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 124 85) (xy 124 99) (xy 131 99) (xy 137 105) (xy 137 113)
        (xy 136 116) (xy 144 120) (xy 147 114) (xy 147 103) (xy 138 104)
        (xy 133 98) (xy 139 91) (xy 132 86) (xy 124 85)
      )
    )
  )
  (zone (net 2) (net_name "Net-(C1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122 99) (xy 122 85) (xy 114 86) (xy 107 91) (xy 112 97)
        (xy 110 102) (xy 95 95) (xy 93 101) (xy 92 106) (xy 92 110)
        (xy 112 110) (xy 112 108) (xy 112 104) (xy 122 104) (xy 122 99)
      )
    )
  )
)
