(kicad_pcb (version 20170922) (host pcbnew no-vcs-found-72d4889~60~ubuntu17.04.1)
(general
  (thickness 1.6)
  (drawings 409)
  (tracks 75)
  (zones 0)
  (modules 21)
  (nets 6)
)
(page A4)
(layers
  (0 F.Cu signal)
  (31 B.Cu signal)
  (32 B.Adhes user)
  (33 F.Adhes user)
  (34 B.Paste user)
  (35 F.Paste user)
  (36 B.SilkS user)
  (37 F.SilkS user)
  (38 B.Mask user)
  (39 F.Mask user)
  (40 Dwgs.User user)
  (41 Cmts.User user)
  (42 Eco1.User user)
  (43 Eco2.User user)
  (44 Edge.Cuts user)
  (45 Margin user)
  (46 B.CrtYd user)
  (47 F.CrtYd user)
  (48 B.Fab user)
  (49 F.Fab user)
)
(setup
  (last_trace_width 0.25)
  (trace_clearance 0.1525)
  (zone_clearance 0.508)
  (zone_45_only no)
  (trace_min 0.1525)
  (segment_width 0.2)
  (edge_width 0.15)
  (via_size 0.6)
  (via_drill 0.4)
  (via_min_size 0.4)
  (via_min_drill 0.3)
  (uvia_size 0.3)
  (uvia_drill 0.1)
  (uvias_allowed no)
  (uvia_min_size 0.2)
  (uvia_min_drill 0.1)
  (pcb_text_width 0.3)
  (pcb_text_size 1.5 1.5)
  (mod_edge_width 0.15)
  (mod_text_size 1 1)
  (mod_text_width 0.15)
  (pad_size 4 4)
  (pad_drill 0)
  (pad_to_mask_clearance 0.2)
  (aux_axis_origin 0 0)
  (visible_elements FFFFFF7F)
  (pcbplotparams
    (layerselection 0x01000_7fffffff)
    (usegerberextensions false)
    (usegerberattributes true)
    (usegerberadvancedattributes true)
    (creategerberjobfile true)
    (excludeedgelayer true)
    (linewidth 0.100000)
    (plotframeref false)
    (viasonmask false)
    (mode 1)
    (useauxorigin true)
    (hpglpennumber 1)
    (hpglpenspeed 20)
    (hpglpendiameter 15)
    (psnegative false)
    (psa4output false)
    (plotreference false)
    (plotvalue false)
    (plotinvisibletext false)
    (padsonsilk false)
    (subtractmaskfromsilk false)
    (outputformat 3)
    (mirror false)
    (drillshape 0)
    (scaleselection 1)
    (outputdirectory ""))
)
(net 0 "")
(net 1 BAT+)
(net 2 BAT-)
(net 3 B2OUT+)
(net 4 "Net-(SW1-Pad3)")
(net 5 "Net-(BT1-Pad2)")
(net_class Default "This is the default net class."
  (clearance 0.1525)
  (trace_width 0.25)
  (via_dia 0.6)
  (via_drill 0.4)
  (uvia_dia 0.3)
  (uvia_drill 0.1)
  (add_net B2OUT+)
  (add_net BAT+)
  (add_net BAT-)
  (add_net "Net-(BT1-Pad2)")
  (add_net "Net-(SW1-Pad3)")
)
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer B.Cu) (tedit 59650532)
    (at 227.1 98.81 90)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at -8.24 -4.35 90) (layer B.SilkS))
    (fp_text value Pin_Header_Straight_1x01_Pitch2.54mm (at 0 -2.33 90) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Battery_Holders:Keystone_3034_1x20mm-CoinCell (layer B.Cu) (tedit 595D9565)
    (at 237.125 110.125 270)
    (descr "Keystone 3034 SMD battery holder for 2020, 2025 and 2032 coincell batteries. http://www.keyelco.com/product-pdf.cfm?p=798")
    (tags "Keystone type 3034 coin cell retainer")
    (attr smd)
    (fp_text reference BT1 (at 0.025 15.875 270) (layer B.SilkS))
    (fp_text value Battery_Cell (at 0 -11.5 270) (layer B.Fab))
    (fp_text user %R (at 0 2.9 270) (layer B.Fab))
    (pad 2 smd rect (at 0 0 270) (size 3.96 3.96) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(BT1-Pad2)"))
    (pad 1 smd rect (at 10.985 0 270) (size 1.27 5.08) (layers B.Cu B.Paste B.Mask)
      (net 3 B2OUT+))
    (pad 1 smd rect (at -10.985 0 270) (size 1.27 5.08) (layers B.Cu B.Paste B.Mask)
      (net 3 B2OUT+))
    (model ${KISYS3DMOD}/Battery_Holders.3dshapes/Keystone_3034_1x20mm-CoinCell.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:GS2 (layer B.Cu) (tedit 0)
    (at 230.95 108.63 270)
    (descr "Pontet Goute de soudure")
    (attr virtual)
    (fp_text reference J5 (at 2.62 8.5 180) (layer B.SilkS))
    (fp_text value B1OUT (at -4.83 -0.15 180) (layer B.Fab))
    (pad 2 smd rect (at 0 -0.635 270) (size 1.27 0.9652) (layers B.Cu B.Paste B.Mask)
      (net 2 BAT-))
    (pad 1 smd rect (at 0 0.635 270) (size 1.27 0.9652) (layers B.Cu B.Paste B.Mask)
      (net 3 B2OUT+))
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 586134A1)
    (at 237.505 90.3)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J9 (at 9.445 1.25 90) (layer F.SilkS))
    (fp_text value B3IN (at -3.11 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0 0.64) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 2 BAT-))
    (pad 1 smd rect (at 0 -0.64) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 B2OUT+))
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 586134A1)
    (at 240.515 90.29 180)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J1 (at -11.785 -2.11 270) (layer F.SilkS))
    (fp_text value B3IN2 (at 3.08 -0.01 270) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 B2OUT+))
    (pad 2 smd rect (at 0 0.64 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 2 BAT-))
  )
  (module Connectors:GS2 (layer B.Cu) (tedit 586134A1)
    (at 230.97 111.61 90)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J8 (at -0.99 -9.37) (layer B.SilkS))
    (fp_text value B1OUT2 (at -1.8 0) (layer B.Fab))
    (pad 1 smd rect (at 0 0.64 90) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 3 B2OUT+))
    (pad 2 smd rect (at 0 -0.64 90) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 2 BAT-))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer B.Cu) (tedit 59650532)
    (at 246.89 98.81 90)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at -3.09 4.11 90) (layer B.SilkS))
    (fp_text value Pin_Header_Straight_1x01_Pitch2.54mm (at 0 -2.33 90) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer B.Cu) (tedit 59650532)
    (at 246.9 121.41 90)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at 1.71 4.55 90) (layer B.SilkS))
    (fp_text value Pin_Header_Straight_1x01_Pitch2.54mm (at 0 -2.33 90) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer B.Cu) (tedit 59650532)
    (at 227.1 121.41 90)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference REF** (at -0.94 -5 90) (layer B.SilkS))
    (fp_text value Pin_Header_Straight_1x01_Pitch2.54mm (at 0 -2.33 90) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 0)
    (at 230.975 108.64 90)
    (descr "Pontet Goute de soudure")
    (attr virtual)
    (fp_text reference J5 (at 0.74 -8.075 180) (layer F.SilkS))
    (fp_text value B1OUT (at -2.7438 0 180) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.635 90) (size 1.27 0.9652) (layers F.Cu F.Paste F.Mask)
      (net 1 BAT+))
    (pad 2 smd rect (at 0 0.635 90) (size 1.27 0.9652) (layers F.Cu F.Paste F.Mask)
      (net 2 BAT-))
  )
  (module LEDs:LED_0805_HandSoldering (layer F.Cu) (tedit 59EBE887)
    (at 239.061 85.731 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D1 (at -12.189 -6.319 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 BAT-))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 B2OUT+))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:GS2 (layer B.Cu) (tedit 586134A1)
    (at 240.515 90.29)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J1 (at 8.635 0.81 -90) (layer B.SilkS))
    (fp_text value B3IN2 (at 3.08 0.01 -90) (layer B.Fab))
    (pad 2 smd rect (at 0 -0.64) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 2 BAT-))
    (pad 1 smd rect (at 0 0.64) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 3 B2OUT+))
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 586134A1)
    (at 247.45 84.4258 270)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J6 (at 9.8242 -1.1) (layer F.SilkS))
    (fp_text value B2OUT2 (at -1.8 0) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 B2OUT+))
    (pad 2 smd rect (at 0 0.64 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 2 BAT-))
  )
  (module Connectors:GS2 (layer B.Cu) (tedit 586134A1)
    (at 222.4988 101.529189 270)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J7 (at -1.279189 5.0488 180) (layer B.SilkS))
    (fp_text value B2IN2 (at -1.8 0 180) (layer B.Fab))
    (pad 1 smd rect (at 0 0.64 270) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 3 B2OUT+))
    (pad 2 smd rect (at 0 -0.64 270) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 2 BAT-))
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 586134A1)
    (at 230.986901 111.6087 270)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J8 (at -2.1087 8.086901) (layer F.SilkS))
    (fp_text value B1OUT2 (at -1.4087 -0.763099) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 1 BAT+))
    (pad 2 smd rect (at 0 0.64 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 2 BAT-))
  )
  (module LEDs:LED_0805_HandSoldering (layer F.Cu) (tedit 595FCA25)
    (at 238.755 94.86 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D2 (at -12.495 0.46 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 B2OUT+))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 BAT-))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:GS2 (layer B.Cu) (tedit 586134A1)
    (at 247.450001 84.4233 270)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J3 (at 5.7767 -0.099999 180) (layer B.SilkS))
    (fp_text value B2OUT (at -1.8 0 180) (layer B.Fab))
    (pad 1 smd rect (at 0 0.64 270) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 3 B2OUT+))
    (pad 2 smd rect (at 0 -0.64 270) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 2 BAT-))
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 59F814B2)
    (at 222.4988 101.529189 270)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J4 (at -2.879189 4.2988) (layer F.SilkS))
    (fp_text value B2IN (at -1.8 0) (layer F.Fab))
    (pad 2 smd rect (at 0 0.64 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 2 BAT-))
    (pad 1 smd rect (at 0 -0.64 270) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 B2OUT+))
  )
  (module Connectors:GS2 (layer B.Cu) (tedit 586134A1)
    (at 237.505 90.309786 180)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J9 (at -14.995 -4.090214 180) (layer B.SilkS))
    (fp_text value B3IN (at -5.195 0.009786 90) (layer B.Fab))
    (pad 1 smd rect (at 0 0.64 180) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 3 B2OUT+))
    (pad 2 smd rect (at 0 -0.64 180) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 2 BAT-))
  )
  (module Buttons_Switches_SMD:JS202011SCQN (layer F.Cu) (tedit 59EEDBE5)
    (at 239.37 102.51)
    (fp_text reference 401-2002-1-ND (at 0 5.461) (layer F.SilkS))
    (fp_text value SW_SPDT (at 0 -5.5) (layer F.Fab))
    (fp_text user C&K (at 11.03 2.99) (layer F.SilkS))
    (pad 1 smd rect (at -2.5 3) (size 1.2 3) (layers F.Cu F.Paste F.Mask)
      (net 2 BAT-))
    (pad 2 smd rect (at 0 3) (size 1.2 3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(BT1-Pad2)"))
    (pad 3 smd rect (at 2.5 3) (size 1.2 3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(SW1-Pad3)"))
    (pad 4 smd rect (at -2.5 -3) (size 1.2 3) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 0 -3) (size 1.2 3) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 2.5 -3) (size 1.2 3) (layers F.Cu F.Paste F.Mask))
  )
  (module AnyColorButton:GS2-no-mask (layer F.Cu) (tedit 59EED95E)
    (at 233.23 103.27)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J2 (at 17.37 -0.22 90) (layer F.SilkS))
    (fp_text value PWR_BRIDGE (at -1.8 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 2 BAT-))
    (pad 2 smd rect (at 0 0.64) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(BT1-Pad2)"))
  )
  (dimension 24.652485 (width 0.3) (layer Eco1.User)
    (gr_text "24.652 mm" (at 276.279439 110.571919 89.18652433) (layer Eco1.User))
    (feature1 (pts (xy 248.15 122.5) (xy 277.454303 122.916086)))
    (feature2 (pts (xy 248.5 97.85) (xy 277.804303 98.266086)))
    (crossbar (pts (xy 275.104575 98.227753) (xy 274.754575 122.877753)))
    (arrow1a (pts (xy 274.754575 122.877753) (xy 274.184207 121.743037)))
    (arrow1b (pts (xy 274.754575 122.877753) (xy 275.35693 121.759688)))
    (arrow2a (pts (xy 275.104575 98.227753) (xy 274.50222 99.345818)))
    (arrow2b (pts (xy 275.104575 98.227753) (xy 275.674943 99.362469)))
  )
  (dimension 22.150508 (width 0.3) (layer Eco1.User)
    (gr_text "22.151 mm" (at 236.786291 135.27443 -0.388001605) (layer Eco1.User))
    (feature1 (pts (xy 225.8 122.1) (xy 225.702149 136.549399)))
    (feature2 (pts (xy 247.95 122.25) (xy 247.852149 136.699399)))
    (crossbar (pts (xy 247.870433 133.999461) (xy 225.720433 133.849461)))
    (arrow1a (pts (xy 225.720433 133.849461) (xy 226.850882 133.270682)))
    (arrow1b (pts (xy 225.720433 133.849461) (xy 226.84294 134.443497)))
    (arrow2a (pts (xy 247.870433 133.999461) (xy 246.747926 133.405425)))
    (arrow2b (pts (xy 247.870433 133.999461) (xy 246.739984 134.57824)))
  )
  (gr_text LAMPSTER (at 237.05 119.9) (layer F.SilkS))
  (dimension 1.25 (width 0.3) (layer Eco1.User)
    (gr_text "1.250 mm" (at 259.7 85.675 270) (layer Eco1.User))
    (feature1 (pts (xy 247.5 86.3) (xy 261.05 86.3)))
    (feature2 (pts (xy 247.5 85.05) (xy 261.05 85.05)))
    (crossbar (pts (xy 258.35 85.05) (xy 258.35 86.3)))
    (arrow1a (pts (xy 258.35 86.3) (xy 257.763579 85.173496)))
    (arrow1b (pts (xy 258.35 86.3) (xy 258.936421 85.173496)))
    (arrow2a (pts (xy 258.35 85.05) (xy 257.763579 86.176504)))
    (arrow2b (pts (xy 258.35 85.05) (xy 258.936421 86.176504)))
  )
  (dimension 1.3 (width 0.3) (layer Eco1.User)
    (gr_text "1.300 mm" (at 214.95 102.85 270) (layer Eco1.User))
    (feature1 (pts (xy 220.35 103.5) (xy 213.6 103.5)))
    (feature2 (pts (xy 220.35 102.2) (xy 213.6 102.2)))
    (crossbar (pts (xy 216.3 102.2) (xy 216.3 103.5)))
    (arrow1a (pts (xy 216.3 103.5) (xy 215.713579 102.373496)))
    (arrow1b (pts (xy 216.3 103.5) (xy 216.886421 102.373496)))
    (arrow2a (pts (xy 216.3 102.2) (xy 215.713579 103.326504)))
    (arrow2b (pts (xy 216.3 102.2) (xy 216.886421 103.326504)))
  )
  (gr_line (start 226.401 94.15309) (end 226.9 93) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 225.9754 95.33525) (end 226.401 94.15309) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 225.036 100.25978) (end 225.1542 99.00893) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 225.1542 99.00893) (end 225.3508 97.76796) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 225.6248 96.54179) (end 225.9754 95.33525) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 225.3508 97.76796) (end 225.6248 96.54179) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 224.9965 101.51558) (end 225.036 100.25978) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 233.5238 111.04268) (end 228.4692 111.04268) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 233.5238 109.18848) (end 233.5238 111.04268) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 228.4692 109.18848) (end 233.5238 109.18848) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 228.4692 111.04268) (end 228.4692 109.18848) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 247.99648 122.51558) (end 247.9965 97.71561) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 225.9965 122.51558) (end 247.99648 122.51558) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 225.9965 97.71559) (end 225.9965 122.51558) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 247.9965 97.71561) (end 225.9965 97.71559) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 239.92359 93.04288) (end 238.06941 93.04288) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 239.92359 87.98828) (end 239.92359 93.04288) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 238.06941 87.98828) (end 239.92359 87.98828) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 238.06941 93.04288) (end 238.06941 87.98828) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 238.9965 97.18224) (end 239.41509 97.16908) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 238.57791 97.16908) (end 238.9965 97.18224) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 238.16096 97.12967) (end 238.57791 97.16908) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 237.74729 97.06415) (end 238.16096 97.12967) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 237.33857 96.97279) (end 237.74729 97.06415) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 236.9364 96.85594) (end 237.33857 96.97279) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 236.54234 96.71408) (end 236.9364 96.85594) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 236.15798 96.54775) (end 236.54234 96.71408) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 235.78481 96.35762) (end 236.15798 96.54775) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 235.42433 96.14443) (end 235.78481 96.35762) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 235.07794 95.90901) (end 235.42433 96.14443) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 234.747 95.65233) (end 235.07794 95.90901) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 234.4329 95.37537) (end 234.747 95.65233) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 234.1367 95.07922) (end 234.4329 95.37537) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 233.8598 94.76506) (end 234.1367 95.07922) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 233.6031 94.43414) (end 233.8598 94.76506) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 233.3677 94.08775) (end 233.6031 94.43414) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 233.1545 93.72727) (end 233.3677 94.08775) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 232.9643 93.3541) (end 233.1545 93.72727) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 232.798 92.96974) (end 232.9643 93.3541) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 232.6561 92.57568) (end 232.798 92.96974) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 232.5393 92.17351) (end 232.6561 92.57568) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 232.4479 91.76479) (end 232.5393 92.17351) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 232.3824 91.35108) (end 232.4479 91.76479) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 232.343 90.93418) (end 232.3824 91.35108) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 232.3298 90.51558) (end 232.343 90.93418) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 232.343 90.09698) (end 232.3298 90.51558) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 232.3824 89.68008) (end 232.343 90.09698) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 232.4479 89.26638) (end 232.3824 89.68008) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 232.5393 88.85768) (end 232.4479 89.26638) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 232.6561 88.45548) (end 232.5393 88.85768) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 232.798 88.06138) (end 232.6561 88.45548) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 232.9643 87.67708) (end 232.798 88.06138) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 233.1545 87.30388) (end 232.9643 87.67708) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 233.3677 86.94338) (end 233.1545 87.30388) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 233.6031 86.59698) (end 233.3677 86.94338) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 233.8598 86.26608) (end 233.6031 86.59698) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 234.1367 85.95198) (end 233.8598 86.26608) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 234.4329 85.65578) (end 234.1367 85.95198) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 234.747 85.37888) (end 234.4329 85.65578) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 235.07794 85.12218) (end 234.747 85.37888) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 235.42433 84.88678) (end 235.07794 85.12218) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 235.78481 84.67358) (end 235.42433 84.88678) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 236.15798 84.48338) (end 235.78481 84.67358) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 236.54234 84.31708) (end 236.15798 84.48338) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 236.9364 84.17518) (end 236.54234 84.31708) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 237.33857 84.05838) (end 236.9364 84.17518) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 237.74729 83.96698) (end 237.33857 84.05838) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 238.16096 83.90148) (end 237.74729 83.96698) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 238.57791 83.86208) (end 238.16096 83.90148) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 238.9965 83.84888) (end 238.57791 83.86208) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 239.41509 83.86208) (end 238.9965 83.84888) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 239.83204 83.90148) (end 239.41509 83.86208) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 240.24571 83.96698) (end 239.83204 83.90148) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 240.65443 84.05838) (end 240.24571 83.96698) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 241.0566 84.17518) (end 240.65443 84.05838) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 241.45066 84.31708) (end 241.0566 84.17518) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 241.83502 84.48338) (end 241.45066 84.31708) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 242.20819 84.67358) (end 241.83502 84.48338) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 242.56867 84.88678) (end 242.20819 84.67358) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 242.91506 85.12218) (end 242.56867 84.88678) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 243.24598 85.37888) (end 242.91506 85.12218) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 243.56014 85.65578) (end 243.24598 85.37888) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 243.85629 85.95198) (end 243.56014 85.65578) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 244.133249 86.26608) (end 243.85629 85.95198) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 244.389933 86.59698) (end 244.133249 86.26608) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 244.625345 86.94338) (end 244.389933 86.59698) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 244.838541 87.30388) (end 244.625345 86.94338) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 245.028665 87.67708) (end 244.838541 87.30388) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 245.195002 88.06138) (end 245.028665 87.67708) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 245.336863 88.45548) (end 245.195002 88.06138) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 245.453714 88.85768) (end 245.336863 88.45548) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 245.545069 89.26638) (end 245.453714 88.85768) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 245.61059 89.68008) (end 245.545069 89.26638) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 245.650003 90.09698) (end 245.61059 89.68008) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 245.663156 90.51558) (end 245.650003 90.09698) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 245.650003 90.93418) (end 245.663156 90.51558) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 245.61059 91.35108) (end 245.650003 90.93418) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 245.545069 91.76479) (end 245.61059 91.35108) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 245.453714 92.17351) (end 245.545069 91.76479) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 245.336863 92.57568) (end 245.453714 92.17351) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 245.195002 92.96974) (end 245.336863 92.57568) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 245.028665 93.3541) (end 245.195002 92.96974) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 244.838541 93.72727) (end 245.028665 93.3541) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 244.625345 94.08775) (end 244.838541 93.72727) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 244.389933 94.43414) (end 244.625345 94.08775) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 244.133249 94.76506) (end 244.389933 94.43414) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 243.85629 95.07922) (end 244.133249 94.76506) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 243.56014 95.37537) (end 243.85629 95.07922) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 243.24598 95.65233) (end 243.56014 95.37537) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 242.91506 95.90901) (end 243.24598 95.65233) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 242.56867 96.14443) (end 242.91506 95.90901) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 242.20819 96.35762) (end 242.56867 96.14443) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 241.83502 96.54775) (end 242.20819 96.35762) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 241.45066 96.71408) (end 241.83502 96.54775) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 241.0566 96.85594) (end 241.45066 96.71408) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 240.65443 96.97279) (end 241.0566 96.85594) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 240.24571 97.06415) (end 240.65443 96.97279) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 239.83204 97.12967) (end 240.24571 97.06415) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 239.41509 97.16908) (end 239.83204 97.12967) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 224.9965 103.51582) (end 224.9965 101.51558) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 220.1959 103.51582) (end 224.9965 103.51582) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 220.1959 101.51558) (end 220.1959 103.51582) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 220.2449 99.95834) (end 220.1959 101.51558) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 220.3915 98.40724) (end 220.2449 99.95834) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 220.6352 96.86842) (end 220.3915 98.40724) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 220.9751 95.34793) (end 220.6352 96.86842) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 221.4097 93.85178) (end 220.9751 95.34793) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 221.9375 92.38588) (end 221.4097 93.85178) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 222.5563 90.95598) (end 221.9375 92.38588) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 223.2636 89.56778) (end 222.5563 90.95598) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 224.0567 88.22678) (end 223.2636 89.56778) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 224.9324 86.93818) (end 224.0567 88.22678) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 225.8873 85.70708) (end 224.9324 86.93818) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 226.9176 84.53838) (end 225.8873 85.70708) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 228.0193 83.43668) (end 226.9176 84.53838) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 229.188 82.40638) (end 228.0193 83.43668) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 230.4191 81.45148) (end 229.188 82.40638) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 231.7077 80.57578) (end 230.4191 81.45148) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 233.0487 79.78268) (end 231.7077 80.57578) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 234.4369 79.07538) (end 233.0487 79.78268) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 235.8668 78.45658) (end 234.4369 79.07538) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 237.3327 77.92878) (end 235.8668 78.45658) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 238.82885 77.49418) (end 237.3327 77.92878) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 240.34934 77.15428) (end 238.82885 77.49418) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 241.88816 76.91058) (end 240.34934 77.15428) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 243.43926 76.76398) (end 241.88816 76.91058) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 244.9965 76.71498) (end 243.43926 76.76398) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 249.7971 76.71498) (end 244.9965 76.71498) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 249.7971 86.31618) (end 249.7971 76.71498) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 244.9965 86.31618) (end 249.7971 86.31618) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 244.9965 81.51558) (end 244.9965 86.31618) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 243.7407 81.55508) (end 244.9965 81.51558) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 242.48985 81.67328) (end 243.7407 81.55508) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 241.24888 81.86988) (end 242.48985 81.67328) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 240.02271 82.14388) (end 241.24888 81.86988) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 238.81617 82.49448) (end 240.02271 82.14388) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 237.63401 82.92008) (end 238.81617 82.49448) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 236.48092 83.41908) (end 237.63401 82.92008) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 235.36143 83.98948) (end 236.48092 83.41908) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 234.28 84.62898) (end 235.36143 83.98948) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 233.2408 85.33528) (end 234.28 84.62898) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 232.248 86.10528) (end 233.2408 85.33528) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 231.3056 86.93618) (end 232.248 86.10528) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 230.4171 87.82468) (end 231.3056 86.93618) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 229.5862 88.76708) (end 230.4171 87.82468) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 228.8162 89.75988) (end 229.5862 88.76708) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 228.1099 90.79908) (end 228.8162 89.75988) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 227.4704 91.88051) (end 228.1099 90.79908) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 226.9 93) (end 227.4704 91.88051) (layer Edge.Cuts) (width 0.1))
  (gr_text "THAT WAY" (at 244.65 110.95) (layer F.SilkS))
  (gr_text "< OR" (at 243.7 109.43) (layer F.SilkS))
  (gr_text "ALWAYS ON" (at 231.77 103.3 90) (layer F.SilkS))
  (gr_text ARM> (at 237.95 110.4) (layer F.SilkS))
  (gr_text BAT- (at 221.88 98.74 90) (layer F.SilkS))
  (gr_text BAT+ (at 223.34 98.74 90) (layer F.SilkS))
  (zone (net 2) (net_name BAT-) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 255 70) (xy 255 135) (xy 215 135) (xy 215 70)
      )
    )
  )
)
