(kicad_pcb (version 20171130) (host pcbnew "(5.0.2)-1")
  (general
    (thickness 1.6)
    (drawings 11)
    (tracks 29)
    (zones 0)
    (modules 8)
    (nets 3)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 2)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad2)")
  (net 2 "Net-(J1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 2)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5C27F509)
    (at 138.43 96.52 90)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J1 (at 0 -2.77 90) (layer F.SilkS) hide)
    (fp_text value TEST (at 0 5.31 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5C2800A6)
    (at 138.43 79.375 90)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference PCM (at -0.381 5.207 270) (layer F.SilkS))
    (fp_text value PCM (at 0 5.31 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad2)"))
  )
  (module Button_Switch_SMD:SW_SPST_EVQQ2 (layer F.Cu) (tedit 5C27F505)
    (at 139.7 96.52)
    (descr "Light Touch Switch, https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE28.pdf")
    (attr smd)
    (fp_text reference TEST (at 0 2.286) (layer F.SilkS))
    (fp_text value TEST (at 0 4.25) (layer F.Fab))
    (fp_text user %R (at 0.05 -3.95) (layer F.Fab))
    (pad 1 smd rect (at 3.4 -2) (size 3.2 1) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at -3.4 -2) (size 3.2 1) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad2)"))
    (pad 2 smd rect (at -3.4 2) (size 3.2 1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 3.4 2) (size 3.2 1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_EVQQ2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module small_gear_footprints:12mm_gear (layer F.Cu) (tedit 0)
    (at 139.7 86.995)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module small_gear_footprints:12mm_wings_fcu (layer F.Cu) (tedit 5C27FDBF)
    (at 139.7 86.995)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module small_gear_footprints:12mm_wings_fmask (layer F.Cu) (tedit 5C27FE22)
    (at 139.7 86.995)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module small_gear_footprints:12mm_gear (layer B.Cu) (tedit 0)
    (at 139.7 86.995 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module small_gear_footprints:12mm_wings (layer B.Cu) (tedit 0)
    (at 139.7 86.995 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (gr_arc (start 139.7 88.9) (end 132.080001 97.789999) (angle -81.20258929) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 139.7 88.9) (end 147.319999 80.010001) (angle -81.20258929) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.32 80.01) (end 147.32 97.79) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 132.08 80.01) (end 132.08 97.79) (layer Edge.Cuts) (width 0.15))
  (gr_text "Thanks Marshall" (at 133.096 88.9 270) (layer B.Cu))
  (gr_text 190122.01 (at 139.7 98.933) (layer B.SilkS))
  (gr_text PRESSer (at 139.7 94.615) (layer B.SilkS))
  (gr_text er (at 133.35 92.71 90) (layer F.SilkS))
  (gr_text PRESS (at 133.35 98.425 90) (layer F.SilkS))
)
