(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 22)
    (tracks 65)
    (zones 0)
    (modules 8)
    (nets 12)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.1)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "../Panels/ICE-Adapter-Video/Video Gerbers/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 /NSYNC)
  (net 4 /VIDEO)
  (net 5 "Net-(P3-Pad1)")
  (net 6 "Net-(Q1-Pad2)")
  (net 7 "Net-(Q1-Pad3)")
  (net 8 "Net-(RV1-Pad3)")
  (net 9 "Net-(RV1-Pad1)")
  (net 10 "Net-(U1-Pad10)")
  (net 11 "Net-(U1-Pad12)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /NSYNC)
    (add_net /VIDEO)
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(RV1-Pad1)")
    (add_net "Net-(RV1-Pad3)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad12)")
  )
  (net_class HiPower ""
    (clearance 0.2)
    (trace_width 0.6)
    (via_dia 1)
    (via_drill 0.8)
    (uvia_dia 0.4)
    (uvia_drill 0.2)
    (add_net GND)
    (add_net VCC)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.4)
    (uvia_drill 0.2)
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 58A0772D)
    (at 94.79 120.99 90)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 0.91 -3.66 -90) (layer F.SilkS))
    (fp_text value BC237 (at 1.13 3.07 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 1.27 -1.27 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 6 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 7 "Net-(Q1-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (offset (xyz 1.269999980926514 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Discret:R3 (layer F.Cu) (tedit 58A0776D)
    (at 95.95 115.03 180)
    (descr "Resitance 3 pas")
    (tags R)
    (fp_text reference R1 (at 1.51 -0.04 180) (layer F.SilkS))
    (fp_text value 75R (at -1.39 -0.04 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 7 "Net-(Q1-Pad3)"))
    (pad 2 thru_hole circle (at 3.81 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 "Net-(P3-Pad1)"))
    (model Discret.3dshapes/R3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:R3 (layer F.Cu) (tedit 58A07766)
    (at 84.77 135.49)
    (descr "Resitance 3 pas")
    (tags R)
    (fp_text reference R2 (at -1.54 0.04) (layer F.SilkS))
    (fp_text value 1K (at 1.2 0.12) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 7 "Net-(Q1-Pad3)"))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Discret.3dshapes/R3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-14_W7.62mm (layer F.Cu) (tedit 58A07747)
    (at 81.788 116.078)
    (descr "14-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 3.842 1.082) (layer F.SilkS))
    (fp_text value 7400 (at 3.872 7.692 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /VIDEO))
    (pad 8 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(RV1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 /VIDEO))
    (pad 9 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(U1-Pad10)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(U1-Pad12)"))
    (pad 10 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(U1-Pad10)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /NSYNC))
    (pad 11 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(RV1-Pad1)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /NSYNC))
    (pad 12 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(U1-Pad12)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(U1-Pad10)"))
    (pad 13 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(U1-Pad12)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model Housings_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Trimmer-Suntan-TSR-3386P (layer F.Cu) (tedit 58A076C8)
    (at 98.48 128.1 180)
    (fp_text reference RV1 (at -0.69 3.65 180) (layer F.SilkS))
    (fp_text value 10K (at -0.05 -3.6 180) (layer F.SilkS))
    (pad 3 thru_hole circle (at 5.08 0 180) (size 1.51 1.51) (drill 0.51) (layers *.Cu *.Mask)
      (net 8 "Net-(RV1-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.51 1.51) (drill 0.51) (layers *.Cu *.Mask)
      (net 9 "Net-(RV1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 2.54 180) (size 1.51 1.51) (drill 0.51) (layers *.Cu *.Mask)
      (net 6 "Net-(Q1-Pad2)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 54EA090C)
    (at 82.4 111.62 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J1 (at -2.426 -1.882 180) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 -3.1 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (offset (xyz 0 -1.269999980926514 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 5BADDDD5)
    (at 99.26 135.49 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J2 (at -1.24 -2.8) (layer Dwgs.User))
    (fp_text value Conn_01x04 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /NSYNC))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 /VIDEO))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (offset (xyz 0 -3.809999942779541 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 54EA090C)
    (at 97.5 111.57 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 1.968 -2.83) (layer F.SilkS))
    (fp_text value "Composite Video" (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(P3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (offset (xyz 0 -1.269999980926514 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text Video► (at 87.884 110.744) (layer F.SilkS))
  (gr_text GND (at 90.47 137.74) (layer F.SilkS))
  (gr_text NSYNC (at 98.13 137.7) (layer F.SilkS))
  (gr_text Video (at 93.2 137.7) (layer F.SilkS))
  (gr_text GND (at 95.94 137.74) (layer F.SilkS))
  (gr_text "JonB\nRetro" (at 85.848 116.532624) (layer B.SilkS))
  (gr_text ◄Pwr (at 86.868 112.522) (layer F.SilkS))
  (gr_text Video (at 99.84 112.64 90) (layer F.SilkS))
  (gr_text GND (at 92.72 112.98 90) (layer F.SilkS))
  (gr_text 5v (at 84.328 113.538) (layer F.SilkS))
  (gr_text GND (at 80.09 112.41 90) (layer F.SilkS))
  (gr_text "Video Mixer\n" (at 85.648 133.822624 90) (layer B.SilkS))
  (gr_line (start 79.5 138.22) (end 79.5 109.51) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.35 138.22) (end 79.5 138.22) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.33 109.5) (end 101.35 138.22) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 79.5 109.51) (end 101.33 109.51) (angle 90) (layer Edge.Cuts) (width 0.1))
)
