(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "/RST")
  (net 2 "/TMS")
  (net 3 "/TCK")
  (net 4 "/GND")
  (net 5 "/TDO")
  (net 6 "/TDI")
  (net 7 "unconnected-(J2-Pin_4-Pad4)")
  (net 8 "unconnected-(J2-Pin_7-Pad7)")
  (net 9 "unconnected-(J2-Pin_8-Pad8)")
  (footprint "custom:Sidecar-6" (layer "F.Cu")
    (at 140.97 90.17)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (property "Sheetfile" "jtag-sidecar.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "Conn_01x06" (at 0 15.03) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 6.35 90) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0) (size 3.2 1.6) (drill 1 (offset 0.8 0)) (layers "*.Cu" "*.Mask")
      (net 1 "/RST") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 3.2 1.6) (drill 1 (offset 0.8 0)) (layers "*.Cu" "*.Mask")
      (net 2 "/TMS") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 3.2 1.6) (drill 1 (offset 0.8 0)) (layers "*.Cu" "*.Mask")
      (net 3 "/TCK") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole rect (at 0 7.62) (size 3.2 1.6) (drill 1 (offset 0.8 0)) (layers "*.Cu" "*.Mask")
      (net 4 "/GND") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16) (size 3.2 1.6) (drill 1 (offset 0.8 0)) (layers "*.Cu" "*.Mask")
      (net 5 "/TDO") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7) (size 3.2 1.6) (drill 1 (offset 0.8 0)) (layers "*.Cu" "*.Mask")
      (net 6 "/TDI") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical" (layer "F.Cu")
    (at 147.315 91.44)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (property "Sheetfile" "jtag-sidecar.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x05, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2" (at 1.27 -3.556) (layer "F.SilkS"))
    (fp_text value "Conn_02x05_Odd_Even" (at 1.27 12.49) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 5.08 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "/TCK") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "/GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "/TDO") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "unconnected-(J2-Pin_4-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "/TMS") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "/RST") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "unconnected-(J2-Pin_7-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "unconnected-(J2-Pin_8-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "/TDI") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "/GND") (pinfunction "Pin_10") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 152.4 102.87) (mid 152.028026 103.768026) (end 151.13 104.14)
    (layer "Edge.Cuts"))
  (gr_line (start 151.13 88.9) (end 139.7 88.9)
    (layer "Edge.Cuts"))
  (gr_line (start 139.7 104.14) (end 151.13 104.14)
    (layer "Edge.Cuts"))
  (gr_line (start 152.4 90.17) (end 152.4 102.87)
    (layer "Edge.Cuts"))
  (gr_arc (start 151.13 88.9) (mid 152.028026 89.271974) (end 152.4 90.17)
    (layer "Edge.Cuts"))
  (gr_line (start 139.7 88.9) (end 139.7 104.14)
    (layer "Edge.Cuts"))
  (gr_text "GND" (at 150.876 91.44 270) (layer "B.SilkS"))
  (gr_text "RST" (at 150.876 96.52 270) (layer "B.SilkS"))
  (gr_text "TCK" (at 146.05 91.44 90) (layer "B.SilkS"))
  (gr_text "GND" (at 150.876 101.6 270) (layer "B.SilkS"))
  (gr_text "VCC" (at 150.876 93.98 270) (layer "B.SilkS"))
  (gr_text "TDI" (at 146.05 101.6 90) (layer "B.SilkS"))
  (gr_text "TDO" (at 146.05 93.98 90) (layer "B.SilkS"))
  (gr_text "TMS" (at 146.05 96.52 90) (layer "B.SilkS"))
  (gr_text "GND" (at 143.51 97.79) (layer "F.SilkS"))
  (gr_text "TMS" (at 143.51 92.71) (layer "F.SilkS"))
  (gr_text "TDI" (at 143.51 102.87) (layer "F.SilkS"))
  (gr_text "TDO" (at 143.51 100.33) (layer "F.SilkS"))
  (gr_text "RST" (at 143.51 90.17) (layer "F.SilkS"))
  (gr_text "TCK" (at 143.51 95.25) (layer "F.SilkS"))
  (zone (net 4) (net_name "/GND") (layer "B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139.7 88.9)
        (xy 152.4 88.9)
        (xy 152.4 104.14)
        (xy 139.7 104.14)
      )
    )
  )
)
