(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 1.6)
    (drawings 7)
    (tracks 104)
    (zones 0)
    (modules 3)
    (nets 24)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /GND-GPIB)
  (net 2 /DIO1)
  (net 3 /REN)
  (net 4 /DIO2)
  (net 5 /DIO3)
  (net 6 /DIO4)
  (net 7 /DIO5)
  (net 8 /DIO6)
  (net 9 /DIO7)
  (net 10 /~CS)
  (net 11 /DIO8)
  (net 12 /5V_SD)
  (net 13 /EOI)
  (net 14 /GND_SD)
  (net 15 /DAV)
  (net 16 /NRFD)
  (net 17 /DI)
  (net 18 /DO)
  (net 19 /SCK)
  (net 20 /NDAC)
  (net 21 /IFC)
  (net 22 /SRQ)
  (net 23 /ATN)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /5V_SD)
    (add_net /ATN)
    (add_net /DAV)
    (add_net /DI)
    (add_net /DIO1)
    (add_net /DIO2)
    (add_net /DIO3)
    (add_net /DIO4)
    (add_net /DIO5)
    (add_net /DIO6)
    (add_net /DIO7)
    (add_net /DIO8)
    (add_net /DO)
    (add_net /EOI)
    (add_net /GND-GPIB)
    (add_net /GND_SD)
    (add_net /IFC)
    (add_net /NDAC)
    (add_net /NRFD)
    (add_net /REN)
    (add_net /SCK)
    (add_net /SRQ)
    (add_net /~CS)
  )
  (module 111-024-113L001-no-MH:111-024-113L001-no-MHs-courtyardY (layer B.Cu) (tedit 6061D1F4)
    (at 172.72 48.26 180)
    (descr 111-024-113L001-2)
    (tags Connector)
    (fp_text reference J1 (at 11.88 -1.623) (layer B.SilkS))
    (fp_text value 111-024-113L001-no-MHs (at 11.88 -1.623) (layer B.SilkS) hide)
    (pad 24 thru_hole circle (at 23.76 -4.29 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 1 /GND-GPIB))
    (pad 23 thru_hole circle (at 21.6 -4.29 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 1 /GND-GPIB))
    (pad 22 thru_hole circle (at 19.44 -4.29 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 1 /GND-GPIB))
    (pad 21 thru_hole circle (at 17.28 -4.29 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 1 /GND-GPIB))
    (pad 20 thru_hole circle (at 15.12 -4.29 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 1 /GND-GPIB))
    (pad 19 thru_hole circle (at 12.96 -4.29 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 1 /GND-GPIB))
    (pad 18 thru_hole circle (at 10.8 -4.29 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 1 /GND-GPIB))
    (pad 17 thru_hole circle (at 8.64 -4.29 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 3 /REN))
    (pad 16 thru_hole circle (at 6.48 -4.29 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 11 /DIO8))
    (pad 15 thru_hole circle (at 4.32 -4.29 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 9 /DIO7))
    (pad 14 thru_hole circle (at 2.16 -4.29 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 8 /DIO6))
    (pad 13 thru_hole circle (at 0 -4.29 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 7 /DIO5))
    (pad 12 thru_hole circle (at 23.76 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask B.SilkS))
    (pad 11 thru_hole circle (at 21.6 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 23 /ATN))
    (pad 10 thru_hole circle (at 19.44 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 22 /SRQ))
    (pad 9 thru_hole circle (at 17.28 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 21 /IFC))
    (pad 8 thru_hole circle (at 15.12 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 20 /NDAC))
    (pad 7 thru_hole circle (at 12.96 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 16 /NRFD))
    (pad 6 thru_hole circle (at 10.8 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 15 /DAV))
    (pad 5 thru_hole circle (at 8.64 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 13 /EOI))
    (pad 4 thru_hole circle (at 6.48 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 6 /DIO4))
    (pad 3 thru_hole circle (at 4.32 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 5 /DIO3))
    (pad 2 thru_hole circle (at 2.16 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 4 /DIO2))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask B.SilkS)
      (net 2 /DIO1))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x09_P2.54mm_Vertical (layer F.Cu) (tedit 6061CEF5)
    (at 187.96 59.69 180)
    (descr "Through hole straight pin header, 1x09, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x09 2.54mm single row")
    (fp_text reference J2 (at 2.86 -0.95) (layer F.SilkS))
    (fp_text value Conn_01x09_Male (at 2.499999 10.299999 90) (layer F.Fab))
    (fp_text user %R (at 0 10.16 90) (layer F.Fab))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /~CS))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /SCK))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /DO))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /DI))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /5V_SD))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /GND_SD))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x09_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pandauino_644-Narrow:644-Narrow (layer F.Cu) (tedit 605FD562)
    (at 180.699999 40.130001 270)
    (descr "Pandauino 644-Narrow")
    (tags "Arduino ATmega644 ATmega1284")
    (fp_text reference A1 (at 0.509999 -3.450001 180) (layer F.SilkS))
    (fp_text value 644-Narrow (at 15.241999 24.489999) (layer F.Fab))
    (fp_text user %R (at 15.241999 31.093999) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 23 thru_hole oval (at 17.78 33.02 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 24 thru_hole oval (at 17.78 30.48 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 25 thru_hole oval (at 17.78 27.94 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GND-GPIB))
    (pad 26 thru_hole oval (at 17.78 25.4 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 /DIO1))
    (pad 27 thru_hole oval (at 17.78 22.86 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 3 /REN))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 /DIO2))
    (pad 28 thru_hole oval (at 17.78 20.32 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 5 /DIO3))
    (pad 29 thru_hole oval (at 17.78 17.78 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 6 /DIO4))
    (pad 30 thru_hole oval (at 17.78 15.24 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 7 /DIO5))
    (pad 31 thru_hole oval (at 17.78 12.7 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 8 /DIO6))
    (pad 32 thru_hole oval (at 17.78 10.16 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 9 /DIO7))
    (pad 33 thru_hole oval (at 17.78 7.62 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 10 /~CS))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 11 /DIO8))
    (pad 34 thru_hole oval (at 17.78 5.08 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 12 /5V_SD))
    (pad 13 thru_hole oval (at 0 30.48 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 13 /EOI))
    (pad 35 thru_hole oval (at 17.78 2.54 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 14 /GND_SD))
    (pad 14 thru_hole oval (at 0 33.02 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 15 /DAV))
    (pad 36 thru_hole oval (at 17.78 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 0 35.56 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 16 /NRFD))
    (pad 22 thru_hole oval (at 17.78 35.56 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 38 thru_hole circle (at 8.89 1.27 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 17 /DI))
    (pad 39 thru_hole circle (at 6.35 1.27 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 37 thru_hole rect (at 11.43 1.27 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 40 thru_hole circle (at 11.43 -1.27 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 18 /DO))
    (pad 41 thru_hole circle (at 8.89 -1.27 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 19 /SCK))
    (pad 42 thru_hole circle (at 6.35 -1.27 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at 0 38.1 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 20 /NDAC))
    (pad 17 thru_hole circle (at 0 40.64 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 21 /IFC))
    (pad 18 thru_hole circle (at 0 43.18 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 22 /SRQ))
    (pad 19 thru_hole circle (at 17.78 43.18 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad 20 thru_hole circle (at 17.78 40.64 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 23 /ATN))
    (pad 21 thru_hole circle (at 17.78 38.1 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Module.3dshapes/Arduino_Nano_WithMountingHoles.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 132.08 37.592) (end 132.08 38.862) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 189.738 37.592) (end 132.08 37.592) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 189.738 61.468) (end 189.738 37.592) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 132.08 38.862) (end 132.08 38.608) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 132.08 61.468) (end 132.08 38.608) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 189.738 61.468) (end 132.08 61.468) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_text "Tektronix 4050 Flash Drive" (at 160.02 60.5) (layer F.SilkS))
)
