(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 26)
    (no_connects 1)
    (area 107.899999 108.229999 173.000001 138.330001)
    (thickness 1.6)
    (drawings 34)
    (tracks 105)
    (zones 0)
    (modules 14)
    (nets 52)
  )
  (page A4)
  (title_block
    (title "Raspberry Pi Hat Template")
    (date 2015-12-24)
    (rev 0.1)
    (company OpenFet)
    (comment 1 "Author: Julien")
    (comment 2 "License: CERN OHL V1.2")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.1)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (trace_clearance 0.15)
    (zone_clearance 0.2)
    (zone_45_only yes)
    (trace_min 0.1)
    (segment_width 0.35)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.26)
    (via_min_drill 0.16)
    (user_via 0.6 0.32)
    (user_via 1.5 0.8)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.2 1.2)
    (pad_drill 0.5)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 211.1 101.7)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory /home/mangokid/Desktop/hat_gerber/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(P3-Pad28)")
  (net 3 "Net-(P3-Pad3)")
  (net 4 "Net-(P3-Pad5)")
  (net 5 "Net-(P3-Pad7)")
  (net 6 "Net-(P3-Pad12)")
  (net 7 "Net-(P3-Pad17)")
  (net 8 "Net-(P3-Pad26)")
  (net 9 "Net-(P3-Pad32)")
  (net 10 "Net-(P3-Pad33)")
  (net 11 "Net-(P3-Pad35)")
  (net 12 "Net-(P3-Pad36)")
  (net 13 "Net-(P3-Pad40)")
  (net 14 VCC)
  (net 15 VCC5)
  (net 16 "Net-(P3-Pad8)")
  (net 17 "Net-(P3-Pad10)")
  (net 18 GPIO_17)
  (net 19 SD_D3)
  (net 20 SD_CLK)
  (net 21 SD_CMD)
  (net 22 MISO)
  (net 23 "Net-(P3-Pad19)")
  (net 24 "Net-(P3-Pad21)")
  (net 25 MOSI)
  (net 26 "Net-(P3-Pad23)")
  (net 27 "Net-(P3-Pad24)")
  (net 28 ID_SD)
  (net 29 "Net-(P3-Pad29)")
  (net 30 "Net-(P3-Pad31)")
  (net 31 SD_D2)
  (net 32 "Net-(R1-Pad1)")
  (net 33 "Net-(R2-Pad1)")
  (net 34 "Net-(R3-Pad1)")
  (net 35 "Net-(R4-Pad1)")
  (net 36 "Net-(R5-Pad1)")
  (net 37 "Net-(R6-Pad1)")
  (net 38 "Net-(R7-Pad1)")
  (net 39 "Net-(SW1-Pad1)")
  (net 40 "Net-(U1-Pad2)")
  (net 41 "Net-(U1-Pad4)")
  (net 42 "Net-(U1-Pad5)")
  (net 43 "Net-(U1-Pad6)")
  (net 44 "Net-(U1-Pad7)")
  (net 45 "Net-(U1-Pad16)")
  (net 46 "Net-(U1-Pad17)")
  (net 47 "Net-(U1-Pad18)")
  (net 48 "Net-(U1-Pad19)")
  (net 49 "Net-(U1-Pad20)")
  (net 50 "Net-(U1-Pad21)")
  (net 51 "Net-(U1-Pad22)")
  (net_class Default "This is the default net class."
    (clearance 0.15)
    (trace_width 0.2)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net GND)
    (add_net GPIO_17)
    (add_net ID_SD)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(P3-Pad10)")
    (add_net "Net-(P3-Pad12)")
    (add_net "Net-(P3-Pad17)")
    (add_net "Net-(P3-Pad19)")
    (add_net "Net-(P3-Pad21)")
    (add_net "Net-(P3-Pad23)")
    (add_net "Net-(P3-Pad24)")
    (add_net "Net-(P3-Pad26)")
    (add_net "Net-(P3-Pad28)")
    (add_net "Net-(P3-Pad29)")
    (add_net "Net-(P3-Pad3)")
    (add_net "Net-(P3-Pad31)")
    (add_net "Net-(P3-Pad32)")
    (add_net "Net-(P3-Pad33)")
    (add_net "Net-(P3-Pad35)")
    (add_net "Net-(P3-Pad36)")
    (add_net "Net-(P3-Pad40)")
    (add_net "Net-(P3-Pad5)")
    (add_net "Net-(P3-Pad7)")
    (add_net "Net-(P3-Pad8)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(SW1-Pad1)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net SD_CLK)
    (add_net SD_CMD)
    (add_net SD_D2)
    (add_net SD_D3)
    (add_net VCC)
    (add_net VCC5)
  )
  (module w_pin_strip:pin_socket_20x2 (layer F.Cu) (tedit 567B9DD9)
    (at 140.45 111.78)
    (descr "Pin socket 20x2pin")
    (tags "CONN DEV")
    (fp_text reference P3 (at 25 3.1 180) (layer F.SilkS))
    (fp_text value Raspberry_Pi_+_Conn (at 0 -5.08) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -24.13 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 14 VCC))
    (pad 2 thru_hole oval (at -24.13 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 15 VCC5))
    (pad 3 thru_hole oval (at -21.59 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P3-Pad3)"))
    (pad 4 thru_hole oval (at -21.59 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 15 VCC5))
    (pad 5 thru_hole oval (at -19.05 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(P3-Pad5)"))
    (pad 6 thru_hole oval (at -19.05 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 7 thru_hole oval (at -16.51 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P3-Pad7)"))
    (pad 8 thru_hole oval (at -16.51 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(P3-Pad8)"))
    (pad 9 thru_hole oval (at -13.97 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 10 thru_hole oval (at -13.97 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(P3-Pad10)"))
    (pad 11 thru_hole oval (at -11.43 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 18 GPIO_17))
    (pad 12 thru_hole oval (at -11.43 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P3-Pad12)"))
    (pad 13 thru_hole oval (at -8.89 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 19 SD_D3))
    (pad 14 thru_hole oval (at -8.89 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 15 thru_hole oval (at -6.35 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 20 SD_CLK))
    (pad 16 thru_hole oval (at -6.35 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 21 SD_CMD))
    (pad 17 thru_hole oval (at -3.81 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P3-Pad17)"))
    (pad 18 thru_hole oval (at -3.81 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 22 MISO))
    (pad 19 thru_hole oval (at -1.27 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(P3-Pad19)"))
    (pad 20 thru_hole oval (at -1.27 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 21 thru_hole oval (at 1.27 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(P3-Pad21)"))
    (pad 22 thru_hole oval (at 1.27 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 25 MOSI))
    (pad 23 thru_hole oval (at 3.81 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(P3-Pad23)"))
    (pad 24 thru_hole oval (at 3.81 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(P3-Pad24)"))
    (pad 25 thru_hole oval (at 6.35 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 26 thru_hole oval (at 6.35 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P3-Pad26)"))
    (pad 27 thru_hole oval (at 8.89 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 28 ID_SD))
    (pad 28 thru_hole oval (at 8.89 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P3-Pad28)"))
    (pad 29 thru_hole oval (at 11.43 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(P3-Pad29)"))
    (pad 30 thru_hole oval (at 11.43 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 31 thru_hole oval (at 13.97 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(P3-Pad31)"))
    (pad 32 thru_hole oval (at 13.97 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P3-Pad32)"))
    (pad 33 thru_hole oval (at 16.51 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P3-Pad33)"))
    (pad 34 thru_hole oval (at 16.51 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 35 thru_hole oval (at 19.05 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P3-Pad35)"))
    (pad 36 thru_hole oval (at 19.05 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P3-Pad36)"))
    (pad 37 thru_hole oval (at 21.59 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 31 SD_D2))
    (pad 38 thru_hole oval (at 21.59 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS))
    (pad 39 thru_hole oval (at 24.13 1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 40 thru_hole oval (at 24.13 -1.27) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(P3-Pad40)"))
    (model ../../../../../home/mangokid/kicad_libs/modules/packages3d/walter/pin_strip/pin_socket_20x2.wrl
      (at (xyz 0 0 -0.025))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 5687A909)
    (at 111.45 111.78)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 1.00076 5.00126) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers))
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 5687A906)
    (at 169.45 111.78)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 1.00076 5.00126) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers))
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 5687A5B1)
    (at 169.45 134.78)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 1.00076 5.00126) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers))
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 5687A904)
    (at 111.45 134.78)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 1.00076 5.00126) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers))
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5415CFA7)
    (at 125.576 135.228)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 0.127) (layer F.SilkS))
    (fp_text value 0 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 18 GPIO_17))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5415CFA7)
    (at 136.604 129.132)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 0) (layer F.SilkS))
    (fp_text value 33 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 21 SD_CMD))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5415CFA7)
    (at 136.604 126.719)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 0 -0.127) (layer F.SilkS))
    (fp_text value 33 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 22 MISO))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5415CFA7)
    (at 136.604 124.306)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at 0.074 0) (layer F.SilkS))
    (fp_text value 33 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 31 SD_D2))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5415CFA7)
    (at 136.604 121.893)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R5 (at 0 -0.127) (layer F.SilkS))
    (fp_text value 33 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R5-Pad1)"))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 19 SD_D3))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5415CFA7)
    (at 136.604 119.48)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R6 (at 0.074 0) (layer F.SilkS))
    (fp_text value 33 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R6-Pad1)"))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 25 MOSI))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 5415CFA7)
    (at 136.604 117.067)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R7 (at 0.074 0.127) (layer F.SilkS))
    (fp_text value 33 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R7-Pad1)"))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 20 SD_CLK))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPDT_PCM12 (layer F.Cu) (tedit 5788B26D)
    (at 118.931 136.384)
    (descr "Ultraminiature Surface Mount Slide Switch")
    (attr smd)
    (fp_text reference SW1 (at -0.033 0.368) (layer F.SilkS))
    (fp_text value SPST (at -0.287 0.368) (layer F.Fab))
    (pad "" np_thru_hole circle (at -1.5 0.325) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.5 0.325) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
    (pad 1 smd rect (at -2.25 -1.425) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(SW1-Pad1)"))
    (pad 2 smd rect (at 0.75 -1.425) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 14 VCC))
    (pad 3 smd rect (at 2.25 -1.425) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -3.65 1.425) (size 1 0.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 3.65 1.425) (size 1 0.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 3.65 -0.775) (size 1 0.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -3.65 -0.775) (size 1 0.8) (layers F.Cu F.Paste F.Mask))
  )
  (module ESP:ESP-12E (layer F.Cu) (tedit 559F8D21)
    (at 116.328 130.94 90)
    (descr "Module, ESP-8266, ESP-12, 16 pad, SMD")
    (tags "Module ESP-8266 ESP8266")
    (fp_text reference U1 (at 2.57 0.284 90) (layer F.SilkS))
    (fp_text value ESP-12E (at 8 1 90) (layer F.Fab))
    (fp_text user "No Copper" (at 6.892 -5.4 90) (layer F.CrtYd))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(R1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2 90) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(U1-Pad2)"))
    (pad 3 thru_hole oval (at 0 4 90) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 28 ID_SD))
    (pad 4 thru_hole oval (at 0 6 90) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(U1-Pad4)"))
    (pad 5 thru_hole oval (at 0 8 90) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(U1-Pad5)"))
    (pad 6 thru_hole oval (at 0 10 90) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(U1-Pad6)"))
    (pad 7 thru_hole oval (at 0 12 90) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(U1-Pad7)"))
    (pad 8 thru_hole oval (at 0 14 90) (size 2.5 1.1) (drill 0.65 (offset -0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(SW1-Pad1)"))
    (pad 9 smd oval (at 1.99 15.75 180) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R2-Pad1)"))
    (pad 10 smd oval (at 3.99 15.75 180) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R3-Pad1)"))
    (pad 11 smd oval (at 5.99 15.75 180) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R4-Pad1)"))
    (pad 12 smd oval (at 7.99 15.75 180) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R5-Pad1)"))
    (pad 13 smd oval (at 9.99 15.75 180) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R6-Pad1)"))
    (pad 14 smd oval (at 11.99 15.75 180) (size 2.4 1.1) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R7-Pad1)"))
    (pad 15 thru_hole oval (at 14 14 90) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 16 thru_hole oval (at 14 12 90) (size 2.5 1.1) (drill 0.65 (offset 0.6 0)) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(U1-Pad16)"))
    (pad 17 thru_hole oval (at 14 10 90) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(U1-Pad17)"))
    (pad 18 thru_hole oval (at 14 8 90) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(U1-Pad18)"))
    (pad 19 thru_hole oval (at 14 6 90) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(U1-Pad19)"))
    (pad 20 thru_hole oval (at 14 4 90) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(U1-Pad20)"))
    (pad 21 thru_hole oval (at 14 2 90) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(U1-Pad21)"))
    (pad 22 thru_hole oval (at 14 0 90) (size 2.5 1.1) (drill 0.65 (offset 0.7 0)) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(U1-Pad22)"))
    (model ${ESPLIB}/ESP8266.3dshapes/ESP-12.wrl
      (at (xyz 0.04 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "By Eikacy" (at 123.724 127.608) (layer F.SilkS))
  (gr_text ESP-12E/F (at 123.47 124.687) (layer F.SilkS))
  (gr_text "R0=0\nR1/R6=33" (at 122.962 119.861) (layer F.SilkS))
  (dimension 30 (width 0.3) (layer Dwgs.User)
    (gr_text "30.000 mm" (at 187.3 123.28 270) (layer Dwgs.User))
    (feature1 (pts (xy 169.95 138.28) (xy 188.65 138.28)))
    (feature2 (pts (xy 169.95 108.28) (xy 188.65 108.28)))
    (crossbar (pts (xy 185.95 108.28) (xy 185.95 138.28)))
    (arrow1a (pts (xy 185.95 138.28) (xy 185.363579 137.153496)))
    (arrow1b (pts (xy 185.95 138.28) (xy 186.536421 137.153496)))
    (arrow2a (pts (xy 185.95 108.28) (xy 185.363579 109.406504)))
    (arrow2b (pts (xy 185.95 108.28) (xy 186.536421 109.406504)))
  )
  (dimension 65 (width 0.3) (layer Dwgs.User)
    (gr_text "65.000 mm" (at 140.45 84.430001) (layer Dwgs.User))
    (feature1 (pts (xy 107.95 111.28) (xy 107.95 83.080001)))
    (feature2 (pts (xy 172.95 111.28) (xy 172.95 83.080001)))
    (crossbar (pts (xy 172.95 85.780001) (xy 107.95 85.780001)))
    (arrow1a (pts (xy 107.95 85.780001) (xy 109.076504 85.19358)))
    (arrow1b (pts (xy 107.95 85.780001) (xy 109.076504 86.366422)))
    (arrow2a (pts (xy 172.95 85.780001) (xy 171.823496 85.19358)))
    (arrow2b (pts (xy 172.95 85.780001) (xy 171.823496 86.366422)))
  )
  (gr_line (start 110.95 138.28) (end 169.95 138.28) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 107.95 111.28) (end 107.95 135.28) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.95 108.28) (end 110.95 108.28) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 172.95 135.28) (end 172.95 111.28) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 169.95 111.28) (end 169.95 108.28) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 169.95 135.28) (end 172.95 135.28) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 110.95 135.28) (end 110.95 138.28) (angle 90) (layer Edge.Cuts) (width 0.1))
  (dimension 58 (width 0.3) (layer Dwgs.User)
    (gr_text "58.000 mm" (at 140.45 94.93) (layer Dwgs.User))
    (feature1 (pts (xy 169.45 111.78) (xy 169.45 93.58)))
    (feature2 (pts (xy 111.45 111.78) (xy 111.45 93.58)))
    (crossbar (pts (xy 111.45 96.28) (xy 169.45 96.28)))
    (arrow1a (pts (xy 169.45 96.28) (xy 168.323496 96.866421)))
    (arrow1b (pts (xy 169.45 96.28) (xy 168.323496 95.693579)))
    (arrow2a (pts (xy 111.45 96.28) (xy 112.576504 96.866421)))
    (arrow2b (pts (xy 111.45 96.28) (xy 112.576504 95.693579)))
  )
  (gr_arc (start 110.95 111.28) (end 107.95 111.28) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.976 131.418) (xy 113.945 131.418) (xy 113.945 115.289) (xy 107.976 115.289)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.976 131.418) (xy 113.945 131.418) (xy 113.945 115.289) (xy 107.976 115.289)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.707 108.304) (xy 114.707 138.276) (xy 166.142 138.276) (xy 166.142 108.304)
      )
    )
  )
)
