(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(D1-K)")
  (net 2 "+BATT")
  (net 3 "GND")
  (net 4 "Net-(D1-A)")
  (net 5 "Net-(JP1-B)")
  (net 6 "Net-(JP2-B)")
  (net 7 "Net-(J1-Pin_1)")
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 151.9936 97.8297 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Bachmann Shay Chuff Trigger.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at 2.944648 -0.026672) (layer "F.SilkS"))
    (fp_text value ".01uf" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 2 "+BATT") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 3 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 177.075639 97.756318 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Bachmann Shay Chuff Trigger.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C3" (at 2.948082 0.068429) (layer "F.SilkS"))
    (fp_text value ".01uf" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 2 "+BATT") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 3 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (at 139.7651 94.5388 180)
    (descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "Bachmann Shay Chuff Trigger.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr smd)
    (fp_text reference "LED" (at 0 -1.82 180) (layer "F.SilkS"))
    (fp_text value "RED LED" (at 0 1.82 180) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.175439)
      (net 1 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.175439)
      (net 4 "Net-(D1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3mm" (layer "F.Cu")
    (at 116.69268 97.48266)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (property "Sheetfile" "Bachmann Shay Chuff Trigger.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -4) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "MountingHole:MountingHole_3mm" (layer "F.Cu")
    (at 146.13128 97.74428)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (property "Sheetfile" "Bachmann Shay Chuff Trigger.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -4) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "MountingHole:MountingHole_3mm" (layer "F.Cu")
    (at 186.59602 97.69856)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (property "Sheetfile" "Bachmann Shay Chuff Trigger.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -4) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 134.6448 94.5642)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Bachmann Shay Chuff Trigger.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at 0.026 1.6764) (layer "F.SilkS") hide)
    (fp_text value "2.5k" (at 0 1.82) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 6 "Net-(JP2-B)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.192308)
      (net 4 "Net-(D1-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92Flat" (layer "F.Cu")
    (at 124.3457 94.225)
    (descr "TO-92Flat package, often used for hall sensors, drill 0.75mm (see e.g. http://www.ti.com/lit/ds/symlink/drv5023.pdf)")
    (tags "to-92Flat hall sensor")
    (property "Sheetfile" "Bachmann Shay Chuff Trigger.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at 1.3335 1.45542) (layer "F.SilkS") hide)
    (fp_text value "DRV5033" (at 1.25 1.7) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 1.27 -2.06) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 180) (size 1.05 1.3) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 2 "+BATT") (pinfunction "VCC") (pintype "power_in"))
    (pad "2" thru_hole oval (at 1.27 0 180) (size 1.05 1.3) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 3 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole oval (at 2.54 0 180) (size 1.05 1.3) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(D1-K)") (pinfunction "Vout") (pintype "open_collector"))
    (model "${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92Flat.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92Flat" (layer "F.Cu")
    (at 153.43886 94.21114)
    (descr "TO-92Flat package, often used for hall sensors, drill 0.75mm (see e.g. http://www.ti.com/lit/ds/symlink/drv5023.pdf)")
    (tags "to-92Flat hall sensor")
    (property "Sheetfile" "Bachmann Shay Chuff Trigger.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 1.06934 1.44526) (layer "F.SilkS") hide)
    (fp_text value "DRV5033" (at 1.25 1.7) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 1.27 -2.06) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 180) (size 1.05 1.3) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 2 "+BATT") (pinfunction "VCC") (pintype "power_in"))
    (pad "2" thru_hole oval (at 1.27 0 180) (size 1.05 1.3) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 3 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole oval (at 2.54 0 180) (size 1.05 1.3) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(D1-K)") (pinfunction "Vout") (pintype "open_collector"))
    (model "${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92Flat.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92Flat" (layer "F.Cu")
    (at 177.09896 94.225)
    (descr "TO-92Flat package, often used for hall sensors, drill 0.75mm (see e.g. http://www.ti.com/lit/ds/symlink/drv5023.pdf)")
    (tags "to-92Flat hall sensor")
    (property "Sheetfile" "Bachmann Shay Chuff Trigger.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U3" (at 1.15824 1.41732) (layer "F.SilkS") hide)
    (fp_text value "DRV5033" (at 1.25 1.7) (layer "B.SilkS"))
    (fp_text user "${REFERENCE}" (at 1.27 -2.06) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 180) (size 1.05 1.3) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 2 "+BATT") (pinfunction "VCC") (pintype "power_in"))
    (pad "2" thru_hole oval (at 1.27 0 180) (size 1.05 1.3) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 3 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole oval (at 2.54 0 180) (size 1.05 1.3) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(D1-K)") (pinfunction "Vout") (pintype "open_collector"))
    (model "${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92Flat.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (at 139.05 98.4375 -90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "Bachmann Shay Chuff Trigger.kicad_sch")
    (property "Sheetname" "")
    (property "ki_keywords" "ZXTR2105F-7")
    (attr smd)
    (fp_text reference "Q1" (at 0.0485 2.159 90) (layer "F.SilkS") hide)
    (fp_text value "ZXTR2105F-7" (at 0 2.4 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9375 -0.95 270) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "2" smd roundrect (at -0.9375 0.95 270) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(JP1-B)") (pinfunction "VOUT") (pintype "output"))
    (pad "3" smd roundrect (at 0.9375 0 270) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+BATT") (pinfunction "VIN") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (at 122.7328 97.6122 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "Bachmann Shay Chuff Trigger.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at 3.184852 -0.019217) (layer "F.SilkS"))
    (fp_text value ".01uf" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 2 "+BATT") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 3 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (at 126.216206 98.5125 -90)
    (descr "Fuse SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse handsolder")
    (property "Sheetfile" "Bachmann Shay Chuff Trigger.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resettable fuse, polymeric positive temperature coefficient, small symbol")
    (property "ki_keywords" "resettable fuse PTC PPTC polyfuse polyswitch")
    (attr smd)
    (fp_text reference "F1" (at 3.226344 0.018611) (layer "F.SilkS"))
    (fp_text value "100ma" (at 0 1.82 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.175439)
      (net 2 "+BATT") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.175439)
      (net 7 "Net-(J1-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuse_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (at 134.85 98 90)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "Bachmann Shay Chuff Trigger.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Solder Jumper, 2-pole, open")
    (property "ki_keywords" "solder jumper SPST")
    (attr exclude_from_pos_files)
    (fp_text reference "JP1" (at -2.314671 0.030454 180) (layer "F.SilkS"))
    (fp_text value "SolderJumper_2_Open" (at 0 1.9 90) (layer "F.Fab") hide)
    (pad "1" smd custom (at -0.65 0 90) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 2 "+BATT") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0.5 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.5 -0.75)
          )
          (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.65 0 90) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 5 "Net-(JP1-B)") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0 -0.75)
          )
          (width 0) (fill yes))
      ))
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (at 130.3424 94.1324)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "Bachmann Shay Chuff Trigger.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Solder Jumper, 2-pole, open")
    (property "ki_keywords" "solder jumper SPST")
    (attr exclude_from_pos_files)
    (fp_text reference "JP2" (at -0.1674 1.905) (layer "F.SilkS"))
    (fp_text value "SolderJumper_2_Open" (at 0 1.9) (layer "F.Fab") hide)
    (pad "1" smd custom (at -0.65 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 5 "Net-(JP1-B)") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0.5 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.5 -0.75)
          )
          (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.65 0) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 6 "Net-(JP2-B)") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly
          (pts
            (xy 0 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0 -0.75)
          )
          (width 0) (fill yes))
      ))
  )
  (footprint "Connector_PinHeader_1.27mm:PinHeader_1x03_P1.27mm_Vertical" (layer "F.Cu")
    (at 129.1844 100.0506 90)
    (descr "Through hole straight pin header, 1x03, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x03 1.27mm single row")
    (property "Sheetfile" "Bachmann Shay Chuff Trigger.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J1" (at 0.127 -1.8034 180) (layer "F.SilkS") hide)
    (fp_text value "Wire Harness" (at 0 4.235 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 90) (size 1 1) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(J1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 1.27 90) (size 1 1) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 3 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54 90) (size 1 1) (drill 0.65) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(D1-K)") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x03_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 186.5249 92.53982) (end 186.5249 94.09684)
    (layer "Edge.Cuts"))
  (gr_line (start 193.294 102.93858) (end 181.26964 102.94366)
    (layer "Edge.Cuts"))
  (gr_line (start 153.05786 102.81158) (end 111.15802 102.82936)
    (layer "Edge.Cuts"))
  (gr_line (start 181.26964 102.94366) (end 181.26202 101.43744)
    (layer "Edge.Cuts"))
  (gr_line (start 181.26202 101.43744) (end 153.05786 101.44506)
    (layer "Edge.Cuts"))
  (gr_line (start 111.15802 92.48902) (end 186.52236 92.54744)
    (layer "Edge.Cuts"))
  (gr_line (start 111.15802 102.82936) (end 111.15802 92.48902)
    (layer "Edge.Cuts"))
  (gr_line (start 153.05786 101.44506) (end 153.05786 102.81158)
    (layer "Edge.Cuts"))
  (gr_line (start 193.29908 94.107) (end 193.294 102.93858)
    (layer "Edge.Cuts"))
  (gr_line (start 186.5249 94.09684) (end 193.29908 94.107)
    (layer "Edge.Cuts"))
  (gr_text "Sensors \non this \nside!" (at 125.313175 99.018776) (layer "B.SilkS"))
  (gr_text "Set lead \nlength to \n~12mm!" (at 155 99) (layer "B.SilkS"))
  (gr_text "Gnd" (at 130.4544 97.8662 90) (layer "F.SilkS"))
  (gr_text "+V" (at 129.1844 98.3234 90) (layer "F.SilkS"))
  (gr_text "Hall Effect Chuff Sensor\n5-36VDC/Open Collector SW\nCopyright 2024  \nEric Timberlake\nVersion 1.4" (at 158 97) (layer "F.SilkS"))
  (gr_text "Out" (at 131.6736 97.9424 90) (layer "F.SilkS"))
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 178.308 91.98356) (xy 111.11484 91.99372))
    (height 11.851646)
    (gr_text "67.1932 mm" (at 144.709356 78.336994 0.008663457939) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 2) (units_format 1) (precision 4))
    (style (thickness 0.3) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 181.12232 93.9419) (xy 193.21526 94.04858))
    (height -6.889986)
    (gr_text "12.0934 mm" (at 187.245447 85.305592 359.4945683) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 2) (units_format 1) (precision 4))
    (style (thickness 0.3) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 154.71394 92.09786) (xy 111.21898 92.1258))
    (height 6.993078)
    (gr_text "43.4950 mm" (at 132.960812 83.318753 0.0368052726) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 2) (units_format 1) (precision 4))
    (style (thickness 0.3) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 125.6792 92.39504) (xy 111.1377 92.32646))
    (height 2.666562)
    (gr_text "14.5417 mm" (at 118.429515 87.894238 -0.2702139) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 2) (units_format 1) (precision 4))
    (style (thickness 0.3) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 111.05896 102.88778) (xy 192.80886 102.80904))
    (height 5.398024)
    (gr_text "81.7499 mm" (at 151.937375 106.446432 0.05518622388) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 2) (units_format 1) (precision 4))
    (style (thickness 0.3) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 153.10866 102.88524) (xy 181.25186 102.78364))
    (height 10.769896)
    (gr_text "28.1434 mm" (at 167.212642 111.804278 0.2068430708) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 2) (units_format 1) (precision 4))
    (style (thickness 0.3) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 192.8749 92.63888) (xy 192.8749 102.6541))
    (height -6.97484)
    (gr_text "10.0152 mm" (at 198.04974 97.64649 90) (layer "Dwgs.User"))
    (format (prefix "") (suffix "") (units 2) (units_format 1) (precision 4))
    (style (thickness 0.3) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (zone (net 3) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.63402 90.75674)
        (xy 195.8467 90.46718)
        (xy 195.99148 105.36936)
        (xy 109.34192 103.76916)
      )
    )
  )
  (zone (net 3) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.92612 91.11996)
        (xy 195.55714 90.61196)
        (xy 195.55714 104.64292)
        (xy 110.21568 104.35082)
      )
    )
  )
)
