(kicad_pcb (version 4) (host pcbnew 4.0.5+dfsg1-4)
  (general
    (links 77)
    (no_connects 2)
    (area 122.491499 95.364299 183.832501 119.875301)
    (thickness 1.6)
    (drawings 10)
    (tracks 376)
    (zones 0)
    (modules 24)
    (nets 38)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.15)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.381)
    (edge_width 1.00076)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3048)
    (pcb_text_size 1.524 2.032)
    (mod_edge_width 0.381)
    (mod_text_size 1.524 1.524)
    (mod_text_width 0.3048)
    (pad_size 1.524 1.524)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF3F)
    (pcbplotparams
      (layerselection 0x012f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory output/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C2-Pad1)")
  (net 3 PA12)
  (net 4 PA11)
  (net 5 "Net-(D1-Pad2)")
  (net 6 "Net-(J1-Pad3)")
  (net 7 "Net-(J1-Pad2)")
  (net 8 PC13)
  (net 9 PC14)
  (net 10 PC15)
  (net 11 NRST)
  (net 12 PA0)
  (net 13 PA1)
  (net 14 PA2)
  (net 15 PA3)
  (net 16 PA4)
  (net 17 PA5)
  (net 18 PA6)
  (net 19 PA7)
  (net 20 PB1)
  (net 21 PB9)
  (net 22 PB8)
  (net 23 PB7)
  (net 24 PB6)
  (net 25 PB5)
  (net 26 PB4)
  (net 27 PB3)
  (net 28 PA15)
  (net 29 PA14)
  (net 30 PA13)
  (net 31 PA10)
  (net 32 PA9)
  (net 33 PA8)
  (net 34 "Net-(R1-Pad2)")
  (net 35 GND)
  (net 36 +3V3)
  (net 37 "Net-(C8-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.15)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net +3V3)
    (add_net GND)
    (add_net NRST)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(R1-Pad2)")
    (add_net PA0)
    (add_net PA1)
    (add_net PA10)
    (add_net PA11)
    (add_net PA12)
    (add_net PA13)
    (add_net PA14)
    (add_net PA15)
    (add_net PA2)
    (add_net PA3)
    (add_net PA4)
    (add_net PA5)
    (add_net PA6)
    (add_net PA7)
    (add_net PA8)
    (add_net PA9)
    (add_net PB1)
    (add_net PB3)
    (add_net PB4)
    (add_net PB5)
    (add_net PB6)
    (add_net PB7)
    (add_net PB8)
    (add_net PB9)
    (add_net PC13)
    (add_net PC14)
    (add_net PC15)
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5AAE6E46)
    (at 138.81862 103.60152 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at 0.03048 -0.04318 270) (layer F.SilkS))
    (fp_text value 1.5k (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 36 +3V3))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad3)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:LQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 5AAE6DCF)
    (at 159.4612 107.62488 270)
    (descr "48 LEAD LQFP 7x7mm (see MICREL LQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (autoplace_cost90 2)
    (attr smd)
    (fp_text reference U1 (at -0.14478 -0.04318 360) (layer F.SilkS))
    (fp_text value STM32F103CB (at 0 6 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -4.35 -2.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -4.35 -2.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 PC13))
    (pad 3 smd rect (at -4.35 -1.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 PC14))
    (pad 4 smd rect (at -4.35 -1.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 PC15))
    (pad 5 smd rect (at -4.35 -0.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 6 smd rect (at -4.35 -0.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 7 smd rect (at -4.35 0.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 NRST))
    (pad 8 smd rect (at -4.35 0.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 35 GND))
    (pad 9 smd rect (at -4.35 1.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 36 +3V3))
    (pad 10 smd rect (at -4.35 1.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 PA0))
    (pad 11 smd rect (at -4.35 2.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 PA1))
    (pad 12 smd rect (at -4.35 2.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 PA2))
    (pad 13 smd rect (at -2.75 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 PA3))
    (pad 14 smd rect (at -2.25 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 16 PA4))
    (pad 15 smd rect (at -1.75 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 17 PA5))
    (pad 16 smd rect (at -1.25 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 PA6))
    (pad 17 smd rect (at -0.75 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 PA7))
    (pad 18 smd rect (at -0.25 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R1-Pad2)"))
    (pad 19 smd rect (at 0.25 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 PB1))
    (pad 20 smd rect (at 0.75 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 35 GND))
    (pad 21 smd rect (at 1.25 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 1.75 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 2.25 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 35 GND))
    (pad 24 smd rect (at 2.75 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 36 +3V3))
    (pad 25 smd rect (at 4.35 2.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 26 smd rect (at 4.35 2.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 27 smd rect (at 4.35 1.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 28 smd rect (at 4.35 1.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 29 smd rect (at 4.35 0.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 33 PA8))
    (pad 30 smd rect (at 4.35 0.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 PA9))
    (pad 31 smd rect (at 4.35 -0.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 31 PA10))
    (pad 32 smd rect (at 4.35 -0.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 PA11))
    (pad 33 smd rect (at 4.35 -1.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 PA12))
    (pad 34 smd rect (at 4.35 -1.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 PA13))
    (pad 35 smd rect (at 4.35 -2.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 35 GND))
    (pad 36 smd rect (at 4.35 -2.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 36 +3V3))
    (pad 37 smd rect (at 2.75 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 PA14))
    (pad 38 smd rect (at 2.25 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 PA15))
    (pad 39 smd rect (at 1.75 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 PB3))
    (pad 40 smd rect (at 1.25 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 PB4))
    (pad 41 smd rect (at 0.75 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 PB5))
    (pad 42 smd rect (at 0.25 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 PB6))
    (pad 43 smd rect (at -0.25 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 PB7))
    (pad 44 smd rect (at -0.75 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 35 GND))
    (pad 45 smd rect (at -1.25 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 PB8))
    (pad 46 smd rect (at -1.75 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 PB9))
    (pad 47 smd rect (at -2.25 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 35 GND))
    (pad 48 smd rect (at -2.75 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 36 +3V3))
    (model Housings_QFP.3dshapes/LQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5AAE6DEA)
    (at 169.7482 105.3338 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at -0.0762 -0.0381 180) (layer F.SilkS))
    (fp_text value 27pF (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 35 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5AAE6DD9)
    (at 169.7228 101.1936)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at -0.0381 -0.0381) (layer F.SilkS))
    (fp_text value 27pF (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 35 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5AAE6DE4)
    (at 169.7482 110.1852)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at 0 -0.0381) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 35 GND))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 36 +3V3))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5AAE6DF1)
    (at 169.7482 114.1984 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C4 (at 0 -0.0381 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 35 GND))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 36 +3V3))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5AAE6E38)
    (at 143.0274 103.6574 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C5 (at 0.03556 -0.0762 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 36 +3V3))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 35 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5AAE6E1A)
    (at 149.3774 101.1936)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C6 (at -0.0381 0.0635) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 36 +3V3))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 35 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-1206_Pol (layer F.Cu) (tedit 0)
    (at 132.8674 102.6668)
    (attr smd)
    (fp_text reference C8 (at 0 0) (layer F.SilkS))
    (fp_text value 10uF (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.651 0) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 1.651 0) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 35 GND))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-1206_Pol (layer F.Cu) (tedit 5AAE6E72)
    (at 132.8674 112.522 180)
    (attr smd)
    (fp_text reference C9 (at 0.03048 -0.01778 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.651 0 180) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 36 +3V3))
    (pad 2 smd rect (at 1.651 0 180) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 35 GND))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5AAE6E4A)
    (at 143.0528 111.6076 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C11 (at 0 0.0254 90) (layer F.SilkS))
    (fp_text value 47p (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 PA12))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 35 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5AAE6E31)
    (at 149.3901 114.2238)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C12 (at -0.0762 0) (layer F.SilkS))
    (fp_text value 47p (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 PA11))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 35 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 5AAE6E23)
    (at 149.352 107.5944 180)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D1 (at -0.0762 -0.1143 180) (layer F.SilkS))
    (fp_text value LED (at 0 2 180) (layer F.Fab))
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 35 GND))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x16 (layer F.Cu) (tedit 5AAE5131)
    (at 176.29 97.31 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -0.11176 -2.57048 270) (layer F.SilkS))
    (fp_text value CONN_01X16 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 36 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 35 GND))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 PC13))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 PC14))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 PC15))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 NRST))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 PA0))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 PA1))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 PA2))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 PA3))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 PA4))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 PA5))
    (pad 13 thru_hole oval (at 0 30.48 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 PA6))
    (pad 14 thru_hole oval (at 0 33.02 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 PA7))
    (pad 15 thru_hole oval (at 0 35.56 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 PB1))
    (pad 16 thru_hole oval (at 0 38.1 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 PB9))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x16.wrl
      (at (xyz 0 -0.75 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x16 (layer F.Cu) (tedit 5AAE6E0A)
    (at 176.29 117.88 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at -0.0762 -2.5146 270) (layer F.SilkS))
    (fp_text value CONN_01X16 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 36 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 35 GND))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 PB8))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 PB7))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 PB6))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 PB5))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 PB4))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 PB3))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 PA15))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 PA14))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 PA13))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 PA12))
    (pad 13 thru_hole oval (at 0 30.48 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 PA11))
    (pad 14 thru_hole oval (at 0 33.02 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 PA10))
    (pad 15 thru_hole oval (at 0 35.56 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 PA9))
    (pad 16 thru_hole oval (at 0 38.1 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 PA8))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x16.wrl
      (at (xyz 0 -0.75 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5AAE6E13)
    (at 149.352 104.267)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0.0254 0.0254) (layer F.SilkS))
    (fp_text value 1K (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5AAE6E6A)
    (at 138.811 111.601 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 0 270) (layer F.SilkS))
    (fp_text value 22R (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad3)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 PA12))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5AAE6E57)
    (at 149.352 110.8964)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 0.02794 -0.02794) (layer F.SilkS))
    (fp_text value 22R (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad2)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 PA11))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_HC49-4H_Vertical (layer F.Cu) (tedit 5AAE6DC6)
    (at 177.25136 105.3338 270)
    (descr "Crystal THT HC-49-4H http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-49-4H")
    (fp_text reference Y1 (at 2.3749 -0.02794 270) (layer F.SilkS))
    (fp_text value 12MHz (at 2.44 3.525 270) (layer F.Fab))
    (fp_text user %R (at 2.44 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 4.88 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_HC49-4H_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module diynuk-extras:USB-A-PLUG (layer F.Cu) (tedit 57C64714)
    (at 127.381 107.6198)
    (descr "USB A PLUG Through Hole")
    (tags USB)
    (fp_text reference J1 (at -7.62 0 90) (layer F.SilkS))
    (fp_text value USB_A (at -3.81 -10.16) (layer F.SilkS) hide)
    (pad 5 thru_hole oval (at -2.10058 5.69976) (size 3.50012 1.50114) (drill oval 2.49936 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 35 GND))
    (pad 5 thru_hole oval (at -2.10058 -5.69976) (size 3.50012 1.50114) (drill oval 2.49936 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 35 GND))
    (pad 3 thru_hole circle (at 0 -1.00076) (size 1.39954 1.39954) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J1-Pad3)"))
    (pad 2 thru_hole circle (at 0 1.00076) (size 1.39954 1.39954) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J1-Pad2)"))
    (pad 4 thru_hole circle (at 0 -3.50012) (size 1.51892 1.51892) (drill 0.91948) (layers *.Cu *.Mask F.SilkS)
      (net 35 GND))
    (pad 1 thru_hole circle (at 0 3.50012) (size 1.51892 1.51892) (drill 0.91948) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(C8-Pad1)"))
    (pad 7 thru_hole circle (at -2.10058 -2.25044) (size 1.09982 1.09982) (drill 1.09982) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole circle (at -2.10058 2.25044) (size 1.09982 1.09982) (drill 1.09982) (layers *.Cu *.Mask F.SilkS))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E)
    (at 134.45 107.63 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U2 (at -0.397 0.0254 180) (layer F.SilkS))
    (fp_text value AP7333-33SRG-7 (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 35 GND))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 36 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module diynuk-extras:logo_front_silk (layer F.Cu) (tedit 0)
    (at 182.06 107.61 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module diynuk-extras:mai68-art (layer B.Cu) (tedit 0)
    (at 136.28 107.24)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module diynuk-extras:logo_back_silk (layer B.Cu) (tedit 0)
    (at 157.29 107.61)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (gr_line (start 124.56612 113.32464) (end 125.98476 113.32464) (angle 90) (layer Edge.Cuts) (width 1))
  (gr_line (start 124.58136 101.9175) (end 126 101.9175) (angle 90) (layer Edge.Cuts) (width 1))
  (gr_line (start 127.762 95.5548) (end 178.562 95.5548) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 122.682 114.6048) (end 122.682 100.6348) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 178.562 119.6848) (end 127.762 119.6848) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_line (start 183.642 114.6048) (end 183.642 100.6348) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_arc (start 178.562 100.6348) (end 178.562 95.5548) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_arc (start 178.562 114.6048) (end 183.642 114.6048) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_arc (start 127.762 100.6348) (end 122.682 100.6348) (angle 90) (layer Edge.Cuts) (width 0.381))
  (gr_arc (start 127.762 114.6048) (end 127.762 119.6848) (angle 90) (layer Edge.Cuts) (width 0.381))
  (zone (net 36) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 178.90236 96.12122) (xy 180.90896 99.24542) (xy 180.78196 115.50142) (xy 178.16576 118.75262) (xy 126.70536 118.72722)
        (xy 122.74296 114.18062) (xy 122.79376 100.82022) (xy 126.32436 96.27362)
      )
    )
  )
  (zone (net 35) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 179.01412 96.12122) (xy 181.02072 99.24542) (xy 180.89372 115.50142) (xy 178.27752 118.75262) (xy 126.81712 118.72722)
        (xy 122.85472 114.18062) (xy 122.90552 100.82022) (xy 126.43612 96.27362)
      )
    )
  )
)
