(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 38)
    (no_connects 0)
    (area 137.634 97.714999 173.306174 163.397001)
    (thickness 1.6)
    (drawings 22)
    (tracks 209)
    (zones 0)
    (modules 9)
    (nets 30)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.8)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.5)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.75)
    (via_drill 0.5)
    (via_min_size 0.6)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1 1)
    (pad_drill 0.635)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x01520_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 MISO)
  (net 3 MOSI)
  (net 4 CLK)
  (net 5 D10)
  (net 6 "Net-(U1-Pad6)")
  (net 7 D6)
  (net 8 "Net-(U1-Pad11)")
  (net 9 "Net-(U1-Pad12)")
  (net 10 +3V3)
  (net 11 D4)
  (net 12 D5)
  (net 13 D7)
  (net 14 "Net-(uP1-Pad22)")
  (net 15 Ant)
  (net 16 TX0)
  (net 17 RX1)
  (net 18 RESET)
  (net 19 D2)
  (net 20 D3)
  (net 21 D8)
  (net 22 D9)
  (net 23 A0)
  (net 24 A1)
  (net 25 A2)
  (net 26 A3)
  (net 27 "Net-(P2-Pad1)")
  (net 28 SDA)
  (net 29 SCL)
  (net_class Default "This is the default net class."
    (clearance 0.8)
    (trace_width 0.5)
    (via_dia 0.75)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net A0)
    (add_net A1)
    (add_net A2)
    (add_net A3)
    (add_net Ant)
    (add_net CLK)
    (add_net D10)
    (add_net D2)
    (add_net D3)
    (add_net D4)
    (add_net D5)
    (add_net D6)
    (add_net D7)
    (add_net D8)
    (add_net D9)
    (add_net GND)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(uP1-Pad22)")
    (add_net RESET)
    (add_net RX1)
    (add_net SCL)
    (add_net SDA)
    (add_net TX0)
  )
  (module Connect:PINTST (layer F.Cu) (tedit 5819560E)
    (at 144.018 143.256)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P7 (at 0 -1.26746) (layer F.SilkS))
    (fp_text value Ant (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.253 1.253) (drill 0.85) (layers *.Cu *.Mask F.SilkS)
      (net 15 Ant))
    (model Connect.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5818D5E6)
    (at 144.526 130.302)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 0.254 5.334) (layer F.SilkS))
    (fp_text value CONN_2 (at -2.826 1.398 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 D8))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 D9))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module mysensors_connectors:SMA_EDGE (layer F.Cu) (tedit 58111359)
    (at 138.684 143.256 270)
    (fp_text reference P1 (at 0 -6.35 270) (layer F.SilkS) hide)
    (fp_text value Ant_SMA (at 8.382 -2.286 450) (layer F.SilkS))
    (pad 2 smd rect (at -2.1463 -2.0955 270) (size 1.27 4.191) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.1463 -2.0955 270) (size 1.27 4.191) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 -1.8415 270) (size 1.27 3.683) (layers F.Cu F.Paste F.Mask)
      (net 15 Ant))
    (pad 2 smd rect (at -2.1463 -2.0955 270) (size 1.27 4.191) (layers B.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.1463 -2.0955 270) (size 1.27 4.191) (layers B.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module Connect:PINHEAD1-3 (layer F.Cu) (tedit 5818D5CC)
    (at 168.148 107.442 270)
    (attr virtual)
    (fp_text reference P2 (at 4.953 0.381 360) (layer F.SilkS))
    (fp_text value "3.3v Gnd Raw" (at 0 -2.794 270) (layer F.Fab))
    (pad 1 thru_hole oval (at -2.54 0 270) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 27 "Net-(P2-Pad1)"))
    (pad 2 thru_hole oval (at 0 0 270) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 1.50622 3.01498) (drill 0.99822) (layers *.Cu *.Mask)
      (net 10 +3V3))
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 5818D24D)
    (at 143.51 104.902)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 15.24) (layer F.SilkS))
    (fp_text value CONN_1 (at -3.048 5.842 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 TX0))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 RX1))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 RESET))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 D2))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 D3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 5818D25E)
    (at 168.656 115.062)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at 0.254 10.16) (layer F.SilkS))
    (fp_text value CONN_3 (at 2.794 4.064 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 A3))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 A2))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 A1))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 A0))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module mysensors_radios:RFM69HW_SMD_Handsoldering-Narrow (layer F.Cu) (tedit 58142CD3)
    (at 163.2 157.3 180)
    (descr RFM69HW)
    (tags "RFM69HW, RF69")
    (fp_text reference U1 (at 0.254 -1.778 180) (layer F.SilkS))
    (fp_text value RFM95HW (at 7.1628 6.8072 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.4 0 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.4 2 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 MISO))
    (pad 3 smd rect (at -1.4 4 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 MOSI))
    (pad 4 smd rect (at -1.4 6 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 CLK))
    (pad 5 smd rect (at -1.4 8 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 D10))
    (pad 6 smd rect (at -1.4 10 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U1-Pad6)"))
    (pad 7 smd rect (at -1.4 12 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 D6))
    (pad 8 smd rect (at -1.4 14 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 14.6932 14 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 15 Ant))
    (pad 10 smd rect (at 14.6932 12 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 14.6932 10 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U1-Pad11)"))
    (pad 12 smd rect (at 14.6932 8 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(U1-Pad12)"))
    (pad 13 smd rect (at 14.6932 6 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 10 +3V3))
    (pad 14 smd rect (at 14.6932 4 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 11 D4))
    (pad 15 smd rect (at 14.6932 2 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 12 D5))
    (pad 16 smd rect (at 14.6932 0 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 13 D7))
    (model ${MYSLOCAL}/mysensors.3dshapes/mysensors_radios.3dshapes/rfm69hw.wrl
      (at (xyz 0.332 -0.275 0.03))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 180))
    )
    (model Crystals.3dshapes/crystal_FA238-TSX3225.wrl
      (at (xyz 0.332 -0.08 0.06))
      (scale (xyz 0.24 0.24 0.24))
      (rotate (xyz 0 0 90))
    )
    (model Housings_DFN_QFN.3dshapes/QFN-28-1EP_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0.204 -0.445 0.06))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 5818D606)
    (at 152.654 160.782 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P6 (at 0.762 -3.175 180) (layer F.SilkS))
    (fp_text value "" (at 0.254 -4.572 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 SDA))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 SCL))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 +3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module mysensors_arduino:pro_mini-26 (layer F.Cu) (tedit 58152BFB)
    (at 155.956 118.872 270)
    (descr "IC, ARDUINO_PRO_MINI x 0,6\"")
    (tags "DIL ARDUINO PRO MINI")
    (fp_text reference uP1 (at -18.288 -0.254 360) (layer F.SilkS))
    (fp_text value ARDUPROMINI-6-2 (at 0 0 270) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at -13.97 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 16 TX0))
    (pad 2 thru_hole oval (at -11.43 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 17 RX1))
    (pad 3 thru_hole oval (at -8.89 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 18 RESET))
    (pad 4 thru_hole oval (at -6.35 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole oval (at -3.81 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 19 D2))
    (pad 6 thru_hole oval (at -1.27 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 20 D3))
    (pad 7 thru_hole oval (at 1.27 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 11 D4))
    (pad 8 thru_hole oval (at 3.81 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 12 D5))
    (pad 9 thru_hole oval (at 6.35 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 7 D6))
    (pad 10 thru_hole oval (at 8.89 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 13 D7))
    (pad 11 thru_hole oval (at 11.43 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 21 D8))
    (pad 12 thru_hole oval (at 13.97 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 22 D9))
    (pad 13 thru_hole oval (at 13.97 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 5 D10))
    (pad 14 thru_hole oval (at 11.43 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 3 MOSI))
    (pad 15 thru_hole oval (at 8.89 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 MISO))
    (pad 16 thru_hole oval (at 6.35 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 4 CLK))
    (pad 17 thru_hole oval (at 3.81 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 23 A0))
    (pad 18 thru_hole oval (at 1.27 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 24 A1))
    (pad 19 thru_hole oval (at -1.27 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 25 A2))
    (pad 20 thru_hole oval (at -3.81 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 26 A3))
    (pad 21 thru_hole oval (at -6.35 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 10 +3V3))
    (pad 22 thru_hole oval (at -8.89 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(uP1-Pad22)"))
    (pad 23 thru_hole oval (at -11.43 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 24 thru_hole oval (at -13.97 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(P2-Pad1)"))
    (pad 25 thru_hole oval (at -2.54 -5.08 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 28 SDA))
    (pad 26 thru_hole oval (at -5.08 -5.08 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 29 SCL))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz -0.15 0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x03.wrl
      (at (xyz 0.55 0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x12.wrl
      (at (xyz 0 0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x12.wrl
      (at (xyz 0 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.25 0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/mysensors_arduino.3dshapes/arduino_pro_mini.wrl
      (at (xyz -0.05 0 0.48))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 180))
    )
    (model SMD_Packages.3dshapes/TQFP-32.wrl
      (at (xyz 0.05 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 315))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x12.wrl
      (at (xyz 0 -0.3 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x12.wrl
      (at (xyz 0 0.3 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0.55 0.1 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0.25 0.2 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz -0.15 0.2 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/smd_leds/led_0603.wrl
      (at (xyz -0.3 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/smd_leds/led_0603.wrl
      (at (xyz 0.55 -0.175 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x06.wrl
      (at (xyz -0.65 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz -0.3 -0.05 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0.55 -0.125 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz -0.3 0.05 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeS_EIA-3216.wrl
      (at (xyz -0.35 0.15 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeS_EIA-3216.wrl
      (at (xyz -0.35 -0.15 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz -0.4 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz -0.5 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_arc (start 170.688 160.782) (end 173.228 160.782) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 140.97 160.782) (end 140.97 163.322) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 140.97 100.33) (end 138.43 100.33) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 170.688 100.33) (end 170.815 97.79) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 173.228 160.782) (end 173.228 100.33) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140.97 163.322) (end 170.688 163.322) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138.43 100.33) (end 138.43 160.782) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170.688 97.79) (end 140.97 97.79) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text " SCN v0.1" (at 167.005 160.655) (layer F.SilkS))
  (gr_text I2C (at 149.479 161.544) (layer F.SilkS))
  (gr_text ProMini (at 156.464 102.616) (layer F.SilkS))
  (gr_text SCL (at 156.718 122.682) (layer F.SilkS))
  (gr_text SDA (at 157.988 118.872) (layer F.SilkS))
  (gr_text 3.3V (at 158.75 109.982) (layer F.SilkS))
  (gr_text GND (at 171.3 125.8) (layer F.SilkS))
  (gr_text GND (at 166.2 138) (layer F.SilkS))
  (gr_text D6 (at 152.7 133.7) (layer F.SilkS))
  (gr_text D6 (at 163.1 136.7) (layer F.SilkS))
  (gr_text 3.3V (at 149.3 140.8) (layer F.SilkS))
  (gr_text 3.3V (at 156.6 138.3) (layer F.SilkS))
  (gr_text "ProMini\nLoRaWAN" (at 143.51 160.528) (layer F.SilkS))
  (gr_text RFM95W (at 157.48 156.21) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 172.974 100.203) (xy 172.974 160.782) (xy 170.815 163.068) (xy 140.716 163.068) (xy 138.811 161.036)
        (xy 138.684 100.33) (xy 140.843 98.044) (xy 170.815 98.044) (xy 172.974 100.203)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 172.974 100.203) (xy 172.974 160.782) (xy 170.815 163.068) (xy 140.716 163.068) (xy 138.811 161.036)
        (xy 138.684 100.33) (xy 140.843 98.044) (xy 170.815 98.044) (xy 172.974 100.203)
      )
    )
  )
)
