<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<text>Arduino Pro Mini</text>
<text>9</text>
<text>7</text>
<text>6</text>
<text>5</text>
<text>4</text>
<text>3</text>
<text>2</text>
<text>GND</text>
<text>RST</text>
<text>RXI</text>
<text>TXO</text>
<text>RAW</text>
<text>GND</text>
<text>RST</text>
<text>VCC</text>
<text>A3</text>
<text>A2</text>
<text>A1</text>
<text>A0</text>
<text>13</text>
<text>12</text>
<text>11</text>
<text>10</text>
<text>A5</text>
<text>A4</text>
<text>Valid combinations:</text>
<text>168V / 3.3V Reg / 8MHz</text>
<text>168 / 5V Reg / 16MHz</text>
<text>168 / 5V Reg / 20MHz</text>
<text>Mark back accordingly</text>
<text>A7</text>
<text>A6</text>
<hole x="8" y="56" drill="4.8"/>
<hole x="40" y="56" drill="4.8"/>
<hole x="8" y="0" drill="4.8"/>
<hole x="40" y="0" drill="4.8"/>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="1X12">
</package>
<package name="1X02">
</package>
<package name="0805">
</package>
<package name="PSOP-8">
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="2X3-NS">
</package>
<package name="1X06_LONGPADS">
</package>
</packages>
</library>
<library name="Dexter_Industries_Eagle_Library_Female_Sockets">
<description>&lt;b&gt;WENZHOU YIHUA COMMUNICATED CONNECTOR CO.,LTD&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="YH-55-10">
<description>&lt;b&gt;RJ11&lt;/b&gt; 6 connects&lt;p&gt;
Source: YH-55-10.pdf</description>
</package>
</packages>
</library>
<library name="74xx-little-us">
<description>&lt;b&gt;Single and Dual Gates Family, US symbols&lt;/b&gt;&lt;p&gt;
Little logic devices from Texas Instruments&lt;br&gt;
TinyLogic(R) from FAIRCHILD Semiconductor TM
&lt;p&gt;
&lt;author&gt;Created by evgeni@eniks.com&lt;/author&gt;&lt;br&gt;
&lt;author&gt;Extended by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;&lt;p&gt;
SOT753 - Philips Semiconductors&lt;br&gt;
Source: http://www.semiconductors.philips.com/acrobat_download/datasheets/74HC_HCT1G66_3.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X13">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP6" library="SparkFun" package="1X12" value=""/>
<element name="JP7" library="SparkFun" package="1X12" value=""/>
<element name="JP2" library="SparkFun" package="1X02" value=""/>
<element name="JP3" library="SparkFun" package="1X02" value=""/>
<element name="X1" library="Dexter_Industries_Eagle_Library_Female_Sockets" package="YH-55-10" value="YH-55-10">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="R1" library="SparkFun" package="0805" value="220"/>
<element name="C1" library="SparkFun" package="0805" value="330pf"/>
<element name="IC1" library="74xx-little-us" package="SOT23-5" value="74AHC1G125DBV"/>
<element name="C2" library="SparkFun" package="0805" value="22pf"/>
<element name="R2" library="SparkFun" package="0805" value="2.2K"/>
<element name="C3" library="SparkFun" package="0805" value="10uf"/>
<element name="C4" library="SparkFun" package="0805" value="100nf"/>
<element name="U$1" library="SparkFun" package="PSOP-8" value="PCA9306"/>
<element name="R3" library="SparkFun" package="0805" value="1k"/>
<element name="R4" library="SparkFun" package="0805" value="1k"/>
<element name="R7" library="SparkFun" package="0805" value="200K"/>
<element name="IC2" library="SparkFun" package="SOT23-5" value=""/>
<element name="C5" library="SparkFun" package="0805" value="1u"/>
<element name="JP8" library="SparkFun" package="1X12" value=""/>
<element name="JP9" library="SparkFun" package="1X12" value=""/>
<element name="J1" library="SparkFun" package="2X3-NS" value="AVR_SPI_PRG_6NS"/>
<element name="JP1" library="SparkFun-Connectors" package="1X13" value="M13"/>
<element name="R5" library="SparkFun" package="0805" value="220"/>
<element name="R6" library="SparkFun" package="0805" value="220"/>
<element name="JP4" library="SparkFun" package="1X06_LONGPADS" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="JP7" pad="9"/>
<contactref element="JP6" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="IC1" pad="3"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="IC2" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="U$1" pad="1"/>
<contactref element="JP8" pad="2"/>
<contactref element="JP9" pad="9"/>
<contactref element="IC1" pad="1"/>
<contactref element="J1" pad="6"/>
<contactref element="JP1" pad="6"/>
<contactref element="X1" pad="3"/>
<contactref element="JP4" pad="6"/>
</signal>
<signal name="RESET">
<contactref element="JP7" pad="10"/>
<contactref element="JP6" pad="3"/>
<contactref element="JP8" pad="3"/>
<contactref element="JP9" pad="10"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="SCK">
<contactref element="JP6" pad="9"/>
<contactref element="JP8" pad="9"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="MISO">
<contactref element="JP6" pad="10"/>
<contactref element="JP8" pad="10"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="JP6" pad="11"/>
<contactref element="JP8" pad="11"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="TXO">
<contactref element="JP7" pad="12"/>
<contactref element="R1" pad="2"/>
<contactref element="JP9" pad="12"/>
</signal>
<signal name="VCC">
<contactref element="JP6" pad="4"/>
<contactref element="X1" pad="4"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="IC2" pad="1"/>
<contactref element="IC2" pad="3"/>
<contactref element="U$1" pad="7"/>
<contactref element="R7" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="IC1" pad="5"/>
<contactref element="C4" pad="1"/>
<contactref element="JP8" pad="4"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="RAW">
<contactref element="JP6" pad="1"/>
<contactref element="JP8" pad="1"/>
</signal>
<signal name="D9">
<contactref element="JP7" pad="1"/>
<contactref element="JP9" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="D8">
<contactref element="JP7" pad="2"/>
<contactref element="JP9" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="A5">
<contactref element="JP2" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="A4">
<contactref element="JP2" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="A3">
<contactref element="JP6" pad="5"/>
<contactref element="JP8" pad="5"/>
</signal>
<signal name="A2">
<contactref element="JP6" pad="6"/>
<contactref element="JP8" pad="6"/>
</signal>
<signal name="A1">
<contactref element="JP6" pad="7"/>
<contactref element="JP8" pad="7"/>
</signal>
<signal name="A0">
<contactref element="JP6" pad="8"/>
<contactref element="JP8" pad="8"/>
</signal>
<signal name="D2">
<contactref element="JP7" pad="8"/>
<contactref element="JP9" pad="8"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="D3">
<contactref element="JP7" pad="7"/>
<contactref element="JP9" pad="7"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="D4">
<contactref element="JP7" pad="6"/>
<contactref element="JP9" pad="6"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="D5">
<contactref element="JP7" pad="5"/>
<contactref element="JP9" pad="5"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="D6">
<contactref element="JP7" pad="4"/>
<contactref element="JP9" pad="4"/>
</signal>
<signal name="D7">
<contactref element="JP7" pad="3"/>
<contactref element="JP9" pad="3"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="D10">
<contactref element="JP6" pad="12"/>
<contactref element="JP8" pad="12"/>
</signal>
<signal name="RXI">
<contactref element="JP7" pad="11"/>
<contactref element="JP9" pad="11"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="A6">
<contactref element="JP3" pad="1"/>
</signal>
<signal name="A7">
<contactref element="JP3" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="1"/>
<contactref element="X1" pad="6"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="X1" pad="5"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="SDA">
<contactref element="U$1" pad="4"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="SCL">
<contactref element="U$1" pad="3"/>
<contactref element="JP1" pad="9"/>
</signal>
<signal name="N$11">
<contactref element="U$1" pad="8"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="U$1" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="IC2" pad="5"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="INT_G">
<contactref element="JP1" pad="4"/>
</signal>
<signal name="DEN_G">
<contactref element="JP1" pad="5"/>
</signal>
<signal name="CS_G">
<contactref element="JP1" pad="13"/>
</signal>
<signal name="SDO_G">
<contactref element="JP1" pad="11"/>
</signal>
<signal name="CS_XM">
<contactref element="JP1" pad="12"/>
</signal>
<signal name="SDO_XM">
<contactref element="JP1" pad="10"/>
</signal>
<signal name="N$1">
<contactref element="X1" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R6" pad="2"/>
<contactref element="X1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
