(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "USLetter")
	(title_block
		(title "W850adapter")
		(date "2024-09-27")
		(rev "1b")
	)
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "NINT")
	(net 3 "NRST")
	(net 4 "+3V3")
	(net 5 "CE0")
	(net 6 "unconnected-(WIZ1-NC-Pad10)")
	(net 7 "SCLK")
	(net 8 "MISO")
	(net 9 "MOSI")
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(locked yes)
		(layer "F.Cu")
		(at 3.81 3.81)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "H1"
			(at -0.0762 0.0762 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at -0.0762 1.6002 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "W850adapter_v1b.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(locked yes)
		(layer "F.Cu")
		(at 34.29 26.67)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "H4"
			(at -0.0762 0.0762 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at -0.0762 1.6002 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "W850adapter_v1b.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(locked yes)
		(layer "F.Cu")
		(at 3.81 26.67)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "H2"
			(at -0.0762 0.0762 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at -0.0762 1.6002 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "W850adapter_v1b.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "Connector_JST:JST_SH_BM04B-SRSS-TB_1x04-1MP_P1.00mm_Vertical"
		(layer "F.Cu")
		(at 23.7744 27.6098 180)
		(descr "JST SH series connector, BM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH vertical")
		(property "Reference" "JP_N1"
			(at -4.421 -0.0466 -90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04"
			(at 0.0254 2.4892 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_JST:JST_SH_BM04B-SRSS-TB_1x04-1MP_P1.00mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connectable mounting pin connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Root")
		(sheetfile "W850adapter_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.25 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1.5 1.325 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.5 1.325 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3V3")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.5 1.325 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "NINT")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.5 1.325 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "NRST")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.8 -1.2 180)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at 2.8 -1.2 180)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_BM04B-SRSS-TB_1x04-1MP_P1.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_SH_BM04B-SRSS-TB_1x04-1MP_P1.00mm_Vertical"
		(layer "F.Cu")
		(at 14.3002 27.6098 180)
		(descr "JST SH series connector, BM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH vertical")
		(property "Reference" "JP_N2"
			(at 4.3674 0.1058 -90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04"
			(at 0.0254 2.4892 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_JST:JST_SH_BM04B-SRSS-TB_1x04-1MP_P1.00mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connectable mounting pin connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1MP*")
		(sheetname "Root")
		(sheetfile "W850adapter_v1b.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.25 180)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" smd roundrect
			(at -1.5 1.325 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "CE0")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.5 1.325 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "SCLK")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.5 1.325 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "MISO")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.5 1.325 180)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "MOSI")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.8 -1.2 180)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at 2.8 -1.2 180)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "MountPin")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_BM04B-SRSS-TB_1x04-1MP_P1.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(locked yes)
		(layer "F.Cu")
		(at 34.29 3.81)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "H3"
			(at -0.0762 0.0762 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at -0.0762 1.6002 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Root")
		(sheetfile "W850adapter_v1b.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "ioPiZero:WIZ850io"
		(locked yes)
		(layer "F.Cu")
		(at 8.89 5.588)
		(descr "WIZ850io Driver")
		(tags "WIZ850io Driver")
		(property "Reference" "WIZ1"
			(at 10.54 -2.94 0)
			(layer "F.SilkS")
		)
		(property "Value" "WIZ850io"
			(at 10.01 -0.81 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "ioPiZero:WIZ850io"
			(at 6.35 8.89 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 6.35 8.89 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 6.35 8.89 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "1278-1043-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part#" "WIZ850IO"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "W850adapter_v1b.kicad_sch")
		(attr through_hole)
		(fp_text user "SCSn"
			(at 2.2 10.1 0)
			(layer "F.SilkS")
		)
		(fp_text user "3.3V"
			(at 18.1 2.5346 0)
			(layer "F.SilkS")
		)
		(fp_text user "3.3V"
			(at 18.1 5.1 0)
			(layer "F.SilkS")
		)
		(fp_text user "RSTn"
			(at 18.1 10.3 0)
			(layer "F.SilkS")
		)
		(fp_text user "MOSI"
			(at 2.2 5.2 0)
			(layer "F.SilkS")
		)
		(fp_text user "N/C"
			(at 18.1 7.7 0)
			(layer "F.SilkS")
		)
		(fp_text user "SCLK"
			(at 2.2 7.6 0)
			(layer "F.SilkS")
		)
		(fp_text user "MISO"
			(at 18.1 12.8 0)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at 2.4 2.7 0)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at 18.1 0 0)
			(layer "F.SilkS")
		)
		(fp_text user "INTn"
			(at 2.2 12.7 0)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at 2.3 0.1 0)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "MOSI")
			(pinfunction "MOSI")
			(pintype "bidirectional")
		)
		(pad "4" thru_hole circle
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "SCLK")
			(pinfunction "SCLK")
			(pintype "bidirectional")
		)
		(pad "5" thru_hole circle
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "CE0")
			(pinfunction "SCSn")
			(pintype "bidirectional")
		)
		(pad "6" thru_hole circle
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "NINT")
			(pinfunction "INTn")
			(pintype "bidirectional")
		)
		(pad "7" thru_hole circle
			(at 20.32 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "8" thru_hole circle
			(at 20.32 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "+3V3")
			(pinfunction "3.3V")
			(pintype "power_in")
		)
		(pad "9" thru_hole circle
			(at 20.32 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "+3V3")
			(pinfunction "3.3V")
			(pintype "power_in")
		)
		(pad "10" thru_hole circle
			(at 20.32 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "unconnected-(WIZ1-NC-Pad10)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "11" thru_hole circle
			(at 20.32 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "NRST")
			(pinfunction "RSTn")
			(pintype "bidirectional")
		)
		(pad "12" thru_hole circle
			(at 20.32 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "MISO")
			(pinfunction "MISO")
			(pintype "bidirectional")
		)
	)
	(gr_arc
		(start 3.81 30.48)
		(mid 1.115923 29.364077)
		(end 0 26.67)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 38.1 26.67)
		(mid 36.984077 29.364077)
		(end 34.29 30.48)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 34.29 0)
		(mid 36.984077 1.115923)
		(end 38.1 3.81)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 38.1 3.81)
		(end 38.1 26.67)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 0 3.81)
		(mid 1.115923 1.115923)
		(end 3.81 0)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 3.81 0)
		(end 34.29 0)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 34.29 30.48)
		(end 3.81 30.48)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 0 26.67)
		(end 0 3.81)
		(layer "Edge.Cuts")
	)
	(gr_text "W850adapter\nVersion 1b\n30sept2024"
		(at 6.604 9.8298 90)
		(layer "B.SilkS")
	)
	(gr_text "Copyright S. Cooper 2024.\nCERN OHL v.1.2  (Open Hardware Licence)\nhttp://ohwr.org/cernohl"
		(at 20.574 13.3858 90)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 25.8572 24.9936 90)
		(layer "F.SilkS")
	)
	(gr_text "WIZ850io"
		(at 16.0274 5.0038 0)
		(layer "F.SilkS")
	)
	(gr_text "W850adapter\nVersion 1b\n30sept2024"
		(at 36.2712 19.5834 90)
		(layer "F.SilkS")
	)
	(gr_text "NRST"
		(at 22.7076 24.9936 90)
		(layer "F.SilkS")
	)
	(gr_text "MOSI"
		(at 13.2588 25.0444 90)
		(layer "F.SilkS")
	)
	(gr_text "NINT"
		(at 23.749 25.019 90)
		(layer "F.SilkS")
	)
	(gr_text "SCLK"
		(at 15.2654 24.9936 90)
		(layer "F.SilkS")
	)
	(gr_text "MISO"
		(at 14.3256 25.0444 90)
		(layer "F.SilkS")
	)
	(gr_text "CE0"
		(at 16.2814 25.019 90)
		(layer "F.SilkS")
	)
	(gr_text "+3V"
		(at 24.765 25.0952 90)
		(layer "F.SilkS")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy -0.635 -0.635) (xy 38.735 -0.635) (xy 38.735 31.115) (xy -0.635 31.115)
			)
		)
	)
)
