(kicad_pcb (version 20171130) (host pcbnew "(5.0.0-3-g5ebb6b6)")
  (general
    (thickness 1.6)
    (drawings 23)
    (tracks 297)
    (zones 0)
    (modules 23)
    (nets 52)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.1651)
    (zone_clearance 0.01)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.6 2.4)
    (pad_drill 2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 137.16 69.85)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J2-Pad16)")
  (net 2 "Net-(J2-Pad15)")
  (net 3 "Net-(J2-Pad14)")
  (net 4 "Net-(J2-Pad13)")
  (net 5 "Net-(J2-Pad12)")
  (net 6 "Net-(J2-Pad11)")
  (net 7 "Net-(J2-Pad7)")
  (net 8 "Net-(J2-Pad6)")
  (net 9 "Net-(J2-Pad5)")
  (net 10 "Net-(J2-Pad3)")
  (net 11 "Net-(J2-Pad1)")
  (net 12 "Net-(J1-Pad10)")
  (net 13 "Net-(J1-Pad9)")
  (net 14 "Net-(J1-Pad8)")
  (net 15 "Net-(J1-Pad7)")
  (net 16 "Net-(J1-Pad6)")
  (net 17 "Net-(J1-Pad5)")
  (net 18 "Net-(J1-Pad4)")
  (net 19 "Net-(J1-Pad3)")
  (net 20 "Net-(J1-Pad2)")
  (net 21 "Net-(J1-Pad1)")
  (net 22 /SDA)
  (net 23 /SCL)
  (net 24 +3V3)
  (net 25 GND)
  (net 26 /SWDIO)
  (net 27 /SWCLK)
  (net 28 "Net-(U1-Pad5)")
  (net 29 /POT2)
  (net 30 /POT1)
  (net 31 "Net-(SW7-Pad2)")
  (net 32 /B1)
  (net 33 /B2)
  (net 34 /B3)
  (net 35 /B4)
  (net 36 "Net-(J6-Pad1)")
  (net 37 "Net-(J5-Pad1)")
  (net 38 "Net-(J4-Pad1)")
  (net 39 "Net-(J3-Pad1)")
  (net 40 /RESET)
  (net 41 /S11)
  (net 42 /S21)
  (net 43 /RA1)
  (net 44 /RB1)
  (net 45 /S12)
  (net 46 /S22)
  (net 47 /RA2)
  (net 48 /RB2)
  (net 49 /B5)
  (net 50 "Net-(D1-Pad2)")
  (net 51 /LED)
  (net_class Default "This is the default net class."
    (clearance 0.1651)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /B1)
    (add_net /B2)
    (add_net /B3)
    (add_net /B4)
    (add_net /B5)
    (add_net /LED)
    (add_net /POT1)
    (add_net /POT2)
    (add_net /RA1)
    (add_net /RA2)
    (add_net /RB1)
    (add_net /RB2)
    (add_net /RESET)
    (add_net /S11)
    (add_net /S12)
    (add_net /S21)
    (add_net /S22)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /SWCLK)
    (add_net /SWDIO)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad14)")
    (add_net "Net-(J2-Pad15)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(SW7-Pad2)")
    (add_net "Net-(U1-Pad5)")
  )
  (module "Alps Pots:RK09D-AllOrientations" (layer F.Cu) (tedit 5BE88C40)
    (at 137.16 84.85)
    (fp_text reference SW9 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Rotary_Encoder_Switch (at 0 -0.5) (layer F.Fab))
    (pad S1 thru_hole oval (at -2.5 7) (size 2 2) (drill 1 (offset 0 0.3)) (layers *.Cu *.Mask)
      (net 45 /S12))
    (pad C thru_hole circle (at 0 7) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 30 /POT1))
    (pad S2 thru_hole oval (at 2.5 7) (size 2 2) (drill 1 (offset 0 0.3)) (layers *.Cu *.Mask)
      (net 46 /S22))
    (pad "" thru_hole oval (at -4.4 0) (size 2.6 2.4) (drill 2.1) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 4.4 0) (size 2.6 2.4) (drill 2.1) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 0 -4.4) (size 2.4 2.6) (drill 2.1) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 0 4.4) (size 2.4 2.6) (drill 2.1) (layers *.Cu *.Mask))
    (pad A thru_hole circle (at -7 -2.5) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 47 /RA2))
    (pad C thru_hole circle (at -7 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 30 /POT1))
    (pad B thru_hole circle (at -7 2.5) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 48 /RB2))
    (pad S2 thru_hole circle (at 7 2.5) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 46 /S22))
    (pad C thru_hole circle (at 7 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 30 /POT1))
    (pad S1 thru_hole circle (at 7 -2.5) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 45 /S12))
    (pad B thru_hole oval (at 2.5 -7) (size 2 2) (drill 1 (offset 0 -0.3)) (layers *.Cu *.Mask)
      (net 48 /RB2))
    (pad C thru_hole circle (at 0 -7) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 30 /POT1))
    (pad A thru_hole oval (at -2.5 -7) (size 2 2) (drill 1 (offset 0 -0.3)) (layers *.Cu *.Mask)
      (net 47 /RA2))
  )
  (module "Alps Pots:RK09D-AllOrientations" (layer F.Cu) (tedit 5BE88C40)
    (at 137.16 54.85 180)
    (fp_text reference SW8 (at 0 0.5 180) (layer F.SilkS) hide)
    (fp_text value Rotary_Encoder_Switch (at 0 -0.5 180) (layer F.Fab))
    (pad S1 thru_hole oval (at -2.5 7 180) (size 2 2) (drill 1 (offset 0 0.3)) (layers *.Cu *.Mask)
      (net 41 /S11))
    (pad C thru_hole circle (at 0 7 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 29 /POT2))
    (pad S2 thru_hole oval (at 2.5 7 180) (size 2 2) (drill 1 (offset 0 0.3)) (layers *.Cu *.Mask)
      (net 42 /S21))
    (pad "" thru_hole oval (at -4.4 0 180) (size 2.6 2.4) (drill 2.1) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 4.4 0 180) (size 2.6 2.4) (drill 2.1) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 0 -4.4 180) (size 2.4 2.6) (drill 2.1) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 0 4.4 180) (size 2.4 2.6) (drill 2.1) (layers *.Cu *.Mask))
    (pad A thru_hole circle (at -7 -2.5 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 43 /RA1))
    (pad C thru_hole circle (at -7 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 29 /POT2))
    (pad B thru_hole circle (at -7 2.5 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 44 /RB1))
    (pad S2 thru_hole circle (at 7 2.5 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 42 /S21))
    (pad C thru_hole circle (at 7 0 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 29 /POT2))
    (pad S1 thru_hole circle (at 7 -2.5 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 41 /S11))
    (pad B thru_hole oval (at 2.5 -7 180) (size 2 2) (drill 1 (offset 0 -0.3)) (layers *.Cu *.Mask)
      (net 44 /RB1))
    (pad C thru_hole circle (at 0 -7 180) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 29 /POT2))
    (pad A thru_hole oval (at -2.5 -7 180) (size 2 2) (drill 1 (offset 0 -0.3)) (layers *.Cu *.Mask)
      (net 43 /RA1))
  )
  (module LED_SMD:LED_0603_1608Metric_Castellated (layer B.Cu) (tedit 5B301BBE)
    (at 130.56 70.45 180)
    (descr "LED SMD 0603 (1608 Metric), castellated end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED castellated")
    (attr smd)
    (fp_text reference D1 (at -2.6 0 180) (layer B.SilkS))
    (fp_text value LED_Small (at 0 -1.38 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.8125 0 180) (size 1.225 0.85) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 51 /LED))
    (pad 2 smd roundrect (at 0.8125 0 180) (size 1.225 0.85) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 50 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric_Castellated.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 130.16 68.05 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0.4 1.43 270) (layer B.SilkS))
    (fp_text value 1k (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 +3V3))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 50 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 143.36 76.25)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 1.43) (layer B.SilkS))
    (fp_text value 4.7k (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 /SDA))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 143.36 74.65 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0.4 1.4 180) (layer B.SilkS))
    (fp_text value 4.7k (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 /SCL))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Adafruit:Feather Mounting Hole" (layer F.Cu) (tedit 5BE87E64)
    (at 146.05 92.71)
    (fp_text reference J3 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 2.54) (layers *.Cu *.Mask)
      (net 39 "Net-(J3-Pad1)"))
  )
  (module "Adafruit:Feather Mounting Hole" (layer F.Cu) (tedit 5BE87E8F)
    (at 128.27 46.99)
    (fp_text reference J4 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 2.54) (layers *.Cu *.Mask)
      (net 38 "Net-(J4-Pad1)"))
  )
  (module "Adafruit:Feather Mounting Hole" (layer F.Cu) (tedit 5BE87E6C)
    (at 128.27 92.71)
    (fp_text reference J5 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 2.54) (layers *.Cu *.Mask)
      (net 37 "Net-(J5-Pad1)"))
  )
  (module "Adafruit:Feather Mounting Hole" (layer F.Cu) (tedit 5BE87E7E)
    (at 146.05 46.99)
    (fp_text reference J6 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 2.54) (layers *.Cu *.Mask)
      (net 36 "Net-(J6-Pad1)"))
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 130.16 65.65)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.4) (layer B.SilkS))
    (fp_text value 10uF (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 24 +3V3))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 25 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59958EE7)
    (at 132.56 67.45)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 1.5) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 25 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 24 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module E-Switch:TL3301-GullWing (layer F.Cu) (tedit 5BE87E49)
    (at 137.16 69.85)
    (fp_text reference SW7 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value SW_Push (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at -4.55 2.25) (size 2.1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (pad 3 smd rect (at 4.55 2.25) (size 2.1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 25 GND))
    (pad 4 smd rect (at 4.55 -2.25) (size 2.1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 49 /B5))
    (pad 2 smd rect (at -4.55 -2.25) (size 2.1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(SW7-Pad2)"))
  )
  (module Housings_DFN_QFN:QFN-24-1EP_4x4mm_Pitch0.5mm (layer B.Cu) (tedit 54130A77)
    (at 137.16 69.1825 270)
    (descr "24-Lead Plastic Quad Flat, No Lead Package (MJ) - 4x4x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U1 (at 3.4675 0) (layer B.SilkS))
    (fp_text value SAMD09D (at 0 -3.375 270) (layer B.Fab))
    (pad 25 smd rect (at -0.65 0.65 270) (size 1.3 1.3) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at -0.65 -0.65 270) (size 1.3 1.3) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at 0.65 0.65 270) (size 1.3 1.3) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 25 smd rect (at 0.65 -0.65 270) (size 1.3 1.3) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 24 smd rect (at -1.25 1.95 180) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 24 +3V3))
    (pad 23 smd rect (at -0.75 1.95 180) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 25 GND))
    (pad 22 smd rect (at -0.25 1.95 180) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 51 /LED))
    (pad 21 smd rect (at 0.25 1.95 180) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 35 /B4))
    (pad 20 smd rect (at 0.75 1.95 180) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 26 /SWDIO))
    (pad 19 smd rect (at 1.25 1.95 180) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 27 /SWCLK))
    (pad 18 smd rect (at 1.95 1.25 270) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 40 /RESET))
    (pad 17 smd rect (at 1.95 0.75 270) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 34 /B3))
    (pad 16 smd rect (at 1.95 0.25 270) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 47 /RA2))
    (pad 15 smd rect (at 1.95 -0.25 270) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 48 /RB2))
    (pad 14 smd rect (at 1.95 -0.75 270) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 45 /S12))
    (pad 13 smd rect (at 1.95 -1.25 270) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 46 /S22))
    (pad 12 smd rect (at 1.25 -1.95 180) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 23 /SCL))
    (pad 11 smd rect (at 0.75 -1.95 180) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 22 /SDA))
    (pad 10 smd rect (at 0.25 -1.95 180) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 30 /POT1))
    (pad 9 smd rect (at -0.25 -1.95 180) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 49 /B5))
    (pad 8 smd rect (at -0.75 -1.95 180) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 32 /B1))
    (pad 7 smd rect (at -1.25 -1.95 180) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 33 /B2))
    (pad 6 smd rect (at -1.95 -1.25 270) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 29 /POT2))
    (pad 5 smd rect (at -1.95 -0.75 270) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(U1-Pad5)"))
    (pad 4 smd rect (at -1.95 -0.25 270) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 43 /RA1))
    (pad 3 smd rect (at -1.95 0.25 270) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 44 /RB1))
    (pad 2 smd rect (at -1.95 0.75 270) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 41 /S11))
    (pad 1 smd rect (at -1.95 1.25 270) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 42 /S21))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/QFN-24-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Adafruit:SW_PUSH_6mm_Centered (layer F.Cu) (tedit 5BE87ECA)
    (at 137.16 84.85)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW6 (at 0 -4.25) (layer F.SilkS) hide)
    (fp_text value SW_Push (at 0.5 4.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 3.25 -2.25 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 25 GND))
    (pad 2 thru_hole circle (at 3.25 2.25 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 30 /POT1))
    (pad 1 thru_hole circle (at -3.25 -2.25 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 25 GND))
    (pad 2 thru_hole circle (at -3.25 2.25 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 30 /POT1))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (offset (xyz -3.25 2.25 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Adafruit:SW_PUSH_6mm_Centered (layer F.Cu) (tedit 5BE87E98)
    (at 137.16 54.85)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW5 (at 0 -4.25) (layer F.SilkS) hide)
    (fp_text value SW_Push (at 0.5 4.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 thru_hole circle (at -3.25 2.25 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 25 GND))
    (pad 1 thru_hole circle (at -3.25 -2.25 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 29 /POT2))
    (pad 2 thru_hole circle (at 3.25 2.25 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 25 GND))
    (pad 1 thru_hole circle (at 3.25 -2.25 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 29 /POT2))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (offset (xyz -3.25 2.25 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Adafruit:SW_PUSH_6mm_Centered (layer F.Cu) (tedit 5BE87E5D)
    (at 137.16 92.35)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW4 (at 0 -4.25) (layer F.SilkS) hide)
    (fp_text value SW_Push (at 0.5 4.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" thru_hole circle (at 3.25 -2.25 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 3.25 2.25 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 25 GND))
    (pad 1 thru_hole circle (at -3.25 -2.25 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 35 /B4))
    (pad 2 thru_hole circle (at -3.25 2.25 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 25 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (offset (xyz -3.25 2.25 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Adafruit:SW_PUSH_6mm_Centered (layer F.Cu) (tedit 5BE87E40)
    (at 137.16 77.35)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW3 (at 0 -4.25) (layer F.SilkS) hide)
    (fp_text value SW_Push (at 0.5 4.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 thru_hole circle (at -3.25 2.25 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 25 GND))
    (pad 1 thru_hole circle (at -3.25 -2.25 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 34 /B3))
    (pad 2 thru_hole circle (at 3.25 2.25 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 25 GND))
    (pad "" thru_hole circle (at 3.25 -2.25 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (offset (xyz -3.25 2.25 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Adafruit:SW_PUSH_6mm_Centered (layer F.Cu) (tedit 5BE87EA6)
    (at 137.16 62.35)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW2 (at 0 -4.25) (layer F.SilkS) hide)
    (fp_text value SW_Push (at 0.5 4.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 3.25 -2.25 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 25 GND))
    (pad 2 thru_hole circle (at 3.25 2.25 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 33 /B2))
    (pad 1 thru_hole circle (at -3.25 -2.25 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 25 GND))
    (pad "" thru_hole circle (at -3.25 2.25 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (offset (xyz -3.25 2.25 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Adafruit:SW_PUSH_6mm_Centered (layer F.Cu) (tedit 5BE88579)
    (at 137.16 47.35)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW1 (at 0 -4.25) (layer F.SilkS) hide)
    (fp_text value SW_Push (at 0.5 4.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" thru_hole circle (at -3.25 2.25 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -3.25 -2.25 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 25 GND))
    (pad 2 thru_hole circle (at 3.25 2.25 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 32 /B1))
    (pad 1 thru_hole circle (at 3.25 -2.25 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 25 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (offset (xyz -3.25 2.25 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 5BE87E88)
    (at 147.32 60.96)
    (descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x12 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value FeatherTop (at 0 30.27) (layer F.Fab))
    (fp_text user %R (at 0 13.97 90) (layer F.Fab))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /SDA))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /SCL))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad10)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad9)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x16_Pitch2.54mm (layer F.Cu) (tedit 5BE87E83)
    (at 127 50.8)
    (descr "Through hole straight pin header, 1x16, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x16 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value FeatherBottom (at 0 40.43) (layer F.Fab))
    (fp_text user %R (at 0 19.05 90) (layer F.Fab))
    (pad 16 thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J2-Pad16)"))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad15)"))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad14)"))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad13)"))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad12)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad11)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /RESET))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /SWCLK))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /SWDIO))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 +3V3))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x16_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module chickadee:chickadee_3mm_fcu (layer F.Cu) (tedit 0)
    (at 137.56 69.85)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value "Chickadee 3mm" (at 0.75 0) (layer F.SilkS) hide)
  )
  (gr_text ckd.tech/knobs/v1 (at 130.16 70.45 90) (layer F.SilkS))
  (gr_text OK (at 130.56 73.05) (layer B.SilkS))
  (gr_text P1 (at 130.56 89.85) (layer F.SilkS))
  (gr_text B4 (at 143.16 92.25) (layer F.SilkS))
  (gr_text B3 (at 144.56 77.25) (layer F.SilkS))
  (gr_text P2 (at 146.96 55.05) (layer F.SilkS))
  (gr_text B1 (at 143.16 47.45) (layer F.SilkS))
  (gr_text B2 (at 144.36 62.05) (layer F.SilkS))
  (gr_text B5 (at 144.56 69.85) (layer F.SilkS))
  (gr_arc (start 128.27 46.99) (end 128.27 44.45) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 146.05 46.99) (end 148.59 46.99) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.27 44.45) (end 146.05 44.45) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.59 92.71) (end 148.59 46.99) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125.73 92.71) (end 125.73 46.99) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 128.27 92.71) (end 125.73 92.71) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 146.05 92.71) (end 146.05 95.25) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.27 95.25) (end 146.05 95.25) (layer Edge.Cuts) (width 0.15))
  (zone (net 25) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.01))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.66 44.35) (xy 148.66 44.35) (xy 148.66 95.35) (xy 125.66 95.35)
      )
    )
  )
  (zone (net 25) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.01))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.76 44.45) (xy 148.56 44.45) (xy 148.76 95.45) (xy 125.76 95.45) (xy 125.56 95.45)
      )
    )
  )
)
