(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 140)
    (no_connects 0)
    (area 44.867074 79.2501 109.534446 142.58066)
    (thickness 1.6)
    (drawings 79)
    (tracks 577)
    (zones 0)
    (modules 42)
    (nets 67)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.2032)
    (pcb_text_size 1.016 1.016)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x001f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerber/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCAP1)
  (net 3 NRST)
  (net 4 VCAP2)
  (net 5 VDD1)
  (net 6 OSCIN)
  (net 7 "Net-(C7-Pad2)")
  (net 8 OSC32_IN)
  (net 9 OSC32_OUT)
  (net 10 5V_IN)
  (net 11 "Net-(C19-Pad2)")
  (net 12 PB10)
  (net 13 "Net-(D1-Pad1)")
  (net 14 "Net-(D2-Pad2)")
  (net 15 "Net-(D4-Pad1)")
  (net 16 SWCLK)
  (net 17 SWDIO)
  (net 18 TRACESWO)
  (net 19 PB5)
  (net 20 PB6)
  (net 21 PB7)
  (net 22 BOOT0)
  (net 23 PB8)
  (net 24 PB9)
  (net 25 PC13)
  (net 26 PC0)
  (net 27 PC1)
  (net 28 PC2)
  (net 29 PC3)
  (net 30 PA0)
  (net 31 PA1)
  (net 32 PA2)
  (net 33 PA3)
  (net 34 PA4)
  (net 35 PA5)
  (net 36 PA6)
  (net 37 PA7)
  (net 38 PC4)
  (net 39 PC5)
  (net 40 PB0)
  (net 41 PB1)
  (net 42 PB2)
  (net 43 PB4)
  (net 44 PD2)
  (net 45 PC12)
  (net 46 PC11)
  (net 47 PC10)
  (net 48 PA15)
  (net 49 PA12)
  (net 50 PA11)
  (net 51 PA10)
  (net 52 PA9)
  (net 53 PA8)
  (net 54 PC9)
  (net 55 PC8)
  (net 56 PC7)
  (net 57 PC6)
  (net 58 PB15)
  (net 59 PB14)
  (net 60 PB13)
  (net 61 PB12)
  (net 62 OSCOUT)
  (net 63 VBAT)
  (net 64 "Net-(R6-Pad1)")
  (net 65 "Net-(R7-Pad1)")
  (net 66 PB11_VCAP1)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net BOOT0)
    (add_net GND)
    (add_net NRST)
    (add_net "Net-(C19-Pad2)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(R7-Pad1)")
    (add_net OSC32_IN)
    (add_net OSC32_OUT)
    (add_net OSCIN)
    (add_net OSCOUT)
    (add_net PB11_VCAP1)
    (add_net SWCLK)
    (add_net SWDIO)
    (add_net TRACESWO)
    (add_net VBAT)
    (add_net VCAP1)
    (add_net VCAP2)
  )
  (net_class Power ""
    (clearance 0.1524)
    (trace_width 0.508)
    (via_dia 0.8382)
    (via_drill 0.381)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net 5V_IN)
    (add_net "Net-(D2-Pad2)")
    (add_net VDD1)
  )
  (net_class Thin ""
    (clearance 0.1524)
    (trace_width 0.2032)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net PA0)
    (add_net PA1)
    (add_net PA10)
    (add_net PA11)
    (add_net PA12)
    (add_net PA15)
    (add_net PA2)
    (add_net PA3)
    (add_net PA4)
    (add_net PA5)
    (add_net PA6)
    (add_net PA7)
    (add_net PA8)
    (add_net PA9)
    (add_net PB0)
    (add_net PB1)
    (add_net PB10)
    (add_net PB12)
    (add_net PB13)
    (add_net PB14)
    (add_net PB15)
    (add_net PB2)
    (add_net PB4)
    (add_net PB5)
    (add_net PB6)
    (add_net PB7)
    (add_net PB8)
    (add_net PB9)
    (add_net PC0)
    (add_net PC1)
    (add_net PC10)
    (add_net PC11)
    (add_net PC12)
    (add_net PC13)
    (add_net PC2)
    (add_net PC3)
    (add_net PC4)
    (add_net PC5)
    (add_net PC6)
    (add_net PC7)
    (add_net PC8)
    (add_net PC9)
    (add_net PD2)
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 76.454 85.471 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at -2.413 0 360) (layer F.SilkS))
    (fp_text value 12pF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C7-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:LQFP-64_10x10mm_Pitch0.5mm (layer F.Cu) (tedit 5649442E)
    (at 75.311 105.029 270)
    (descr "64 LEAD LQFP 10x10mm (see MICREL LQFP10x10-64LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U1 (at 4.826 -7.493 360) (layer F.SilkS))
    (fp_text value STM32F405RG (at 0 7.2 270) (layer F.Fab))
    (pad 1 smd rect (at -5.7 -3.75 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 63 VBAT) (solder_mask_margin 0.0508))
    (pad 2 smd rect (at -5.7 -3.25 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 PC13) (solder_mask_margin 0.0508))
    (pad 3 smd rect (at -5.7 -2.75 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 OSC32_IN) (solder_mask_margin 0.0508))
    (pad 4 smd rect (at -5.7 -2.25 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 OSC32_OUT) (solder_mask_margin 0.0508))
    (pad 5 smd rect (at -5.7 -1.75 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 OSCIN) (solder_mask_margin 0.0508))
    (pad 6 smd rect (at -5.7 -1.25 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 62 OSCOUT) (solder_mask_margin 0.0508))
    (pad 7 smd rect (at -5.7 -0.75 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 NRST) (solder_mask_margin 0.0508))
    (pad 8 smd rect (at -5.7 -0.25 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 PC0) (solder_mask_margin 0.0508))
    (pad 9 smd rect (at -5.7 0.25 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 PC1) (solder_mask_margin 0.0508))
    (pad 10 smd rect (at -5.7 0.75 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 PC2) (solder_mask_margin 0.0508))
    (pad 11 smd rect (at -5.7 1.25 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 PC3) (solder_mask_margin 0.0508))
    (pad 12 smd rect (at -5.7 1.75 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad 13 smd rect (at -5.7 2.25 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 VDD1) (solder_mask_margin 0.0508))
    (pad 14 smd rect (at -5.7 2.75 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 PA0) (solder_mask_margin 0.0508))
    (pad 15 smd rect (at -5.7 3.25 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 31 PA1) (solder_mask_margin 0.0508))
    (pad 16 smd rect (at -5.7 3.75 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 PA2) (solder_mask_margin 0.0508))
    (pad 17 smd rect (at -3.75 5.7) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 33 PA3) (solder_mask_margin 0.0508))
    (pad 18 smd rect (at -3.25 5.7) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad 19 smd rect (at -2.75 5.7) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 VDD1) (solder_mask_margin 0.0508))
    (pad 20 smd rect (at -2.25 5.7) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 34 PA4) (solder_mask_margin 0.0508))
    (pad 21 smd rect (at -1.75 5.7) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 35 PA5) (solder_mask_margin 0.0508))
    (pad 22 smd rect (at -1.25 5.7) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 36 PA6) (solder_mask_margin 0.0508))
    (pad 23 smd rect (at -0.75 5.7) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 37 PA7) (solder_mask_margin 0.0508))
    (pad 24 smd rect (at -0.25 5.7) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 38 PC4) (solder_mask_margin 0.0508))
    (pad 25 smd rect (at 0.25 5.7) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 39 PC5) (solder_mask_margin 0.0508))
    (pad 26 smd rect (at 0.75 5.7) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 PB0) (solder_mask_margin 0.0508))
    (pad 27 smd rect (at 1.25 5.7) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 41 PB1) (solder_mask_margin 0.0508))
    (pad 28 smd rect (at 1.75 5.7) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 42 PB2) (solder_mask_margin 0.0508))
    (pad 29 smd rect (at 2.25 5.7) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 PB10) (solder_mask_margin 0.0508))
    (pad 30 smd rect (at 2.75 5.7) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 66 PB11_VCAP1) (solder_mask_margin 0.0508))
    (pad 31 smd rect (at 3.25 5.7) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 VCAP1) (solder_mask_margin 0.0508))
    (pad 32 smd rect (at 3.75 5.7) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 VDD1) (solder_mask_margin 0.0508))
    (pad 33 smd rect (at 5.7 3.75 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 61 PB12) (solder_mask_margin 0.0508))
    (pad 34 smd rect (at 5.7 3.25 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 60 PB13) (solder_mask_margin 0.0508))
    (pad 35 smd rect (at 5.7 2.75 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 59 PB14) (solder_mask_margin 0.0508))
    (pad 36 smd rect (at 5.7 2.25 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 58 PB15) (solder_mask_margin 0.0508))
    (pad 37 smd rect (at 5.7 1.75 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 57 PC6) (solder_mask_margin 0.0508))
    (pad 38 smd rect (at 5.7 1.25 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 56 PC7) (solder_mask_margin 0.0508))
    (pad 39 smd rect (at 5.7 0.75 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 55 PC8) (solder_mask_margin 0.0508))
    (pad 40 smd rect (at 5.7 0.25 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 54 PC9) (solder_mask_margin 0.0508))
    (pad 41 smd rect (at 5.7 -0.25 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 53 PA8) (solder_mask_margin 0.0508))
    (pad 42 smd rect (at 5.7 -0.75 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 52 PA9) (solder_mask_margin 0.0508))
    (pad 43 smd rect (at 5.7 -1.25 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 51 PA10) (solder_mask_margin 0.0508))
    (pad 44 smd rect (at 5.7 -1.75 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 50 PA11) (solder_mask_margin 0.0508))
    (pad 45 smd rect (at 5.7 -2.25 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 49 PA12) (solder_mask_margin 0.0508))
    (pad 46 smd rect (at 5.7 -2.75 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 17 SWDIO) (solder_mask_margin 0.0508))
    (pad 47 smd rect (at 5.7 -3.25 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 VCAP2) (solder_mask_margin 0.0508))
    (pad 48 smd rect (at 5.7 -3.75 270) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 VDD1) (solder_mask_margin 0.0508))
    (pad 49 smd rect (at 3.75 -5.7) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 16 SWCLK) (solder_mask_margin 0.0508))
    (pad 50 smd rect (at 3.25 -5.7) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 48 PA15) (solder_mask_margin 0.0508))
    (pad 51 smd rect (at 2.75 -5.7) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 47 PC10) (solder_mask_margin 0.0508))
    (pad 52 smd rect (at 2.25 -5.7) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 46 PC11) (solder_mask_margin 0.0508))
    (pad 53 smd rect (at 1.75 -5.7) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 45 PC12) (solder_mask_margin 0.0508))
    (pad 54 smd rect (at 1.25 -5.7) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 44 PD2) (solder_mask_margin 0.0508))
    (pad 55 smd rect (at 0.75 -5.7) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 TRACESWO) (solder_mask_margin 0.0508))
    (pad 56 smd rect (at 0.25 -5.7) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 43 PB4) (solder_mask_margin 0.0508))
    (pad 57 smd rect (at -0.25 -5.7) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 PB5) (solder_mask_margin 0.0508))
    (pad 58 smd rect (at -0.75 -5.7) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 PB6) (solder_mask_margin 0.0508))
    (pad 59 smd rect (at -1.25 -5.7) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 PB7) (solder_mask_margin 0.0508))
    (pad 60 smd rect (at -1.75 -5.7) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 BOOT0) (solder_mask_margin 0.0508))
    (pad 61 smd rect (at -2.25 -5.7) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 23 PB8) (solder_mask_margin 0.0508))
    (pad 62 smd rect (at -2.75 -5.7) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 24 PB9) (solder_mask_margin 0.0508))
    (pad 63 smd rect (at -3.25 -5.7) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad 64 smd rect (at -3.75 -5.7) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 VDD1) (solder_mask_margin 0.0508))
    (model Housings_QFP.3dshapes/LQFP-64_10x10mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:Symbol_OSHW-Logo_SilkScreen (layer F.Cu) (tedit 5654ACB2)
    (at 64.77 85.09)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference REF** (at 0.09906 -4.38912) (layer F.SilkS) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 0.30988 6.56082) (layer F.Fab))
  )
  (module LEDs:LED-0805 (layer F.Cu) (tedit 55BDE1C2)
    (at 68.1355 117.856 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D1 (at 1.143 -1.905 360) (layer F.SilkS))
    (fp_text value LED (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 55 PC8))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-1206_Pol (layer F.Cu) (tedit 0)
    (at 66.167 129.667)
    (attr smd)
    (fp_text reference D2 (at 3.556 -0.508) (layer F.SilkS))
    (fp_text value D (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.651 0) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 10 5V_IN))
    (pad 2 smd rect (at 1.651 0) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D2-Pad2)"))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_FSMSM (layer F.Cu) (tedit 555C8B1B)
    (at 68.072 125.857 180)
    (descr http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=1437566-3&DocType=Customer+Drawing&DocLang=English)
    (tags "SPST button tactile switch")
    (attr smd)
    (fp_text reference SW2 (at 4.572 2.54 180) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0.01011 -0.00022 180) (layer F.Fab))
    (pad 1 smd rect (at -4.60243 -0.00232 180) (size 2.18 1.6) (layers F.Cu F.Paste F.Mask)
      (net 22 BOOT0))
    (pad 2 smd rect (at 4.60243 0.00232 180) (size 2.18 1.6) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(R7-Pad1)"))
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 562ABFC7)
    (at 62.103 133.35 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U2 (at -0.05 -2.55 180) (layer F.SilkS))
    (fp_text value LT1761 (at -0.05 2.35 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 5V_IN) (solder_mask_margin 0.0508))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 5V_IN) (solder_mask_margin 0.0508))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C19-Pad2)") (solder_mask_margin 0.0508))
    (pad 5 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 VDD1) (solder_mask_margin 0.0508))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:USB_Mini-B (layer F.Cu) (tedit 562ABF85)
    (at 75.438 134.747 90)
    (descr "USB Mini-B 5-pin SMD connector")
    (tags "USB USB_B USB_Mini connector")
    (attr smd)
    (fp_text reference P4 (at 5.715 3.302 180) (layer F.SilkS))
    (fp_text value USB_B (at 0 -7.0993 90) (layer F.Fab))
    (pad 1 smd rect (at 3.44932 -1.6002 90) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D2-Pad2)") (solder_mask_margin 0.0508))
    (pad 2 smd rect (at 3.44932 -0.8001 90) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 50 PA11) (solder_mask_margin 0.0508))
    (pad 3 smd rect (at 3.44932 0 90) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 49 PA12) (solder_mask_margin 0.0508))
    (pad 4 smd rect (at 3.44932 0.8001 90) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad 5 smd rect (at 3.44932 1.6002 90) (size 2.30124 0.50038) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.0508))
    (pad 6 smd rect (at 3.35026 -4.45008 90) (size 2.49936 1.99898) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -2.14884 -4.45008 90) (size 2.49936 1.99898) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 3.35026 4.45008 90) (size 2.49936 1.99898) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -2.14884 4.45008 90) (size 2.49936 1.99898) (layers F.Cu F.Paste F.Mask))
    (pad "" np_thru_hole circle (at 0.8509 -2.19964 90) (size 0.89916 0.89916) (drill 0.89916) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0.8509 2.19964 90) (size 0.89916 0.89916) (drill 0.89916) (layers *.Cu *.Mask F.SilkS))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 84.1375 100.9015)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C14 (at 1.032 -1.651) (layer F.SilkS))
    (fp_text value .1uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 VDD1))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 79.248 113.665 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 2.54 0.016 360) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 VCAP2))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 81.588768 113.721682 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C16 (at 2.610318 -0.072232 360) (layer F.SilkS))
    (fp_text value .1uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 VDD1))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 66.564 108.966)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -0.016 -1.651) (layer F.SilkS))
    (fp_text value 2.2uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 VCAP1))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 74.295 95.504 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 2.397 0.127 180) (layer F.SilkS))
    (fp_text value .1uF (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 NRST))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 66.6115 111.4425 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at -0.079026 -1.698122 180) (layer F.SilkS))
    (fp_text value .1uF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 VDD1))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 80.772 85.471 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at -2.413 0 360) (layer F.SilkS))
    (fp_text value 12pF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 OSCIN))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 89.154 85.598 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at -2.413 0.016 360) (layer F.SilkS))
    (fp_text value 12pF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 OSC32_IN))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 85.852 85.598 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at -2.413 0.016 360) (layer F.SilkS))
    (fp_text value 12pF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 OSC32_OUT))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 67.183 100.7905 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at -2.627462 -0.225952 180) (layer F.SilkS))
    (fp_text value .1uF (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 VDD1))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 71.204875 96.507365 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at 3.413 0 180) (layer F.SilkS))
    (fp_text value .1uF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 VDD1))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210 (layer F.Cu) (tedit 5415D85D)
    (at 66.675 133.985 270)
    (descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C18 (at 3.175 -0.127 540) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.7 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 10 5V_IN))
    (pad 2 smd rect (at 1.5 0 270) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 58.801 133.477 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C19 (at -2.556 -0.127 180) (layer F.SilkS))
    (fp_text value 10nF (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 VDD1))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C19-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210 (layer F.Cu) (tedit 5415D85D)
    (at 55.245 132.969 90)
    (descr "Capacitor SMD 1210, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C20 (at -3.175 0 360) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.7 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 90) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 5 VDD1))
    (pad 2 smd rect (at 1.5 0 90) (size 1 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED-0805 (layer F.Cu) (tedit 55BDE1C2)
    (at 70.6755 117.856 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D4 (at 1.143 1.9685 360) (layer F.SilkS))
    (fp_text value LED (at 0 1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 54 PC9))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D4-Pad1)"))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 0)
    (at 84.074 134.62 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -2.286 0.127 180) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 VDD1))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 SWCLK))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 SWDIO))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 NRST))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 TRACESWO))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x16 (layer F.Cu) (tedit 0)
    (at 54.61 88.9)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 2.286 40.513) (layer F.SilkS))
    (fp_text value CONN_01X32 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 VDD1))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 VDD1))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 PC0))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 PC1))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 PC2))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 PC3))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 PA0))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 PA1))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 PA2))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 PA3))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 PA4))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 PA5))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 PA6))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 PA7))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 PC4))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 PC5))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 PB0))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 PB1))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 PB2))
    (pad 22 thru_hole oval (at 2.54 25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 PB10))
    (pad 23 thru_hole oval (at 0 27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 66 PB11_VCAP1))
    (pad 24 thru_hole oval (at 2.54 27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 61 PB12))
    (pad 25 thru_hole oval (at 0 30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 PB13))
    (pad 26 thru_hole oval (at 2.54 30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 59 PB14))
    (pad 27 thru_hole oval (at 0 33.02) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 58 PB15))
    (pad 28 thru_hole oval (at 2.54 33.02) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 PC6))
    (pad 29 thru_hole oval (at 0 35.56) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 56 PC7))
    (pad 30 thru_hole oval (at 2.54 35.56) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 55 PC8))
    (pad 31 thru_hole oval (at 0 38.1) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 VDD1))
    (pad 32 thru_hole oval (at 2.54 38.1) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x16.wrl
      (at (xyz 0.05 -0.75 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x16 (layer F.Cu) (tedit 0)
    (at 95.25 88.9)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 3.556 40.513) (layer F.SilkS))
    (fp_text value CONN_01X32 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 VDD1))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 VDD1))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 PC13))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 NRST))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 63 VBAT))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 PB9))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 PB8))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 BOOT0))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 PB7))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 PB6))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 PB5))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 PB4))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 TRACESWO))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 PD2))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 PC12))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 PC11))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 PC10))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 PA15))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 SWCLK))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 SWDIO))
    (pad 22 thru_hole oval (at 2.54 25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 PA12))
    (pad 23 thru_hole oval (at 0 27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 PA11))
    (pad 24 thru_hole oval (at 2.54 27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 PA10))
    (pad 25 thru_hole oval (at 0 30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 PA9))
    (pad 26 thru_hole oval (at 2.54 30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 PA8))
    (pad 27 thru_hole oval (at 0 33.02) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 PC9))
    (pad 28 thru_hole oval (at 2.54 33.02) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 5V_IN))
    (pad 29 thru_hole oval (at 0 35.56) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 VDD1))
    (pad 30 thru_hole oval (at 2.54 35.56) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 VDD1))
    (pad 31 thru_hole oval (at 0 38.1) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 32 thru_hole oval (at 2.54 38.1) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x16.wrl
      (at (xyz 0.05 -0.75 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module SMD_Packages:SMD-1206_Pol (layer F.Cu) (tedit 0)
    (at 87.539869 89.554317 180)
    (attr smd)
    (fp_text reference Y2 (at -0.090131 -1.885683 180) (layer F.SilkS))
    (fp_text value Crystal (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.651 0 180) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 8 OSC32_IN))
    (pad 2 smd rect (at 1.651 0 180) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 9 OSC32_OUT))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 91.186 129.032 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R1 (at 2.667 0.127 180) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 NRST))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 VDD1))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 76.581 95.504 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -2.1 360) (layer F.SilkS))
    (fp_text value 0 (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C7-Pad2)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 62 OSCOUT))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 75.7555 123.063 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R3 (at 2.54 0.127 360) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 22 BOOT0))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 66.929 121.285)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R4 (at -1.143 -1.651) (layer F.SilkS))
    (fp_text value 470 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 71.6915 121.285 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R5 (at -1.27 1.651 360) (layer F.SilkS))
    (fp_text value 470 (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 80.899 122.301)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 -1.651) (layer F.SilkS))
    (fp_text value 1k (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(R6-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 59.563 130.048 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R7 (at -2.794 -0.127 180) (layer F.SilkS))
    (fp_text value 1k (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(R7-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 VDD1))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_FSMSM (layer F.Cu) (tedit 555C8B1B)
    (at 84.455 125.857 180)
    (descr http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=1437566-3&DocType=Customer+Drawing&DocLang=English)
    (tags "SPST button tactile switch")
    (attr smd)
    (fp_text reference SW1 (at 0.127 -2.667 180) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0.01011 -0.00022 180) (layer F.Fab))
    (pad 1 smd rect (at -4.60243 -0.00232 180) (size 2.18 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 NRST))
    (pad 2 smd rect (at 4.60243 0.00232 180) (size 2.18 1.6) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(R6-Pad1)"))
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 5654AAFC)
    (at 51.308 84.328)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 1.00076 5.00126) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers))
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 5654AAF7)
    (at 101.092 84.328)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 1.00076 5.00126) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers))
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 5654AAF9)
    (at 101.092 136.652)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 1.00076 5.00126) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers))
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 5654AAFF)
    (at 51.308 136.652)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 1.00076 5.00126) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 576F4D07)
    (at 63.5 109.982 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 2.54 -0.127 180) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 66 PB11_VCAP1))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 84.82 114.681 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R9 (at -0.143 -1.651 180) (layer F.SilkS))
    (fp_text value DNP (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 VCAP2))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_SMD_5032_2Pads (layer F.Cu) (tedit 56D4CA47)
    (at 78.595 89.916)
    (descr "Ceramic SMD crystal, 5.0x3.2mm, 2 Pads")
    (tags "crystal oscillator quartz SMD SMT 5032")
    (attr smd)
    (fp_text reference Y1 (at 0 -2.8) (layer F.SilkS))
    (fp_text value Crystal (at 0 2.9) (layer F.Fab))
    (pad 1 smd rect (at -2.05 0) (size 2 2.4) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C7-Pad2)"))
    (pad 2 smd rect (at 2.05 0) (size 2 2.4) (layers F.Cu F.Paste F.Mask)
      (net 6 OSCIN))
    (model Crystals.3dshapes/Crystal_SMD_5032_2Pads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 104.14 81.28) (end 104.14 139.7) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 48.26 81.28) (end 104.14 81.28) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 48.26 139.7) (end 48.26 81.28) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104.14 139.7) (end 48.26 139.7) (layer Edge.Cuts) (width 0.15))
  (gr_text "2016 MR" (at 93.726 137.668) (layer F.Cu))
  (gr_text OSHW (at 64.643 88.011) (layer F.SilkS))
  (gr_text 5V (at 100.457 121.9835) (layer F.SilkS))
  (gr_text "RESET\n" (at 85.0265 123.19) (layer F.SilkS))
  (gr_text BOOT (at 68.072 123.19) (layer F.SilkS))
  (gr_text VBAT (at 91.694 91.44) (layer F.SilkS))
  (gr_text SWO (at 96.774 131.318 90) (layer F.SilkS))
  (gr_text RST (at 94.361 131.572 90) (layer F.SilkS))
  (gr_text DIO (at 91.694 131.572 90) (layer F.SilkS))
  (gr_text GND (at 89.281 131.318 90) (layer F.SilkS))
  (gr_text CLK (at 86.741 131.445 90) (layer F.SilkS))
  (gr_text VDD (at 84.201 131.445 90) (layer F.SilkS))
  (gr_text ARMKit2 (at 57.785 85.09) (layer F.SilkS))
  (gr_text PC9 (at 91.948 121.92) (layer F.SilkS))
  (gr_text VDD (at 92.075 124.587) (layer F.SilkS))
  (gr_text GND (at 91.948 127.127) (layer F.SilkS))
  (gr_text GND (at 101.092 127) (layer F.SilkS))
  (gr_text VDD (at 101.092 124.5235) (layer F.SilkS))
  (gr_text PA9 (at 91.948 119.507) (layer F.SilkS))
  (gr_text PA8 (at 100.965 119.38) (layer F.SilkS))
  (gr_text PA11 (at 91.567 116.84) (layer F.SilkS))
  (gr_text PA10 (at 101.473 116.84) (layer F.SilkS))
  (gr_text PA12 (at 101.473 114.427) (layer F.SilkS))
  (gr_text SWDIO (at 91.186 114.3) (layer F.SilkS))
  (gr_text PA15 (at 91.567 111.887) (layer F.SilkS))
  (gr_text PC11 (at 91.567 109.22) (layer F.SilkS))
  (gr_text CLK (at 100.965 111.76) (layer F.SilkS))
  (gr_text PD2 (at 91.948 106.68) (layer F.SilkS))
  (gr_text PB4 (at 91.948 104.14) (layer F.SilkS))
  (gr_text PB6 (at 91.948 101.727) (layer F.SilkS))
  (gr_text PC10 (at 101.473 109.347) (layer F.SilkS))
  (gr_text PC12 (at 101.473 106.807) (layer F.SilkS))
  (gr_text SWO (at 101.092 104.267) (layer F.SilkS))
  (gr_text PB5 (at 100.965 101.727) (layer F.SilkS))
  (gr_text BOOT0 (at 91.059 99.187) (layer F.SilkS))
  (gr_text PB7 (at 100.965 99.06) (layer F.SilkS))
  (gr_text PB9 (at 91.948 96.52) (layer F.SilkS))
  (gr_text NRST (at 91.694 94.107) (layer F.SilkS))
  (gr_text PB8 (at 100.965 96.647) (layer F.SilkS))
  (gr_text PC13 (at 101.473 94.107) (layer F.SilkS))
  (gr_text GND (at 101.092 91.44) (layer F.SilkS))
  (gr_text VDD (at 101.092 88.9) (layer F.SilkS))
  (gr_text VDD (at 92.202 88.9) (layer F.SilkS))
  (gr_text GND (at 60.579 127) (layer F.SilkS))
  (gr_text VDD (at 51.308 127.127) (layer F.SilkS))
  (gr_text PC8 (at 60.452 124.587) (layer F.SilkS))
  (gr_text PC7 (at 51.181 124.587) (layer F.SilkS))
  (gr_text PC6 (at 60.452 122.047) (layer F.SilkS))
  (gr_text PB15 (at 50.8 122.047) (layer F.SilkS))
  (gr_text PB14 (at 60.96 119.38) (layer F.SilkS))
  (gr_text PB13 (at 50.8 119.38) (layer F.SilkS))
  (gr_text PB12 (at 60.96 116.84) (layer F.SilkS))
  (gr_text PB11 (at 50.673 116.84) (layer F.SilkS))
  (gr_text PB10 (at 60.96 114.427) (layer F.SilkS))
  (gr_text PB2 (at 51.181 114.427) (layer F.SilkS))
  (gr_text PB1 (at 60.452 111.76) (layer F.SilkS))
  (gr_text PB0 (at 51.181 112.014) (layer F.SilkS))
  (gr_text PC5 (at 60.452 109.22) (layer F.SilkS))
  (gr_text PC4 (at 51.181 109.347) (layer F.SilkS))
  (gr_text PA7 (at 60.325 106.68) (layer F.SilkS))
  (gr_text PA6 (at 51.181 106.68) (layer F.SilkS))
  (gr_text PA5 (at 60.325 104.14) (layer F.SilkS))
  (gr_text PA4 (at 51.308 104.14) (layer F.SilkS))
  (gr_text PA3 (at 60.452 101.6) (layer F.SilkS))
  (gr_text PA2 (at 51.181 101.6) (layer F.SilkS))
  (gr_text PA1 (at 60.452 99.06) (layer F.SilkS))
  (gr_text PA0 (at 51.308 99.187) (layer F.SilkS))
  (gr_text PC3 (at 60.452 96.52) (layer F.SilkS))
  (gr_text PC2 (at 51.308 96.774) (layer F.SilkS))
  (gr_text PC1 (at 60.452 93.98) (layer F.SilkS))
  (gr_text PC0 (at 51.308 94.107) (layer F.SilkS))
  (gr_text GND (at 51.308 91.567) (layer F.SilkS))
  (gr_text GND (at 60.579 91.44) (layer F.SilkS))
  (gr_text VDD (at 60.579 89.027) (layer F.SilkS))
  (gr_text VDD (at 51.308 88.9) (layer F.SilkS))
  (zone (net 5) (net_name VDD1) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 52.832 90.17) (xy 59.69 90.17) (xy 61.341 91.821) (xy 65.151 91.821) (xy 66.04 92.71)
        (xy 67.31 92.71) (xy 67.31 82.55) (xy 52.07 82.55) (xy 52.07 90.17) (xy 52.959 90.17)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 52.07 82.55) (xy 100.33 82.55) (xy 100.33 138.43) (xy 52.07 138.43)
      )
    )
  )
)
