(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~58~ubuntu16.04.1)
  (general
    (links 190)
    (no_connects 1)
    (area 99.924999 60.924999 148.075001 136.075001)
    (thickness 1.6)
    (drawings 40)
    (tracks 996)
    (zones 0)
    (modules 69)
    (nets 45)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.4)
    (trace_clearance 0.17)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.16)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5.5 5.5)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory /home/kolijn/Desktop/gerbers/))
  )
  (net 0 "")
  (net 1 +BATT)
  (net 2 GND)
  (net 3 +3V3)
  (net 4 "Net-(C14-Pad1)")
  (net 5 "Net-(C15-Pad1)")
  (net 6 "Net-(C16-Pad1)")
  (net 7 "Net-(C17-Pad1)")
  (net 8 /V_Charger)
  (net 9 /BAT_MEASURE)
  (net 10 /REG_ENABLE)
  (net 11 /V_Solar)
  (net 12 VBUS)
  (net 13 "Net-(D6-Pad1)")
  (net 14 /charge_status)
  (net 15 "Net-(F1-Pad2)")
  (net 16 /MISO)
  (net 17 /SCK)
  (net 18 /MOSI)
  (net 19 /RESET)
  (net 20 /UART_AT_TO_RN)
  (net 21 /UART_RN_TO_AT)
  (net 22 /UART_GPS_OUT)
  (net 23 /UART_GPS_IN)
  (net 24 "Net-(R3-Pad2)")
  (net 25 /USBD+)
  (net 26 /USBD-)
  (net 27 "Net-(U2-Pad16)")
  (net 28 /RN_RESET)
  (net 29 /BUTTON_1)
  (net 30 /V_RN)
  (net 31 /V_bak)
  (net 32 /LED_OUT_GRN)
  (net 33 /LED_OUT_RED)
  (net 34 "Net-(C1-Pad3)")
  (net 35 "Net-(D5-Pad2)")
  (net 36 "Net-(IC1-Pad5)")
  (net 37 "Net-(J6-Pad2)")
  (net 38 "Net-(J6-Pad3)")
  (net 39 "Net-(J16-Pad4)")
  (net 40 "Net-(J16-Pad5)")
  (net 41 "Net-(J17-Pad1)")
  (net 42 "Net-(R2-Pad2)")
  (net 43 "Net-(D3-Pad2)")
  (net 44 "Net-(D4-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.17)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +BATT)
    (add_net /BAT_MEASURE)
    (add_net /BUTTON_1)
    (add_net /LED_OUT_GRN)
    (add_net /LED_OUT_RED)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /REG_ENABLE)
    (add_net /RESET)
    (add_net /RN_RESET)
    (add_net /SCK)
    (add_net /UART_AT_TO_RN)
    (add_net /UART_GPS_IN)
    (add_net /UART_GPS_OUT)
    (add_net /UART_RN_TO_AT)
    (add_net /USBD+)
    (add_net /USBD-)
    (add_net /V_Charger)
    (add_net /V_RN)
    (add_net /V_Solar)
    (add_net /V_bak)
    (add_net /charge_status)
    (add_net GND)
    (add_net "Net-(C1-Pad3)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(IC1-Pad5)")
    (add_net "Net-(J16-Pad4)")
    (add_net "Net-(J16-Pad5)")
    (add_net "Net-(J17-Pad1)")
    (add_net "Net-(J6-Pad2)")
    (add_net "Net-(J6-Pad3)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(U2-Pad16)")
    (add_net VBUS)
  )
  (net_class 50_OHM_line ""
    (clearance 0.12)
    (trace_width 0.35)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Diodes_SMD:D_SOT-23_ANK (layer F.Cu) (tedit 5B76EFE8)
    (at 111.506 114.046 180)
    (descr "SOT-23, Single Diode")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D2 (at -2.594 0.046 180) (layer F.SilkS))
    (fp_text value "BAS K73" (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.5 180) (layer F.Fab))
    (pad 2 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 12 VBUS))
    (pad "" smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 /V_Charger))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOT-23_ANK (layer F.Cu) (tedit 5B76EFEC)
    (at 111.506 110.49 180)
    (descr "SOT-23, Single Diode")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D1 (at -2.594 -0.11 180) (layer F.SilkS))
    (fp_text value "BAS K73" (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.5 180) (layer F.Fab))
    (pad 2 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 11 /V_Solar))
    (pad "" smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 /V_Charger))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_PicoBlade_53047-0210_02x1.25mm_Straight (layer F.Cu) (tedit 5B76F044)
    (at 102.616 88.646 90)
    (descr "Molex PicoBlade, single row, top entry type, through hole, PN:53047-0210")
    (tags "connector molex picoblade")
    (fp_text reference J14 (at -3.354 0.584 90) (layer F.SilkS))
    (fp_text value SOLAR (at 0.625 -3.25 90) (layer F.Fab))
    (fp_text user %R (at 0.625 -1.25 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 11 /V_Solar))
    (pad 2 thru_hole circle (at 1.25 0 90) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_PicoBlade_53047-0210_02x1.25mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_PicoBlade_53047-0210_02x1.25mm_Straight (layer F.Cu) (tedit 5B76F2D0)
    (at 102.616 83.058 90)
    (descr "Molex PicoBlade, single row, top entry type, through hole, PN:53047-0210")
    (tags "connector molex picoblade")
    (fp_text reference J13 (at 2.458 2.384 90) (layer F.SilkS))
    (fp_text value LIPO_BAT (at 0.625 -3.25 90) (layer F.Fab))
    (fp_text user %R (at 0.625 -1.25 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 +BATT))
    (pad 2 thru_hole circle (at 1.25 0 90) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_PicoBlade_53047-0210_02x1.25mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 135.382 73.66)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C21 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 31 /V_bak))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5B76EFBE)
    (at 107.696 121.92 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R17 (at -1.28 -1.596 90) (layer F.SilkS))
    (fp_text value 470 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 /V_Charger))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5B76F28A)
    (at 111.506 87.63 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 2.23 1.994 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5B76F28F)
    (at 113.538 88.138 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at -0.162 1.662 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5B76F090)
    (at 132.842 68.072)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 3.058 0.028) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C1-Pad3)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 58AA8463)
    (at 111.252 117.602 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 1.5 180) (layer B.SilkS))
    (fp_text value 4.7uF (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.5 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 30 /V_RN))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5B76F24F)
    (at 113.538 91.694 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at -0.106 1.562 90) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 123.571 79.375 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5B76F0AA)
    (at 126.619 85.09 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 3.19 -0.019 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5B76F02C)
    (at 125.476 102.489 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 2.776 -0.111 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 135.89 85.09 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 0 -1.5 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 139.954 97.028)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5B76F1D5)
    (at 136.398 115.062)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at 3.402 -0.062) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.75) (layer B.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 30 /V_RN))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5B76F095)
    (at 132.842 69.85)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C13 (at 3.358 -0.05) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C1-Pad3)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5B76F025)
    (at 133.096 105.664)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C14 (at -0.096 -1.764) (layer F.SilkS))
    (fp_text value 22pF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C14-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5B76F030)
    (at 125.476 105.664 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C15 (at 3.376 -0.036 180) (layer F.SilkS))
    (fp_text value 22pF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C15-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5B76F25C)
    (at 122.682 93.726 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C16 (at 3.182 -0.174 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C16-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5B76F0A7)
    (at 128.397 85.09 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C17 (at 3.29 0.103 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C17-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 108.839 110.236 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C18 (at 0 -1.5 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 /V_Charger))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 119.8245 82.3595)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C20 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /BAT_MEASURE))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5B76F0D3)
    (at 113.03 118.364 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at 0.036 -1.57 270) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5B76EFCC)
    (at 107.696 118.364 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D5 (at 0.036 -1.804 360) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(D5-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 14 /charge_status))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5B76EFC5)
    (at 109.474 118.364 90)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D6 (at -0.136 -3.374 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 14 /charge_status))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D6-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module "gps_node_components:bourns polyfuse" (layer F.Cu) (tedit 5B76F26A)
    (at 107.569 97.409 270)
    (fp_text reference F1 (at -1.309 2.369 270) (layer F.SilkS))
    (fp_text value Polyfuse (at 0 -6.35 270) (layer F.Fab))
    (pad 1 smd rect (at -2.35 0 270) (size 2 3.2) (layers F.Cu F.Paste F.Mask)
      (net 12 VBUS))
    (pad 2 smd rect (at 2.35 0 270) (size 2 3.2) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(F1-Pad2)"))
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 5B76EFF8)
    (at 107.95 114.046 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference IC1 (at -0.854 -2.65 90) (layer F.SilkS))
    (fp_text value MCP73831/2 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 14 /charge_status))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 /V_Charger))
    (pad 5 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(IC1-Pad5)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module gps_node_components:Molex_Microusb (layer F.Cu) (tedit 5B76F011)
    (at 103.886 103.124 270)
    (fp_text reference J6 (at -5.724 2.486 270) (layer F.SilkS))
    (fp_text value USB_OTG (at 0 -7.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.3 -0.325 270) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(F1-Pad2)"))
    (pad 2 smd rect (at -0.65 -0.325 270) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(J6-Pad2)"))
    (pad 3 smd rect (at 0 -0.325 270) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(J6-Pad3)"))
    (pad 4 smd rect (at 0.65 -0.325 270) (size 0.4 2) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.3 -0.325 270) (size 0.4 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at -2.5 0 270) (size 1.45 1.45) (drill 0.85) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at 2.5 0 270) (size 1.45 1.45) (drill 0.85) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at -3.5 2.7 270) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at 3.5 2.7 270) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 142.494 84.074)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J11 (at 1.27 -2.33) (layer F.SilkS))
    (fp_text value "AVR ICSP" (at 1.27 7.41) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /MISO))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /SCK))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /MOSI))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /RESET))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 102.108 110.998)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J16 (at 0 -2.33) (layer F.SilkS))
    (fp_text value FW_UPDATE (at 0 15.03) (layer F.Fab))
    (fp_text user %R (at 0 6.35 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /RN_RESET))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /V_RN))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J16-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J16-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO14580_Pad (layer F.Cu) (tedit 5B76EE3A)
    (at 105 76)
    (descr "Mounting Hole 3.2mm, M3, ISO14580")
    (tags "mounting hole 3.2mm m3 iso14580")
    (attr virtual)
    (fp_text reference J1 (at 0 -3.75) (layer F.SilkS))
    (fp_text value "Mounting Hole" (at 0 3.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO14580_Pad (layer F.Cu) (tedit 5B76EE2F)
    (at 133 131)
    (descr "Mounting Hole 3.2mm, M3, ISO14580")
    (tags "mounting hole 3.2mm m3 iso14580")
    (attr virtual)
    (fp_text reference J2 (at 0 -3.75) (layer F.SilkS))
    (fp_text value "Mounting Hole" (at 0 3.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO14580_Pad (layer F.Cu) (tedit 5B76EE34)
    (at 143 76)
    (descr "Mounting Hole 3.2mm, M3, ISO14580")
    (tags "mounting hole 3.2mm m3 iso14580")
    (attr virtual)
    (fp_text reference J3 (at 0 -3.75) (layer F.SilkS))
    (fp_text value "Mounting Hole" (at 0 3.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO14580_Pad (layer F.Cu) (tedit 5B76EE29)
    (at 115 131)
    (descr "Mounting Hole 3.2mm, M3, ISO14580")
    (tags "mounting hole 3.2mm m3 iso14580")
    (attr virtual)
    (fp_text reference J4 (at 0 -3.75) (layer F.SilkS))
    (fp_text value "Mounting Hole" (at 0 3.75) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5B76F2CA)
    (at 106.045 86.614)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (fp_text reference J5 (at -0.845 -2.514) (layer F.SilkS))
    (fp_text value "TEST Vbatt" (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +BATT))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5B76F255)
    (at 112.903 95.377)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (fp_text reference J7 (at 1.697 2.523) (layer F.SilkS))
    (fp_text value "Test 3.3v" (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5B76F048)
    (at 106.045 90.17)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (fp_text reference J8 (at -0.245 2.63) (layer F.SilkS))
    (fp_text value "Test Gnd" (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 146.05 109.22 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J12 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value "UART RF" (at 0 7.41 180) (layer F.Fab))
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /UART_AT_TO_RN))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /UART_RN_TO_AT))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 110.744 73.152)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J15 (at 0 -2.33) (layer F.SilkS))
    (fp_text value "UART GPS" (at 0 7.41) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /UART_GPS_OUT))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /UART_GPS_IN))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5B76F294)
    (at 109.474 88.392 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 2.492 0.026 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /REG_ENABLE))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5B76EFAE)
    (at 111.252 121.92 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at 2.88 -0.248 270) (layer F.SilkS))
    (fp_text value 470 (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(D4-Pad2)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 32 /LED_OUT_GRN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5B76F07F)
    (at 117.602 76.708 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 2.508 -0.102 90) (layer F.SilkS))
    (fp_text value 220 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 23 /UART_GPS_IN))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5B76F07B)
    (at 115.824 76.708 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 2.508 0.076 90) (layer F.SilkS))
    (fp_text value 220 (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 22 /UART_GPS_OUT))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5B76F00C)
    (at 108.204 103.759 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at -2.396 0.159 180) (layer F.SilkS))
    (fp_text value 22 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 25 /USBD+))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(J6-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5B76F008)
    (at 108.204 101.981 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at -2.396 0.081 180) (layer F.SilkS))
    (fp_text value 22 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 26 /USBD-))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(J6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 127.762 112.268 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 -1.65 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 /RESET))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5B76EFB7)
    (at 113.03 121.92 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at 2.88 -0.37 270) (layer F.SilkS))
    (fp_text value 470 (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 33 /LED_OUT_RED))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5B76EFF4)
    (at 106.934 110.49 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at 3.09 0.066 90) (layer F.SilkS))
    (fp_text value 2k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(IC1-Pad5)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 116.7765 80.4545)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R15 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 100k (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 /BAT_MEASURE))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 120.0785 80.4545)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R16 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 100k (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 /BAT_MEASURE))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5B76EFA1)
    (at 109.474 121.92 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R18 (at 2.88 -0.326 270) (layer F.SilkS))
    (fp_text value 470 (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D6-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_PTS645 (layer F.Cu) (tedit 5B76EF88)
    (at 130 119 270)
    (descr "C&K Components SPST SMD PTS645 Series 6mm Tact Switch")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference SW2 (at 6.1 0.1 360) (layer F.SilkS))
    (fp_text value RESET (at 0 4.15 270) (layer F.Fab))
    (fp_text user %R (at 0 -4.05 270) (layer F.Fab))
    (pad 2 smd rect (at -3.98 2.25 270) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 /RESET))
    (pad 1 smd rect (at -3.98 -2.25 270) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 3.98 -2.25 270) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 3.98 2.25 270) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 /RESET))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_PTS645.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 5B76F266)
    (at 110.49 91.948 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U1 (at 2.752 0.29 270) (layer F.SilkS))
    (fp_text value TLV71333PDBV (at 0 2.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 /REG_ENABLE))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module drawn_by_jpmeijers:ublox-cam-m8q-0 (layer F.Cu) (tedit 5B76F065)
    (at 124 75 90)
    (fp_text reference U2 (at 3.1 -6.3 90) (layer F.SilkS))
    (fp_text value ublox-cam-m8q-0 (at 7.15 -6.35 90) (layer F.Fab))
    (pad 1 smd rect (at 0.8 4.4 90) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C1-Pad3)"))
    (pad 2 smd rect (at 1.8 4.4 90) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 2.8 4.4 90) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 3.8 4.4 90) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 4.8 4.4 90) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 5.8 4.4 90) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 6.8 4.4 90) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 7.8 4.4 90) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 31 /V_bak))
    (pad 9 smd rect (at 8.8 4.4 90) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C1-Pad3)"))
    (pad 10 smd rect (at 9.8 4.4 90) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 10.8 4.4 90) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 12 smd rect (at 11.8 4.4 90) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 13 smd rect (at 12.95 4.4 90) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 14 smd rect (at 12.95 -4.4 90) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 15 smd rect (at 11.8 -4.4 90) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 16 smd rect (at 10.8 -4.4 90) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U2-Pad16)"))
    (pad 17 smd rect (at 9.8 -4.4 90) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U2-Pad16)"))
    (pad 18 smd rect (at 8.8 -4.4 90) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 19 smd rect (at 7.8 -4.4 90) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 20 smd rect (at 6.8 -4.4 90) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 5.8 -4.4 90) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 22 smd rect (at 4.8 -4.4 90) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 23 smd rect (at 3.8 -4.4 90) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 24 smd rect (at 2.8 -4.4 90) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 25 smd rect (at 1.8 -4.4 90) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R3-Pad2)"))
    (pad 26 smd rect (at 0.8 -4.4 90) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R2-Pad2)"))
    (pad 27 smd rect (at 0.4 -2 180) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 28 smd rect (at 0.4 -1 180) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 29 smd rect (at 0.4 0 180) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at 0.4 1 180) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask))
    (pad 31 smd rect (at 0.4 2 180) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Housings_QFP:TQFP-44_10x10mm_Pitch0.8mm (layer F.Cu) (tedit 58CC9A48)
    (at 131.318 93.726)
    (descr "44-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1.0 mm Body [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U4 (at 0 -7.45) (layer F.SilkS))
    (fp_text value ATMEGA32U4-AU (at 0 7.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -5.7 -4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -5.7 -3.2) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 VBUS))
    (pad 3 smd rect (at -5.7 -2.4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 26 /USBD-))
    (pad 4 smd rect (at -5.7 -1.6) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 25 /USBD+))
    (pad 5 smd rect (at -5.7 -0.8) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -5.7 0) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C16-Pad1)"))
    (pad 7 smd rect (at -5.7 0.8) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 VBUS))
    (pad 8 smd rect (at -5.7 1.6) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at -5.7 2.4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 /SCK))
    (pad 10 smd rect (at -5.7 3.2) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 /MISO))
    (pad 11 smd rect (at -5.7 4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 /MOSI))
    (pad 12 smd rect (at -4 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -3.2 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 19 /RESET))
    (pad 14 smd rect (at -2.4 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 15 smd rect (at -1.6 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 16 smd rect (at -0.8 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C15-Pad1)"))
    (pad 17 smd rect (at 0 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C14-Pad1)"))
    (pad 18 smd rect (at 0.8 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 29 /BUTTON_1))
    (pad 19 smd rect (at 1.6 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 2.4 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 21 /UART_RN_TO_AT))
    (pad 21 smd rect (at 3.2 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 20 /UART_AT_TO_RN))
    (pad 22 smd rect (at 4 5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 5.7 4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 24 smd rect (at 5.7 3.2) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 25 smd rect (at 5.7 2.4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 26 smd rect (at 5.7 1.6) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 27 smd rect (at 5.7 0.8) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 28 smd rect (at 5.7 0) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 29 smd rect (at 5.7 -0.8) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 22 /UART_GPS_OUT))
    (pad 30 smd rect (at 5.7 -1.6) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 /UART_GPS_IN))
    (pad 31 smd rect (at 5.7 -2.4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 28 /RN_RESET))
    (pad 32 smd rect (at 5.7 -3.2) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 33 smd rect (at 5.7 -4) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 34 smd rect (at 4 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 35 smd rect (at 3.2 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 36 smd rect (at 2.4 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 32 /LED_OUT_GRN))
    (pad 37 smd rect (at 1.6 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 33 /LED_OUT_RED))
    (pad 38 smd rect (at 0.8 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 0 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 40 smd rect (at -0.8 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 /charge_status))
    (pad 41 smd rect (at -1.6 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 /BAT_MEASURE))
    (pad 42 smd rect (at -2.4 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C17-Pad1)"))
    (pad 43 smd rect (at -3.2 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 44 smd rect (at -4 -5.7 90) (size 1.5 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Housings_QFP.3dshapes/TQFP-44_10x10mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module drawn_by_jpmeijers:RN2483 (layer B.Cu) (tedit 5643193A)
    (at 115 100)
    (fp_text reference U5 (at 2.8956 1.4478) (layer B.SilkS))
    (fp_text value RN2483 (at 4.7752 24.2062) (layer B.Fab) hide)
    (pad 47 smd rect (at 0 1.27) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 46 smd rect (at 0 2.54) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask))
    (pad 45 smd rect (at 0 3.81) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask))
    (pad 44 smd rect (at 0 5.08) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask))
    (pad 43 smd rect (at 0 6.35) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask))
    (pad 42 smd rect (at 0 7.62) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask))
    (pad 41 smd rect (at 0 8.89) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 40 smd rect (at 0 10.16) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask))
    (pad 39 smd rect (at 0 11.43) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask))
    (pad 38 smd rect (at 0 12.7) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask))
    (pad 37 smd rect (at 0 13.97) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask))
    (pad 36 smd rect (at 0 15.24) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask))
    (pad 35 smd rect (at 0 16.51) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask))
    (pad 34 smd rect (at 0 17.78) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask)
      (net 30 /V_RN))
    (pad 33 smd rect (at 0 19.05) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 32 smd rect (at 0 20.32) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask)
      (net 28 /RN_RESET))
    (pad 31 smd rect (at 0 21.59) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(J16-Pad4)"))
    (pad 30 smd rect (at 0 22.86) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(J16-Pad5)"))
    (pad 29 smd rect (at 0 24.13) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask))
    (pad 28 smd rect (at 0 25.4) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 20 smd rect (at 17.78 25.4) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 27 smd rect (at 5.08 26.67) (size 1.016 1.524) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 26 smd rect (at 6.35 26.67) (size 1.016 1.524) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 25 smd rect (at 7.62 26.67) (size 1.016 1.524) (layers B.Cu B.Paste B.Mask))
    (pad 24 smd rect (at 8.89 26.67) (size 1.016 1.524) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 23 smd rect (at 10.16 26.67) (size 1.016 1.524) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(J17-Pad1)"))
    (pad 22 smd rect (at 11.43 26.67) (size 1.016 1.524) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 21 smd rect (at 12.7 26.67) (size 1.016 1.524) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 19 smd rect (at 17.78 24.13) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask))
    (pad 18 smd rect (at 17.78 22.86) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask))
    (pad 17 smd rect (at 17.78 21.59) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask))
    (pad 16 smd rect (at 17.78 20.32) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask))
    (pad 15 smd rect (at 17.78 19.05) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask))
    (pad 14 smd rect (at 17.78 17.78) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask))
    (pad 13 smd rect (at 17.78 16.51) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask))
    (pad 12 smd rect (at 17.78 15.24) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask)
      (net 30 /V_RN))
    (pad 11 smd rect (at 17.78 13.97) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 17.78 12.7) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask))
    (pad 9 smd rect (at 17.78 11.43) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask))
    (pad 8 smd rect (at 17.78 10.16) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 17.78 8.89) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask)
      (net 20 /UART_AT_TO_RN))
    (pad 6 smd rect (at 17.78 7.62) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask)
      (net 21 /UART_RN_TO_AT))
    (pad 5 smd rect (at 17.78 6.35) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at 17.78 5.08) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd rect (at 17.78 3.81) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 17.78 2.54) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask))
    (pad 1 smd rect (at 17.78 1.27) (size 1.524 1.016) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
  )
  (module gps_node_components:QC3CA_16MHz (layer F.Cu) (tedit 5B76F022)
    (at 129.286 104.394 90)
    (fp_text reference Y1 (at -3.006 -0.186 90) (layer F.SilkS))
    (fp_text value 16MHz (at 0 -2.8 90) (layer F.Fab))
    (pad 1 smd rect (at -1.2 0.95 90) (size 1.5 1.4) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C14-Pad1)"))
    (pad 2 smd rect (at 1.2 -0.95 90) (size 1.5 1.4) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C15-Pad1)"))
    (pad "" smd rect (at 1.2 0.95 90) (size 1.5 1.4) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -1.2 -0.95 90) (size 1.5 1.4) (layers F.Cu F.Paste F.Mask))
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 58E0A804)
    (at 105.156 112.014 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 0 1.65 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 28 /RN_RESET))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 30 /V_RN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 121.412 112.268 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 0 -1.65 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /BUTTON_1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_PTS645 (layer F.Cu) (tedit 5B76F0CA)
    (at 119 119 90)
    (descr "C&K Components SPST SMD PTS645 Series 6mm Tact Switch")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference SW3 (at -6.1 0.1 180) (layer F.SilkS))
    (fp_text value MODE (at 0 4.15 90) (layer F.Fab))
    (fp_text user %R (at 0 -4.05 90) (layer F.Fab))
    (pad 2 smd rect (at -3.98 2.25 90) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /BUTTON_1))
    (pad 1 smd rect (at -3.98 -2.25 90) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 3.98 -2.25 90) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 3.98 2.25 90) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 /BUTTON_1))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_PTS645.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5B76EFDB)
    (at 111.252 118.364 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D4 (at 0.036 -0.048 360) (layer F.SilkS))
    (fp_text value LED_Small_ALT (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module gps_node_components:CONN-RF-UFL (layer F.Cu) (tedit 5B76EF96)
    (at 127 132 180)
    (fp_text reference J17 (at -0.9 2.9 180) (layer F.SilkS))
    (fp_text value "u.FL connector" (at 2.159 -2.032 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.55 0 180) (size 1.1 2.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 3.45 0 180) (size 1.1 2.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 2 1.75 180) (size 1.2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(J17-Pad1)"))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 58CD5446)
    (at 131.699 74.168)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (fp_text reference J9 (at 0 -2.33) (layer F.SilkS))
    (fp_text value "Test V_bak" (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /V_bak))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5B76F275)
    (at 113.03 82.804 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference SW1 (at 0.296 -2.47 270) (layer F.SilkS))
    (fp_text value "RS stock no. 448-0747" (at 0 7.41 270) (layer F.Fab))
    (fp_text user %R (at 0 2.54 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +BATT))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /REG_ENABLE))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 5B76F08B)
    (at 135.382 76.962 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U3 (at 0.262 2.618 90) (layer F.SilkS))
    (fp_text value TLV71333PDBV (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 +BATT))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 31 /V_bak))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module gps_node_components:C_FEEDTHROUGH_0805 (layer B.Cu) (tedit 5B76F1C7)
    (at 136.398 118.11 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C19 (at -2.802 -0.89 180) (layer B.SilkS))
    (fp_text value NFM21HC105R1C3D (at 0 -2.1 180) (layer B.Fab))
    (pad 2 thru_hole circle (at 0 -1.15 180) (size 0.4 0.4) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0 1.15 180) (size 0.4 0.4) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
    (pad 2 smd rect (at 0 0.625 180) (size 0.6 0.65) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 1 smd rect (at -1 0 180) (size 0.6 0.8) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 3 smd rect (at 1 0 180) (size 0.6 0.8) (layers B.Cu B.Paste B.Mask)
      (net 30 /V_RN))
    (pad 2 smd rect (at 0 -0.625 180) (size 0.6 0.65) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0 0 180) (size 0.4 0.4) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module gps_node_components:C_FEEDTHROUGH_0805 (layer F.Cu) (tedit 5B76EAD0)
    (at 130.302 77.47 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -2 90) (layer F.SilkS))
    (fp_text value NFM21HC105R1C3D (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at 0 -2 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 1.15 90) (size 0.4 0.4) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0 -1.15 90) (size 0.4 0.4) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
    (pad 2 smd rect (at 0 -0.625 90) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 1 smd rect (at -1 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 3 smd rect (at 1 0 90) (size 0.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(C1-Pad3)"))
    (pad 2 smd rect (at 0 0.625 90) (size 0.6 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 0 0 90) (size 0.4 0.4) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "TTN Tracker Node \nv1.2\nhttp://ttntracker.com" (at 138 123.9 90) (layer F.SilkS))
  (gr_text "⇈\nGPS\nKeep upright" (at 133.4 63.5) (layer F.SilkS))
  (gr_text "868MHz Antenna" (at 124.8 134.3) (layer F.SilkS))
  (gr_text Solar (at 101.3 92.3 90) (layer F.SilkS))
  (gr_text Batt (at 101.3 78.4 90) (layer F.SilkS))
  (gr_text Off (at 112.9 80.5) (layer F.SilkS))
  (gr_text ON (at 107.8 80.5) (layer F.SilkS))
  (gr_text "TTN Tracker Node \nv1.2\nhttp://ttntracker.com" (at 137 85) (layer B.SilkS))
  (gr_text LORA (at 145.6 101.5) (layer F.SilkS))
  (gr_text GPS (at 113.8 72) (layer F.SilkS))
  (gr_text Out (at 113.6 73.3) (layer F.SilkS))
  (gr_text In (at 113.2 75.7) (layer F.SilkS))
  (gr_text IN (at 142.9 109.3) (layer F.SilkS))
  (gr_text OUT (at 143 106.8) (layer F.SilkS))
  (gr_text Gnd (at 143.1 104.2) (layer F.SilkS))
  (gr_text Gnd (at 113.7 78.4) (layer F.SilkS))
  (gr_arc (start 146 124) (end 148 124) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140 126) (end 146 126) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138 134) (end 138 128) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 112 136) (end 136 136) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 110 128) (end 110 134) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 102 126) (end 108 126) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148 73) (end 148 124) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138 63) (end 138 69) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140 71) (end 146 71) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 124) (end 100 73) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 102 124) (end 102 126) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 108 128) (end 108 126) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 112 134) (end 112 136) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 136 134) (end 138 134) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 140 128) (end 138 128) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 146 73) (end 146 71) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 140 69) (end 140 71) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 112 61) (end 136 61) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 110 69) (end 110 63) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 102 71) (end 108 71) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 102 73) (end 100 73) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 108 69) (end 110 69) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 136 63) (end 136 61) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 112 63) (end 110 63) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100 61) (xy 148 61) (xy 148 136) (xy 100 136)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100 136) (xy 100 61) (xy 148 61) (xy 148 136)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.6 61.1) (xy 127.6 65.8) (xy 120.4 65.8) (xy 120.4 61)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120.4 61) (xy 120.4 65.8) (xy 127.6 65.8) (xy 127.6 61)
      )
    )
  )
)
