<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="46.345" x2="0" y2="-6.35" width="0" layer="20"/>
<wire x1="0" y1="-6.35" x2="2.54" y2="-8.89" width="0" layer="20" curve="90"/>
<wire x1="2.54" y1="-8.89" x2="28.245" y2="-8.89" width="0" layer="20"/>
<wire x1="28.245" y1="-8.89" x2="30.785" y2="-6.35" width="0" layer="20" curve="90"/>
<wire x1="30.785" y1="-6.35" x2="30.785" y2="46.345" width="0" layer="20"/>
<wire x1="30.785" y1="46.345" x2="28.245" y2="48.885" width="0" layer="20" curve="90"/>
<wire x1="28.245" y1="48.885" x2="2.54" y2="48.885" width="0" layer="20"/>
<wire x1="2.54" y1="48.885" x2="0" y2="46.345" width="0" layer="20" curve="90"/>
<text>red</text>
<text>banana power
to eurorack</text>
<text>john slee
revision 2</text>
</plain>
<libraries>
<library name="jslee-approved">
<packages>
<package name="PCB-BANANA">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X8">
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,2">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.2 mm with drill center</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="5V" library="jslee-approved" package="PCB-BANANA" value="PCB-BANANA">
<attribute name="NAME"/>
</element>
<element name="GND" library="jslee-approved" package="PCB-BANANA" value="PCB-BANANA">
<attribute name="NAME"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="2X8" value="">
<attribute name="VALUE"/>
</element>
<element name="V+" library="jslee-approved" package="PCB-BANANA" value="PCB-BANANA">
<attribute name="NAME"/>
</element>
<element name="V-" library="jslee-approved" package="PCB-BANANA" value="PCB-BANANA">
<attribute name="NAME"/>
</element>
<element name="U$1" library="holes" package="3,2" value=""/>
<element name="U$2" library="holes" package="3,2" value=""/>
<element name="U$3" library="holes" package="3,2" value=""/>
<element name="U$4" library="holes" package="3,2" value=""/>
</elements>
<signals>
<signal name="+5V">
<contactref element="5V" pad="P$1"/>
<contactref element="5V" pad="P$2"/>
<contactref element="J1" pad="11"/>
<contactref element="J1" pad="12"/>
</signal>
<signal name="-12V">
<contactref element="V-" pad="P$1"/>
<contactref element="V-" pad="P$2"/>
<contactref element="J1" pad="1"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="GND" pad="P$1"/>
<contactref element="GND" pad="P$2"/>
<contactref element="J1" pad="3"/>
<contactref element="J1" pad="7"/>
<contactref element="J1" pad="5"/>
<contactref element="J1" pad="4"/>
<contactref element="J1" pad="8"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="+12V">
<contactref element="V+" pad="P$1"/>
<contactref element="V+" pad="P$2"/>
<contactref element="J1" pad="9"/>
<contactref element="J1" pad="10"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
