(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "unconnected-(J1-Pad28)")
  (net 3 "unconnected-(J1-Pad29)")
  (net 4 "unconnected-(J1-Pad30)")
  (net 5 "unconnected-(J1-Pad10)")
  (net 6 "Net-(C1-Pad3)")
  (net 7 "Net-(C5-Pad3)")
  (net 8 "Net-(C5-Pad4)")
  (net 9 "Net-(C6-Pad1)")
  (net 10 "Net-(C6-Pad2)")
  (net 11 "Net-(C6-Pad3)")
  (net 12 "Net-(C6-Pad4)")
  (net 13 "Net-(C7-Pad1)")
  (net 14 "Net-(C7-Pad2)")
  (net 15 "Net-(C7-Pad3)")
  (net 16 "Net-(C7-Pad4)")
  (net 17 "Net-(C1-Pad4)")
  (net 18 "Net-(C8-Pad2)")
  (net 19 "Net-(C5-Pad1)")
  (net 20 "Net-(C5-Pad2)")
  (net 21 "Net-(C8-Pad1)")
  (net 22 "unconnected-(J1-Pad27)")
  (net 23 "Net-(C1-Pad1)")
  (net 24 "Net-(C1-Pad2)")
  (net 25 "Net-(C8-Pad3)")
  (net 26 "Net-(C8-Pad4)")
  (net 27 "Net-(C2-Pad1)")
  (net 28 "Net-(C2-Pad2)")
  (net 29 "Net-(C2-Pad3)")
  (net 30 "Net-(C2-Pad4)")
  (net 31 "Net-(C3-Pad1)")
  (net 32 "Net-(C3-Pad2)")
  (net 33 "Net-(C3-Pad3)")
  (net 34 "Net-(C3-Pad4)")
  (net 35 "Net-(C4-Pad1)")
  (net 36 "Net-(C4-Pad2)")
  (net 37 "Net-(C4-Pad3)")
  (net 38 "Net-(C4-Pad4)")
  (footprint "Omnetics_microD:OMNETICS_A98055-037" locked (layer "F.Cu")
    (tedit 68C49557)
    (at 234.1118 97.5055 90)
    (property "Availability" "In Stock")
    (property "CREATOR" "DIZAR")
    (property "Check_prices" "https://www.snapeda.com/parts/A98055-037/Omnetics/view-part/?ref=eda")
    (property "Description" "\n                        \n                            MMDP-037-H2-.11-N00, Micro-D Dual Row 37 Pin Contact Horizontal Thru Hole (2 Row) Plug Connector w/ No Hardware\n                        \n")
    (property "MANUFACTURER" "Omnetics")
    (property "MAXIMUM_PACKAGE_HEIGHT" "8.13mm")
    (property "MF" "Omnetics")
    (property "MP" "A98055-037")
    (property "PARTREV" "B")
    (property "Package" "Package")
    (property "Price" "None")
    (property "STANDARD" "IPC-7351B")
    (property "Sheetfile" "Thermometry_PCB_v2.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/A98055-037/Omnetics/view-part/?ref=snap")
    (property "VERIFIER" "")
    (attr through_hole)
    (fp_text reference "J1" (at -16.7945 -3.6068 90) (layer "F.SilkS"))
    (fp_text value "A98055-037" (at -6.9175 -4.1348 90) (layer "F.Fab"))
    (fp_text user "PCB Edge" (at 19.05 10.795 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at -11.43 0 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 26 "Net-(C8-Pad4)") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.102))
    (pad "2" thru_hole circle locked (at -10.16 0 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 18 "Net-(C8-Pad2)") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.102))
    (pad "3" thru_hole circle locked (at -8.89 0 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 16 "Net-(C7-Pad4)") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.102))
    (pad "4" thru_hole circle locked (at -7.62 0 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 14 "Net-(C7-Pad2)") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.102))
    (pad "5" thru_hole circle locked (at -6.35 0 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 12 "Net-(C6-Pad4)") (pinfunction "5") (pintype "passive") (solder_mask_margin 0.102))
    (pad "6" thru_hole circle locked (at -5.08 0 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 10 "Net-(C6-Pad2)") (pinfunction "6") (pintype "passive") (solder_mask_margin 0.102))
    (pad "7" thru_hole circle locked (at -3.81 0 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 8 "Net-(C5-Pad4)") (pinfunction "7") (pintype "passive") (solder_mask_margin 0.102))
    (pad "8" thru_hole circle locked (at -2.54 0 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 20 "Net-(C5-Pad2)") (pinfunction "8") (pintype "passive") (solder_mask_margin 0.102))
    (pad "9" thru_hole circle locked (at -1.27 0 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 19 "Net-(C5-Pad1)") (pinfunction "9") (pintype "passive") (solder_mask_margin 0.102))
    (pad "10" thru_hole circle locked (at 0 0 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 5 "unconnected-(J1-Pad10)") (pinfunction "10") (pintype "passive") (solder_mask_margin 0.102))
    (pad "11" thru_hole circle locked (at 1.27 0 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad3)") (pinfunction "11") (pintype "passive") (solder_mask_margin 0.102))
    (pad "12" thru_hole circle locked (at 2.54 0 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 17 "Net-(C1-Pad4)") (pinfunction "12") (pintype "passive") (solder_mask_margin 0.102))
    (pad "13" thru_hole circle locked (at 3.81 0 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 24 "Net-(C1-Pad2)") (pinfunction "13") (pintype "passive") (solder_mask_margin 0.102))
    (pad "14" thru_hole circle locked (at 5.08 0 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 30 "Net-(C2-Pad4)") (pinfunction "14") (pintype "passive") (solder_mask_margin 0.102))
    (pad "15" thru_hole circle locked (at 6.35 0 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 28 "Net-(C2-Pad2)") (pinfunction "15") (pintype "passive") (solder_mask_margin 0.102))
    (pad "16" thru_hole circle locked (at 7.62 0 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 34 "Net-(C3-Pad4)") (pinfunction "16") (pintype "passive") (solder_mask_margin 0.102))
    (pad "17" thru_hole circle locked (at 8.89 0 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 32 "Net-(C3-Pad2)") (pinfunction "17") (pintype "passive") (solder_mask_margin 0.102))
    (pad "18" thru_hole circle locked (at 10.16 0 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 38 "Net-(C4-Pad4)") (pinfunction "18") (pintype "passive") (solder_mask_margin 0.102))
    (pad "19" thru_hole circle locked (at 11.43 0 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 36 "Net-(C4-Pad2)") (pinfunction "19") (pintype "passive") (solder_mask_margin 0.102))
    (pad "20" thru_hole circle locked (at -10.795 1.27 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 25 "Net-(C8-Pad3)") (pinfunction "20") (pintype "passive") (solder_mask_margin 0.102))
    (pad "21" thru_hole circle locked (at -9.525 1.27 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 21 "Net-(C8-Pad1)") (pinfunction "21") (pintype "passive") (solder_mask_margin 0.102))
    (pad "22" thru_hole circle locked (at -8.255 1.27 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 15 "Net-(C7-Pad3)") (pinfunction "22") (pintype "passive") (solder_mask_margin 0.102))
    (pad "23" thru_hole circle locked (at -6.985 1.27 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 13 "Net-(C7-Pad1)") (pinfunction "23") (pintype "passive") (solder_mask_margin 0.102))
    (pad "24" thru_hole circle locked (at -5.715 1.27 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 11 "Net-(C6-Pad3)") (pinfunction "24") (pintype "passive") (solder_mask_margin 0.102))
    (pad "25" thru_hole circle locked (at -4.445 1.27 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 9 "Net-(C6-Pad1)") (pinfunction "25") (pintype "passive") (solder_mask_margin 0.102))
    (pad "26" thru_hole circle locked (at -3.175 1.27 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 7 "Net-(C5-Pad3)") (pinfunction "26") (pintype "passive") (solder_mask_margin 0.102))
    (pad "27" thru_hole circle locked (at -1.905 1.27 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 22 "unconnected-(J1-Pad27)") (pinfunction "27") (pintype "passive") (solder_mask_margin 0.102))
    (pad "28" thru_hole circle locked (at -0.635 1.27 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 2 "unconnected-(J1-Pad28)") (pinfunction "28") (pintype "passive") (solder_mask_margin 0.102))
    (pad "29" thru_hole circle locked (at 0.635 1.27 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 3 "unconnected-(J1-Pad29)") (pinfunction "29") (pintype "passive") (solder_mask_margin 0.102))
    (pad "30" thru_hole circle locked (at 1.905 1.27 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 4 "unconnected-(J1-Pad30)") (pinfunction "30") (pintype "passive") (solder_mask_margin 0.102))
    (pad "31" thru_hole circle locked (at 3.175 1.27 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 23 "Net-(C1-Pad1)") (pinfunction "31") (pintype "passive") (solder_mask_margin 0.102))
    (pad "32" thru_hole circle locked (at 4.445 1.27 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 29 "Net-(C2-Pad3)") (pinfunction "32") (pintype "passive") (solder_mask_margin 0.102))
    (pad "33" thru_hole circle locked (at 5.715 1.27 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 27 "Net-(C2-Pad1)") (pinfunction "33") (pintype "passive") (solder_mask_margin 0.102))
    (pad "34" thru_hole circle locked (at 6.985 1.27 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 33 "Net-(C3-Pad3)") (pinfunction "34") (pintype "passive") (solder_mask_margin 0.102))
    (pad "35" thru_hole circle locked (at 8.255 1.27 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 31 "Net-(C3-Pad1)") (pinfunction "35") (pintype "passive") (solder_mask_margin 0.102))
    (pad "36" thru_hole circle locked (at 9.525 1.27 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 37 "Net-(C4-Pad3)") (pinfunction "36") (pintype "passive") (solder_mask_margin 0.102))
    (pad "37" thru_hole circle locked (at 10.795 1.27 90) (size 1.1176 1.1176) (drill 0.7112) (layers *.Cu *.Mask)
      (net 35 "Net-(C4-Pad1)") (pinfunction "37") (pintype "passive") (solder_mask_margin 0.102))
    (pad "SH1" thru_hole circle locked (at -16.0655 0 90) (size 3.3528 3.3528) (drill 2.3368) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "SHIELD") (pintype "passive") (solder_mask_margin 0.102))
    (pad "SH2" thru_hole circle locked (at 16.0655 0 90) (size 3.3528 3.3528) (drill 2.3368) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "SHIELD") (pintype "passive") (solder_mask_margin 0.102))
  )
  (footprint "MountingHole:MountingHole_6.5mm_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 183.769 97.663)
    (descr "Mounting Hole 6.5mm")
    (tags "mounting hole 6.5mm")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "MOUNT" (at 0 -7.5) (layer "F.SilkS"))
    (fp_text value "MountingHole_6.5mm_Pad" (at 0 7.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 13 13) (drill 6.5) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_6.5mm_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 210.82 97.79)
    (descr "Mounting Hole 6.5mm")
    (tags "mounting hole 6.5mm")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "MOUNT" (at 0 -7.5) (layer "F.SilkS"))
    (fp_text value "MountingHole_6.5mm_Pad" (at 0 7.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 13 13) (drill 6.5) (layers F&B.Cu *.Mask))
  )
  (footprint "Glenair_Connectors:171-006-6P-.110-BL" (layer "F.Cu")
    (tedit 0)
    (at 179.705 115.286 180)
    (property "Sheetfile" "Thermometry_PCB_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C5" (at -1.27 -6.35 180 unlocked) (layer "F.SilkS"))
    (fp_text value "171-006-6P-.110-BL" (at 0 -2.54 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.04 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 19 "Net-(C5-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -1.27 2.54 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 20 "Net-(C5-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -2.54 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 "Net-(C5-Pad3)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at -3.81 2.54 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 "Net-(C5-Pad4)") (pinfunction "4") (pintype "passive"))
  )
  (footprint "Glenair_Connectors:171-006-6P-.110-BL" (layer "F.Cu")
    (tedit 0)
    (at 222.25 79.659)
    (property "Sheetfile" "Thermometry_PCB_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C4" (at -1.27 -6.35 unlocked) (layer "F.SilkS"))
    (fp_text value "171-006-6P-.110-BL" (at 0 -2.54 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.04 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 35 "Net-(C4-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -1.27 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 36 "Net-(C4-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -2.54 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 37 "Net-(C4-Pad3)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at -3.81 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 38 "Net-(C4-Pad4)") (pinfunction "4") (pintype "passive"))
  )
  (footprint "Glenair_Connectors:171-006-6P-.110-BL" (layer "F.Cu")
    (tedit 0)
    (at 218.44 115.286 180)
    (property "Sheetfile" "Thermometry_PCB_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C8" (at -1.27 -6.35 180 unlocked) (layer "F.SilkS"))
    (fp_text value "171-006-6P-.110-BL" (at 0 -2.54 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.04 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 21 "Net-(C8-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -1.27 2.54 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 18 "Net-(C8-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -2.54 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 25 "Net-(C8-Pad3)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at -3.81 2.54 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 26 "Net-(C8-Pad4)") (pinfunction "4") (pintype "passive"))
  )
  (footprint "Glenair_Connectors:171-006-6P-.110-BL" (layer "F.Cu")
    (tedit 0)
    (at 208.915 79.659)
    (property "Sheetfile" "Thermometry_PCB_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C3" (at -1.27 -6.35 unlocked) (layer "F.SilkS"))
    (fp_text value "171-006-6P-.110-BL" (at 0 -2.54 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.04 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 "Net-(C3-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -1.27 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 32 "Net-(C3-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -2.54 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 "Net-(C3-Pad3)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at -3.81 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 34 "Net-(C3-Pad4)") (pinfunction "4") (pintype "passive"))
  )
  (footprint "Glenair_Connectors:171-006-6P-.110-BL" (layer "F.Cu")
    (tedit 0)
    (at 195.58 79.659)
    (property "Sheetfile" "Thermometry_PCB_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C2" (at -1.27 -6.35 unlocked) (layer "F.SilkS"))
    (fp_text value "171-006-6P-.110-BL" (at 0 -2.54 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.04 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 27 "Net-(C2-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -1.27 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 "Net-(C2-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -2.54 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 29 "Net-(C2-Pad3)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at -3.81 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 30 "Net-(C2-Pad4)") (pinfunction "4") (pintype "passive"))
  )
  (footprint "Glenair_Connectors:171-006-6P-.110-BL" (layer "F.Cu")
    (tedit 0)
    (at 205.105 115.286 180)
    (property "Sheetfile" "Thermometry_PCB_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C7" (at -1.27 -6.35 180 unlocked) (layer "F.SilkS"))
    (fp_text value "171-006-6P-.110-BL" (at 0 -2.54 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.04 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 "Net-(C7-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -1.27 2.54 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 "Net-(C7-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -2.54 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 15 "Net-(C7-Pad3)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at -3.81 2.54 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 16 "Net-(C7-Pad4)") (pinfunction "4") (pintype "passive"))
  )
  (footprint "Glenair_Connectors:171-006-6P-.110-BL" (layer "F.Cu")
    (tedit 0)
    (at 191.77 115.286 180)
    (property "Sheetfile" "Thermometry_PCB_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C6" (at -1.27 -6.35 180 unlocked) (layer "F.SilkS"))
    (fp_text value "171-006-6P-.110-BL" (at 0 -2.54 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.04 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 "Net-(C6-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -1.27 2.54 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 "Net-(C6-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -2.54 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 "Net-(C6-Pad3)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at -3.81 2.54 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 "Net-(C6-Pad4)") (pinfunction "4") (pintype "passive"))
  )
  (footprint "Glenair_Connectors:171-006-6P-.110-BL" (layer "F.Cu")
    (tedit 0)
    (at 182.245 79.659)
    (property "Sheetfile" "Thermometry_PCB_v2.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C1" (at -1.27 -6.35 unlocked) (layer "F.SilkS"))
    (fp_text value "171-006-6P-.110-BL" (at 0 -2.54 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.04 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 "Net-(C1-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -1.27 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 24 "Net-(C1-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -2.54 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(C1-Pad3)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at -3.81 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 17 "Net-(C1-Pad4)") (pinfunction "4") (pintype "passive"))
  )
  (gr_rect locked (start 241.3 69.215) (end 172.72 125.73) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "Taj Dyson\n9-17-2025\nSLAC National Accelerator Laboratory" (at 197.485 105.41) (layer "F.SilkS"))
  (zone locked (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 240.665 125.095)
        (xy 173.355 125.095)
        (xy 173.355 69.85)
        (xy 240.665 69.85)
      )
    )
  )
)
