(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 107)
    (no_connects 0)
    (area 117.314567 71.1505 159.5247 123.540501)
    (thickness 1.6)
    (drawings 26)
    (tracks 346)
    (zones 0)
    (modules 70)
    (nets 46)
  )
  (page A)
  (title_block
    (title "Triple Bypass")
    (date 2018-08-07)
    (rev 0.3)
    (company "db Electronics")
    (comment 1 https://github.com/db-electronics/triple-bypass-kicad)
    (comment 2 "Licensed under CERN OHL v.1.2")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1778)
    (trace_clearance 0.1778)
    (zone_clearance 0.3048)
    (zone_45_only no)
    (trace_min 0.1778)
    (segment_width 0.2)
    (edge_width 0.2032)
    (via_size 0.6096)
    (via_drill 0.3048)
    (via_min_size 0.6096)
    (via_min_drill 0.3048)
    (uvia_size 0.6096)
    (uvia_drill 0.3048)
    (uvias_allowed no)
    (uvia_min_size 0.6096)
    (uvia_min_drill 0.3048)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 125.095 117.602)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/0.3))
  )
  (net 0 "")
  (net 1 /SYNC-75)
  (net 2 "Net-(C101-Pad1)")
  (net 3 "Net-(C102-Pad1)")
  (net 4 "Net-(C103-Pad2)")
  (net 5 "Net-(C104-Pad2)")
  (net 6 "Net-(C105-Pad2)")
  (net 7 "Net-(C106-Pad2)")
  (net 8 "Net-(C107-Pad2)")
  (net 9 "Net-(C108-Pad2)")
  (net 10 "Net-(C109-Pad1)")
  (net 11 GND)
  (net 12 "Net-(C110-Pad2)")
  (net 13 "Net-(C111-Pad1)")
  (net 14 "Net-(C111-Pad2)")
  (net 15 "Net-(C112-Pad1)")
  (net 16 "Net-(C112-Pad2)")
  (net 17 "Net-(C113-Pad1)")
  (net 18 /SR)
  (net 19 "Net-(C114-Pad1)")
  (net 20 /SL)
  (net 21 +5V)
  (net 22 /SYNC-OUT)
  (net 23 "Net-(CON101-Pad6)")
  (net 24 "Net-(J101-Pad2)")
  (net 25 /SYNC-TTL)
  (net 26 "Net-(R103-Pad1)")
  (net 27 "Net-(R104-Pad1)")
  (net 28 "Net-(R105-Pad1)")
  (net 29 "Net-(R106-Pad1)")
  (net 30 "Net-(R112-Pad2)")
  (net 31 "Net-(U101-Pad7)")
  (net 32 "Net-(U101-Pad8)")
  (net 33 /B-In)
  (net 34 /YM-Left)
  (net 35 /SCD-Left)
  (net 36 /32X-Left)
  (net 37 /PSG)
  (net 38 /32X-Right)
  (net 39 /SCD-Right)
  (net 40 /YM-Right)
  (net 41 /R-Out)
  (net 42 /G-Out)
  (net 43 /B-Out)
  (net 44 /G-In)
  (net 45 /R-In)
  (net_class Default "This is the default net class."
    (clearance 0.1778)
    (trace_width 0.1778)
    (via_dia 0.6096)
    (via_drill 0.3048)
    (uvia_dia 0.6096)
    (uvia_drill 0.3048)
    (add_net /32X-Left)
    (add_net /32X-Right)
    (add_net /B-In)
    (add_net /B-Out)
    (add_net /G-In)
    (add_net /G-Out)
    (add_net /PSG)
    (add_net /R-In)
    (add_net /R-Out)
    (add_net /SCD-Left)
    (add_net /SCD-Right)
    (add_net /SL)
    (add_net /SR)
    (add_net /SYNC-75)
    (add_net /SYNC-OUT)
    (add_net /SYNC-TTL)
    (add_net /YM-Left)
    (add_net /YM-Right)
    (add_net "Net-(C101-Pad1)")
    (add_net "Net-(C102-Pad1)")
    (add_net "Net-(C103-Pad2)")
    (add_net "Net-(C104-Pad2)")
    (add_net "Net-(C105-Pad2)")
    (add_net "Net-(C106-Pad2)")
    (add_net "Net-(C107-Pad2)")
    (add_net "Net-(C108-Pad2)")
    (add_net "Net-(C109-Pad1)")
    (add_net "Net-(C110-Pad2)")
    (add_net "Net-(C111-Pad1)")
    (add_net "Net-(C111-Pad2)")
    (add_net "Net-(C112-Pad1)")
    (add_net "Net-(C112-Pad2)")
    (add_net "Net-(C113-Pad1)")
    (add_net "Net-(C114-Pad1)")
    (add_net "Net-(CON101-Pad6)")
    (add_net "Net-(J101-Pad2)")
    (add_net "Net-(R103-Pad1)")
    (add_net "Net-(R104-Pad1)")
    (add_net "Net-(R105-Pad1)")
    (add_net "Net-(R106-Pad1)")
    (add_net "Net-(R112-Pad2)")
    (add_net "Net-(U101-Pad7)")
    (add_net "Net-(U101-Pad8)")
  )
  (net_class Power ""
    (clearance 0.1778)
    (trace_width 0.254)
    (via_dia 0.6096)
    (via_drill 0.3048)
    (uvia_dia 0.6096)
    (uvia_drill 0.3048)
    (add_net +5V)
    (add_net GND)
  )
  (module db-smt:TSSOP-14 (layer F.Cu) (tedit 5B61BE66)
    (at 150.495 98.933 90)
    (solder_mask_margin 0.1)
    (fp_text reference U101 (at 2.921 2.159 180) (layer F.SilkS))
    (fp_text value THS7374IPWR (at 2.4 -2.7 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 90) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R106-Pad1)"))
    (pad 2 smd rect (at 0 0.65 90) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R103-Pad1)"))
    (pad 3 smd rect (at 0 1.3 90) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R104-Pad1)"))
    (pad 4 smd rect (at 0 1.95 90) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R105-Pad1)"))
    (pad 5 smd rect (at 0 2.6 90) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 6 smd rect (at 0 3.25 90) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 7 smd rect (at 0 3.9 90) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U101-Pad7)"))
    (pad 8 smd rect (at 6 3.9 90) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U101-Pad8)"))
    (pad 9 smd rect (at 6 3.25 90) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J101-Pad2)"))
    (pad 10 smd rect (at 6 2.6 90) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 21 +5V))
    (pad 11 smd rect (at 6 1.95 90) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 43 /B-Out))
    (pad 12 smd rect (at 6 1.3 90) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 42 /G-Out))
    (pad 13 smd rect (at 6 0.65 90) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 41 /R-Out))
    (pad 14 smd rect (at 6 0 90) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R112-Pad2)"))
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B619BFB)
    (at 155.3845 105.283 90)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference R109 (at 3.302 -0.0508 90) (layer F.SilkS))
    (fp_text value 1.00k (at 0.508 -2.54 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 2 smd rect (at 0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R105-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:TP50 (layer F.Cu) (tedit 5B61A578)
    (at 155.448 115.951)
    (solder_mask_margin 0.1016)
    (fp_text reference B1 (at 0 -1.397) (layer F.SilkS) hide)
    (fp_text value TP_50 (at 0 -3.25) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1.27 1.27) (layers F.Cu F.Paste F.Mask)
      (net 33 /B-In))
  )
  (module db-smt:SMD-6.6x6.6 (layer F.Cu) (tedit 5A6BE195)
    (at 142.4305 90.551 270)
    (solder_mask_margin 0.1016)
    (fp_text reference C101 (at -1.143 2.794 540) (layer F.SilkS))
    (fp_text value 220uF/10V (at 4.064 -5.334 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 0 0 270) (size 3.7 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 /SYNC-75))
    (pad 1 smd rect (at 5.8 0 270) (size 3.7 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C101-Pad1)"))
  )
  (module db-smt:0805 (layer F.Cu) (tedit 5B61BB87)
    (at 140.97 110.998 270)
    (tags 0805)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference C102 (at -2.286 0 270) (layer F.SilkS))
    (fp_text value 10uF/10V (at 1.016 -2.54 270) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 270) (size 1.016 1.27) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C102-Pad1)"))
    (pad 2 smd rect (at 2.159 0 270) (size 1.016 1.27) (layers F.Cu F.Paste F.Mask)
      (net 34 /YM-Left))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B61BB4E)
    (at 143.891 111.887 90)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference C103 (at 3.175 0 90) (layer F.SilkS))
    (fp_text value 1uF/16V (at 0.508 -2.54 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 35 /SCD-Left))
    (pad 2 smd rect (at 0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C103-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B61BB1F)
    (at 146.685 111.887 90)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference C104 (at 3.175 0 90) (layer F.SilkS))
    (fp_text value 1uF/16V (at 0.508 -2.54 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 36 /32X-Left))
    (pad 2 smd rect (at 0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C104-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B61BBBB)
    (at 138.049 111.887 90)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference C105 (at 3.175 0 90) (layer F.SilkS))
    (fp_text value 1uF/16V (at 0.508 -2.54 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 37 /PSG))
    (pad 2 smd rect (at 0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C105-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B61BBBD)
    (at 136.652 111.887 90)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference C106 (at 3.175 0 90) (layer F.SilkS))
    (fp_text value 1uF/16V (at 0.508 -2.54 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 37 /PSG))
    (pad 2 smd rect (at 0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C106-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B61BBC8)
    (at 133.858 111.887 90)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference C107 (at 3.175 0 90) (layer F.SilkS))
    (fp_text value 1uF/16V (at 0.508 -2.54 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 38 /32X-Right))
    (pad 2 smd rect (at 0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C107-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B61BBEC)
    (at 131.064 111.887 90)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference C108 (at 3.175 0 90) (layer F.SilkS))
    (fp_text value 1uF/16V (at 0.508 -2.54 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 39 /SCD-Right))
    (pad 2 smd rect (at 0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C108-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0805 (layer F.Cu) (tedit 5B61BC41)
    (at 128.143 110.998 270)
    (tags 0805)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference C109 (at -2.286 0 270) (layer F.SilkS))
    (fp_text value 10uF/10V (at 1.016 -2.54 270) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 270) (size 1.016 1.27) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C109-Pad1)"))
    (pad 2 smd rect (at 2.159 0 270) (size 1.016 1.27) (layers F.Cu F.Paste F.Mask)
      (net 40 /YM-Right))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0805 (layer F.Cu) (tedit 5AA1DFC6)
    (at 133.35 99.695)
    (tags 0805)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference C110 (at -2.286 0.127) (layer F.SilkS))
    (fp_text value 10uF/10V (at 1.016 -2.54) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1.016 1.27) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 2 smd rect (at 2.159 0) (size 1.016 1.27) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C110-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5AA6C7C1)
    (at 140.081 101.4095)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference C111 (at 3.175 0) (layer F.SilkS))
    (fp_text value 270pF/50V (at 0.508 -2.54) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C111-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C111-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5AA6C7C1)
    (at 128.651 97.917 90)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference C112 (at 3.175 0 90) (layer F.SilkS))
    (fp_text value 270pF/50V (at 0.508 -2.54 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C112-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C112-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:1206_P (layer F.Cu) (tedit 5B619FDA)
    (at 127.762 90.297)
    (solder_mask_margin 0.1016)
    (fp_text reference C113 (at 0.127 -2.032) (layer F.SilkS))
    (fp_text value 22uF/10V (at 0.8 -3.2) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1.6 1.8) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C113-Pad1)"))
    (pad 2 smd rect (at 2.8 0) (size 1.6 1.8) (layers F.Cu F.Paste F.Mask)
      (net 18 /SR))
  )
  (module db-smt:1206_P (layer F.Cu) (tedit 5B619FE0)
    (at 135.763 90.297 180)
    (solder_mask_margin 0.1016)
    (fp_text reference C114 (at 0 2.032 180) (layer F.SilkS))
    (fp_text value 22uF/10V (at 0.8 -3.2 180) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 1.6 1.8) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C114-Pad1)"))
    (pad 2 smd rect (at 2.8 0 180) (size 1.6 1.8) (layers F.Cu F.Paste F.Mask)
      (net 20 /SL))
  )
  (module db-smt:1206_P (layer F.Cu) (tedit 5B61BEC2)
    (at 148.59 95.631 270)
    (solder_mask_margin 0.1016)
    (fp_text reference C115 (at 5.588 0 450) (layer F.SilkS))
    (fp_text value 22uF/10V (at 0.8 -3.2 270) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 270) (size 1.6 1.8) (layers F.Cu F.Paste F.Mask)
      (net 21 +5V))
    (pad 2 smd rect (at 2.8 0 270) (size 1.6 1.8) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B61BEC5)
    (at 146.558 97.028 270)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference C116 (at 4.191 -0.0635 270) (layer F.SilkS))
    (fp_text value 0.1uF/50V (at 0.508 -2.54 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 270) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 21 +5V))
    (pad 2 smd rect (at 0.95 0 270) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B61BA7C)
    (at 136.271 94.107 180)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference C117 (at 3.175 0 180) (layer F.SilkS))
    (fp_text value 0.1uF/50V (at 0.508 -2.54 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 180) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 21 +5V))
    (pad 2 smd rect (at 0.95 0 180) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:TP50 (layer F.Cu) (tedit 5B61A57C)
    (at 153.289 115.951)
    (solder_mask_margin 0.1016)
    (fp_text reference G1 (at 0 -1.397) (layer F.SilkS) hide)
    (fp_text value TP_50 (at 0 -3.25) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1.27 1.27) (layers F.Cu F.Paste F.Mask)
      (net 44 /G-In))
  )
  (module db-thparts:HDR1X2 (layer F.Cu) (tedit 5B619F9C)
    (at 155.321 88.2015 270)
    (solder_mask_margin 0.1016)
    (fp_text reference J101 (at -0.254 4.572 450) (layer F.SilkS))
    (fp_text value HDR1X2 (at 1.27 -3.302 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 GND) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 0 2.54 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 "Net-(J101-Pad2)") (solder_mask_margin 0.1016))
  )
  (module db-smt:TP50 (layer F.Cu) (tedit 5B61A576)
    (at 151.13 115.951)
    (solder_mask_margin 0.1016)
    (fp_text reference R1 (at 0 -1.397) (layer F.SilkS) hide)
    (fp_text value TP_50 (at 0 -3.25) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1.27 1.27) (layers F.Cu F.Paste F.Mask)
      (net 45 /R-In))
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B610592)
    (at 149.86 111.887 90)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference R102 (at 3.175 0 90) (layer F.SilkS))
    (fp_text value 2.20k (at 0.508 -2.54 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 25 /SYNC-TTL))
    (pad 2 smd rect (at 0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 21 +5V))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B6104BF)
    (at 152.654 111.887 270)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference R103 (at -3.175 0 270) (layer F.SilkS))
    (fp_text value 5.62k (at 0.508 -2.54 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 270) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R103-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 45 /R-In))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B6104D5)
    (at 154.051 111.887 270)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference R104 (at -3.175 0 270) (layer F.SilkS))
    (fp_text value 5.62k (at 0.508 -2.54 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 270) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R104-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 44 /G-In))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B6104E3)
    (at 155.448 111.887 270)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference R105 (at -3.175 0 270) (layer F.SilkS))
    (fp_text value 5.62k (at 0.508 -2.54 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 270) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R105-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 33 /B-In))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B6104F8)
    (at 151.257 111.887 270)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference R106 (at -3.175 0 270) (layer F.SilkS))
    (fp_text value 5.62k (at 0.508 -2.54 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 270) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R106-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 25 /SYNC-TTL))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B619C02)
    (at 151.765 105.283 90)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference R107 (at 3.302 0 90) (layer F.SilkS))
    (fp_text value 1.00k (at 0.508 -2.54 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 2 smd rect (at 0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R103-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B619BED)
    (at 153.543 105.283 90)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference R108 (at 3.2512 0 90) (layer F.SilkS))
    (fp_text value 1.00k (at 0.508 -2.54 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 2 smd rect (at 0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R104-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B619C0F)
    (at 149.86 105.283 90)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference R110 (at 3.302 0.0508 90) (layer F.SilkS))
    (fp_text value 1.00k (at 0.508 -2.54 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 2 smd rect (at 0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R106-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B61BE79)
    (at 154.1145 90.424)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference R111 (at -3.2385 0.0635) (layer F.SilkS))
    (fp_text value 100k (at 0.508 -2.54) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 21 +5V))
    (pad 2 smd rect (at 0.95 0) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J101-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B61BDC5)
    (at 148.336 92.964)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference R112 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 75.0 (at 0.508 -2.54) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C101-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R112-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B61BB85)
    (at 139.446 111.887 90)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference R113 (at 3.175 0 90) (layer F.SilkS))
    (fp_text value 2.20k (at 0.508 -2.54 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 34 /YM-Left))
    (pad 2 smd rect (at 0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B61BB51)
    (at 142.494 111.887 90)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference R114 (at 3.175 0 90) (layer F.SilkS))
    (fp_text value 75.0 (at 0.508 -2.54 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 35 /SCD-Left))
    (pad 2 smd rect (at 0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B61BB1B)
    (at 145.288 111.887 90)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference R115 (at 3.175 0 90) (layer F.SilkS))
    (fp_text value 75.0 (at 0.508 -2.54 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 36 /32X-Left))
    (pad 2 smd rect (at 0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B61BBB9)
    (at 135.255 111.887 90)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference R116 (at 3.175 0 90) (layer F.SilkS))
    (fp_text value 1.30k (at 0.508 -2.54 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 37 /PSG))
    (pad 2 smd rect (at 0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B61BBD6)
    (at 132.461 111.887 90)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference R117 (at 3.175 0 90) (layer F.SilkS))
    (fp_text value 75.0 (at 0.508 -2.54 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 38 /32X-Right))
    (pad 2 smd rect (at 0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B61BBEA)
    (at 129.667 111.887 90)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference R118 (at 3.175 0 90) (layer F.SilkS))
    (fp_text value 75.0 (at 0.508 -2.54 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 39 /SCD-Right))
    (pad 2 smd rect (at 0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B61BC3F)
    (at 126.619 111.887 90)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference R119 (at 3.175 0 90) (layer F.SilkS))
    (fp_text value 2.20k (at 0.508 -2.54 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 40 /YM-Right))
    (pad 2 smd rect (at 0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B61BEFC)
    (at 140.97 105.283 90)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference R120 (at 0.127 -1.27 90) (layer F.SilkS))
    (fp_text value 6.19k (at 0.508 -2.54 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C102-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C111-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B61BEFE)
    (at 143.891 105.283 90)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference R121 (at 0.127 -1.27 90) (layer F.SilkS))
    (fp_text value 130k (at 0.508 -2.54 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C103-Pad2)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C111-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B61BF01)
    (at 146.685 105.283 90)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference R122 (at 0.127 -1.27 90) (layer F.SilkS))
    (fp_text value 130k (at 0.508 -2.54 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C104-Pad2)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C111-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B61BA77)
    (at 138.049 105.283 90)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference R123 (at 3.302 0 90) (layer F.SilkS))
    (fp_text value 100k (at 0.508 -2.54 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C105-Pad2)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C111-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B61BA79)
    (at 136.652 105.283 90)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference R124 (at 3.175 0 90) (layer F.SilkS))
    (fp_text value 100k (at 0.508 -2.54 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C106-Pad2)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C112-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B61BEF8)
    (at 135.255 105.283 90)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference R125 (at 0.127 -1.27 90) (layer F.SilkS))
    (fp_text value 130k (at 0.508 -2.54 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C107-Pad2)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C112-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B61BEF6)
    (at 132.334 105.283 90)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference R126 (at 0.127 -1.27 90) (layer F.SilkS))
    (fp_text value 130k (at 0.508 -2.54 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C108-Pad2)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C112-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B61BEF4)
    (at 129.54 105.283 90)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference R127 (at 0.127 -1.27 90) (layer F.SilkS))
    (fp_text value 6.19k (at 0.508 -2.54 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C109-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C112-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B61A923)
    (at 134.239 102.616)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference R128 (at -3.175 0) (layer F.SilkS))
    (fp_text value 10.0k (at 0.508 -2.54) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 21 +5V))
    (pad 2 smd rect (at 0.95 0) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C110-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B61A921)
    (at 134.239 101.219 180)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference R129 (at 3.175 0 180) (layer F.SilkS))
    (fp_text value 10.0k (at 0.508 -2.54 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 180) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C110-Pad2)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5AA6C7C1)
    (at 140.081 102.8065)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference R130 (at 3.175 0) (layer F.SilkS))
    (fp_text value 162k (at 0.508 -2.54) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C111-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C111-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5AA6C7C1)
    (at 127.127 97.917 90)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference R131 (at 3.175 0.127 90) (layer F.SilkS))
    (fp_text value 162k (at 0.508 -2.54 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C112-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C112-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B619FF8)
    (at 130.81 92.456 180)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference R132 (at 3.175 0 180) (layer F.SilkS))
    (fp_text value 332 (at 0.508 -2.54 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 180) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C112-Pad2)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C113-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B61A001)
    (at 134.366 92.456)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference R133 (at 3.175 0) (layer F.SilkS))
    (fp_text value 332 (at 0.508 -2.54) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C111-Pad2)"))
    (pad 2 smd rect (at 0.95 0) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C114-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-smt:TP50 (layer F.Cu) (tedit 5B61A57E)
    (at 149.0345 115.951)
    (solder_mask_margin 0.1016)
    (fp_text reference S1 (at 0 -1.397) (layer F.SilkS) hide)
    (fp_text value TP_50 (at 0 -3.25) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1.27 1.27) (layers F.Cu F.Paste F.Mask)
      (net 25 /SYNC-TTL))
  )
  (module db-smt:TP50 (layer F.Cu) (tedit 5B61A56B)
    (at 140.843 115.951)
    (solder_mask_margin 0.1016)
    (fp_text reference SL1 (at 0 -1.397) (layer F.SilkS) hide)
    (fp_text value TP_50 (at 0 -3.25) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1.27 1.27) (layers F.Cu F.Paste F.Mask)
      (net 35 /SCD-Left))
  )
  (module db-smt:TP50 (layer F.Cu) (tedit 5B61A561)
    (at 129.921 115.951)
    (solder_mask_margin 0.1016)
    (fp_text reference SR2 (at 0.0635 -1.397) (layer F.SilkS) hide)
    (fp_text value TP_50 (at 0 -3.25) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1.27 1.27) (layers F.Cu F.Paste F.Mask)
      (net 39 /SCD-Right))
  )
  (module db-smt:TP50 (layer F.Cu) (tedit 5B61A566)
    (at 135.382 115.951)
    (solder_mask_margin 0.1016)
    (fp_text reference SN1 (at 0 -1.397) (layer F.SilkS) hide)
    (fp_text value TP_50 (at 0 -3.25) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1.27 1.27) (layers F.Cu F.Paste F.Mask)
      (net 37 /PSG))
  )
  (module db-smt:TSSOP-8_3.0mm (layer F.Cu) (tedit 5A6BE324)
    (at 131.66 96.236)
    (solder_mask_margin 0.1)
    (fp_text reference U102 (at -0.596 -0.986 180) (layer F.SilkS))
    (fp_text value LMV358M8G-13 (at 2.4 -2.7) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C112-Pad2)"))
    (pad 2 smd rect (at 0 0.65) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C112-Pad1)"))
    (pad 3 smd rect (at 0 1.3) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C110-Pad2)"))
    (pad 4 smd rect (at 0 1.95) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 5 smd rect (at 5.5 1.95) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C110-Pad2)"))
    (pad 6 smd rect (at 5.5 1.3) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C111-Pad1)"))
    (pad 7 smd rect (at 5.5 0.65) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C111-Pad2)"))
    (pad 8 smd rect (at 5.5 0) (size 2 0.3) (layers F.Cu F.Paste F.Mask)
      (net 21 +5V))
  )
  (module db-smt:TP50 (layer F.Cu) (tedit 5B61A56E)
    (at 143.51 115.951)
    (solder_mask_margin 0.1016)
    (fp_text reference XL1 (at 0 -1.397) (layer F.SilkS) hide)
    (fp_text value TP_50 (at 0 -3.25) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1.27 1.27) (layers F.Cu F.Paste F.Mask)
      (net 36 /32X-Left))
  )
  (module db-smt:TP50 (layer F.Cu) (tedit 5B61A564)
    (at 132.588 115.951)
    (solder_mask_margin 0.1016)
    (fp_text reference XR2 (at 0.0635 -1.397) (layer F.SilkS) hide)
    (fp_text value TP_50 (at 0 -3.25) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1.27 1.27) (layers F.Cu F.Paste F.Mask)
      (net 38 /32X-Right))
  )
  (module db-smt:TP50 (layer F.Cu) (tedit 5B61A569)
    (at 138.176 115.951)
    (solder_mask_margin 0.1016)
    (fp_text reference YL1 (at 0 -1.397) (layer F.SilkS) hide)
    (fp_text value TP_50 (at 0 -3.25) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1.27 1.27) (layers F.Cu F.Paste F.Mask)
      (net 34 /YM-Left))
  )
  (module db-smt:TP50 (layer F.Cu) (tedit 5B61A55E)
    (at 127.254 115.951)
    (solder_mask_margin 0.1016)
    (fp_text reference YR2 (at 0.0635 -1.397) (layer F.SilkS) hide)
    (fp_text value TP_50 (at 0 -3.25) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1.27 1.27) (layers F.Cu F.Paste F.Mask)
      (net 40 /YM-Right))
  )
  (module db-smt:TP50 (layer F.Cu) (tedit 5B61A589)
    (at 127.254 101.727)
    (solder_mask_margin 0.1016)
    (fp_text reference 0V1 (at 0.25 -1.75) (layer F.SilkS) hide)
    (fp_text value TP_50 (at 0 -3.25) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1.27 1.27) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
  )
  (module db-smt:TP50 (layer F.Cu) (tedit 5B61A573)
    (at 146.304 115.951)
    (solder_mask_margin 0.1016)
    (fp_text reference 5V1 (at 0.127 -1.397) (layer F.SilkS) hide)
    (fp_text value TP_50 (at 0 -3.25) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1.27 1.27) (layers F.Cu F.Paste F.Mask)
      (net 21 +5V))
  )
  (module db-smt:0603 (layer F.Cu) (tedit 5B61BB20)
    (at 148.082 111.887 90)
    (tags 0603)
    (solder_mask_margin 0.1016)
    (attr smd)
    (fp_text reference C100 (at 3.175 0 90) (layer F.SilkS))
    (fp_text value 0.1uF/50V (at 0.508 -2.54 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 21 +5V))
    (pad 2 smd rect (at 0.95 0 90) (size 0.8 1) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module db-artwork:oshw-logo_5mm (layer F.Cu) (tedit 0)
    (at 145.923 81.28)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module db-artwork:db-logo_7.5mm (layer F.Cu) (tedit 0)
    (at 152.654 80.3275)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module db-smt:JMP-PCB-3POS (layer F.Cu) (tedit 5B62F675)
    (at 145.415 88.9)
    (solder_mask_margin 0.1016)
    (fp_text reference J102 (at 0.0635 -1.651 180) (layer F.SilkS))
    (fp_text value JMP-PCB-3POS (at -0.0508 -2.9464) (layer F.Fab) hide)
    (pad 1 smd oval (at -0.8128 0) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 /SYNC-75))
    (pad 2 smd oval (at 0 0) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask)
      (net 22 /SYNC-OUT))
    (pad 3 smd oval (at 0.8128 0) (size 0.635 1.27) (layers F.Cu F.Paste F.Mask)
      (net 25 /SYNC-TTL))
  )
  (module db-thparts:MD-90SM (layer B.Cu) (tedit 5B630365)
    (at 134.493 86.614 180)
    (solder_mask_margin 0.1016)
    (fp_text reference CON101 (at -4.8895 -3.175 180) (layer B.SilkS))
    (fp_text value MD-90SM (at -2.54 -5.08 180) (layer B.Fab) hide)
    (pad 5 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 /SYNC-OUT))
    (pad 8 thru_hole circle (at 2.032 0 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 /SL))
    (pad 9 thru_hole circle (at 4.064 0 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 /SR))
    (pad 4 thru_hole circle (at -2.032 0 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 /SYNC-75))
    (pad 7 thru_hole circle (at -4.064 0 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 41 /R-Out))
    (pad 3 thru_hole circle (at -4.064 2.54 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 42 /G-Out))
    (pad 6 thru_hole circle (at 4.064 2.54 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 "Net-(CON101-Pad6)"))
    (pad 1 thru_hole circle (at -1.27 2.54 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 43 /B-Out))
    (pad 2 thru_hole circle (at 0.762 2.54 180) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 +5V))
    (pad 10 thru_hole circle (at 0 6.096 180) (size 3.048 3.048) (drill 2.286) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 10 thru_hole circle (at 7.239 5.334 180) (size 3.048 3.048) (drill 2.286) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 10 thru_hole circle (at -7.239 5.334 180) (size 3.048 3.048) (drill 2.286) (layers *.Cu *.Mask)
      (net 11 GND))
  )
  (dimension 9.398 (width 0.2032) (layer Dwgs.User)
    (gr_text "0.3700 in" (at 129.794 72.5005) (layer Dwgs.User))
    (feature1 (pts (xy 134.493 78.232) (xy 134.493 71.1505)))
    (feature2 (pts (xy 125.095 78.232) (xy 125.095 71.1505)))
    (crossbar (pts (xy 125.095 73.8505) (xy 134.493 73.8505)))
    (arrow1a (pts (xy 134.493 73.8505) (xy 133.366496 74.436921)))
    (arrow1b (pts (xy 134.493 73.8505) (xy 133.366496 73.264079)))
    (arrow2a (pts (xy 125.095 73.8505) (xy 126.221504 74.436921)))
    (arrow2b (pts (xy 125.095 73.8505) (xy 126.221504 73.264079)))
  )
  (dimension 39.37 (width 0.2032) (layer Dwgs.User)
    (gr_text "1.5500 in" (at 120.697 97.917 270) (layer Dwgs.User))
    (feature1 (pts (xy 125.095 117.602) (xy 119.347 117.602)))
    (feature2 (pts (xy 125.095 78.232) (xy 119.347 78.232)))
    (crossbar (pts (xy 122.047 78.232) (xy 122.047 117.602)))
    (arrow1a (pts (xy 122.047 117.602) (xy 121.460579 116.475496)))
    (arrow1b (pts (xy 122.047 117.602) (xy 122.633421 116.475496)))
    (arrow2a (pts (xy 122.047 78.232) (xy 121.460579 79.358504)))
    (arrow2b (pts (xy 122.047 78.232) (xy 122.633421 79.358504)))
  )
  (dimension 32.004 (width 0.2032) (layer Dwgs.User)
    (gr_text "1.2600 in" (at 141.097 122.1905) (layer Dwgs.User))
    (feature1 (pts (xy 157.099 117.602) (xy 157.099 123.5405)))
    (feature2 (pts (xy 125.095 117.602) (xy 125.095 123.5405)))
    (crossbar (pts (xy 125.095 120.8405) (xy 157.099 120.8405)))
    (arrow1a (pts (xy 157.099 120.8405) (xy 155.972496 121.426921)))
    (arrow1b (pts (xy 157.099 120.8405) (xy 155.972496 120.254079)))
    (arrow2a (pts (xy 125.095 120.8405) (xy 126.221504 121.426921)))
    (arrow2b (pts (xy 125.095 120.8405) (xy 126.221504 120.254079)))
  )
  (gr_text "Licensed under CERN OHL v.1.2" (at 139.5095 111.252) (layer B.SilkS))
  (gr_text "https://github.com/db-eletronics/\ntriple-bypass-kicad" (at 138.303 113.6015) (layer B.SilkS))
  (gr_text "install MD-90SM on\nthis side of PCB" (at 134.8105 92.5195) (layer B.SilkS))
  (gr_text db-electronics.ca (at 150.495 85.4075) (layer F.SilkS))
  (gr_text "triple bypass" (at 152.654 82.6135) (layer F.SilkS))
  (gr_text v0.3 (at 155.067 84.1375) (layer F.SilkS))
  (gr_text GND (at 126.3015 103.759 90) (layer F.SilkS))
  (gr_text YR (at 127.254 114.427) (layer F.SilkS))
  (gr_text CR (at 129.921 114.427) (layer F.SilkS))
  (gr_text XR (at 132.588 114.427) (layer F.SilkS))
  (gr_text PSG (at 135.382 114.427) (layer F.SilkS))
  (gr_text YL (at 138.176 114.427) (layer F.SilkS))
  (gr_text CL (at 140.843 114.427) (layer F.SilkS))
  (gr_text XL (at 143.51 114.427) (layer F.SilkS))
  (gr_text 5V (at 146.304 114.427) (layer F.SilkS))
  (gr_text S (at 149.0345 114.4905) (layer F.SilkS))
  (gr_text B (at 155.448 114.4905) (layer F.SilkS))
  (gr_text G (at 153.2255 114.4905) (layer F.SilkS))
  (gr_text R (at 151.0665 114.4905) (layer F.SilkS))
  (gr_line (start 157.099 78.232) (end 157.099 117.602) (angle 90) (layer Edge.Cuts) (width 0.2032))
  (gr_line (start 125.095 78.232) (end 157.099 78.232) (angle 90) (layer Edge.Cuts) (width 0.2032))
  (gr_line (start 125.095 117.602) (end 125.095 78.232) (angle 90) (layer Edge.Cuts) (width 0.2032))
  (gr_line (start 125.095 117.602) (end 157.099 117.602) (angle 90) (layer Edge.Cuts) (width 0.2032))
  (zone (net 11) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.1778)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 125.603 78.74) (xy 125.603 116.967) (xy 156.464 116.967) (xy 156.464 78.74)
      )
    )
  )
  (zone (net 11) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.1778)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 125.603 78.74) (xy 125.603 116.967) (xy 156.464 116.967) (xy 156.464 78.74)
      )
    )
  )
)
