(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu16.04.1)
  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 54)
    (zones 0)
    (modules 6)
    (nets 4)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.381)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.6 0.3)
    (user_via 0.6 0.4)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /A)
  (net 2 /B)
  (net 3 /C)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /A)
    (add_net /B)
    (add_net /C)
  )
  (module simple_pad:TestPoint_Pad_2.0x2.0mm (layer F.Cu) (tedit 5D1692A9)
    (at 121 95)
    (descr "SMD rectangular pad as test Point, square 2.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference J3 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers F.Cu F.Mask)
      (net 2 /B))
  )
  (module simple_pad:TestPoint_Pad_2.0x2.0mm (layer F.Cu) (tedit 5D1692A4)
    (at 121 92.5)
    (descr "SMD rectangular pad as test Point, square 2.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference J1 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers F.Cu F.Mask)
      (net 1 /A))
  )
  (module simple_pad:TestPoint_Pad_2.0x2.0mm (layer F.Cu) (tedit 5D1692AF)
    (at 132 92.5)
    (descr "SMD rectangular pad as test Point, square 2.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference J2 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers F.Cu F.Mask)
      (net 1 /A))
  )
  (module simple_pad:TestPoint_Pad_2.0x2.0mm (layer F.Cu) (tedit 5D1692B2)
    (at 132 95)
    (descr "SMD rectangular pad as test Point, square 2.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference J4 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers F.Cu F.Mask)
      (net 2 /B))
  )
  (module simple_pad:TestPoint_Pad_2.0x2.0mm (layer F.Cu) (tedit 5D1692AC)
    (at 121 97.5)
    (descr "SMD rectangular pad as test Point, square 2.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference J5 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers F.Cu F.Mask)
      (net 3 /C))
  )
  (module simple_pad:TestPoint_Pad_2.0x2.0mm (layer F.Cu) (tedit 5D1692B4)
    (at 132 97.5)
    (descr "SMD rectangular pad as test Point, square 2.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference J6 (at 0 -1.998) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers F.Cu F.Mask)
      (net 3 /C))
  )
  (gr_line (start 119.5 91) (end 119.5 99) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 133.5 91) (end 119.5 91) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 133.5 99) (end 133.5 91) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 119.5 99) (end 133.5 99) (layer Edge.Cuts) (width 0.2))
  (zone (net 1) (net_name /A) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120 93.5) (xy 133 93.5) (xy 133 91.5) (xy 120 91.5)
      )
    )
  )
  (zone (net 2) (net_name /B) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.75 96) (xy 133 96) (xy 133 94) (xy 119.75 94)
      )
    )
  )
  (zone (net 3) (net_name /C) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120 98.5) (xy 133 98.5) (xy 133 96.5) (xy 120 96.5)
      )
    )
  )
  (zone (net 3) (net_name /C) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120.044966 98.5) (xy 133.044966 98.5) (xy 133.044966 96.5) (xy 120.044966 96.5)
      )
    )
  )
  (zone (net 2) (net_name /B) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120 96) (xy 133 96) (xy 133 94) (xy 120 94)
      )
    )
  )
  (zone (net 1) (net_name /A) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120 93.5) (xy 133 93.5) (xy 133 91.5) (xy 120 91.5)
      )
    )
  )
)
