(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 17)
    (tracks 35)
    (zones 0)
    (modules 21)
    (nets 15)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.3)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.65 1.1)
    (pad_drill 0.7)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 "Net-(D1-Pad2)")
  (net 3 "Net-(D2-Pad1)")
  (net 4 "Net-(D3-Pad1)")
  (net 5 "Net-(D4-Pad1)")
  (net 6 "Net-(D2-Pad2)")
  (net 7 "Net-(D3-Pad2)")
  (net 8 "Net-(D4-Pad2)")
  (net 9 "Net-(J1-Pad3)")
  (net 10 "Net-(J1-Pad4)")
  (net 11 "Net-(J1-Pad2)")
  (net 12 "Net-(J1-PadSH)")
  (net 13 GND)
  (net 14 +5V)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-PadSH)")
  )
  (module digikey-footprints:USB_Mini_B_Female_548190519 (layer F.Cu) (tedit 5E34ABA2)
    (at 103.5685 62.5475)
    (fp_text reference J1 (at -3.65 -5.325) (layer F.SilkS))
    (fp_text value 0548190519 (at -4.2 6.35) (layer F.Fab))
    (fp_text user %R (at -5.7 -0.075) (layer F.Fab))
    (pad SH thru_hole oval (at -5.05 3.65) (size 2.7 1.7) (drill oval 1.9 0.7) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-PadSH)"))
    (pad SH thru_hole oval (at -5.05 -3.65) (size 2.7 1.7) (drill oval 1.9 0.7) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-PadSH)"))
    (pad 2 thru_hole oval (at -1.2 0.8) (size 1.65 1.1) (drill 0.7 (offset -0.275 0)) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad2)"))
    (pad 4 thru_hole oval (at -1.2 -0.8) (size 1.65 1.1) (drill 0.7 (offset -0.275 0)) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad4)"))
    (pad 1 thru_hole oval (at 0 1.6) (size 1.65 1.1) (drill 0.7 (offset 0.275 0)) (layers *.Cu *.Mask)
      (net 14 +5V))
    (pad 5 thru_hole oval (at 0 -1.6) (size 1.65 1.1) (drill 0.7 (offset 0.275 0)) (layers *.Cu *.Mask)
      (net 13 GND))
    (pad 3 thru_hole oval (at 0 0) (size 1.65 1.1) (drill 0.7 (offset 0.275 0)) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad3)"))
  )
  (module LogoLibrary:HugeVLogo1.0 (layer B.Cu) (tedit 0)
    (at 107.188 66.294 180)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module LogoLibrary:HugeVLogo1.0 (layer F.Cu) (tedit 0)
    (at 80.518 65.532)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via (layer F.Cu) (tedit 56DDB9C7)
    (at 96.7486 40.8178)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference " " (at 0 -3.81) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2_Pad_Via (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via (layer F.Cu) (tedit 56DDB9C7)
    (at 96.773 86.106)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference " " (at 0 -3.81) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2_Pad_Via (at -0.38 3.048) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via (layer F.Cu) (tedit 56DDB9C7)
    (at 183.8706 104.4448)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference " " (at 0 -3.81) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2_Pad_Via (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via (layer F.Cu) (tedit 56DDB9C7)
    (at 218.82 104.521)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference " " (at 0 -3.81) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2_Pad_Via (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.2mm_M2_Pad_Via (layer F.Cu) (tedit 56DDB9C7)
    (at 218.821 40.8178)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (attr virtual)
    (fp_text reference " " (at 0 -3.81) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2_Pad_Via (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 -1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.166726 -1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 1.65) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.166726 1.166726) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.65 0) (size 0.7 0.7) (drill 0.4) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module "" (layer F.Cu) (tedit 0)
    (at 106.045 66.675)
    (fp_text reference "" (at 121.79 63.5) (layer F.SilkS))
    (fp_text value "" (at 121.79 63.5) (layer F.SilkS))
  )
  (module LED_SMD:LED_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 121.663 60.96 180)
    (descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D1 (at 0 -1.82) (layer F.SilkS))
    (fp_text value LED (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 121.793 65.913 180)
    (descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D2 (at 0 -1.82) (layer F.SilkS))
    (fp_text value LED (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 6 "Net-(D2-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 121.92 76.2 180)
    (descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D4 (at 0 -1.82) (layer F.SilkS))
    (fp_text value LED (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 5 "Net-(D4-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 8 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 121.796 71.12 180)
    (descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D3 (at 0 -1.82) (layer F.SilkS))
    (fp_text value LED (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 7 "Net-(D3-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 4 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CustomLibrary:SL_70541_3 (layer F.Cu) (tedit 0)
    (at 212.852 48.514 90)
    (descr "<b>Vertical Header w/ Latch & Pegs</b>\n\n<p>With Split Pegs:</p>\n<ul>\n<li> 70541-0002 </li>\n<li> 70541-0037 </li>\n<li> 70541-0072 </li>\n</ul>\n<p>With Tri-Pegs:</p>\n<ul>\n<li> 70545-0002 </li>\n<li> 70545-0037 </li>\n<li> 70545-0072 </li>\n<li> 70545-0142 </li>\n<li> 70545-0177 </li>\n</ul>")
    (fp_text reference J4 (at -0.889 -4.445 90) (layer F.SilkS))
    (fp_text value Conn_01x03 (at -5.08 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.54 -1.27 270) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 GND) (solder_mask_margin 0.0508))
    (pad 2 thru_hole circle (at 0 -1.27 90) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 GND) (solder_mask_margin 0.0508))
    (pad 3 thru_hole circle (at 2.54 -1.27 90) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 GND) (solder_mask_margin 0.0508))
    (pad "" np_thru_hole circle (at -6.604 -0.508 90) (size 3.4036 3.4036) (drill 3.4036) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 6.604 -0.508 90) (size 3.4036 3.4036) (drill 3.4036) (layers *.Cu *.Mask))
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 113.919 60.96 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R_Small (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 14 +5V))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 114.046 65.913 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R_Small (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 6 "Net-(D2-Pad2)"))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 14 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 114.3 71.12 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R_Small (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 14 +5V))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 7 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 114.3 76.2 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 -1.82) (layer F.SilkS))
    (fp_text value R_Small (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 8 "Net-(D4-Pad2)"))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 14 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CustomLibrary:SL_70541_4 (layer F.Cu) (tedit 0)
    (at 212.725 68.961 90)
    (descr "<b>Vertical Header w/ Latch & Pegs</b>\n\n<p>With Split Pegs:</p>\n<ul>\n<li> 70541-0003 </li>\n<li> 70541-0038 </li>\n<li> 70541-0073 </li>\n</ul>\n<p>With Tri-Pegs:</p>\n<ul>\n<li> 70545-0003 </li>\n<li> 70545-0038 </li>\n<li> 70545-0073 </li>\n<li> 70545-0143 </li>\n<li> 70545-0178 </li>\n</ul>")
    (fp_text reference J3 (at 2.54 -4.572 90) (layer F.SilkS))
    (fp_text value Conn_01x04 (at -6.35 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -3.81 -1.27 270) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 GND) (solder_mask_margin 0.0508))
    (pad 2 thru_hole circle (at -1.27 -1.27 90) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 GND) (solder_mask_margin 0.0508))
    (pad 3 thru_hole circle (at 1.27 -1.27 90) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 GND) (solder_mask_margin 0.0508))
    (pad 4 thru_hole circle (at 3.81 -1.27 90) (size 1.9304 1.9304) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 GND) (solder_mask_margin 0.0508))
    (pad "" np_thru_hole circle (at -7.874 -0.508 90) (size 3.4036 3.4036) (drill 3.4036) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.874 -0.508 90) (size 3.4036 3.4036) (drill 3.4036) (layers *.Cu *.Mask))
  )
  (module TerminalBlock_RND:TerminalBlock_RND_205-00289_1x04_P5.08mm_Horizontal (layer F.Cu) (tedit 5B294ED0)
    (at 134.112 60.833 270)
    (descr "terminal block RND 205-00289, 4 pins, pitch 5.08mm, size 20.3x10.6mm^2, drill diamater 1.3mm, pad diameter 2.5mm, see http://cdn-reichelt.de/documents/datenblatt/C151/RND_205-00287_DB_EN.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_RND")
    (tags "THT terminal block RND 205-00289 pitch 5.08mm size 20.3x10.6mm^2 drill 1.3mm pad 2.5mm")
    (fp_text reference J2 (at 7.493 -6.858 90) (layer F.SilkS))
    (fp_text value DIN-4 (at 7.62 6.36 90) (layer F.Fab))
    (fp_text user %R (at 7.62 -6.36 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 3 thru_hole circle (at 10.16 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 4 thru_hole circle (at 15.24 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/TerminalBlock_RND.3dshapes/TerminalBlock_RND_205-00289_1x04_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_RND:TerminalBlock_RND_205-00288_1x03_P5.08mm_Horizontal (layer F.Cu) (tedit 5B294ECF)
    (at 133.985 44.196 270)
    (descr "terminal block RND 205-00288, 3 pins, pitch 5.08mm, size 15.2x10.6mm^2, drill diamater 1.3mm, pad diameter 2.5mm, see http://cdn-reichelt.de/documents/datenblatt/C151/RND_205-00287_DB_EN.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_RND")
    (tags "THT terminal block RND 205-00288 pitch 5.08mm size 15.2x10.6mm^2 drill 1.3mm pad 2.5mm")
    (fp_text reference J5 (at 5.588 -7.239 90) (layer F.SilkS))
    (fp_text value DIN-3 (at 5.08 6.36 90) (layer F.Fab))
    (fp_text user %R (at 5.08 -6.36 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 3 thru_hole circle (at 10.16 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/TerminalBlock_RND.3dshapes/TerminalBlock_RND_205-00288_1x03_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text G (at 117.983 39.878) (layer F.SilkS))
  (gr_text 5V (at 102.489 40.005) (layer F.SilkS))
  (gr_text G (at 100.965 86.868) (layer B.SilkS))
  (gr_text G (at 219.71 86.995) (layer F.SilkS))
  (gr_arc (start 179.705 90.17) (end 180.975 90.17) (angle -90) (layer Edge.Cuts) (width 0.12))
  (gr_arc (start 182.245 106.045) (end 180.975 106.045) (angle -90) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 180.975 106.045) (end 180.975 90.17) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 220.345 107.315) (end 182.245 107.315) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 221.615 87.63) (end 221.615 106.045) (layer Edge.Cuts) (width 0.12))
  (gr_arc (start 95.25 87.63) (end 93.98 87.63) (angle -90) (layer Edge.Cuts) (width 0.12))
  (gr_arc (start 95.25 39.37) (end 95.25 38.1) (angle -90) (layer Edge.Cuts) (width 0.12))
  (gr_arc (start 220.345 39.37) (end 221.615 39.37) (angle -90) (layer Edge.Cuts) (width 0.12))
  (gr_arc (start 220.345 106.045) (end 220.345 107.315) (angle -90) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 220.345 38.1) (end 95.25 38.1) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 221.615 87.63) (end 221.615 39.37) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 95.25 88.9) (end 179.705 88.9) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 93.98 39.37) (end 93.98 87.63) (layer Edge.Cuts) (width 0.12))
  (zone (net 13) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 220.98 39.37) (xy 220.98 87.63) (xy 220.345 88.265) (xy 95.25 88.265) (xy 94.615 87.63)
        (xy 94.615 39.37) (xy 95.123 38.735) (xy 220.287491 38.735)
      )
    )
  )
  (zone (net 14) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.919 39.37) (xy 113.919 87.884) (xy 113.411 88.265) (xy 95.25 88.265) (xy 94.615 87.63)
        (xy 94.615 39.37) (xy 95.123 38.735) (xy 112.688221 38.735)
      )
    )
  )
  (zone (net 13) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 220.98 39.37) (xy 220.98 87.63) (xy 220.345 88.265) (xy 115.1255 88.265) (xy 114.808 87.9475)
        (xy 114.808 78.74) (xy 114.808 39.37) (xy 115.443 38.735) (xy 220.345 38.735)
      )
    )
  )
)
