<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="30.48" y2="0" width="0.4064" layer="20"/>
<wire x1="30.48" y1="0" x2="30.48" y2="43.18" width="0.4064" layer="20"/>
<wire x1="30.48" y1="43.18" x2="0" y2="43.18" width="0.4064" layer="20"/>
<wire x1="0" y1="43.18" x2="0" y2="0" width="0.4064" layer="20"/>
<hole x="2.54" y="40.64" drill="1.5748"/>
<hole x="2.54" y="2.54" drill="1.5748"/>
<hole x="27.94" y="2.54" drill="1.5748"/>
<hole x="27.94" y="40.64" drill="1.5748"/>
<text>V001</text>
<text>Vtarget</text>
<text>Owl Valley
Breakout Board
JTAG Adapter
J5 pins are reversed!</text>
<text>GND</text>
<text>1</text>
<text>1</text>
</plain>
<libraries>
<library name="SilverButte">
<packages>
<package name="TPAD37">
</package>
<package name="2X5-SHROUDED">
</package>
<package name="2X10-SHROUDED">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J3" library="SilverButte" package="2X10-SHROUDED" value="2x10 JTAG">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="TP2" library="SilverButte" package="TPAD37" value="VTARGET">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="TP4" library="SilverButte" package="TPAD37" value="GND">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="SilverButte" package="2X5-SHROUDED" value="2x5 JTAG">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="TDI">
<contactref element="J3" pad="5"/>
<contactref element="J5" pad="7"/>
</signal>
<signal name="TMS">
<contactref element="J3" pad="7"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="TCK">
<contactref element="J3" pad="9"/>
<contactref element="J5" pad="3"/>
</signal>
<signal name="TRST_N">
<contactref element="J3" pad="3"/>
<contactref element="J5" pad="8"/>
</signal>
<signal name="TDO">
<contactref element="J3" pad="13"/>
<contactref element="J5" pad="5"/>
</signal>
<signal name="GND">
<contactref element="J3" pad="4"/>
<contactref element="J3" pad="6"/>
<contactref element="J3" pad="8"/>
<contactref element="J3" pad="10"/>
<contactref element="J3" pad="12"/>
<contactref element="J3" pad="14"/>
<contactref element="J3" pad="16"/>
<contactref element="J3" pad="18"/>
<contactref element="J3" pad="20"/>
<contactref element="TP4" pad="TP"/>
<contactref element="J5" pad="4"/>
<contactref element="J5" pad="6"/>
<contactref element="J5" pad="10"/>
</signal>
<signal name="SECURE">
<contactref element="J3" pad="11"/>
</signal>
<signal name="TXD">
<contactref element="J3" pad="19"/>
</signal>
<signal name="RXD">
<contactref element="J3" pad="17"/>
</signal>
<signal name="VTARGET">
<contactref element="J3" pad="1"/>
<contactref element="J3" pad="2"/>
<contactref element="TP2" pad="TP"/>
<contactref element="J5" pad="2"/>
</signal>
<signal name="N_RESET">
<contactref element="J3" pad="15"/>
<contactref element="J5" pad="9"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
