(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~61~ubuntu18.04.1)
  (general
    (links 50)
    (no_connects 0)
    (area 121.336999 66.980999 175.335001 103.707001)
    (thickness 1.6)
    (drawings 20)
    (tracks 92)
    (zones 0)
    (modules 24)
    (nets 22)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /Red_A)
  (net 2 "Net-(C1-Pad2)")
  (net 3 /Green_A)
  (net 4 "Net-(C2-Pad2)")
  (net 5 /Blue_A)
  (net 6 "Net-(C3-Pad2)")
  (net 7 /Sync_A)
  (net 8 "Net-(C4-Pad2)")
  (net 9 /Sync)
  (net 10 GND)
  (net 11 /Blanking)
  (net 12 /Audio_R)
  (net 13 /Audio_L)
  (net 14 /Red)
  (net 15 /Green)
  (net 16 /Blue)
  (net 17 /Audio_R_EXT)
  (net 18 /Audio_L_EXT)
  (net 19 /Audio_Mono)
  (net 20 /Audio_L_INT)
  (net 21 /Audio_R_INT)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /Audio_L)
    (add_net /Audio_L_EXT)
    (add_net /Audio_L_INT)
    (add_net /Audio_Mono)
    (add_net /Audio_R)
    (add_net /Audio_R_EXT)
    (add_net /Audio_R_INT)
    (add_net /Blanking)
    (add_net /Blue)
    (add_net /Blue_A)
    (add_net /Green)
    (add_net /Green_A)
    (add_net /Red)
    (add_net /Red_A)
    (add_net /Sync)
    (add_net /Sync_A)
    (add_net GND)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad2)")
  )
  (module eswitch-dpdt:eswitch-dpdt-m2 (layer F.Cu) (tedit 5C7C028F)
    (at 173.101 71.501 270)
    (fp_text reference SW1 (at 7.62 9.3345 360) (layer F.SilkS))
    (fp_text value SW_DPDT_x2 (at 2.55 -2.8 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.5 2.5) (drill 1.85) (layers *.Cu *.Mask)
      (net 21 /Audio_R_INT))
    (pad 4 thru_hole circle (at 4.83 0 270) (size 2.5 2.5) (drill 1.85) (layers *.Cu *.Mask)
      (net 20 /Audio_L_INT))
    (pad 2 thru_hole circle (at 0 4.7 270) (size 2.5 2.5) (drill 1.85) (layers *.Cu *.Mask)
      (net 12 /Audio_R))
    (pad 5 thru_hole circle (at 4.83 4.7 270) (size 2.5 2.5) (drill 1.85) (layers *.Cu *.Mask)
      (net 13 /Audio_L))
    (pad 3 thru_hole circle (at 0 9.4 270) (size 2.5 2.5) (drill 1.85) (layers *.Cu *.Mask)
      (net 17 /Audio_R_EXT))
    (pad 6 thru_hole circle (at 4.83 9.4 270) (size 2.5 2.5) (drill 1.85) (layers *.Cu *.Mask)
      (net 18 /Audio_L_EXT))
  )
  (module k-scartx-024:K-SCARTX-024 (layer F.Cu) (tedit 5C7BF0A9)
    (at 148.75 86.25)
    (fp_text reference J1 (at -25.6235 -4.9065) (layer F.SilkS))
    (fp_text value SCART-F (at -26.035 2.54 90) (layer F.Fab))
    (pad "" np_thru_hole oval (at -22.86 2.54) (size 2 4.8) (drill oval 2 4.8) (layers *.Cu *.SilkS *.Mask Dwgs.User Eco1.User Eco2.User))
    (pad 20 thru_hole circle (at -17.145 0) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 9 /Sync))
    (pad 18 thru_hole circle (at -13.335 0) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 10 GND))
    (pad 16 thru_hole circle (at -9.525 0) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 11 /Blanking))
    (pad 14 thru_hole circle (at -5.715 0) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
    (pad 12 thru_hole circle (at -1.905 0) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
    (pad 10 thru_hole circle (at 1.905 0) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole circle (at 5.715 0) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole circle (at 9.525 0) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 13 /Audio_L))
    (pad 4 thru_hole circle (at 13.335 0) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 10 GND))
    (pad 2 thru_hole circle (at 17.145 0) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 12 /Audio_R))
    (pad 21 thru_hole circle (at -19.04 5.08) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 10 GND))
    (pad 19 thru_hole circle (at -15.23 5.08) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
    (pad 17 thru_hole circle (at -11.42 5.08) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 10 GND))
    (pad 15 thru_hole circle (at -7.61 5.08) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 14 /Red))
    (pad 13 thru_hole circle (at -3.8 5.08) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 10 GND))
    (pad 11 thru_hole circle (at 0.01 5.08) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 15 /Green))
    (pad 9 thru_hole circle (at 3.82 5.08) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 10 GND))
    (pad 7 thru_hole circle (at 7.63 5.08) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 16 /Blue))
    (pad 5 thru_hole circle (at 11.44 5.08) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 10 GND))
    (pad 3 thru_hole circle (at 15.25 5.08) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at 19.06 5.08) (size 2.2 2.2) (drill 1.3) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole oval (at 22.86 2.54) (size 2 4.8) (drill oval 2 4.8) (layers *.Cu *.Mask))
    (model /home/martin/k-scartx-024.wrl
      (at (xyz -0.01 -0.1 0.2))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x10_Pitch2.54mm (layer F.Cu) (tedit 5C7BF22A)
    (at 159.1945 98.9965 270)
    (descr "Through hole angled pin header, 1x10, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x10 2.54mm single row")
    (fp_text reference J4 (at 2.921 -2.4765 270) (layer F.SilkS))
    (fp_text value Conn_01x10 (at 4.385 25.13 270) (layer F.Fab))
    (fp_text user %R (at 2.77 11.43 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /Audio_Mono))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /Audio_L_INT))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /Audio_R_INT))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /Blanking))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /Sync_A))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /Blue_A))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Green_A))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /Red_A))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_1x10_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5C7C0383)
    (at 138.3665 94.4245)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 1.5875) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.5) (layer B.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 /Red_A))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5C7C038E)
    (at 145.9865 94.4245)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 1.5875) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.5) (layer B.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 /Green_A))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5C7C0395)
    (at 153.6065 94.4245)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 1.5875) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.5) (layer B.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 5 /Blue_A))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5C7BFB51)
    (at 132.461 96.9645 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at -2.794 -0.0635 360) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.5 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 7 /Sync_A))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module rca:RCJ-02 (layer F.Cu) (tedit 5C7C029A)
    (at 134.9375 70.231)
    (fp_text reference J2 (at 5.0165 -1.5875) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at -4.15 -2.25) (layer F.Fab))
    (pad 2 thru_hole circle (at -5.15 1.6) (size 3 3) (drill 2) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 2 thru_hole circle (at 5.15 1.6) (size 3 3) (drill 2) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.7) (layers *.Cu *.Mask)
      (net 17 /Audio_R_EXT))
    (model /home/martin/rca-02x.wrl
      (at (xyz 0 -0.06 0.1))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module rca:RCJ-02 (layer F.Cu) (tedit 5C7C0141)
    (at 154.432 70.231)
    (fp_text reference J3 (at -5.207 -1.397) (layer F.SilkS))
    (fp_text value Conn_Coaxial (at -4.15 -2.25) (layer F.Fab))
    (pad 2 thru_hole circle (at -5.15 1.6) (size 3 3) (drill 2) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 2 thru_hole circle (at 5.15 1.6) (size 3 3) (drill 2) (layers *.Cu *.Mask)
      (net 10 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.7) (layers *.Cu *.Mask)
      (net 18 /Audio_L_EXT))
    (model /home/martin/rca-02x.wrl
      (at (xyz 0 -0.06 0.1))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5C7BF0EB)
    (at 141.1605 94.361 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 2.4765 0 450) (layer B.SilkS))
    (fp_text value 30R (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 14 /Red))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5C7BF0F6)
    (at 148.7805 94.361 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 2.4765 -0.0635 450) (layer B.SilkS))
    (fp_text value 30R (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 15 /Green))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5C7BF103)
    (at 156.4005 94.488 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 2.4765 -0.0635 450) (layer B.SilkS))
    (fp_text value 30R (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 16 /Blue))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5C7BFB90)
    (at 131.6355 94.361 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at -0.762 1.5875 270) (layer B.SilkS))
    (fp_text value 30R (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 9 /Sync))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5C7BFB2A)
    (at 133.6675 94.361 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at -0.762 -1.651 270) (layer B.SilkS))
    (fp_text value 75R (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5C7BF107)
    (at 158.369 94.488 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 2.4765 0 450) (layer B.SilkS))
    (fp_text value 75R (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5C7BF0FB)
    (at 150.749 94.361 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 2.4765 0 450) (layer B.SilkS))
    (fp_text value 75R (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5C7BF0F1)
    (at 143.129 94.361 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 2.4765 0 450) (layer B.SilkS))
    (fp_text value 75R (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5C7BF093)
    (at 171.704 82.296 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 2.4765 0 270) (layer B.SilkS))
    (fp_text value 470R (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 20 /Audio_L_INT))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 19 /Audio_Mono))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5C7BF08A)
    (at 169.7355 82.296 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 2.921 0 270) (layer B.SilkS))
    (fp_text value 470R (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 21 /Audio_R_INT))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 19 /Audio_Mono))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5C7BF09D)
    (at 173.6725 82.296 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 2.921 -0.0635 270) (layer B.SilkS))
    (fp_text value 20K (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 10 GND))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 19 /Audio_Mono))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 5C7BFC2F)
    (at 171.7675 100.2665)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference J5 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 3.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 10 GND))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 5C7BFC1F)
    (at 124.841 100.203)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference J6 (at 3.1115 2.4765) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 3.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 10 GND))
  )
  (module Connectors:GS2 (layer B.Cu) (tedit 586134A1)
    (at 129.413 96.3295 180)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference JP1 (at 1.78 0 450) (layer B.SilkS))
    (fp_text value Jumper (at -1.8 0 450) (layer B.Fab))
    (pad 1 smd rect (at 0 0.64 180) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 9 /Sync))
    (pad 2 smd rect (at 0 -0.64 180) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 7 /Sync_A))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 5C7C0119)
    (at 124.841 70.4215)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference J7 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0 3.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask)
      (net 10 GND))
  )
  (gr_line (start 121.412 69.088) (end 121.412 67.056) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.26 69.088) (end 175.26 67.056) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "RGB SCART BREAKOUT\nMartin Hejnfelt (martin@hejnfelt.com)" (at 144.399 80.137) (layer B.SilkS))
  (gr_text RED (at 136.3345 101.854 90) (layer B.SilkS))
  (gr_text GREEN (at 138.938 101.727 90) (layer B.SilkS))
  (gr_text BLUE (at 141.4145 101.7905 90) (layer B.SilkS))
  (gr_text SYNC (at 143.9545 101.727 90) (layer B.SilkS))
  (gr_text GND (at 146.558 101.6635 90) (layer B.SilkS))
  (gr_text BLANK (at 149.098 101.727 90) (layer B.SilkS))
  (gr_text MONO (at 159.258 101.727 90) (layer B.SilkS))
  (gr_text GND (at 154.1145 101.7905 90) (layer B.SilkS))
  (gr_text RIGHT (at 151.5745 101.727 90) (layer B.SilkS))
  (gr_text LEFT (at 156.6545 101.727 90) (layer B.SilkS))
  (gr_text RIGHT (at 135.001 74.422) (layer B.SilkS))
  (gr_text LEFT (at 154.6225 74.422) (layer B.SilkS))
  (gr_line (start 121.412 103.632) (end 121.92 103.632) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.412 69.088) (end 121.412 103.632) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.26 67.056) (end 121.412 67.056) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.26 103.632) (end 175.26 69.088) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.92 103.632) (end 175.26 103.632) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 10) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.133 103.505) (xy 121.539 103.505) (xy 121.539 67.183) (xy 175.133 67.183)
      )
    )
  )
  (zone (net 10) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.133 103.505) (xy 121.539 103.505) (xy 121.539 67.183) (xy 175.133 67.183)
      )
    )
  )
)
