(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 89)
    (no_connects 0)
    (area 124.24918 56.4436 179.995999 119.171001)
    (thickness 0.8128)
    (drawings 14)
    (tracks 223)
    (zones 0)
    (modules 33)
    (nets 14)
  )
  (page A4)
  (layers
    (0 F.Cu jumper)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.25)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 0.69 0.4)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.6 0.6)
    (pad_drill 0.3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 152.146 85.471)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory board/))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 "Net-(C1-Pad1)")
  (net 4 "Net-(C11-Pad2)")
  (net 5 /SWDIO)
  (net 6 /SWCLK)
  (net 7 /SWO)
  (net 8 /~RESET)
  (net 9 /SDA)
  (net 10 /SCL)
  (net 11 /~SEN_ENABLE)
  (net 12 /RAD_ENABLE)
  (net 13 /RAD_INT)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +3V3)
    (add_net /RAD_ENABLE)
    (add_net /RAD_INT)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /SWCLK)
    (add_net /SWDIO)
    (add_net /SWO)
    (add_net /~RESET)
    (add_net /~SEN_ENABLE)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C11-Pad2)")
  )
  (module sensor-node:via-0.6mm (layer F.Cu) (tedit 58F4F190)
    (at 158.046 96.671)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value via-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module sensor-node:via-0.6mm (layer F.Cu) (tedit 58F4F190)
    (at 154.946 91.471)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value via-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module sensor-node:via-0.6mm (layer F.Cu) (tedit 58F4F190)
    (at 154.146 106.971)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value via-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module sensor-node:via-0.6mm (layer F.Cu) (tedit 58F4F190)
    (at 145.146 104.471)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value via-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module sensor-node:via-0.6mm (layer F.Cu) (tedit 58F4F190)
    (at 148.146 105.471)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value via-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module sensor-node:CORTEX-DEBUG-EDGE (layer F.Cu) (tedit 58890AA3)
    (at 155.106 110.071)
    (fp_text reference CD1 (at 2.44 -2.7) (layer F.SilkS))
    (fp_text value CortexDebug (at 1.778 -2.54) (layer F.Fab))
    (pad 2 smd rect (at 0 0) (size 0.6 3) (layers F.Cu F.Paste F.Mask)
      (net 5 /SWDIO))
    (pad 4 smd rect (at 1.27 0) (size 0.6 3) (layers F.Cu F.Paste F.Mask)
      (net 6 /SWCLK))
    (pad 6 smd rect (at 2.54 0) (size 0.6 3) (layers F.Cu F.Paste F.Mask)
      (net 7 /SWO))
    (pad 8 smd rect (at 3.81 0) (size 0.6 3) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 5.08 0) (size 0.6 3) (layers F.Cu F.Paste F.Mask)
      (net 8 /~RESET))
    (pad 1 smd rect (at 0 0) (size 0.6 3) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 3 smd rect (at 1.27 0) (size 0.6 3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2.54 0) (size 0.6 3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 3.81 0) (size 0.6 3) (layers B.Cu B.Paste B.Mask))
    (pad 9 smd rect (at 5.08 0) (size 0.6 3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model ../../../../../home/hannes/Repository/sensor-node/freecad/shroudedHeader.wrl
      (at (xyz -0.15 -0.065 -0.12))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz -90 0 0))
    )
  )
  (module sensor-node:Si7021BA (layer F.Cu) (tedit 5894D2A2)
    (at 163.046 97.191 90)
    (fp_text reference SBA1 (at -5.98 3.3 90) (layer F.SilkS))
    (fp_text value Si7021-BA (at 0 -5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -5.08 0 90) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at -2.54 0 90) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 0 0 90) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 /~SEN_ENABLE))
    (pad 4 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 /SCL))
    (pad 5 thru_hole circle (at 5.08 0 90) (size 1.8 1.8) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 /SDA))
    (model ../../../../../home/hannes/Repository/sensor-node/freecad/si7021_breakout.wrl
      (at (xyz 0.2 -0.05 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Housings_QFP:TQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 54130A77)
    (at 152.4 100.33 270)
    (descr "48 LEAD TQFP 7x7mm (see MICREL TQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference EFM1 (at 0.041 -0.046 450) (layer F.SilkS))
    (fp_text value EFM32ZG222 (at 0 6 270) (layer F.Fab))
    (pad 1 smd rect (at -4.35 -2.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /SDA))
    (pad 2 smd rect (at -4.35 -2.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 10 /SCL))
    (pad 3 smd rect (at -4.35 -1.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -4.35 -1.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 5 smd rect (at -4.35 -0.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -4.35 -0.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -4.35 0.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -4.35 0.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at -4.35 1.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at -4.35 1.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at -4.35 2.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at -4.35 2.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at -2.75 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at -2.25 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at -1.75 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at -1.25 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 /~RESET))
    (pad 17 smd rect (at -0.75 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at -0.25 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 19 smd rect (at 0.25 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 20 smd rect (at 0.75 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 1.25 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 1.75 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 23 smd rect (at 2.25 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 24 smd rect (at 2.75 4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 25 smd rect (at 4.35 2.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 26 smd rect (at 4.35 2.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 27 smd rect (at 4.35 1.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 28 smd rect (at 4.35 1.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 29 smd rect (at 4.35 0.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C11-Pad2)"))
    (pad 30 smd rect (at 4.35 0.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 31 smd rect (at 4.35 -0.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 32 smd rect (at 4.35 -0.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 33 smd rect (at 4.35 -1.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 34 smd rect (at 4.35 -1.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 35 smd rect (at 4.35 -2.25 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 36 smd rect (at 4.35 -2.75 270) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 37 smd rect (at 2.75 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 /SWCLK))
    (pad 38 smd rect (at 2.25 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 /SWDIO))
    (pad 39 smd rect (at 1.75 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /SWO))
    (pad 40 smd rect (at 1.25 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 41 smd rect (at 0.75 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 42 smd rect (at 0.25 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 43 smd rect (at -0.25 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 44 smd rect (at -0.75 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 45 smd rect (at -1.25 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 46 smd rect (at -1.75 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /~SEN_ENABLE))
    (pad 47 smd rect (at -2.25 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 /RAD_INT))
    (pad 48 smd rect (at -2.75 -4.35) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 /RAD_ENABLE))
    (model Housings_QFP.3dshapes/TQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:MSOP-10_3x3mm_Pitch0.5mm (layer F.Cu) (tedit 54130A77)
    (at 152.4 90.271 270)
    (descr "10-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.5")
    (attr smd)
    (fp_text reference S1 (at 0 -0.046 450) (layer F.SilkS))
    (fp_text value Si4012 (at 0 2.6 270) (layer F.Fab))
    (pad 1 smd rect (at -2.2 -1 270) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -2.2 -0.5 270) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -2.2 0 270) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (pad 4 smd rect (at -2.2 0.5 270) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (pad 5 smd rect (at -2.2 1 270) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 6 smd rect (at 2.2 1 270) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 2.2 0.5 270) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 13 /RAD_INT))
    (pad 8 smd rect (at 2.2 0 270) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 /RAD_ENABLE))
    (pad 9 smd rect (at 2.2 -0.5 270) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /SCL))
    (pad 10 smd rect (at 2.2 -1 270) (size 1.4 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 /SDA))
    (model Housings_SSOP.3dshapes/MSOP-10_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 541A9B8D)
    (at 152.146 59.471)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 2.1) (layer B.SilkS))
    (fp_text value 1pF (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 158.446 88.371 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 3.35 1.1 180) (layer F.SilkS))
    (fp_text value 0.5pF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 147.896 88.071 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 4 -0.15 180) (layer F.SilkS))
    (fp_text value 1µF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 147.896 93.571 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 4 0.1 180) (layer F.SilkS))
    (fp_text value 0.1µF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 147.896 90.871 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 4 -0.1 180) (layer F.SilkS))
    (fp_text value 10µF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 159.946 99.721 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at -2.75 1.5 450) (layer F.SilkS))
    (fp_text value 0.1µF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 144.165 97.282 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 3.769 0.311 180) (layer F.SilkS))
    (fp_text value 10nF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 143.51 100.076 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 3.614 0.127 180) (layer F.SilkS))
    (fp_text value 0.1µF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 143.617 102.87 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 3.471 -0.101 180) (layer F.SilkS))
    (fp_text value 10nF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 141.605 105.664 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at -0.381 -1.807 180) (layer F.SilkS))
    (fp_text value 10µF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 151.896 108.721 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at 1.541 2.562 180) (layer F.SilkS))
    (fp_text value 1µF (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C11-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 147.554 107.315 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at 0.208 1.744 180) (layer F.SilkS))
    (fp_text value 0.1µF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 147.446 109.971 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C13 (at 4.701 0.065 180) (layer F.SilkS))
    (fp_text value 10µF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 152.146 59.471 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C14 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value 1pF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 157.746 93.519 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -1.248 1.9 270) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 /SDA))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 160.346 94.171 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -3.25 -0.05 360) (layer F.SilkS))
    (fp_text value 10k (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /SCL))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 163.696 88.371 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference L1 (at -2.2 -1.6 180) (layer F.SilkS))
    (fp_text value 220nH (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module sensor-node:HU2032-LF (layer B.Cu) (tedit 58891075)
    (at 165.746 98.501 180)
    (fp_text reference BT1 (at 13.208 0 180) (layer B.SilkS))
    (fp_text value CR2032Holder (at 13.208 1.524 180) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 1.27 180) (size 1.524 1.524) (drill 0.94) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 1 thru_hole circle (at 0 -1.27 180) (size 1.524 1.524) (drill 0.94) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 27.2 0 180) (size 1.524 1.524) (drill 0.94) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ../../../../../home/hannes/Repository/sensor-node/freecad/batteryHolder.wrl
      (at (xyz 0.535 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 159.746 104.821 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C15 (at -0.65 1.8 90) (layer F.SilkS))
    (fp_text value 10µF (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module sensor-node-main:frequ (layer F.Cu) (tedit 0)
    (at 152.146 82.971)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module sensor-node-main:logo (layer F.Cu) (tedit 0)
    (at 152.146 70.471)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module sensor-node:mounting (layer F.Cu) (tedit 58F4EB22)
    (at 140.146 88.471)
    (zone_connect 2)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value mounting (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 1.778 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 1.27 -1.27) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 -1.778) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at -1.27 -1.27) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at -1.778 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at -1.27 1.27) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 1.778) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 1.27 1.27) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module sensor-node:mounting (layer F.Cu) (tedit 58F4EC68)
    (at 164.146 108.471)
    (zone_connect 2)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value mounting (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.4) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 1.778 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 1.27 -1.27) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 -1.778) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at -1.27 -1.27) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at -1.778 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at -1.27 1.27) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 1.778) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 1.27 1.27) (size 0.5 0.5) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module sensor-node:via-0.6mm (layer F.Cu) (tedit 58F4F190)
    (at 153.146 102.471)
    (fp_text reference REF** (at 0 1) (layer F.SilkS) hide)
    (fp_text value via-0.6mm (at 0 -1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (gr_text "www.hochreiner.net\nsensor node\nV1.0.1" (at 152.096 70.471) (layer B.SilkS))
  (dimension 25 (width 0.3) (layer F.SilkS)
    (gr_text "25.000 mm" (at 130.749179 98.816981 270) (layer F.SilkS))
    (feature1 (pts (xy 135.099179 111.316981) (xy 129.399179 111.316981)))
    (feature2 (pts (xy 135.099179 86.316981) (xy 129.399179 86.316981)))
    (crossbar (pts (xy 132.099179 86.316981) (xy 132.099179 111.316981)))
    (arrow1a (pts (xy 132.099179 111.316981) (xy 131.512758 110.190477)))
    (arrow1b (pts (xy 132.099179 111.316981) (xy 132.6856 110.190477)))
    (arrow2a (pts (xy 132.099179 86.316981) (xy 131.512758 87.443485)))
    (arrow2b (pts (xy 132.099179 86.316981) (xy 132.6856 87.443485)))
  )
  (dimension 30 (width 0.3) (layer F.SilkS)
    (gr_text "30.000 mm" (at 152.146 117.821) (layer F.SilkS))
    (feature1 (pts (xy 137.146 113.471) (xy 137.146 119.171)))
    (feature2 (pts (xy 167.146 113.471) (xy 167.146 119.171)))
    (crossbar (pts (xy 167.146 116.471) (xy 137.146 116.471)))
    (arrow1a (pts (xy 137.146 116.471) (xy 138.272504 115.884579)))
    (arrow1b (pts (xy 137.146 116.471) (xy 138.272504 117.057421)))
    (arrow2a (pts (xy 167.146 116.471) (xy 166.019496 115.884579)))
    (arrow2b (pts (xy 167.146 116.471) (xy 166.019496 117.057421)))
  )
  (dimension 54 (width 0.3) (layer F.SilkS)
    (gr_text "54.000 mm" (at 173.495999 84.471 270) (layer F.SilkS))
    (feature1 (pts (xy 169.146 111.471) (xy 174.845999 111.471)))
    (feature2 (pts (xy 169.146 57.471) (xy 174.845999 57.471)))
    (crossbar (pts (xy 172.145999 57.471) (xy 172.145999 111.471)))
    (arrow1a (pts (xy 172.145999 111.471) (xy 171.559578 110.344496)))
    (arrow1b (pts (xy 172.145999 111.471) (xy 172.73242 110.344496)))
    (arrow2a (pts (xy 172.145999 57.471) (xy 171.559578 58.597504)))
    (arrow2b (pts (xy 172.145999 57.471) (xy 172.73242 58.597504)))
  )
  (gr_arc (start 139.146 59.471) (end 137.146 59.471) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 165.146 59.471) (end 165.146 57.471) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 165.146 109.471) (end 167.146 109.471) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 139.146 109.471) (end 139.146 111.471) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 165.146 111.471) (end 139.146 111.471) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.146 57.471) (end 165.146 57.471) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.146 109.471) (end 137.146 59.471) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.146 59.471) (end 167.146 109.471) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.146 111.471) (xy 167.146 111.471) (xy 167.146 86.471) (xy 137.146 86.471)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.146 86.471) (xy 167.146 86.471) (xy 167.146 111.471) (xy 137.146 111.471)
      )
    )
  )
)
