(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "USLetter")
  (title_block
    (title "Spectrum Analyzer: VCO and 1st Mixer")
    (date "2022-08-21")
    (rev "0")
    (company "Andy McCann KA3KAF and Doug McCann KA3KAG")
    (comment 2 "Wes Hayward W7ZOI")
    (comment 3 "Original Design by:")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (grid_origin 93.687635 126.212551)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "Net-(C101-Pad2)")
  (net 3 "Net-(C102-Pad2)")
  (net 4 "Net-(C104-Pad1)")
  (net 5 "Net-(C104-Pad2)")
  (net 6 "Net-(C105-Pad2)")
  (net 7 "Net-(C106-Pad1)")
  (net 8 "Net-(C106-Pad2)")
  (net 9 "Net-(C107-Pad1)")
  (net 10 "Net-(C107-Pad2)")
  (net 11 "Net-(C108-Pad2)")
  (net 12 "Net-(C109-Pad2)")
  (net 13 "Net-(C110-Pad1)")
  (net 14 "Net-(C110-Pad2)")
  (net 15 "Net-(J101-Pad1)")
  (net 16 "Net-(J103-Pad1)")
  (net 17 "Net-(J104-Pad1)")
  (net 18 "Net-(JP101-Pad2)")
  (net 19 "Net-(L101-Pad1)")
  (net 20 "Net-(L102-Pad1)")
  (net 21 "Net-(R101-Pad2)")
  (net 22 "Net-(J105-Pad1)")
  (net 23 "Net-(R106-Pad2)")
  (footprint "vco-1stmixer:TUF-1H" (layer "F.Cu")
    (tedit 0)
    (at 170.5256 110.4646 90)
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U104" (at 4.24 1.66 90 unlocked) (layer "F.SilkS"))
    (fp_text value "TUF-1H+" (at 3.79 3.01 90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -1.52 -0.54 90 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 4.25 1.63 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(R101-Pad2)") (pinfunction "RF") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(J104-Pad1)") (pinfunction "IF") (pintype "passive"))
    (pad "3" thru_hole circle (at 5.08 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "4" thru_hole circle (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(JP101-Pad2)") (pinfunction "LO") (pintype "passive"))
    (model "${KIPRJMOD}/vco-1stmixer-models/vco-1stmixer-3D/TUF-1H.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/2ndmixer-2ndlo-models/2ndmixer-2ndlo-3D/Body002.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 147.5356 119.1006)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (attr exclude_from_pos_files)
    (fp_text reference "TP103" (at 0 -1.448) (layer "F.SilkS"))
    (fp_text value "MAV-11A Out" (at 0 1.55) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 7 "Net-(C106-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 152.8696 93.9546)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R113" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "47" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C109-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(J105-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 178.5236 83.7946)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "H102" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 178.5236 121.8946)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "H101" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 100.5456 94.2086)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R102" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "150" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C101-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(J105-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 97.7516 84.0486)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "H103" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_THT:CP_Radial_D8.0mm_P3.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 105.1736 86.5886)
    (descr "CP, Radial series, Radial, pin pitch=3.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 3.50mm  diameter 8mm Electrolytic Capacitor")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C103" (at 1.652651 -5.08) (layer "F.SilkS"))
    (fp_text value "100u" (at 1.75 5.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.75 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C101-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P3.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 152.3616 107.1626)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (attr exclude_from_pos_files)
    (fp_text reference "TP106" (at 0 -1.448) (layer "F.SilkS"))
    (fp_text value "TUF1H Out" (at 0 1.55) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 21 "Net-(R101-Pad2)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 148.8056 95.2246 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R108" (at 3.81 0 90) (layer "F.SilkS"))
    (fp_text value "36" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(R106-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C107-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 158.2036 105.3846 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R111" (at 3.81 0 90) (layer "F.SilkS"))
    (fp_text value "33" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C105-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C108-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 154.9016 116.5606)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R112" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "22" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C108-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(J105-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_THT:L_Toroid_Vertical_L13.0mm_W6.5mm_P5.60mm" (layer "F.Cu")
    (tedit 5AE59B06)
    (at 163.7916 80.4926)
    (descr "L_Toroid, Vertical series, Radial, pin pitch=5.60mm, , length*width=13*6.5mm^2")
    (tags "L_Toroid Vertical series Radial pin pitch 5.60mm  length 13mm width 6.5mm")
    (property "Field4" "T37-6")
    (property "Field5" "10T #30")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "L102" (at 0 2.54) (layer "F.SilkS"))
    (fp_text value ".3u" (at 0 8.15) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.8 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 20 "Net-(L102-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 5.6) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 14 "Net-(C110-Pad2)") (pintype "passive"))
    (model "${KIPRJMOD}/vco-1stmixer-models/vco-1stmixer-3D/T37-6 IND004.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/vco-1stmixer-models/vco-1stmixer-3D/T37-6 IND004.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "vco-1stmixer:691103110002" (layer "F.Cu")
    (tedit 62DE8117)
    (at 123.1516 83.7946)
    (descr "<b>WR-TBL Serie 1031 - 3.50 mm Horiz. Entry Modular<br></b>Max Height = 8.4mm , Pitch 3.5mm , 2 Pins")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Model" "Conn_01x02")
    (property "Spice_Netlist_Enabled" "N")
    (property "Spice_Primitive" "J")
    (attr through_hole)
    (fp_text reference "J105" (at 0 -2.54) (layer "F.SilkS"))
    (fp_text value "Conn_01x02" (at 4.12 4.865) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at -1.75 0) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 22 "Net-(J105-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 1.75 0) (size 1.8 1.8) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KIPRJMOD}/vco-1stmixer-models/vco-1stmixer-3D/691103110002_1.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/vco-1stmixer-models/vco-1stmixer-3D/691103110002_1.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 172.9356 86.0406 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C110" (at 2.5 -0.254 90) (layer "F.SilkS"))
    (fp_text value ".001u" (at 2.5 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C110-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(C110-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 137.4156 89.3826)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C109" (at 2.5 0) (layer "F.SilkS"))
    (fp_text value ".001u" (at 2.5 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C109-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 148.0436 89.3826)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R116" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "220" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(L102-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C109-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 142.2016 95.2246 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R106" (at 3.81 0 90) (layer "F.SilkS"))
    (fp_text value "150" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(R106-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 136.1056 115.7986)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C107" (at 2.540035 0) (layer "F.SilkS"))
    (fp_text value ".01u" (at 2.5 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C107-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C107-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 126.1996 106.4406 -90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C104" (at 2.5 0 90) (layer "F.SilkS"))
    (fp_text value ".001u" (at 2.5 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C104-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C104-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 130.2636 91.9226 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R109" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "220" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(L101-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C105-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 111.7216 97.7646)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R104" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "150" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C104-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 100.7996 97.5106 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R101" (at 3.81 0 90) (layer "F.SilkS"))
    (fp_text value "150" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(R101-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 111.7216 101.3206)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R105" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "1.5k" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(J101-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C102-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "vco-1stmixer:MAV-11BSM&plus_" (layer "F.Cu")
    (tedit 0)
    (at 133.5656 109.4486)
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U102" (at -0.0635 0.0635) (layer "F.SilkS"))
    (fp_text value "MAV-11" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "*" (at -3.6195 -0.9525) (layer "F.SilkS"))
    (fp_text user "*" (at -4.5466 -0.381) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User") hide)
    (fp_text user "0.03in/0.762mm" (at 0 -6.604) (layer "Cmts.User") hide)
    (fp_text user "0in/0mm" (at 6.604 0) (layer "Cmts.User") hide)
    (fp_text user "0.25in/6.35mm" (at -7.4295 0) (layer "Cmts.User") hide)
    (fp_text user "0.25in/6.35mm" (at 0 7.874) (layer "Cmts.User") hide)
    (fp_text user "0.058in/1.473mm" (at 7.4295 -3.175) (layer "Cmts.User") hide)
    (fp_text user "*" (at -1.4605 0) (layer "F.Fab") hide)
    (fp_text user "*" (at -1.4605 0) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at -3.175 0 90) (size 0.762 1.4732) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(C104-Pad2)") (pinfunction "RF_In") (pintype "passive"))
    (pad "2" smd rect locked (at 0 3.175) (size 0.762 1.4732) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "input"))
    (pad "3" smd rect locked (at 3.175 0 90) (size 0.762 1.4732) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(C106-Pad1)") (pinfunction "RF_Out") (pintype "passive"))
    (pad "4" smd rect locked (at 0 -3.175) (size 0.762 1.4732) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "input"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 172.6816 97.2566 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R115" (at 3.81 -0.254 90) (layer "F.SilkS"))
    (fp_text value "470" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(J103-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C110-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 145.5036 95.2246 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R107" (at 3.81 0 90) (layer "F.SilkS"))
    (fp_text value "220" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(L101-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C105-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 108.8876 116.5606 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C101" (at 2.5 0) (layer "F.SilkS"))
    (fp_text value ".01u" (at 2.5 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C101-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 108.8876 97.7646 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C102" (at 2.5 -0.152449) (layer "F.SilkS"))
    (fp_text value ".1u" (at 2.5 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C102-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 111.7216 94.2086)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R103" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "36" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(R101-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C104-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 123.4056 101.2806 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C105" (at 2.5 0 90) (layer "F.SilkS"))
    (fp_text value ".001u" (at 2.5 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C105-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-0.5sqmm_1x02_P4.6mm_D0.9mm_OD2.1mm" (layer "F.Cu")
    (tedit 5EB70B43)
    (at 111.4536 124.1806)
    (descr "Soldered wire connection, for 2 times 0.5 mm² wires, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.5sqmm")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J103" (at 2.3 -2.25) (layer "F.SilkS"))
    (fp_text value "VCO Sample" (at 2.3 2.25) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.3 0 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask) (roundrect_rratio 0.119048)
      (net 16 "Net-(J103-Pad1)") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle (at 4.6 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x02_P4.6mm_D0.9mm_OD2.1mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 125.6916 115.7986)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R110" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "150" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C107-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 95.4656 93.1926)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (attr exclude_from_pos_files)
    (fp_text reference "TP101" (at 0 -1.448) (layer "F.SilkS"))
    (fp_text value "VCC" (at 0 1.55) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 2 "Net-(C101-Pad2)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Connector_Wire:SolderWire-0.5sqmm_1x02_P4.6mm_D0.9mm_OD2.1mm" (layer "F.Cu")
    (tedit 5EB70B43)
    (at 180.0476 98.5266 90)
    (descr "Soldered wire connection, for 2 times 0.5 mm² wires, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.5sqmm")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J104" (at 2.3 -2.25 90) (layer "F.SilkS"))
    (fp_text value "RF In" (at 2.3 2.25 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.3 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask) (roundrect_rratio 0.119048)
      (net 17 "Net-(J104-Pad1)") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle (at 4.6 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x02_P4.6mm_D0.9mm_OD2.1mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-0.5sqmm_1x02_P4.6mm_D0.9mm_OD2.1mm" (layer "F.Cu")
    (tedit 5EB70B43)
    (at 180.0476 115.3046 90)
    (descr "Soldered wire connection, for 2 times 0.5 mm² wires, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.5sqmm")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J102" (at 2.3 -2.25 90) (layer "F.SilkS"))
    (fp_text value "1st IF Out" (at 2.3 2.25 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.3 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask) (roundrect_rratio 0.119048)
      (net 8 "Net-(C106-Pad2)") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle (at 4.6 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x02_P4.6mm_D0.9mm_OD2.1mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 113.7536 118.3386)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (attr exclude_from_pos_files)
    (fp_text reference "TP102" (at 0 -2.286) (layer "F.SilkS"))
    (fp_text value "POS-200 Out" (at 0 1.55) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 23 "Net-(R106-Pad2)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Connector_Wire:SolderWire-0.5sqmm_1x02_P4.6mm_D0.9mm_OD2.1mm" (layer "F.Cu")
    (tedit 5EB70B43)
    (at 95.2116 113.5126 90)
    (descr "Soldered wire connection, for 2 times 0.5 mm² wires, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.5sqmm")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J101" (at 2.3 -2.25 90) (layer "F.SilkS"))
    (fp_text value "VCO Control In" (at 2.3 2.25 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.3 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask) (roundrect_rratio 0.119048)
      (net 15 "Net-(J101-Pad1)") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle (at 4.6 0 90) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x02_P4.6mm_D0.9mm_OD2.1mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 137.4156 85.3186)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C108" (at 2.5 0.254) (layer "F.SilkS"))
    (fp_text value ".001u" (at 2.5 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C108-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 151.3456 82.5246)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (attr exclude_from_pos_files)
    (fp_text reference "TP105" (at 0 -1.448) (layer "F.SilkS"))
    (fp_text value "MAV-11B Out" (at 0 1.55) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 14 "Net-(C110-Pad2)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 97.2436 122.1486)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "H104" (at 0 -4.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 154.6876 120.6246)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C106" (at 2.5 0.254) (layer "F.SilkS"))
    (fp_text value ".001u" (at 2.5 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C106-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C106-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_THT:L_Toroid_Vertical_L13.0mm_W6.5mm_P5.60mm" (layer "F.Cu")
    (tedit 5AE59B06)
    (at 133.3116 95.9806)
    (descr "L_Toroid, Vertical series, Radial, pin pitch=5.60mm, , length*width=13*6.5mm^2")
    (tags "L_Toroid Vertical series Radial pin pitch 5.60mm  length 13mm width 6.5mm")
    (property "Field4" "T37-6")
    (property "Field5" "10T #30")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "L101" (at 0 2.54) (layer "F.SilkS"))
    (fp_text value ".3u" (at 0 8.15) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.8 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 19 "Net-(L101-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 5.6) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 7 "Net-(C106-Pad1)") (pintype "passive"))
    (model "${KIPRJMOD}/vco-1stmixer-models/vco-1stmixer-3D/T37-6 IND004.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/vco-1stmixer-models/vco-1stmixer-3D/T37-6 IND004.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 144.9956 81.2546 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R114" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "220" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(L102-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C109-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "vco-1stmixer:MAV-11BSM&plus_" (layer "F.Cu")
    (tedit 0)
    (at 143.9796 109.4486)
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U103" (at 0 0) (layer "F.SilkS"))
    (fp_text value "MAV-11" (at 5.588 2.54) (layer "F.SilkS") hide)
    (fp_text user "*" (at -3.0226 -0.381) (layer "F.SilkS"))
    (fp_text user "*" (at -2.539965 -1.016) (layer "F.SilkS"))
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User"))
    (fp_text user "0.058in/1.473mm" (at 7.4295 -3.175) (layer "Cmts.User"))
    (fp_text user "0.25in/6.35mm" (at -7.4295 0) (layer "Cmts.User"))
    (fp_text user "0.25in/6.35mm" (at 0 7.874) (layer "Cmts.User"))
    (fp_text user "0in/0mm" (at 6.604 0) (layer "Cmts.User"))
    (fp_text user "0.03in/0.762mm" (at 0 -6.604) (layer "Cmts.User"))
    (fp_text user "*" (at -1.4605 0) (layer "F.Fab"))
    (fp_text user "*" (at -1.4605 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -3.175 0 90) (size 0.762 1.4732) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(C107-Pad2)") (pinfunction "RF_In") (pintype "passive"))
    (pad "2" smd rect locked (at 0 3.175) (size 0.762 1.4732) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "input"))
    (pad "3" smd rect locked (at 3.175 0 90) (size 0.762 1.4732) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(C110-Pad2)") (pinfunction "RF_Out") (pintype "passive"))
    (pad "4" smd rect locked (at 0 -3.175) (size 0.762 1.4732) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "input"))
  )
  (footprint "vco-1stmixer:22284028" (layer "F.Cu")
    (tedit 0)
    (at 157.1876 99.7966)
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Model" "22284028")
    (property "Spice_Netlist_Enabled" "N")
    (property "Spice_Primitive" "J")
    (attr through_hole)
    (fp_text reference "JP101" (at -2.794 2.794) (layer "F.SilkS"))
    (fp_text value "Jumper" (at -1.27 0) (layer "F.SilkS") hide)
    (fp_text user "*" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer "Cmts.User") hide)
    (fp_text user "*" (at 0 0) (layer "F.Fab") hide)
    (pad "1" thru_hole rect locked (at 0 0) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask)
      (net 13 "Net-(C110-Pad1)") (pinfunction "J1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -2.54 0) (size 1.4224 1.4224) (drill 0.9144) (layers *.Cu *.Mask)
      (net 18 "Net-(JP101-Pad2)") (pinfunction "J2") (pintype "passive"))
  )
  (footprint "vco-1stmixer:POS-200" (layer "F.Cu")
    (tedit 0)
    (at 113.4996 108.9406)
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "U101" (at 0 0 180) (layer "F.SilkS"))
    (fp_text value "POS-200" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole oval (at -7.62 2.54) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C101-Pad2)") (pinfunction "VCC") (pintype "power_in"))
    (pad "2" thru_hole oval (at -2.54 2.54) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(R106-Pad2)") (pinfunction "RF_Out") (pintype "passive"))
    (pad "3" thru_hole oval (at 2.54 2.54) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND1") (pintype "power_in"))
    (pad "4" thru_hole oval (at 7.62 2.54) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND2") (pintype "power_in"))
    (pad "5" thru_hole oval (at 7.62 -2.54) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND3") (pintype "power_in"))
    (pad "6" thru_hole oval (at 2.54 -2.54) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND4") (pintype "power_in"))
    (pad "7" thru_hole oval (at -2.54 -2.54) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND5") (pintype "power_in"))
    (pad "8" thru_hole oval (at -7.62 -2.54) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C102-Pad2)") (pinfunction "VTune") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_Pad_1.0x1.0mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 129.5016 119.8626)
    (descr "SMD rectangular pad as test Point, square 1.0mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "vco-1stmixer.kicad_sch")
    (property "Sheetname" "")
    (property "Spice_Netlist_Enabled" "N")
    (attr exclude_from_pos_files)
    (fp_text reference "TP104" (at 0 -1.448) (layer "F.SilkS"))
    (fp_text value "6db Pad Out" (at 0 1.55) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0) (size 1 1) (layers "F.Cu" "F.Mask")
      (net 9 "Net-(C107-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (gr_arc (start 92.061903 82.81941) (mid 93.293988 79.844904) (end 96.268494 78.612819) (layer "Edge.Cuts") (width 0.16))
  (gr_line (start 92.061903 82.81941) (end 92.061903 122.828458) (layer "Edge.Cuts") (width 0.16))
  (gr_line (start 179.246122 78.612819) (end 96.268494 78.612819) (layer "Edge.Cuts") (width 0.16))
  (gr_arc (start 96.614264 127.380819) (mid 93.39527 126.047452) (end 92.061903 122.828458) (layer "Edge.Cuts") (width 0.16))
  (gr_line (start 96.614264 127.380819) (end 179.767228 127.380819) (layer "Edge.Cuts") (width 0.16))
  (gr_line (start 183.755903 123.392144) (end 183.755903 83.1226) (layer "Edge.Cuts") (width 0.16))
  (gr_arc (start 183.755903 123.392144) (mid 182.587635 126.212551) (end 179.767228 127.380819) (layer "Edge.Cuts") (width 0.16))
  (gr_arc (start 179.246122 78.612819) (mid 182.434995 79.933716) (end 183.755903 83.1226) (layer "Edge.Cuts") (width 0.16))
  (gr_text "Andy McCann KA3KAF\nDoug McCann KA3KAG" (at 133.057635 124.688551) (layer "F.SilkS"))
  (gr_text "VCO / 1st Mixer Rev. 0" (at 160.997635 125.704551) (layer "F.SilkS"))
  (zone (net 1) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 182.333635 79.984551)
        (xy 183.857635 82.778551)
        (xy 183.857635 123.418551)
        (xy 182.841635 125.958551)
        (xy 180.301635 127.482551)
        (xy 96.227635 127.228551)
        (xy 93.687635 126.212551)
        (xy 91.909635 122.910551)
        (xy 91.909635 82.524551)
        (xy 93.433635 79.730551)
        (xy 96.227635 78.714551)
        (xy 180.047635 78.714551)
      )
    )
  )
)
