(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0.0508)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(J1-Pin_5)")
	(net 2 "Net-(J1-Pin_8)")
	(net 3 "Net-(J1-Pin_9)")
	(net 4 "Net-(J1-Pin_28)")
	(net 5 "Net-(J1-Pin_17)")
	(net 6 "Net-(J1-Pin_24)")
	(net 7 "Net-(J1-Pin_2)")
	(net 8 "Net-(J1-Pin_10)")
	(net 9 "Net-(J1-Pin_7)")
	(net 10 "Net-(J1-Pin_4)")
	(net 11 "Net-(J1-Pin_11)")
	(net 12 "Net-(J1-Pin_18)")
	(net 13 "Net-(J1-Pin_3)")
	(net 14 "Net-(J1-Pin_27)")
	(net 15 "Net-(J1-Pin_25)")
	(net 16 "Net-(J1-Pin_12)")
	(net 17 "Net-(J1-Pin_21)")
	(net 18 "Net-(J1-Pin_6)")
	(net 19 "Net-(J1-Pin_1)")
	(net 20 "Net-(J1-Pin_15)")
	(net 21 "Net-(J1-Pin_16)")
	(net 22 "Net-(J1-Pin_14)")
	(net 23 "Net-(J1-Pin_20)")
	(net 24 "Net-(J1-Pin_13)")
	(net 25 "Net-(J1-Pin_22)")
	(net 26 "Net-(J1-Pin_23)")
	(net 27 "Net-(J1-Pin_26)")
	(net 28 "Net-(J1-Pin_19)")
	(footprint "Package_DIP:DIP-28_W15.24mm_Socket"
		(layer "F.Cu")
		(at 145.175 80.125)
		(descr "28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket")
		(tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket")
		(property "Reference" "J1"
			(at 7.62 -2.33 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ZIF Socket"
			(at 7.62 35.35 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm_Socket"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x14, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "zif28-breadboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 16.51 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(J1-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(J1-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(J1-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(J1-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(J1-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(J1-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(J1-Pin_7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 17.78)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(J1-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 20.32)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(J1-Pin_9)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 0 22.86)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J1-Pin_10)")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 0 25.4)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(J1-Pin_11)")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at 0 27.94)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(J1-Pin_12)")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at 0 30.48)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "Net-(J1-Pin_13)")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole oval
			(at 0 33.02)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(J1-Pin_14)")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole oval
			(at 15.24 33.02)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(J1-Pin_15)")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" thru_hole oval
			(at 15.24 30.48)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(J1-Pin_16)")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" thru_hole oval
			(at 15.24 27.94)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(J1-Pin_17)")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" thru_hole oval
			(at 15.24 25.4)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(J1-Pin_18)")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" thru_hole oval
			(at 15.24 22.86)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(J1-Pin_19)")
			(pinfunction "Pin_19")
			(pintype "passive")
		)
		(pad "20" thru_hole oval
			(at 15.24 20.32)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(J1-Pin_20)")
			(pinfunction "Pin_20")
			(pintype "passive")
		)
		(pad "21" thru_hole oval
			(at 15.24 17.78)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(J1-Pin_21)")
			(pinfunction "Pin_21")
			(pintype "passive")
		)
		(pad "22" thru_hole oval
			(at 15.24 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(J1-Pin_22)")
			(pinfunction "Pin_22")
			(pintype "passive")
		)
		(pad "23" thru_hole oval
			(at 15.24 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(J1-Pin_23)")
			(pinfunction "Pin_23")
			(pintype "passive")
		)
		(pad "24" thru_hole oval
			(at 15.24 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(J1-Pin_24)")
			(pinfunction "Pin_24")
			(pintype "passive")
		)
		(pad "25" thru_hole oval
			(at 15.24 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(J1-Pin_25)")
			(pinfunction "Pin_25")
			(pintype "passive")
		)
		(pad "26" thru_hole oval
			(at 15.24 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(J1-Pin_26)")
			(pinfunction "Pin_26")
			(pintype "passive")
		)
		(pad "27" thru_hole oval
			(at 15.24 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(J1-Pin_27)")
			(pinfunction "Pin_27")
			(pintype "passive")
		)
		(pad "28" thru_hole oval
			(at 15.24 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(J1-Pin_28)")
			(pinfunction "Pin_28")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-28_W15.24mm_Socket.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x14_P2.54mm_Vertical_SMD_Pin1Left"
		(layer "B.Cu")
		(at 156.61 96.65 180)
		(descr "surface-mounted straight pin header, 1x14, 2.54mm pitch, single row, style 1 (pin 1 left)")
		(tags "Surface mounted pin header SMD 1x14 2.54mm single row style1 pin1 left")
		(property "Reference" "J2"
			(at 0 18.84 0)
			(layer "B.SilkS")
		)
		(property "Value" "Breadboard 2"
			(at 0 -18.84 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x14_P2.54mm_Vertical_SMD_Pin1Left"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x14, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "zif28-breadboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.655 16.51 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 4 "Net-(J1-Pin_28)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.655 13.97 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 14 "Net-(J1-Pin_27)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.655 11.43 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 27 "Net-(J1-Pin_26)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.655 8.89 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 15 "Net-(J1-Pin_25)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -1.655 6.35 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 6 "Net-(J1-Pin_24)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 1.655 3.81 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 26 "Net-(J1-Pin_23)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -1.655 1.27 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 25 "Net-(J1-Pin_22)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 1.655 -1.27 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 17 "Net-(J1-Pin_21)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at -1.655 -3.81 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 23 "Net-(J1-Pin_20)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at 1.655 -6.35 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 28 "Net-(J1-Pin_19)")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at -1.655 -8.89 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 12 "Net-(J1-Pin_18)")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at 1.655 -11.43 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 5 "Net-(J1-Pin_17)")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at -1.655 -13.97 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 21 "Net-(J1-Pin_16)")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at 1.655 -16.51 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 20 "Net-(J1-Pin_15)")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x14_P2.54mm_Vertical_SMD_Pin1Left.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x14_P2.54mm_Vertical_SMD_Pin1Left"
		(layer "B.Cu")
		(at 148.99 96.65 180)
		(descr "surface-mounted straight pin header, 1x14, 2.54mm pitch, single row, style 1 (pin 1 left)")
		(tags "Surface mounted pin header SMD 1x14 2.54mm single row style1 pin1 left")
		(property "Reference" "J3"
			(at 0 18.84 0)
			(layer "B.SilkS")
		)
		(property "Value" "Breadboard 1"
			(at 0 -18.84 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x14_P2.54mm_Vertical_SMD_Pin1Left"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x14, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "zif28-breadboard.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.655 16.51 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 19 "Net-(J1-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.655 13.97 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 7 "Net-(J1-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.655 11.43 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 13 "Net-(J1-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.655 8.89 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 10 "Net-(J1-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -1.655 6.35 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "Net-(J1-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 1.655 3.81 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 18 "Net-(J1-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -1.655 1.27 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 9 "Net-(J1-Pin_7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 1.655 -1.27 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "Net-(J1-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at -1.655 -3.81 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 3 "Net-(J1-Pin_9)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at 1.655 -6.35 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 8 "Net-(J1-Pin_10)")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at -1.655 -8.89 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 11 "Net-(J1-Pin_11)")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at 1.655 -11.43 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 16 "Net-(J1-Pin_12)")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at -1.655 -13.97 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 24 "Net-(J1-Pin_13)")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at 1.655 -16.51 180)
			(size 2.51 1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 22 "Net-(J1-Pin_14)")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x14_P2.54mm_Vertical_SMD_Pin1Left.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Symbol:OSHW-Logo2_7.3x6mm_Copper"
		(layer "B.Cu")
		(at 152.8 117.856 180)
		(descr "Open Source Hardware Symbol")
		(tags "Logo Symbol OSHW")
		(property "Reference" "REF**"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "OSHW-Logo2_7.3x6mm_Copper"
			(at 0.75 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" "Symbol:OSHW-Logo2_7.3x6mm_Copper"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_missing_courtyard)
	)
	(gr_arc
		(start 161.45 71.5)
		(mid 162.97028 72.12972)
		(end 163.6 73.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 161.45 121.8)
		(end 144.15 121.8)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 142 73.65)
		(mid 142.62972 72.12972)
		(end 144.15 71.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 163.6 73.65)
		(end 163.6 119.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 144.15 71.5)
		(end 161.45 71.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 163.6 119.65)
		(mid 162.97028 121.17028)
		(end 161.45 121.8)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 144.15 121.8)
		(mid 142.62972 121.17028)
		(end 142 119.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 142 119.65)
		(end 142 73.65)
		(layer "Edge.Cuts")
	)
	(gr_text "Insert ZIF Socket"
		(at 153.796 106.7 90)
		(layer "F.Cu")
	)
	(gr_text "ZIF-28 to Breadboard\nAdapter"
		(at 152.8 74.676 0)
		(layer "B.Cu")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(mode hatch)
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
			(hatch_thickness 0.5)
			(hatch_gap 0.5)
			(hatch_orientation 45)
			(hatch_border_algorithm hatch_thickness)
			(hatch_min_hole_area 0.3)
		)
		(polygon
			(pts
				(xy 140.462 122.936) (xy 164.846 122.936) (xy 164.846 70.612) (xy 140.462 70.612)
			)
		)
	)
)
