(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-1")
  (general
    (thickness 1.6)
    (drawings 21)
    (tracks 298)
    (zones 0)
    (modules 56)
    (nets 29)
  )
  (page A4)
  (title_block
    (title "Revised Current Servo Circuit for Bias Coils")
    (date 2019-05-15)
    (rev 001)
    (company "Ye Group")
    (comment 1 "Initial Design by A. Kaufman, Regal Group")
    (comment 2 "Revision by J. Scott, Ye Group")
    (comment 3 "JILA, University of Colorado, Boulder")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.381)
    (trace_clearance 0.1778)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 1.016)
    (via_drill 0.508)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.015 3.015)
    (pad_drill 2.01)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 43.18 71.12)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +15V)
  (net 2 GNDA)
  (net 3 "Net-(C5-Pad1)")
  (net 4 -15V)
  (net 5 GNDPWR)
  (net 6 +VHC)
  (net 7 -VHC)
  (net 8 SignalDrive)
  (net 9 SignalFeedback)
  (net 10 "Net-(Q1-Pad1)")
  (net 11 "Net-(Q1-Pad3)")
  (net 12 "Net-(R2-Pad1)")
  (net 13 "Net-(R5-Pad1)")
  (net 14 "Net-(R8-Pad2)")
  (net 15 /Coil_Source)
  (net 16 "Net-(C1-Pad1)")
  (net 17 "Net-(C4-Pad1)")
  (net 18 "Net-(C4-Pad2)")
  (net 19 "Net-(C10-Pad2)")
  (net 20 "Net-(C10-Pad1)")
  (net 21 "Net-(J1-Pad1)")
  (net 22 "Net-(J6-Pad1)")
  (net 23 "Net-(J7-Pad3)")
  (net 24 "Net-(R5-Pad2)")
  (net 25 "Net-(R10-Pad2)")
  (net 26 "Net-(R9-Pad2)")
  (net 27 "Net-(R9-Pad1)")
  (net 28 "Net-(R11-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1778)
    (trace_width 0.381)
    (via_dia 1.016)
    (via_drill 0.508)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J7-Pad3)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(R9-Pad1)")
    (add_net "Net-(R9-Pad2)")
    (add_net SignalDrive)
  )
  (net_class High_I ""
    (clearance 0.1778)
    (trace_width 2.794)
    (via_dia 3.048)
    (via_drill 1.524)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net +VHC)
    (add_net -VHC)
    (add_net /Coil_Source)
    (add_net GNDPWR)
    (add_net "Net-(Q1-Pad3)")
    (add_net SignalFeedback)
  )
  (net_class Power ""
    (clearance 0.1778)
    (trace_width 0.508)
    (via_dia 1.143)
    (via_drill 0.635)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net +15V)
    (add_net -15V)
    (add_net GNDA)
  )
  (module footprints:Molex_KK-6410-04_04x2.54mm_Straight (layer F.Cu) (tedit 5D112675)
    (at 102.362 94.742 90)
    (descr "Connector Headers with Friction Lock, 22-27-2041, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2041")
    (fp_text reference J4 (at 1 -4.5 90) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 3.81 4.5 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 /Coil_Source))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 /Coil_Source))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 SignalFeedback))
    (pad 4 thru_hole oval (at 7.62 0 90) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 SignalFeedback))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_KK-6410-04_04x2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Molex_KK-6410-06_06x2.54mm_Straight (layer F.Cu) (tedit 5D1124AB)
    (at 83.693 118.11)
    (descr "Connector Headers with Friction Lock, 22-27-2061, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2061")
    (fp_text reference J5 (at 6.223 -4.064 180) (layer F.SilkS))
    (fp_text value Conn_01x06 (at 6.35 4.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 +VHC))
    (pad 2 thru_hole oval (at 2.54 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 +VHC))
    (pad 3 thru_hole oval (at 5.08 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 GNDPWR))
    (pad 4 thru_hole oval (at 7.62 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 GNDPWR))
    (pad 5 thru_hole oval (at 10.16 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 -VHC))
    (pad 6 thru_hole oval (at 12.7 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 -VHC))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_KK-6410-06_06x2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Molex_KK-6410-02_02x2.54mm_Straight (layer F.Cu) (tedit 5D112443)
    (at 75.565 111.633 90)
    (descr "Connector Headers with Friction Lock, 22-27-2021, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2021")
    (fp_text reference J6 (at 1.143 4.191 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 1.27 4.5 90) (layer F.Fab))
    (fp_text user %R (at 1.27 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 17 "Net-(C4-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 22 "Net-(J6-Pad1)"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_KK-6410-02_02x2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Molex_KK-6410-03_03x2.54mm_Straight (layer F.Cu) (tedit 5D112389)
    (at 120.142 45.72 270)
    (descr "Connector Headers with Friction Lock, 22-27-2031, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2031")
    (fp_text reference J7 (at 7.62 0 180) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 2.54 4.5 90) (layer F.Fab) hide)
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 20 "Net-(C10-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 23 "Net-(J7-Pad3)"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_KK-6410-03_03x2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Molex_KK-6410-03_03x2.54mm_Straight (layer F.Cu) (tedit 5D112389)
    (at 98.044 61.214 270)
    (descr "Connector Headers with Friction Lock, 22-27-2031, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2031")
    (fp_text reference J8 (at -2.54 -0.254) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 2.54 4.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 +15V))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 -15V))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_KK-6410-03_03x2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Molex_KK-6410-03_03x2.54mm_Straight (layer F.Cu) (tedit 5D112389)
    (at 119.126 61.214 270)
    (descr "Connector Headers with Friction Lock, 22-27-2031, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2031")
    (fp_text reference J2 (at 2.54 4.064 270) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 2.54 4.5 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 +15V))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 -15V))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_KK-6410-03_03x2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Molex_KK-6410-03_03x2.54mm_Straight (layer F.Cu) (tedit 5D112389)
    (at 82.677 76.835 270)
    (descr "Connector Headers with Friction Lock, 22-27-2031, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2031")
    (fp_text reference J9 (at -1.143 -4.445 270) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 2.54 4.5 270) (layer F.Fab))
    (fp_text user %R (at 2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 SignalDrive))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 GNDPWR))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 SignalFeedback))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_KK-6410-03_03x2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Molex_KK-6410-03_03x2.54mm_Straight (layer F.Cu) (tedit 5D112389)
    (at 74.422 86.106 270)
    (descr "Connector Headers with Friction Lock, 22-27-2031, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2031")
    (fp_text reference J3 (at 1.27 4.191 270) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 2.54 4.5 270) (layer F.Fab))
    (fp_text user %R (at 2.54 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 18 "Net-(C4-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 17 "Net-(C4-Pad1)"))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_KK-6410-03_03x2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5CDF3A18)
    (at 112.442 52.324)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R12 (at -1.952 1.778) (layer F.SilkS))
    (fp_text value 2k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J7-Pad3)"))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R11-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:OP27GSZ (layer F.Cu) (tedit 0)
    (at 103.632 49.022 90)
    (fp_text reference U3 (at -2.032 3.556 90) (layer F.SilkS))
    (fp_text value OP27 (at 0 0 180) (layer Cmts.User) hide)
    (fp_text user * (at -2.6162 -3.6068 90) (layer F.SilkS))
    (fp_text user * (at -1.6129 -2.4257 90) (layer F.Fab))
    (pad 1 smd rect (at -2.3622 -1.905 90) (size 2.1844 0.5588) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -2.3622 -0.635 90) (size 2.1844 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R11-Pad1)"))
    (pad 3 smd rect (at -2.3622 0.635 90) (size 2.1844 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R10-Pad2)"))
    (pad 4 smd rect (at -2.3622 1.905 90) (size 2.1844 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 4 -15V))
    (pad 5 smd rect (at 2.3622 1.905 90) (size 2.1844 0.5588) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 2.3622 0.635 90) (size 2.1844 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C10-Pad1)"))
    (pad 7 smd rect (at 2.3622 -0.635 90) (size 2.1844 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 1 +15V))
    (pad 8 smd rect (at 2.3622 -1.905 90) (size 2.1844 0.5588) (layers F.Cu F.Paste F.Mask))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 88.218 60.96)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 3.048 0 90) (layer F.SilkS))
    (fp_text value 5.49k (at 0 1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module BNC_Conn:CONN_1-1337543-0 (layer F.Cu) (tedit 5CDF3AA1)
    (at 81.026 61.214)
    (fp_text reference J1 (at -5.08 -8.128) (layer F.SilkS))
    (fp_text value "Voltage Input" (at -4.826 8.128) (layer F.SilkS))
    (pad P2 thru_hole circle (at -5.08 -5.08 90) (size 3.015 3.015) (drill 2.01) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad P1 thru_hole circle (at -5.08 5.08 90) (size 3.015 3.015) (drill 2.01) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 1.398 1.398) (drill 0.89) (layers *.Cu *.Mask)
      (net 16 "Net-(C1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.398 1.398) (drill 0.89) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad1)"))
  )
  (module UL_Footprints:MountingHole_4-40 (layer F.Cu) (tedit 5CDBAFD7)
    (at 121.92 40.64)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value MountingHole_4-40 (at 0 -2.54) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 3.500001 3.500001) (drill 2.448) (layers *.Cu *.Mask)
      (net 2 GNDA))
  )
  (module UL_Footprints:MountingHole_4-40 (layer F.Cu) (tedit 5CDBAFBF)
    (at 121.92 55.88)
    (fp_text reference REF** (at 0 2.54) (layer F.SilkS) hide)
    (fp_text value MountingHole_4-40 (at 0 -2.54) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 3.500001 3.500001) (drill 2.448) (layers *.Cu *.Mask)
      (net 2 GNDA))
  )
  (module Mounting_Holes:MountingHole_3.7mm_Pad (layer F.Cu) (tedit 5CDBA565)
    (at 73.66 119.38)
    (descr "Mounting Hole 3.7mm")
    (tags "mounting hole 3.7mm")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.7mm_Pad (at 0 4.7) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 7.4 7.4) (drill 3.7) (layers *.Cu *.Mask)
      (net 5 GNDPWR))
  )
  (module Mounting_Holes:MountingHole_3.7mm_Pad (layer F.Cu) (tedit 5CDBA47E)
    (at 73.66 78.74)
    (descr "Mounting Hole 3.7mm")
    (tags "mounting hole 3.7mm")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.7mm_Pad (at 0 4.7) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 7.4 7.4) (drill 3.7) (layers *.Cu *.Mask)
      (net 5 GNDPWR))
  )
  (module TO_SOT_Packages_THT:TO-220-2_Vertical (layer F.Cu) (tedit 58CE52AD)
    (at 116.332 99.314 270)
    (descr "TO-220-2, Vertical, RM 5.08mm")
    (tags "TO-220-2 Vertical RM 5.08mm")
    (fp_text reference R6 (at 2.54 0 270) (layer F.SilkS))
    (fp_text value 1 (at 2.54 3.92 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 15 /Coil_Source))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-2_Vertical.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-2_Vertical (layer F.Cu) (tedit 58CE52AD)
    (at 116.332 77.47 270)
    (descr "TO-220-2, Vertical, RM 5.08mm")
    (tags "TO-220-2 Vertical RM 5.08mm")
    (fp_text reference R7 (at 6.477 2.794 270) (layer F.SilkS))
    (fp_text value 1 (at 2.54 3.92 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 9 SignalFeedback))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 5 GNDPWR))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-2_Vertical.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm (layer F.Cu) (tedit 597C781B)
    (at 111.252 65.786 270)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (fp_text reference C18 (at 0.254 3.302 270) (layer F.SilkS))
    (fp_text value 33uF (at 1.25 3.56 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 -15V))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm (layer F.Cu) (tedit 597C781B)
    (at 111.252 59.182 270)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (fp_text reference C17 (at 2.032 3.302 270) (layer F.SilkS))
    (fp_text value 33uF (at 1.25 3.56 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +15V))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 104.14 66.294 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C16 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDA))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 -15V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 104.14 61.214 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C15 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +15V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 88.372 41.402 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 2.52 1.524 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 -1.778 180) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +15V))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 102.108 42.144 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +15V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 88.118 57.912)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 3.048 0 270) (layer F.SilkS))
    (fp_text value 10nF (at 0 1.778) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 111.252 45.7 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 1.29 1.778 90) (layer F.SilkS))
    (fp_text value C_PI (at 0.254 -1.778 90) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C10-Pad2)"))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C10-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 105.41 55.606 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0.02 1.778 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDA))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 -15V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 91.186 54.356)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 -15V))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDA))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 72.537 94.869 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 2.814 -0.127 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 77.744 94.869 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at -3.028 -0.127 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C4-Pad1)"))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C5-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 86.233 106.553 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at -0.635 -1.651 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 GNDPWR))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 +VHC))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 86.233 102.616 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 GNDPWR))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 +VHC))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm (layer F.Cu) (tedit 597C781B)
    (at 84.963 97.155)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (fp_text reference C13 (at 1.778 3.302) (layer F.SilkS))
    (fp_text value 33uF (at 1.25 3.56) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 GNDPWR))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 +VHC))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 93.853 106.553 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 0.635 -1.651 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 GNDPWR))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 -VHC))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 93.853 102.616 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at 0.127 -1.75 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 GNDPWR))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 -VHC))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_Tantal_D4.5mm_P2.50mm (layer F.Cu) (tedit 597C781B)
    (at 92.583 97.155)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=2.50mm, , diameter=4.5mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 2.50mm  diameter 4.5mm Tantal Electrolytic Capacitor")
    (fp_text reference C14 (at 0.762 3.302) (layer F.SilkS))
    (fp_text value 33uF (at -2.54 -5.08) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 GNDPWR))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 -VHC))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 58CE52AD)
    (at 116.332 88.392 270)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q1 (at 2.286 3.048 270) (layer F.SilkS))
    (fp_text value IRF530N (at 2.54 3.92 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 6 +VHC))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 58CE52AD)
    (at 116.332 110.236 270)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q2 (at 6.604 -1.905 270) (layer F.SilkS))
    (fp_text value IRF9530N (at 2.54 3.92 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 270) (layer F.Fab))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(Q1-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 7 -VHC))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (offset (xyz 2.539999961853027 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 95.504 45.212 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at -3.302 0 180) (layer F.SilkS))
    (fp_text value 30k (at 0 -1.778 180) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R8-Pad2)"))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 95.504 49.276)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 3.302 0) (layer F.SilkS))
    (fp_text value 2k (at 0 -1.524) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 83.312 43.514 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 2.874 0 180) (layer F.SilkS))
    (fp_text value DNI (at 0 1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R5-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 79.248 51.054)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 1.778) (layer F.SilkS))
    (fp_text value 0 (at 0 -1.524) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J1-Pad1)"))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 112.442 49.784)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 2.112 -1.778 180) (layer F.SilkS))
    (fp_text value R_PI (at 0 1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C10-Pad2)"))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R11-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 79.248 48.514)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 1.016 -1.524) (layer F.SilkS))
    (fp_text value DNI (at 0 -1.778) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 75.311 105.156)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 3.175 0 90) (layer F.SilkS))
    (fp_text value DNI (at 0 1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R9-Pad2)"))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R9-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 89.488 79.756 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value 51 (at 0 1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 SignalDrive))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Measurement_Points:Test_Point_Keystone_5010-5014_Multipurpose (layer F.Cu) (tedit 56E5DE99)
    (at 94.234 41.656)
    (descr "Keystone Miniature THM Test Point 5010-5014, http://www.keyelco.com/product-pdf.cfm?p=1319")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference TP5 (at 3.556 0) (layer F.SilkS))
    (fp_text value TestPoint (at 0.254 -2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.8 2.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 14 "Net-(R8-Pad2)"))
  )
  (module Measurement_Points:Test_Point_Keystone_5010-5014_Multipurpose (layer F.Cu) (tedit 56E5DE99)
    (at 79.248 42.926)
    (descr "Keystone Miniature THM Test Point 5010-5014, http://www.keyelco.com/product-pdf.cfm?p=1319")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference TP1 (at -3.302 2.032) (layer F.SilkS))
    (fp_text value TestPoint (at 0 -2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.8 2.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 12 "Net-(R2-Pad1)"))
  )
  (module Measurement_Points:Test_Point_Keystone_5010-5014_Multipurpose (layer F.Cu) (tedit 56E5DE99)
    (at 116.332 55.88)
    (descr "Keystone Miniature THM Test Point 5010-5014, http://www.keyelco.com/product-pdf.cfm?p=1319")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference TP8 (at -3.302 0) (layer F.SilkS))
    (fp_text value TestPoint (at 0 -2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.8 2.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 28 "Net-(R11-Pad1)"))
  )
  (module Measurement_Points:Test_Point_Keystone_5010-5014_Multipurpose (layer F.Cu) (tedit 56E5DE99)
    (at 90.932 76.2)
    (descr "Keystone Miniature THM Test Point 5010-5014, http://www.keyelco.com/product-pdf.cfm?p=1319")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference TP2 (at 3.302 -0.762) (layer F.SilkS))
    (fp_text value TestPoint (at 0 2.75) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.8 2.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 10 "Net-(Q1-Pad1)"))
  )
  (module Measurement_Points:Test_Point_Keystone_5010-5014_Multipurpose (layer F.Cu) (tedit 56E5DE99)
    (at 102.997 108.331)
    (descr "Keystone Miniature THM Test Point 5010-5014, http://www.keyelco.com/product-pdf.cfm?p=1319")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference TP3 (at -2.286 -2.286) (layer F.SilkS))
    (fp_text value TestPoint (at 0 2.75) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.8 2.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 11 "Net-(Q1-Pad3)"))
  )
  (module Measurement_Points:Test_Point_Keystone_5010-5014_Multipurpose (layer F.Cu) (tedit 56E5DE99)
    (at 104.14 101.727)
    (descr "Keystone Miniature THM Test Point 5010-5014, http://www.keyelco.com/product-pdf.cfm?p=1319")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference TP4 (at 0 -2.75) (layer F.SilkS))
    (fp_text value TestPoint (at 0 2.75) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.8 2.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 15 /Coil_Source))
  )
  (module Measurement_Points:Test_Point_Keystone_5010-5014_Multipurpose (layer F.Cu) (tedit 56E5DE99)
    (at 108.585 90.932)
    (descr "Keystone Miniature THM Test Point 5010-5014, http://www.keyelco.com/product-pdf.cfm?p=1319")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference TP6 (at 0 -2.75) (layer F.SilkS))
    (fp_text value TestPoint (at 0 2.75) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.8 2.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 9 SignalFeedback))
  )
  (module Measurement_Points:Test_Point_Keystone_5010-5014_Multipurpose (layer F.Cu) (tedit 56E5DE99)
    (at 95.25 87.122)
    (descr "Keystone Miniature THM Test Point 5010-5014, http://www.keyelco.com/product-pdf.cfm?p=1319")
    (tags "Through Hole Mount Test Points")
    (attr virtual)
    (fp_text reference TP7 (at 0 -2.75) (layer F.SilkS))
    (fp_text value TestPoint (at 0 2.75) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.8 2.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 5 GNDPWR))
  )
  (module UL_Footprints:AD620ARZ-REEL7 (layer F.Cu) (tedit 0)
    (at 87.376 48.26 90)
    (fp_text reference U1 (at 1.778 3.556 90) (layer F.SilkS))
    (fp_text value AD620 (at 0 0.381 180) (layer Dwgs.User))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 90) (layer Cmts.User) hide)
    (pad 1 smd rect (at -2.3622 -1.905 90) (size 2.1844 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R5-Pad1)"))
    (pad 2 smd rect (at -2.3622 -0.635 90) (size 2.1844 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C1-Pad1)"))
    (pad 3 smd rect (at -2.3622 0.635 90) (size 2.1844 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R2-Pad1)"))
    (pad 4 smd rect (at -2.3622 1.905 90) (size 2.1844 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 4 -15V))
    (pad 5 smd rect (at 2.3622 1.905 90) (size 2.1844 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDA))
    (pad 6 smd rect (at 2.3622 0.635 90) (size 2.1844 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(R8-Pad2)"))
    (pad 7 smd rect (at 2.3622 -0.635 90) (size 2.1844 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 1 +15V))
    (pad 8 smd rect (at 2.3622 -1.905 90) (size 2.1844 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R5-Pad2)"))
  )
  (module UL_Footprints:AD620ARZ-REEL7 (layer F.Cu) (tedit 0)
    (at 75.311 100.965 180)
    (fp_text reference U2 (at 0 3.429 180) (layer F.SilkS))
    (fp_text value AD620 (at -0.127 0 270) (layer F.SilkS))
    (fp_text user * (at -1.6129 -2.4257 180) (layer F.Fab))
    (pad 1 smd rect (at -2.3622 -1.905 180) (size 2.1844 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R9-Pad2)"))
    (pad 2 smd rect (at -2.3622 -0.635 180) (size 2.1844 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 15 /Coil_Source))
    (pad 3 smd rect (at -2.3622 0.635 180) (size 2.1844 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(Q1-Pad3)"))
    (pad 4 smd rect (at -2.3622 1.905 180) (size 2.1844 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C5-Pad1)"))
    (pad 5 smd rect (at 2.3622 1.905 180) (size 2.1844 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C4-Pad1)"))
    (pad 6 smd rect (at 2.3622 0.635 180) (size 2.1844 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J6-Pad1)"))
    (pad 7 smd rect (at 2.3622 -0.635 180) (size 2.1844 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C4-Pad2)"))
    (pad 8 smd rect (at 2.3622 -1.905 180) (size 2.1844 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R9-Pad1)"))
  )
  (gr_line (start 119.38 124.46) (end 119.38 73.66) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 68.58 124.46) (end 119.38 124.46) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 68.58 73.66) (end 68.58 124.46) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 119.38 73.66) (end 68.58 73.66) (layer Edge.Cuts) (width 0.2))
  (gr_text "Scott Designs\nCurrent Servo - Driver\nRev 1" (at 104.394 122.174) (layer F.SilkS))
  (gr_text "Scott Designs\nCurrent Servo - Control\nRev 1" (at 69.85 38.1) (layer F.SilkS))
  (gr_text "Drive, Gnd\nand Feedback\nTO: J9" (at 124.968 48.514 90) (layer F.SilkS))
  (gr_text "Power Input" (at 93.98 61.722 270) (layer F.SilkS))
  (dimension 5.08 (width 0.15) (layer Cmts.User)
    (gr_text "0.2 in" (at 130.84 38.1 -90) (layer Cmts.User))
    (feature1 (pts (xy 124.46 35.56) (xy 130.126421 35.56)))
    (feature2 (pts (xy 124.46 40.64) (xy 130.126421 40.64)))
    (crossbar (pts (xy 129.54 40.64) (xy 129.54 35.56)))
    (arrow1a (pts (xy 129.54 35.56) (xy 130.126421 36.686504)))
    (arrow1b (pts (xy 129.54 35.56) (xy 128.953579 36.686504)))
    (arrow2a (pts (xy 129.54 40.64) (xy 130.126421 39.513496)))
    (arrow2b (pts (xy 129.54 40.64) (xy 128.953579 39.513496)))
  )
  (dimension 40.64 (width 0.15) (layer Cmts.User)
    (gr_text "1.6000 in" (at 62.2 97.536 90) (layer Cmts.User))
    (feature1 (pts (xy 73.66 77.216) (xy 62.913579 77.216)))
    (feature2 (pts (xy 73.66 117.856) (xy 62.913579 117.856)))
    (crossbar (pts (xy 63.5 117.856) (xy 63.5 77.216)))
    (arrow1a (pts (xy 63.5 77.216) (xy 64.086421 78.342504)))
    (arrow1b (pts (xy 63.5 77.216) (xy 62.913579 78.342504)))
    (arrow2a (pts (xy 63.5 117.856) (xy 64.086421 116.729496)))
    (arrow2b (pts (xy 63.5 117.856) (xy 62.913579 116.729496)))
  )
  (dimension 50.8 (width 0.15) (layer Cmts.User)
    (gr_text "2.0000 in" (at 93.98 133.38) (layer Cmts.User))
    (feature1 (pts (xy 68.58 124.46) (xy 68.58 132.666421)))
    (feature2 (pts (xy 119.38 124.46) (xy 119.38 132.666421)))
    (crossbar (pts (xy 119.38 132.08) (xy 68.58 132.08)))
    (arrow1a (pts (xy 68.58 132.08) (xy 69.706504 131.493579)))
    (arrow1b (pts (xy 68.58 132.08) (xy 69.706504 132.666421)))
    (arrow2a (pts (xy 119.38 132.08) (xy 118.253496 131.493579)))
    (arrow2b (pts (xy 119.38 132.08) (xy 118.253496 132.666421)))
  )
  (dimension 35.56 (width 0.15) (layer Cmts.User)
    (gr_text "1.4000 in" (at 135.92 53.34 270) (layer Cmts.User))
    (feature1 (pts (xy 127 71.12) (xy 135.206421 71.12)))
    (feature2 (pts (xy 127 35.56) (xy 135.206421 35.56)))
    (crossbar (pts (xy 134.62 35.56) (xy 134.62 71.12)))
    (arrow1a (pts (xy 134.62 71.12) (xy 134.033579 69.993496)))
    (arrow1b (pts (xy 134.62 71.12) (xy 135.206421 69.993496)))
    (arrow2a (pts (xy 134.62 35.56) (xy 134.033579 36.686504)))
    (arrow2b (pts (xy 134.62 35.56) (xy 135.206421 36.686504)))
  )
  (dimension 50.8 (width 0.15) (layer Cmts.User)
    (gr_text "2.0000 in" (at 128.3 99.06 270) (layer Cmts.User))
    (feature1 (pts (xy 119.38 124.46) (xy 127.586421 124.46)))
    (feature2 (pts (xy 119.38 73.66) (xy 127.586421 73.66)))
    (crossbar (pts (xy 127 73.66) (xy 127 124.46)))
    (arrow1a (pts (xy 127 124.46) (xy 126.413579 123.333496)))
    (arrow1b (pts (xy 127 124.46) (xy 127.586421 123.333496)))
    (arrow2a (pts (xy 127 73.66) (xy 126.413579 74.786504)))
    (arrow2b (pts (xy 127 73.66) (xy 127.586421 74.786504)))
  )
  (dimension 15.24 (width 0.15) (layer Cmts.User)
    (gr_text "0.6000 in" (at 130.84 48.26 270) (layer Cmts.User))
    (feature1 (pts (xy 124.46 55.88) (xy 130.126421 55.88)))
    (feature2 (pts (xy 124.46 40.64) (xy 130.126421 40.64)))
    (crossbar (pts (xy 129.54 40.64) (xy 129.54 55.88)))
    (arrow1a (pts (xy 129.54 55.88) (xy 128.953579 54.753496)))
    (arrow1b (pts (xy 129.54 55.88) (xy 130.126421 54.753496)))
    (arrow2a (pts (xy 129.54 40.64) (xy 128.953579 41.766504)))
    (arrow2b (pts (xy 129.54 40.64) (xy 130.126421 41.766504)))
  )
  (dimension 58.42 (width 0.15) (layer Cmts.User)
    (gr_text "2.3000 in" (at 97.79 26.64) (layer Cmts.User))
    (feature1 (pts (xy 68.58 35.56) (xy 68.58 27.353579)))
    (feature2 (pts (xy 127 35.56) (xy 127 27.353579)))
    (crossbar (pts (xy 127 27.94) (xy 68.58 27.94)))
    (arrow1a (pts (xy 68.58 27.94) (xy 69.706504 27.353579)))
    (arrow1b (pts (xy 68.58 27.94) (xy 69.706504 28.526421)))
    (arrow2a (pts (xy 127 27.94) (xy 125.873496 27.353579)))
    (arrow2b (pts (xy 127 27.94) (xy 125.873496 28.526421)))
  )
  (dimension 58.42 (width 0.15) (layer Dwgs.User)
    (gr_text "2.3000 in" (at 90.17 54.64) (layer Dwgs.User))
    (feature1 (pts (xy 119.38 53.34) (xy 119.38 53.926421)))
    (feature2 (pts (xy 60.96 53.34) (xy 60.96 53.926421)))
    (crossbar (pts (xy 60.96 53.34) (xy 119.38 53.34)))
    (arrow1a (pts (xy 119.38 53.34) (xy 118.253496 53.926421)))
    (arrow1b (pts (xy 119.38 53.34) (xy 118.253496 52.753579)))
    (arrow2a (pts (xy 60.96 53.34) (xy 62.086504 53.926421)))
    (arrow2b (pts (xy 60.96 53.34) (xy 62.086504 52.753579)))
  )
  (gr_line (start 68.58 71.12) (end 68.58 35.56) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 127 71.12) (end 68.58 71.12) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 127 35.56) (end 127 71.12) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.58 35.56) (end 127 35.56) (layer Edge.Cuts) (width 0.1))
  (gr_text "Power Ouput\nTO: J3" (at 123.698 63.754 90) (layer F.SilkS))
  (zone (net 5) (net_name GNDPWR) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.508)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.635) (smoothing fillet) (radius 1.016))
    (polygon
      (pts
        (xy 87.63 107.696) (xy 87.63 101.346) (xy 92.456 101.346) (xy 92.456 107.696)
      )
    )
  )
  (zone (net 2) (net_name GNDA) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.508))
    (polygon
      (pts
        (xy 71.12 38.1) (xy 124.46 38.1) (xy 124.46 68.58) (xy 71.12 68.58)
      )
    )
  )
  (zone (net 9) (net_name SignalFeedback) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.508)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.635) (smoothing fillet) (radius 1.016))
    (polygon
      (pts
        (xy 117.348 78.74) (xy 117.348 75.946) (xy 116.332 75.946) (xy 113.538 75.946) (xy 113.538 78.74)
        (xy 113.538 78.994) (xy 115.062 78.994) (xy 117.348 78.994)
      )
    )
  )
  (zone (net 5) (net_name GNDPWR) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.508)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.635) (smoothing fillet) (radius 1.016))
    (polygon
      (pts
        (xy 92.456 120.396) (xy 92.456 115.062) (xy 87.63 115.062) (xy 87.63 120.396)
      )
    )
  )
  (zone (net 7) (net_name -VHC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.508)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.635) (smoothing fillet) (radius 1.016))
    (polygon
      (pts
        (xy 92.964 115.062) (xy 97.79 115.062) (xy 97.79 120.396) (xy 92.964 120.396)
      )
    )
  )
  (zone (net 6) (net_name +VHC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.508)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.635) (smoothing fillet) (radius 1.016))
    (polygon
      (pts
        (xy 87.122 115.062) (xy 87.122 120.396) (xy 82.296 120.396) (xy 82.296 115.062)
      )
    )
  )
  (zone (net 15) (net_name /Coil_Source) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.508)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.635) (smoothing fillet) (radius 0.508))
    (polygon
      (pts
        (xy 103.632 91.186) (xy 99.822 91.186) (xy 99.822 95.758) (xy 101.346 97.282) (xy 104.902 97.282)
        (xy 104.902 91.186)
      )
    )
  )
  (zone (net 9) (net_name SignalFeedback) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.508)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.635) (smoothing fillet) (radius 0.508))
    (polygon
      (pts
        (xy 104.902 90.678) (xy 99.822 90.678) (xy 99.822 85.852) (xy 101.092 84.582) (xy 103.632 84.582)
        (xy 104.902 85.852)
      )
    )
  )
)
