(kicad_pcb (version 20171130) (host pcbnew "(5.1.2)-2")
  (general
    (thickness 0.8)
    (drawings 16)
    (tracks 71)
    (zones 0)
    (modules 4)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.01)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1 1.6)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 "Net-(J2-Pad4)")
  (net 2 "Net-(J2-Pad3)")
  (net 3 "Net-(J2-Pad2)")
  (net 4 "Net-(J2-Pad1)")
  (net 5 "Net-(R1-Pad2)")
  (net 6 "Net-(R2-Pad2)")
  (net 7 "Net-(U1-PadB8)")
  (net 8 "Net-(U1-PadA8)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(U1-PadA8)")
    (add_net "Net-(U1-PadB8)")
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BE0F6D3)
    (at 101.288 114.735 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.45 90) (layer F.SilkS) hide)
    (fp_text value 5.1K (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(R1-Pad2)"))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J2-Pad4)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BE0F6CC)
    (at 102.768 114.735 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -0.00442 1.3212 90) (layer F.SilkS) hide)
    (fp_text value 5.1K (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J2-Pad4)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Custom:TYPE-C-31-M-12 (layer F.Cu) (tedit 5E337A34)
    (at 102.742 95.1472 180)
    (fp_text reference U1 (at 0.01016 2.75082) (layer F.SilkS))
    (fp_text value TYPE-C-31-M-12 (at -0.00254 3.88112) (layer F.Fab) hide)
    (pad A4|B9 smd rect (at -2.45 0 180) (size 0.6 1.45) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J2-Pad1)"))
    (pad B8 smd rect (at -1.75 0 180) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U1-PadB8)"))
    (pad A5 smd rect (at -1.25 0 180) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(R1-Pad2)"))
    (pad B7 smd rect (at -0.75 0 180) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J2-Pad2)"))
    (pad A6 smd rect (at -0.25 0 180) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J2-Pad3)"))
    (pad A7 smd rect (at 0.25 0 180) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J2-Pad2)"))
    (pad B6 smd rect (at 0.75 0 180) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J2-Pad3)"))
    (pad A8 smd rect (at 1.25 0 180) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U1-PadA8)"))
    (pad B5 smd rect (at 1.75 0 180) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(R2-Pad2)"))
    (pad B4|A9 smd rect (at 2.45 0 180) (size 0.6 1.45) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J2-Pad1)"))
    (pad B1|A12 smd rect (at 3.25 0 180) (size 0.6 1.45) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J2-Pad4)"))
    (pad A1|B12 smd rect (at -3.25 0 180) (size 0.6 1.45) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J2-Pad4)"))
    (pad GND thru_hole oval (at 4.32 5.095 180) (size 1 1.6) (drill oval 0.6 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(J2-Pad4)"))
    (pad GND thru_hole oval (at 4.32 0.915 180) (size 1 2.1) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 1 "Net-(J2-Pad4)"))
    (pad GND thru_hole oval (at -4.32 0.915 180) (size 1 2.1) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 1 "Net-(J2-Pad4)"))
    (pad GND thru_hole oval (at -4.32 5.095 180) (size 1 1.6) (drill oval 0.6 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(J2-Pad4)"))
    (pad "" np_thru_hole circle (at 2.89 1.445 180) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.89 1.445 180) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 95.1484 124.06 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x05_Male (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at 0 3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J2-Pad4)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 97.409 107.442) (end 93.7387 112.35436) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104.008336 112.35436) (end 108.077 105.664) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104.008336 125.45568) (end 104.008336 112.35436) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 93.7387 125.45568) (end 93.7387 112.35436) (layer Edge.Cuts) (width 0.15))
  (gr_text https://goo.gl/JxeCjH (at 100.65512 110.62208 90) (layer B.SilkS))
  (gr_text GND (at 102.75 122.425) (layer B.SilkS))
  (gr_text D+ (at 100.2 122.375) (layer B.SilkS))
  (gr_text D- (at 97.7 122.375) (layer B.SilkS))
  (gr_text Vcc (at 95.15 122.325) (layer B.SilkS))
  (gr_text "Made by HDR" (at 107.188 101.854 90) (layer F.SilkS))
  (gr_text V1.4 (at 102.7176 101.3968) (layer F.SilkS))
  (gr_text "This side up" (at 94.8182 117.41404 270) (layer F.SilkS))
  (gr_line (start 104.008336 125.4567) (end 93.7387 125.4567) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 97.409 88.773) (end 97.409 107.442) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 108.077 88.773) (end 97.408245 88.773) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 108.077 88.773) (end 108.077 105.664) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name "Net-(J2-Pad4)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 108.3564 88.5952) (xy 108.3564 105.85196) (xy 104.19334 112.53724) (xy 104.19334 125.75794) (xy 93.52026 125.75794)
        (xy 93.52026 112.03432) (xy 97.1042 107.3912) (xy 97.078807 88.5952)
      )
    )
  )
  (zone (net 1) (net_name "Net-(J2-Pad4)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 97.0788 88.5952) (xy 97.0788 88.59012) (xy 97.078807 88.5952)
      )
    )
  )
  (zone (net 1) (net_name "Net-(J2-Pad4)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 97.0788 88.5952) (xy 97.0788 88.59012) (xy 97.078807 88.5952)
      )
    )
  )
  (zone (net 1) (net_name "Net-(J2-Pad4)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 108.35894 88.5952) (xy 108.35894 105.85196) (xy 104.19588 112.53724) (xy 104.19588 125.75794) (xy 93.5228 125.75794)
        (xy 93.5228 112.03432) (xy 97.10674 107.3912) (xy 97.081347 88.5952)
      )
    )
  )
)
