(kicad_pcb (version 4) (host pcbnew 4.0.4+e1-6308~48~ubuntu16.04.1-stable)
  (general
    (links 68)
    (no_connects 0)
    (area 47.650714 79.813839 196.189286 130.135)
    (thickness 1.6)
    (drawings 14)
    (tracks 89)
    (zones 0)
    (modules 35)
    (nets 14)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.6)
    (trace_clearance 0.6)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.4)
    (segment_width 0.2)
    (edge_width 0.2)
    (via_size 0.8)
    (via_drill 0.5)
    (via_min_size 0.5)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5.6 5.6)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C2-Pad2)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C4-Pad2)")
  (net 6 "Net-(C7-Pad1)")
  (net 7 "Net-(C10-Pad2)")
  (net 8 "Net-(D1-Pad2)")
  (net 9 "Net-(F1-Pad1)")
  (net 10 "Net-(P1-Pad3)")
  (net 11 "Net-(P1-Pad1)")
  (net 12 "Net-(R3-Pad2)")
  (net 13 "Net-(R5-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.6)
    (trace_width 0.6)
    (via_dia 0.8)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R5-Pad2)")
  )
  (net_class Power ""
    (clearance 1)
    (trace_width 2)
    (via_dia 1)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad3)")
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 57DEEA1D)
    (at 62.865 124.46)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965_Pad (at 0 3.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 57DEEA18)
    (at 62.865 86.36)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965_Pad (at 0 3.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 57DEEA01)
    (at 113.665 86.36)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965_Pad (at 0 3.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 57DEE9E8)
    (at 113.665 124.46)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965_Pad (at 0 3.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 57DEE9F1)
    (at 180.975 124.46)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965_Pad (at 0 3.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 57DEE9FC)
    (at 180.975 86.36)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965_Pad (at 0 3.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Capacitors_ThroughHole:C_Radial_D16_L30_P7.5 (layer F.Cu) (tedit 57E18652)
    (at 123.19 92.075 270)
    (descr "Radial Electrolytic Capacitor Diameter 16mm x Length 25mm, Pitch 7.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C1 (at -5.715 0 360) (layer F.SilkS))
    (fp_text value 2200uF (at 0.9144 -9.2456 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 7.5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D16_L30_P7.5.wrl
      (at (xyz 0.147638 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D16_L30_P7.5 (layer F.Cu) (tedit 57E18656)
    (at 123.19 111.125 270)
    (descr "Radial Electrolytic Capacitor Diameter 16mm x Length 25mm, Pitch 7.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C2 (at 13.335 0.635 360) (layer F.SilkS))
    (fp_text value 2200uF (at 2.4257 -9.4742 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 7.5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D16_L30_P7.5.wrl
      (at (xyz 0.147638 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D16_L30_P7.5 (layer F.Cu) (tedit 57DEEBC1)
    (at 144.145 92.075 270)
    (descr "Radial Electrolytic Capacitor Diameter 16mm x Length 25mm, Pitch 7.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C3 (at -5.715 0.635 360) (layer F.SilkS))
    (fp_text value 2200uF (at 3.75 9.3 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 7.5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D16_L30_P7.5.wrl
      (at (xyz 0.147638 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D16_L30_P7.5 (layer F.Cu) (tedit 57DEEBD5)
    (at 144.145 111.125 270)
    (descr "Radial Electrolytic Capacitor Diameter 16mm x Length 25mm, Pitch 7.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C4 (at 13.335 -0.635 360) (layer F.SilkS))
    (fp_text value 2200uF (at 3.75 9.3 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 7.5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C4-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D16_L30_P7.5.wrl
      (at (xyz 0.147638 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 57E186C3)
    (at 156.21 99.06 270)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C5 (at 2.54 2.54 270) (layer F.SilkS))
    (fp_text value 100nF (at 3.0861 3.9878 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 57E1866C)
    (at 156.21 123.19 90)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C6 (at 1.0414 -2.7686 180) (layer F.SilkS))
    (fp_text value 100nF (at -0.5842 -4.2672 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C4-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 57E18698)
    (at 175.26 90.805 90)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C7 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value 100nF (at -0.3937 2.2098 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C7-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 57E18683)
    (at 175.26 120.65 90)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C8 (at -2.3368 -0.8001 180) (layer F.SilkS))
    (fp_text value 100nF (at 1.25 2.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C10-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L11_P2 (layer F.Cu) (tedit 57E1869F)
    (at 180.975 96.52 90)
    (descr "Radial Electrolytic Capacitor 5mm x Length 11mm, Pitch 2mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C9 (at 4.6482 -0.0381 180) (layer F.SilkS))
    (fp_text value 10uF (at 6.1087 0.9144 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C7-Pad1)"))
    (pad 2 thru_hole circle (at 2 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L11_P2 (layer F.Cu) (tedit 57E18688)
    (at 181.61 115.57 90)
    (descr "Radial Electrolytic Capacitor 5mm x Length 11mm, Pitch 2mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C10 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 10uF (at -4.2926 -0.508 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C10-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:DO-35 (layer F.Cu) (tedit 57E186F0)
    (at 112.395 95.25 90)
    (descr "Diode 3 pas")
    (tags "DIODE DEV")
    (fp_text reference D1 (at -0.635 -1.905 90) (layer F.SilkS))
    (fp_text value 1N4004 (at -0.5334 1.7145 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 3.81 0 90) (size 1.4224 1.4224) (drill 0.6096) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.4224 1.4224) (drill 0.6096) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(D1-Pad2)"))
    (model Discret.3dshapes/DO-35.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:DO-35 (layer F.Cu) (tedit 57E186DE)
    (at 112.395 115.57 90)
    (descr "Diode 3 pas")
    (tags "DIODE DEV")
    (fp_text reference D2 (at 0 -1.905 90) (layer F.SilkS))
    (fp_text value 1N4004 (at -0.2667 1.9304 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 3.81 0 90) (size 1.4224 1.4224) (drill 0.6096) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(D1-Pad2)"))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.4224 1.4224) (drill 0.6096) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad2)"))
    (model Discret.3dshapes/DO-35.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:DO-35 (layer F.Cu) (tedit 57DEEBF5)
    (at 165.1 101.6 180)
    (descr "Diode 3 pas")
    (tags "DIODE DEV")
    (fp_text reference D3 (at 0 -1.905 180) (layer F.SilkS))
    (fp_text value 1N4004 (at 0 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 3.81 0 180) (size 1.4224 1.4224) (drill 0.6096) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at -3.81 0 180) (size 1.4224 1.4224) (drill 0.6096) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C7-Pad1)"))
    (model Discret.3dshapes/DO-35.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:DO-35 (layer F.Cu) (tedit 57E186BC)
    (at 164.465 123.825)
    (descr "Diode 3 pas")
    (tags "DIODE DEV")
    (fp_text reference D4 (at 0 1.905) (layer F.SilkS))
    (fp_text value 1N4004 (at 0.2159 -2.1717) (layer F.Fab))
    (pad 1 thru_hole rect (at 3.81 0) (size 1.4224 1.4224) (drill 0.6096) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C10-Pad2)"))
    (pad 2 thru_hole circle (at -3.81 0) (size 1.4224 1.4224) (drill 0.6096) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C4-Pad2)"))
    (model Discret.3dshapes/DO-35.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:DO-35 (layer F.Cu) (tedit 57E186CF)
    (at 175.26 99.06 90)
    (descr "Diode 3 pas")
    (tags "DIODE DEV")
    (fp_text reference D5 (at -2.921 -2.1463 90) (layer F.SilkS))
    (fp_text value 1N4004 (at 1.9939 -1.9177 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 3.81 0 90) (size 1.4224 1.4224) (drill 0.6096) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C7-Pad1)"))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.4224 1.4224) (drill 0.6096) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Discret.3dshapes/DO-35.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:DO-35 (layer F.Cu) (tedit 57DEEC28)
    (at 175.26 109.855 90)
    (descr "Diode 3 pas")
    (tags "DIODE DEV")
    (fp_text reference D6 (at -0.635 1.905 90) (layer F.SilkS))
    (fp_text value 1N4004 (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 3.81 0 90) (size 1.4224 1.4224) (drill 0.6096) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 1.4224 1.4224) (drill 0.6096) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C10-Pad2)"))
    (model Discret.3dshapes/DO-35.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D6_P5 (layer F.Cu) (tedit 57E186EB)
    (at 112.395 107.315 90)
    (descr "Capacitor 6mm Disc, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference F1 (at -1.905 -2.54 90) (layer F.SilkS))
    (fp_text value F_Small (at 2.5 3.5 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(F1-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(D1-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D6_P5.wrl
      (at (xyz 0.0984252 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_MKDS1.5-3pol (layer F.Cu) (tedit 57E1FABB)
    (at 64.135 110.49 90)
    (descr "3-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference P1 (at 5 5.9 90) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 5 -6.6 90) (layer F.Fab) hide)
    (pad 3 thru_hole circle (at 10 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P1-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P1-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 90) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MKDS1.5-3pol.wrl
      (at (xyz 0.1968 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Sockets_MOLEX_KK-System:Socket_MOLEX-KK-RM2-54mm_Lock_3pin_straight (layer F.Cu) (tedit 57E1868F)
    (at 181.61 103.505 90)
    (descr "Socket, MOLEX, KK, RM 2.54mm, Lock, 3pin, straight,")
    (tags "Socket, MOLEX, KK, RM 2.54mm, Lock, 3pin, straight,")
    (fp_text reference P2 (at -5.08 0 180) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 5.08 90) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at -2.54 0 90) (size 1.80086 3.50012) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C7-Pad1)"))
    (pad 2 thru_hole oval (at 0 0 90) (size 1.80086 3.50012) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 1.80086 3.50012) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C10-Pad2)"))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_2512_RM10_HandSoldering (layer F.Cu) (tedit 57E18645)
    (at 133.985 85.09 180)
    (descr "Resistor, SMD+THT, 2512, RM10, Hand soldering,")
    (tags "Resistor, SMD+THT, 2512, RM10, Hand soldering,")
    (fp_text reference R1 (at 0.09906 -3.0988 180) (layer F.SilkS))
    (fp_text value 4R7 (at -3.2766 -3.2766 180) (layer F.Fab))
    (pad 1 smd rect (at -3.2004 0 180) (size 1.6002 3.2004) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 3.2004 0 180) (size 1.6002 3.2004) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 1 thru_hole rect (at -5.00126 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 thru_hole rect (at 5.00126 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_2512_RM10_HandSoldering (layer F.Cu) (tedit 57DEEBE5)
    (at 133.985 125.73 180)
    (descr "Resistor, SMD+THT, 2512, RM10, Hand soldering,")
    (tags "Resistor, SMD+THT, 2512, RM10, Hand soldering,")
    (fp_text reference R2 (at 0 2.54 180) (layer F.SilkS))
    (fp_text value 4R7 (at -0.39878 4.20116 180) (layer F.Fab))
    (pad 1 smd rect (at -3.2004 0 180) (size 1.6002 3.2004) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (pad 2 smd rect (at 3.2004 0 180) (size 1.6002 3.2004) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad2)"))
    (pad 1 thru_hole rect (at -5.00126 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C4-Pad2)"))
    (pad 2 thru_hole rect (at 5.00126 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad2)"))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_0805to1206_RM10_HandSoldering (layer F.Cu) (tedit 57E186AB)
    (at 170.815 90.17 90)
    (descr "Resistor, SMD and THT, universal, 0805 to 1206,RM10,  Hand soldering,")
    (tags "Resistor, SMD and THT, universal, 0805 to 1206, RM10, Hand soldering,")
    (fp_text reference R3 (at -6.1087 -2.5019 90) (layer F.SilkS))
    (fp_text value 330R (at 1.27 -2.2225 90) (layer F.Fab))
    (pad 1 smd trapezoid (at -2.413 0 90) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C7-Pad1)"))
    (pad 2 smd trapezoid (at 2.413 0 270) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R3-Pad2)"))
    (pad 1 thru_hole rect (at -5.00126 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C7-Pad1)"))
    (pad 2 thru_hole rect (at 5.00126 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(R3-Pad2)"))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_0805to1206_RM10_HandSoldering (layer F.Cu) (tedit 57E1861D)
    (at 156.845 90.17 90)
    (descr "Resistor, SMD and THT, universal, 0805 to 1206,RM10,  Hand soldering,")
    (tags "Resistor, SMD and THT, universal, 0805 to 1206, RM10, Hand soldering,")
    (fp_text reference R4 (at 4.445 -3.175 90) (layer F.SilkS))
    (fp_text value 2K7 (at 0.1143 -2.4257 90) (layer F.Fab))
    (pad 1 smd trapezoid (at -2.413 0 90) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R3-Pad2)"))
    (pad 2 smd trapezoid (at 2.413 0 270) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at -5.00126 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(R3-Pad2)"))
    (pad 2 thru_hole rect (at 5.00126 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_0805to1206_RM10_HandSoldering (layer F.Cu) (tedit 57E18621)
    (at 156.845 111.125 270)
    (descr "Resistor, SMD and THT, universal, 0805 to 1206,RM10,  Hand soldering,")
    (tags "Resistor, SMD and THT, universal, 0805 to 1206, RM10, Hand soldering,")
    (fp_text reference R5 (at -3.81 2.54 270) (layer F.SilkS))
    (fp_text value 2K7 (at -0.4445 2.8702 270) (layer F.Fab))
    (pad 1 smd trapezoid (at -2.413 0 270) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd trapezoid (at 2.413 0 90) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R5-Pad2)"))
    (pad 1 thru_hole rect (at -5.00126 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 5.00126 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(R5-Pad2)"))
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_0805to1206_RM10_HandSoldering (layer F.Cu) (tedit 57E1867F)
    (at 170.815 113.03 270)
    (descr "Resistor, SMD and THT, universal, 0805 to 1206,RM10,  Hand soldering,")
    (tags "Resistor, SMD and THT, universal, 0805 to 1206, RM10, Hand soldering,")
    (fp_text reference R6 (at -5.08 2.54 270) (layer F.SilkS))
    (fp_text value 330R (at 0.5207 2.3876 270) (layer F.Fab))
    (pad 1 smd trapezoid (at -2.413 0 270) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R5-Pad2)"))
    (pad 2 smd trapezoid (at 2.413 0 90) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C10-Pad2)"))
    (pad 1 thru_hole rect (at -5.00126 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(R5-Pad2)"))
    (pad 2 thru_hole rect (at 5.00126 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C10-Pad2)"))
  )
  (module TO_SOT_Packages_THT:TO-220_Neutral123_Vertical (layer F.Cu) (tedit 57E186AF)
    (at 163.195 92.075 270)
    (descr "TO-220, Neutral, Vertical,")
    (tags "TO-220, Neutral, Vertical,")
    (fp_text reference U1 (at -6.35 0 360) (layer F.SilkS))
    (fp_text value LM317T (at -5.2324 2.7686 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C7-Pad1)"))
    (pad 1 thru_hole oval (at -2.54 0) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(R3-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C3-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-220_Neutral123_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220_Neutral123_Vertical (layer F.Cu) (tedit 57E186B4)
    (at 163.195 114.3 270)
    (descr "TO-220, Neutral, Vertical,")
    (tags "TO-220, Neutral, Vertical,")
    (fp_text reference U2 (at -6.35 0 360) (layer F.SilkS))
    (fp_text value LM337T (at -6.2865 2.6543 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C4-Pad2)"))
    (pad 1 thru_hole oval (at -2.54 0) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(R5-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C10-Pad2)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-220_Neutral123_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 57DEE9D3)
    (at 133.985 105.41)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference REF** (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965_Pad (at 0 3.8) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module "My Shit:Transformer-5VA_1xSec" (layer F.Cu) (tedit 57E21853)
    (at 90.17 105.41)
    (descr "Trafo, Printtrafo, CHK, EI42, 5VA, 1x Sec,")
    (tags "Trafo, Printtrafo, CHK, EI42, 5VA, 1x Sec,")
    (fp_text reference T1 (at 0.0254 -19.5199) (layer F.SilkS))
    (fp_text value MYRRA-TRANSF (at 0 0 90) (layer F.Fab) hide)
    (fp_text user Sec (at 15.99946 0 90) (layer F.SilkS))
    (fp_text user Pri (at -15.99946 0 90) (layer F.SilkS))
    (fp_text user 9 (at 8.001 7.00024) (layer F.SilkS))
    (fp_text user 7 (at 8.001 -7.00024) (layer F.SilkS))
    (fp_text user 5 (at -12.7 -15.24) (layer F.SilkS))
    (fp_text user 1 (at -12.7 15.24) (layer F.SilkS))
    (pad 1 thru_hole circle (at -12.49934 12.5) (size 2.99974 2.99974) (drill 1.50114) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P1-Pad1)"))
    (pad 2 thru_hole circle (at -12.49934 7.5) (size 2.99974 2.99974) (drill 1.50114) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole circle (at -12.49934 0) (size 2.99974 2.99974) (drill 1.50114) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole circle (at -12.49934 -7.5) (size 2.99974 2.99974) (drill 1.50114) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole circle (at -12.49934 -12.5) (size 2.99974 2.99974) (drill 1.50114) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P1-Pad3)"))
    (pad 6 thru_hole circle (at 12.49934 -12.5) (size 2.99974 2.99974) (drill 1.50114) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole circle (at 12.49934 -7.5) (size 2.99974 2.99974) (drill 1.50114) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(F1-Pad1)"))
    (pad 8 thru_hole circle (at 12.49934 0) (size 2.99974 2.99974) (drill 1.50114) (layers *.Cu *.Mask F.SilkS))
    (pad 9 thru_hole circle (at 12.49934 7.5) (size 2.99974 2.99974) (drill 1.50114) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 10 thru_hole circle (at 12.49934 12.5) (size 2.99974 2.99974) (drill 1.50114) (layers *.Cu *.Mask F.SilkS))
  )
  (gr_text https://oshpark.com/profiles/jronen (at 132.4737 115.0366) (layer B.SilkS))
  (gr_text "(C) Jon Ronen-Drori 2016" (at 133.6802 96.1009) (layer B.SilkS))
  (gr_text "CUT OUT" (at 90.1446 105.5243 90) (layer F.SilkS))
  (gr_text + (at 177.3174 107.0991) (layer F.SilkS))
  (gr_text 0 (at 177.3936 103.4796 90) (layer F.SilkS))
  (gr_text - (at 177.165 99.6315 90) (layer F.SilkS))
  (gr_line (start 88.265 90.17) (end 92.075 90.17) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 88.265 121.285) (end 92.075 121.285) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 57.785 129.54) (end 57.785 81.915) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 186.055 129.54) (end 57.785 129.54) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 186.055 81.915) (end 186.055 129.54) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 57.785 81.915) (end 186.055 81.915) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 92.075 90.17) (end 92.075 121.285) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 88.265 121.285) (end 88.265 90.17) (angle 90) (layer Edge.Cuts) (width 0.2))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 183.515 127) (xy 60.325 127) (xy 60.325 83.82) (xy 183.515 83.82)
      )
    )
    (polygon
      (pts        (xy 82.55 88.265) (xy 82.55 123.19) (xy 99.06 123.19) (xy 99.06 88.265)
      )
    )
  )
)
