(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 15)
    (no_connects 0)
    (area 129.401499 66.345999 171.588501 134.758501)
    (thickness 1.6)
    (drawings 11)
    (tracks 46)
    (zones 0)
    (modules 6)
    (nets 19)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 4.7)
    (pad_drill 1.7)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerbers/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 RED)
  (net 3 R_AUD)
  (net 4 SYNC)
  (net 5 GREEN)
  (net 6 L_AUD)
  (net 7 BLUE)
  (net 8 "Net-(SCART1-Pad16)")
  (net 9 "Net-(SCART1-Pad14)")
  (net 10 "Net-(SCART1-Pad10)")
  (net 11 "Net-(SCART1-Pad12)")
  (net 12 "Net-(SCART1-Pad1)")
  (net 13 "Net-(SCART1-Pad3)")
  (net 14 "Net-(SCART1-Pad19)")
  (net 15 "Net-(J1-Pad1)")
  (net 16 "Net-(J2-Pad1)")
  (net 17 "Net-(J3-Pad1)")
  (net 18 "Net-(J4-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net BLUE)
    (add_net GND)
    (add_net GREEN)
    (add_net L_AUD)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(SCART1-Pad1)")
    (add_net "Net-(SCART1-Pad10)")
    (add_net "Net-(SCART1-Pad12)")
    (add_net "Net-(SCART1-Pad14)")
    (add_net "Net-(SCART1-Pad16)")
    (add_net "Net-(SCART1-Pad19)")
    (add_net "Net-(SCART1-Pad3)")
    (add_net RED)
    (add_net R_AUD)
    (add_net SYNC)
  )
  (module SCARTConnectors:3x2_RCA (layer F.Cu) (tedit 5B18BA86)
    (at 150.495 66.421 180)
    (fp_text reference RCA1 (at -11.43 -8.89 180) (layer F.SilkS))
    (fp_text value 3x2_RCA (at 10.16 -7.62 180) (layer F.Fab))
    (pad 9 thru_hole oval (at 17.75 -5.25 180) (size 2.2 4) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 3.75 -5.25 180) (size 2.2 4) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at -10.25 -5.25 180) (size 2.2 4) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 17.75 -12.5 180) (size 2 4) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 RED))
    (pad 5 thru_hole oval (at 10.25 -12.5 180) (size 2 4) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 R_AUD))
    (pad 1 thru_hole oval (at -17.75 -12.5 180) (size 2 4) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 SYNC))
    (pad 2 thru_hole oval (at -10.25 -12.5 180) (size 2 4) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 GREEN))
    (pad 3 thru_hole oval (at -3.75 -12.5 180) (size 2 4) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 L_AUD))
    (pad 4 thru_hole oval (at 3.75 -12.5 180) (size 2 4) (drill 1.3) (layers *.Cu *.Mask)
      (net 7 BLUE))
    (pad "" np_thru_hole oval (at -20.15 -8.75 180) (size 1.7 4.7) (drill oval 1.7 4.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at 20.15 -8.75 180) (size 1.7 4.7) (drill oval 1.7 4.7) (layers *.Cu *.Mask))
  )
  (module SCARTConnectors:SCART_F (layer F.Cu) (tedit 5B18B74C)
    (at 150.495 108.331 270)
    (fp_text reference SCART1 (at 0 6 270) (layer F.SilkS))
    (fp_text value SCART-F (at 0 -6.25 270) (layer F.Fab))
    (pad 20 thru_hole oval (at -17.155 -2.54 270) (size 2 4) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 SYNC))
    (pad 18 thru_hole oval (at -13.345 -2.54 270) (size 2 4) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 16 thru_hole oval (at -9.535 -2.54 270) (size 2 4) (drill 1.3) (layers *.Cu *.Mask)
      (net 8 "Net-(SCART1-Pad16)"))
    (pad 14 thru_hole oval (at -5.725 -2.54 270) (size 2 4) (drill 1.3) (layers *.Cu *.Mask)
      (net 9 "Net-(SCART1-Pad14)"))
    (pad 2 thru_hole oval (at 17.135 -2.54 270) (size 2 4) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 R_AUD))
    (pad 4 thru_hole oval (at 13.325 -2.54 270) (size 2 4) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 9.515 -2.54 270) (size 2 4) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 L_AUD))
    (pad e8 thru_hole oval (at 5.705 -2.54 270) (size 2 4) (drill 1.3) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 1.895 -2.54 270) (size 2 4) (drill 1.3) (layers *.Cu *.Mask)
      (net 10 "Net-(SCART1-Pad10)"))
    (pad 12 thru_hole oval (at -1.915 -2.54 270) (size 2 4) (drill 1.3) (layers *.Cu *.Mask)
      (net 11 "Net-(SCART1-Pad12)"))
    (pad 1 thru_hole oval (at 19.05 2.54 270) (size 2 4) (drill 1.3) (layers *.Cu *.Mask)
      (net 12 "Net-(SCART1-Pad1)"))
    (pad 3 thru_hole oval (at 15.24 2.54 270) (size 2 4) (drill 1.3) (layers *.Cu *.Mask)
      (net 13 "Net-(SCART1-Pad3)"))
    (pad 5 thru_hole oval (at 11.43 2.54 270) (size 2 4) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 7.62 2.54 270) (size 2 4) (drill 1.3) (layers *.Cu *.Mask)
      (net 7 BLUE))
    (pad 9 thru_hole oval (at 3.81 2.54 270) (size 2 4) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 21 thru_hole oval (at -19.05 2.54 270) (size 2 4) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 19 thru_hole oval (at -15.24 2.54 270) (size 2 4) (drill 1.3) (layers *.Cu *.Mask)
      (net 14 "Net-(SCART1-Pad19)"))
    (pad 17 thru_hole oval (at -11.43 2.54 270) (size 2 4) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 15 thru_hole oval (at -7.62 2.54 270) (size 2 4) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 RED))
    (pad 13 thru_hole oval (at -3.81 2.54 270) (size 2 4) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole oval (at 0 2.54 270) (size 2 4) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 GREEN))
    (pad "" np_thru_hole oval (at -22.4 0 270) (size 2 6.8) (drill oval 2 6.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole oval (at 22.4 0 270) (size 2 6.8) (drill oval 2 6.8) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5B19C1E6)
    (at 165.03175 128.40175)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference J1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad1)"))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5B19C1EA)
    (at 135.85825 128.40175)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference J2 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad1)"))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5B19C1DF)
    (at 165.03175 88.26025)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference J3 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask)
      (net 17 "Net-(J3-Pad1)"))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5B19C1F0)
    (at 135.85825 88.26025)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference J4 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask)
      (net 18 "Net-(J4-Pad1)"))
  )
  (gr_text tinkerplunk.com (at 135.85825 108.331 270) (layer F.SilkS))
  (gr_text v0.1 (at 171.0182 68.01104) (layer F.Cu))
  (gr_text "SCART to RCA" (at 165.03175 108.331 270) (layer F.SilkS))
  (gr_line (start 130.345 73.671) (end 130.345 76.671) (angle 90) (layer Edge.Cuts) (width 1.7))
  (gr_line (start 129.4765 134.6835) (end 129.4765 66.421) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 171.5135 66.421) (end 171.5135 134.6835) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 171.5135 134.6835) (end 129.4765 134.6835) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170.645 73.671) (end 170.645 76.671) (angle 90) (layer Edge.Cuts) (width 1.7))
  (gr_line (start 171.5135 66.421) (end 129.4765 66.421) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.095 130.731) (end 152.895 130.731) (angle 90) (layer Edge.Cuts) (width 2))
  (gr_line (start 148.095 85.931) (end 152.895 85.931) (angle 90) (layer Edge.Cuts) (width 2))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.6405 134.8105) (xy 129.3495 134.8105) (xy 129.3495 66.294) (xy 171.6405 66.294)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.6405 134.8105) (xy 129.3495 134.8105) (xy 129.3495 66.294) (xy 171.6405 66.294)
      )
    )
  )
)
