(kicad_pcb (version 4) (host pcbnew 4.0.2-1.fc23-product)
  (general
    (links 3)
    (no_connects 2)
    (area 25.908 69.342 78.740001 112.522001)
    (thickness 1.6002)
    (drawings 4)
    (tracks 2)
    (zones 0)
    (modules 4)
    (nets 3)
  )
  (page A4)
  (title_block
    (date "26 aug 2013")
  )
  (layers
    (0 Front signal)
    (31 Back signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.2032)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2032)
    (segment_width 0.381)
    (edge_width 0.381)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3048)
    (pcb_text_size 1.524 2.032)
    (mod_edge_width 0.381)
    (mod_text_size 1.524 1.524)
    (mod_text_width 0.3048)
    (pad_size 1.80086 1.80086)
    (pad_drill 0.8128)
    (pad_to_mask_clearance 0.254)
    (aux_axis_origin 0 0)
    (grid_origin 96.52 77.724)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions true)
      (excludeedgelayer false)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 0)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory SolderBadge/))
  )
  (net 0 "")
  (net 1 +3.3V)
  (net 2 GND)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.2032)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +3.3V)
    (add_net GND)
  )
  (module LED-5MM (layer Back) (tedit 521B22C0)
    (at 48.8188 104.22382)
    (descr "LED 5mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 5mm 5MM 100mil 2,54mm")
    (fp_text reference "" (at 0 3.81) (layer B.SilkS))
    (fp_text value "" (at 0 -3.81) (layer B.SilkS))
    (pad 1 thru_hole circle (at -1.27 0) (size 1.80086 1.80086) (drill 0.8128) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 1 +3.3V))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.80086 1.80086) (drill 0.8128) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 GND))
    (model discret/leds/led5_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module CR2032 (layer Back) (tedit 51B5F53C)
    (at 48.9204 89.42324 270)
    (fp_text reference "" (at 0 -8.99922 270) (layer B.SilkS))
    (fp_text value "" (at 0 -6.49986 270) (layer B.SilkS))
    (fp_text user "" (at 8.99922 0 270) (layer B.SilkS))
    (fp_text user "" (at -8.99922 0 270) (layer B.SilkS))
    (fp_text user "" (at 0 -4.0005 270) (layer B.SilkS))
    (pad 1 thru_hole circle (at -11.0617 0 270) (size 2.54 2.54) (drill 1.8542) (layers *.Cu *.Mask B.SilkS)
      (net 1 +3.3V))
    (pad 2 thru_hole circle (at 11.0617 0.0508 270) (size 2.54 2.54) (drill 1.8542) (layers *.Cu *.Mask B.SilkS)
      (net 1 +3.3V))
    (pad 3 smd rect (at 0 0 270) (size 5.08 5.08) (layers Back B.Paste B.Mask)
      (net 2 GND))
  )
  (module logo1p5inchFrontMask (layer Front) (tedit 515B2D15)
    (at 48.514 90.551)
    (fp_text reference "" (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS) hide)
  )
  (module PinHole (layer Front) (tedit 51B5F81B)
    (at 48.895 74.803)
    (fp_text reference "" (at 0 -2.49936) (layer F.SilkS))
    (fp_text value "" (at 0 2.49936) (layer F.SilkS))
    (pad 4 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.01092) (layers *.Cu *.Mask F.SilkS))
  )
  (gr_text "Short leg of LED should \npoke out here! -->" (at 56.1975 103.5685) (layer B.SilkS))
  (gr_text www.phenoptix.com (at 62.9285 90.297 90) (layer B.SilkS))
  (gr_circle (center 48.9204 90.62466) (end 46.61916 71.62546) (layer Edge.Cuts) (width 0.381))
  (gr_text "Learn to Solder!" (at 34.29 90.6145 90) (layer B.SilkS))
  (zone (net 2) (net_name GND) (layer Front) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.74 112.522) (xy 76.073 70.358) (xy 26.162 69.34708) (xy 26.162 69.342) (xy 25.908 69.342)
        (xy 26.162 69.34708) (xy 26.162 112.395)
      )
    )
  )
)
