<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="40.18" y1="2.53" x2="40.18" y2="49.87" width="0" layer="20"/>
<wire x1="40.18" y1="49.87" x2="37.64" y2="52.41" width="0" layer="20" curve="90"/>
<wire x1="37.64" y1="52.41" x2="2.54" y2="52.41" width="0" layer="20"/>
<wire x1="2.54" y1="52.41" x2="0" y2="49.87" width="0" layer="20" curve="90"/>
<wire x1="0" y1="49.87" x2="0" y2="2.53" width="0" layer="20"/>
<wire x1="0" y1="2.53" x2="2.54" y2="-0.01" width="0" layer="20" curve="90"/>
<wire x1="2.54" y1="-0.01" x2="37.64" y2="-0.01" width="0" layer="20"/>
<wire x1="37.64" y1="-0.01" x2="40.18" y2="2.53" width="0" layer="20" curve="90"/>
<text>TX</text>
<text>RX</text>
<text>RST</text>
<text>GND</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5~</text>
<text>6~</text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>RAW</text>
<text>GND</text>
<text>RST</text>
<text>VCC</text>
<text>A3</text>
<text>A2</text>
<text>A1</text>
<text>A0</text>
<text>13</text>
<text>12</text>
<text>11</text>
<text>I2C</text>
<text>5V IN</text>
<text>V</text>
<text>G</text>
<text>C</text>
<text>D</text>
<text>G</text>
<text>Rx</text>
<text>Tx</text>
<text>G</text>
<text>V</text>
<text>S</text>
<text>Serial</text>
<text>Digital</text>
<text>A4/D</text>
<text>A5/C</text>
<text>G</text>
<text>V</text>
<text>S</text>
<text>Digital</text>
<text>Analog</text>
<text>S</text>
<text>V</text>
<text>G</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>I2C Servo Breakout </text>
<text>G</text>
<text>OE</text>
<text>C</text>
<text>D</text>
<text>FlthyBreakOut v2.1</text>
<text>Ryan Sondgeroth, 2016</text>
<text>fllthymcnsty</text>
<text>10</text>
<text>11</text>
<text>12</text>
<text>13</text>
<text>A0</text>
<text>A1</text>
<text>A2</text>
<text>A3</text>
<text>+</text>
<text>-</text>
<text>S</text>
<text>V</text>
<text>G</text>
<text>S</text>
<text>V</text>
<text>G</text>
<text>S</text>
<text>V</text>
<text>G</text>
<text>10</text>
<text>A4/D</text>
<text>A5/C</text>
<text>Flthy</text>
<text>BreakOut v2.1</text>
<text>V</text>
<text>cc</text>
<text>V</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X12">
</package>
<package name="1X04">
</package>
<package name="1X02">
</package>
<package name="SCREWTERMINAL-5MM-2">
</package>
<package name="1X03">
</package>
<package name="1X08_ROUND">
</package>
<package name="1X06">
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2,8">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 2.8 mm with drill center</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LEFTIN" library="SparkFun-Connectors" package="1X12" value="M12PTH"/>
<element name="RIGHTIN" library="SparkFun-Connectors" package="1X12" value="M12PTH"/>
<element name="A4A5" library="SparkFun-Connectors" package="1X02" value=""/>
<element name="H1" library="holes" package="2,8" value="MOUNT-HOLE2.8"/>
<element name="H2" library="holes" package="2,8" value="MOUNT-HOLE2.8"/>
<element name="H3" library="holes" package="2,8" value="MOUNT-HOLE2.8"/>
<element name="H4" library="holes" package="2,8" value="MOUNT-HOLE2.8"/>
<element name="POWER" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="">
<attribute name="STOREFRONT_ID" value="PRT-08432"/>
</element>
<element name="I2C1" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="I2C2" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="SERIAL" library="SparkFun-Connectors" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="GROUND_LEFT" library="SparkFun-Connectors" package="1X08_ROUND" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="5V_LEFT1" library="SparkFun-Connectors" package="1X08_ROUND" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="DIGITAL_LEFT" library="SparkFun-Connectors" package="1X08_ROUND" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="GROUND_RIGHT_DIGITAL" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="5V_RIGHT_DIGITAL1" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="DIGITAL_RIGHT" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="5V_RIGHT_ANALOG" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="GROUND_RIGHT_ANALOG" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="ANALOG_RIGHT" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="SERVO" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="VALUE"/>
<attribute name="PROD_ID" value="CONN-08437"/>
</element>
<element name="A4A1" library="SparkFun-Connectors" package="1X02" value=""/>
</elements>
<signals>
<signal name="TX">
<contactref element="LEFTIN" pad="12"/>
</signal>
<signal name="RX">
<contactref element="LEFTIN" pad="11"/>
</signal>
<signal name="GND">
<contactref element="LEFTIN" pad="9"/>
<contactref element="RIGHTIN" pad="2"/>
<contactref element="POWER" pad="1"/>
<contactref element="GROUND_LEFT" pad="1"/>
<contactref element="GROUND_LEFT" pad="2"/>
<contactref element="GROUND_LEFT" pad="3"/>
<contactref element="GROUND_LEFT" pad="4"/>
<contactref element="GROUND_LEFT" pad="5"/>
<contactref element="GROUND_LEFT" pad="7"/>
<contactref element="GROUND_LEFT" pad="6"/>
<contactref element="GROUND_LEFT" pad="8"/>
<contactref element="GROUND_RIGHT_DIGITAL" pad="1"/>
<contactref element="GROUND_RIGHT_DIGITAL" pad="2"/>
<contactref element="GROUND_RIGHT_DIGITAL" pad="3"/>
<contactref element="GROUND_RIGHT_DIGITAL" pad="4"/>
<contactref element="GROUND_RIGHT_ANALOG" pad="1"/>
<contactref element="GROUND_RIGHT_ANALOG" pad="2"/>
<contactref element="GROUND_RIGHT_ANALOG" pad="3"/>
<contactref element="GROUND_RIGHT_ANALOG" pad="4"/>
<contactref element="SERVO" pad="1"/>
<contactref element="I2C1" pad="2"/>
<contactref element="I2C2" pad="2"/>
<contactref element="SERIAL" pad="3"/>
</signal>
<signal name="3">
<contactref element="LEFTIN" pad="7"/>
</signal>
<signal name="4">
<contactref element="LEFTIN" pad="6"/>
</signal>
<signal name="5">
<contactref element="LEFTIN" pad="5"/>
</signal>
<signal name="6">
<contactref element="LEFTIN" pad="4"/>
</signal>
<signal name="7">
<contactref element="LEFTIN" pad="3"/>
</signal>
<signal name="8">
<contactref element="LEFTIN" pad="2"/>
</signal>
<signal name="9">
<contactref element="LEFTIN" pad="1"/>
</signal>
<signal name="A3">
<contactref element="RIGHTIN" pad="5"/>
<contactref element="ANALOG_RIGHT" pad="4"/>
</signal>
<signal name="A2">
<contactref element="RIGHTIN" pad="6"/>
<contactref element="ANALOG_RIGHT" pad="3"/>
</signal>
<signal name="A1">
<contactref element="RIGHTIN" pad="7"/>
<contactref element="ANALOG_RIGHT" pad="2"/>
</signal>
<signal name="A0">
<contactref element="RIGHTIN" pad="8"/>
<contactref element="ANALOG_RIGHT" pad="1"/>
</signal>
<signal name="13">
<contactref element="RIGHTIN" pad="9"/>
<contactref element="DIGITAL_RIGHT" pad="4"/>
</signal>
<signal name="12">
<contactref element="RIGHTIN" pad="10"/>
<contactref element="DIGITAL_RIGHT" pad="3"/>
</signal>
<signal name="11">
<contactref element="RIGHTIN" pad="11"/>
<contactref element="DIGITAL_RIGHT" pad="2"/>
</signal>
<signal name="10">
<contactref element="RIGHTIN" pad="12"/>
<contactref element="DIGITAL_RIGHT" pad="1"/>
<contactref element="SERVO" pad="2"/>
</signal>
<signal name="A5SCL">
<contactref element="A4A5" pad="2"/>
<contactref element="SERVO" pad="3"/>
<contactref element="A4A1" pad="2"/>
</signal>
<signal name="A4SDA">
<contactref element="A4A5" pad="1"/>
<contactref element="SERVO" pad="4"/>
</signal>
<signal name="VIN">
<contactref element="POWER" pad="2"/>
<contactref element="RIGHTIN" pad="1"/>
<contactref element="5V_LEFT1" pad="1"/>
<contactref element="5V_LEFT1" pad="2"/>
<contactref element="5V_LEFT1" pad="3"/>
<contactref element="5V_LEFT1" pad="4"/>
<contactref element="5V_LEFT1" pad="5"/>
<contactref element="5V_LEFT1" pad="6"/>
<contactref element="5V_LEFT1" pad="7"/>
<contactref element="5V_LEFT1" pad="8"/>
<contactref element="5V_RIGHT_DIGITAL1" pad="1"/>
<contactref element="5V_RIGHT_DIGITAL1" pad="2"/>
<contactref element="5V_RIGHT_DIGITAL1" pad="3"/>
<contactref element="5V_RIGHT_DIGITAL1" pad="4"/>
<contactref element="5V_RIGHT_ANALOG" pad="1"/>
<contactref element="5V_RIGHT_ANALOG" pad="2"/>
<contactref element="5V_RIGHT_ANALOG" pad="3"/>
<contactref element="5V_RIGHT_ANALOG" pad="4"/>
<contactref element="SERVO" pad="5"/>
<contactref element="I2C1" pad="1"/>
<contactref element="I2C2" pad="1"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$2">
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
<signal name="2">
<contactref element="LEFTIN" pad="8"/>
</signal>
<signal name="N$5">
</signal>
</signals>
</board>
</drawing>
</eagle>
