(kicad_pcb (version 20171130) (host pcbnew 5.1.7-1.fc32)
  (general
    (thickness 1.6)
    (drawings 6)
    (tracks 19)
    (zones 0)
    (modules 3)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 140.208 60.706 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value PinHeader_1x05_P2.54mm_Vertical (at 0 12.49 90) (layer F.Fab))
    (fp_text user %R (at 0 5.08) (layer F.Fab))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5F68FEEE)
    (at 145.288 56.769 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference " " (at 0 1.43) (layer B.SilkS))
    (fp_text value C_0603_1608Metric (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:SOT-353 (layer F.Cu) (tedit 5D28A629)
    (at 145.288 56.769)
    (attr smd)
    (fp_text reference " " (at -0.025 -3.375) (layer F.SilkS))
    (fp_text value SOT-753 (at 0.35 4.025) (layer F.Fab))
    (fp_text user %R (at 0 0.1) (layer F.Fab))
    (pad 5 smd rect (at -0.95 -1.35) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.07))
    (pad 4 smd rect (at 0.95 -1.35) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.07))
    (pad 3 smd rect (at 0.95 1.35) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.07))
    (pad 2 smd rect (at 0 1.35) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.07))
    (pad 1 smd rect (at -0.95 1.35) (size 0.6 1.05) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.07))
  )
  (gr_line (start 138.811 59.436) (end 143.51 54.61) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 138.811 62.103) (end 138.811 59.436) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 151.765 62.103) (end 138.811 62.103) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 151.765 59.182) (end 151.765 62.103) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 147.066 54.61) (end 151.765 59.182) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 143.51 54.61) (end 147.066 54.61) (layer Edge.Cuts) (width 0.05))
)
