<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.6.0">
<drawing>
<board>
<plain>
<wire x1="24.13" y1="41.91" x2="2.54" y2="41.91" width="0.1524" layer="20"/>
<text>SCL</text>
<text>VIN</text>
<text>GND</text>
<text>SDA</text>
<text>INT</text>
<text>ANL</text>
<wire x1="2.54" y1="41.91" x2="2.54" y2="7.62" width="0.1524" layer="20"/>
<wire x1="2.54" y1="7.62" x2="24.13" y2="7.62" width="0.1524" layer="20"/>
<wire x1="24.13" y1="7.62" x2="24.13" y2="41.91" width="0.1524" layer="20"/>
<text>3.3v</text>
<text>5v</text>
<text>GMR
VexToUNO
V1.1</text>
<text>VIN to Ard</text>
<text>I2C</text>
<text>I2C</text>
<text>INT
10k</text>
</plain>
<libraries>
<library name="con-tycoelectronics">
<description>&lt;b&gt;Tyco Electronics Connector&lt;/b&gt;&lt;p&gt;
http://catalog.tycoelectronics.com&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="RJ11-NO_SHIELD">
<description>&lt;b&gt;RJ11 Low Profile&lt;/b&gt; No Shield&lt;/b&gt;&lt;p&gt;
For all RJ11 N and Z Series Models&lt;br&gt;
Source: www.tycoelectronics.com .. ENG_DS_1654001_1099_RJ_L_0507.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06_LOCK">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin with Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center, locking pins in place during soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02_LOCK">
<description>&lt;h3&gt;Plated Through Hole - Locking Footprint&lt;/h3&gt;
Holes are staggered by 0.005" from center to hold pins while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X05_LOCK">
<description>&lt;h3&gt;Plated Through Hole - 5 Pin with Locking Footprint&lt;/h3&gt;
Holes are offset 0.005" from center, locking pins in place during soldering.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03_LOCK">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin Locking Footprint&lt;/h3&gt;
Pins are staggered 0.005" off center to lock pins while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="con-tycoelectronics" package="RJ11-NO_SHIELD" value="RJ11-2L-B">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RJ11-2L-B"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="83F4463"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X06_LOCK" value=""/>
<element name="J3" library="SparkFun-Connectors" package="1X02_LOCK" value=""/>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="10k">
<attribute name="PROD_ID" value="RES-12183"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X06_LOCK" value=""/>
<element name="J5" library="SparkFun-Connectors" package="1X05_LOCK" value=""/>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3" value="I2C">
<attribute name="PROD_ID" value="RES-12183"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="AXIAL-0.3" value="I2C">
<attribute name="PROD_ID" value="RES-12183"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="1X03_LOCK" value=""/>
</elements>
<signals>
<signal name="INT">
<contactref element="R1" pad="P$2"/>
<contactref element="J2" pad="2"/>
<contactref element="J4" pad="4"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="VIN">
<contactref element="J3" pad="2"/>
<contactref element="J2" pad="5"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="GND">
<contactref element="J2" pad="4"/>
<contactref element="J5" pad="3"/>
<contactref element="J5" pad="4"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="SDA">
<contactref element="J2" pad="3"/>
<contactref element="J4" pad="5"/>
<contactref element="R3" pad="P$1"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="SCL">
<contactref element="J2" pad="6"/>
<contactref element="J4" pad="6"/>
<contactref element="R2" pad="P$1"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="ANALOG">
<contactref element="J2" pad="1"/>
<contactref element="J4" pad="3"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="J5" pad="1"/>
<contactref element="R1" pad="P$1"/>
<contactref element="J6" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="J5" pad="5"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="J6" pad="2"/>
<contactref element="R3" pad="P$2"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="5V">
<contactref element="J5" pad="2"/>
<contactref element="J6" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
